# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2013 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 64-Bit
# Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition
# Date created = 10:48:12  February 22, 2015
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		FGPAmstrad_MiST_top_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "Cyclone III"
set_global_assignment -name DEVICE EP3C25E144C8
set_global_assignment -name TOP_LEVEL_ENTITY Amstrad
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "10:48:12  FEBRUARY 22, 2015"
set_global_assignment -name LAST_QUARTUS_VERSION 13.1
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 1

set_location_assignment PIN_7 -to LED
set_location_assignment PIN_54 -to CLOCK_27[0]
set_location_assignment PIN_55 -to CLOCK_27[1]
set_location_assignment PIN_144 -to VGA_R[5]
set_location_assignment PIN_143 -to VGA_R[4]
set_location_assignment PIN_142 -to VGA_R[3]
set_location_assignment PIN_141 -to VGA_R[2]
set_location_assignment PIN_137 -to VGA_R[1]
set_location_assignment PIN_135 -to VGA_R[0]
set_location_assignment PIN_133 -to VGA_B[5]
set_location_assignment PIN_132 -to VGA_B[4]
set_location_assignment PIN_125 -to VGA_B[3]
set_location_assignment PIN_121 -to VGA_B[2]
set_location_assignment PIN_120 -to VGA_B[1]
set_location_assignment PIN_115 -to VGA_B[0]
set_location_assignment PIN_114 -to VGA_G[5]
set_location_assignment PIN_113 -to VGA_G[4]
set_location_assignment PIN_112 -to VGA_G[3]
set_location_assignment PIN_111 -to VGA_G[2]
set_location_assignment PIN_110 -to VGA_G[1]
set_location_assignment PIN_106 -to VGA_G[0]
set_location_assignment PIN_136 -to VGA_VS
set_location_assignment PIN_119 -to VGA_HS
set_location_assignment PIN_65 -to AUDIO_L
set_location_assignment PIN_80 -to AUDIO_R
set_location_assignment PIN_46 -to UART_TX
set_location_assignment PIN_31 -to UART_RX
set_location_assignment PIN_105 -to SPI_DO
set_location_assignment PIN_88 -to SPI_DI
set_location_assignment PIN_126 -to SPI_SCK
set_location_assignment PIN_127 -to SPI_SS2
set_location_assignment PIN_91 -to SPI_SS3
set_location_assignment PIN_90 -to SPI_SS4
set_location_assignment PIN_13 -to CONF_DATA0

set_location_assignment PIN_49 -to SDRAM_A[0]
set_location_assignment PIN_44 -to SDRAM_A[1]
set_location_assignment PIN_42 -to SDRAM_A[2]
set_location_assignment PIN_39 -to SDRAM_A[3]
set_location_assignment PIN_4 -to SDRAM_A[4]
set_location_assignment PIN_6 -to SDRAM_A[5]
set_location_assignment PIN_8 -to SDRAM_A[6]
set_location_assignment PIN_10 -to SDRAM_A[7]
set_location_assignment PIN_11 -to SDRAM_A[8]
set_location_assignment PIN_28 -to SDRAM_A[9]
set_location_assignment PIN_50 -to SDRAM_A[10]
set_location_assignment PIN_30 -to SDRAM_A[11]
set_location_assignment PIN_32 -to SDRAM_A[12]
set_location_assignment PIN_83 -to SDRAM_DQ[0]
set_location_assignment PIN_79 -to SDRAM_DQ[1]
set_location_assignment PIN_77 -to SDRAM_DQ[2]
set_location_assignment PIN_76 -to SDRAM_DQ[3]
set_location_assignment PIN_72 -to SDRAM_DQ[4]
set_location_assignment PIN_71 -to SDRAM_DQ[5]
set_location_assignment PIN_69 -to SDRAM_DQ[6]
set_location_assignment PIN_68 -to SDRAM_DQ[7]
set_location_assignment PIN_86 -to SDRAM_DQ[8]
set_location_assignment PIN_87 -to SDRAM_DQ[9]
set_location_assignment PIN_98 -to SDRAM_DQ[10]
set_location_assignment PIN_99 -to SDRAM_DQ[11]
set_location_assignment PIN_100 -to SDRAM_DQ[12]
set_location_assignment PIN_101 -to SDRAM_DQ[13]
set_location_assignment PIN_103 -to SDRAM_DQ[14]
set_location_assignment PIN_104 -to SDRAM_DQ[15]
set_location_assignment PIN_58 -to SDRAM_BA[0]
set_location_assignment PIN_51 -to SDRAM_BA[1]
set_location_assignment PIN_85 -to SDRAM_DQMH
set_location_assignment PIN_67 -to SDRAM_DQML
set_location_assignment PIN_60 -to SDRAM_nRAS
set_location_assignment PIN_64 -to SDRAM_nCAS
set_location_assignment PIN_66 -to SDRAM_nWE
set_location_assignment PIN_59 -to SDRAM_nCS
set_location_assignment PIN_33 -to SDRAM_CKE
set_location_assignment PIN_43 -to SDRAM_CLK

set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[0]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[1]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[2]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[3]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[4]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[5]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[6]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[7]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[8]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[9]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[10]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[11]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[12]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[13]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[14]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[15]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[0]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[1]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[2]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[3]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[4]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[5]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[6]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[7]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[8]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[9]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[10]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[11]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[12]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_BA[0]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_BA[1]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQMH
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQML
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nRAS
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nCAS
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nWE
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nCS
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[0]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[1]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[2]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[3]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[4]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[5]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[6]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[7]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[8]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[9]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[10]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[11]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[12]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[13]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[14]
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[15]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[0]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[1]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[2]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[3]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[4]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[5]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[6]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[7]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[8]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[9]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[10]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[11]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[12]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[13]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[14]
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[15]
set_instance_assignment -name GLOBAL_SIGNAL "GLOBAL CLOCK" -to SDRAM_CLK
set_instance_assignment -name GLOBAL_SIGNAL "GLOBAL CLOCK" -to SPI_SCK
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[1]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[2]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[3]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[4]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to SDRAM_A[5]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[6]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[7]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[8]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[9]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[10]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[11]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[12]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[1]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[2]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[3]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[4]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[5]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[6]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[7]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[8]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[9]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[10]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[11]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[12]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[13]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[14]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[15]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_BA[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_BA[1]
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQMH
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQML
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nRAS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nCAS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nWE
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nCS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_CKE
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_CLK
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[5]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[4]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[3]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[2]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[1]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[5]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[4]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[3]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[2]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[1]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[0]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[5]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[4]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[3]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[2]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[1]
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[0]

set_location_assignment PLL_1 -to "pll:pll|altpll:altpll_component"

set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name POWER_PRESET_COOLING_SOLUTION "23 MM HEAT SINK WITH 200 LFPM AIRFLOW"
set_global_assignment -name POWER_BOARD_THERMAL_MODEL "NONE (CONSERVATIVE)"
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 144
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE 8
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF
set_global_assignment -name GENERATE_RBF_FILE ON
set_global_assignment -name CRC_ERROR_OPEN_DRAIN OFF
set_global_assignment -name CYCLONEII_RESERVE_NCEO_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_DATA0_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_DATA1_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_FLASH_NCE_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -rise
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -fall
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -rise
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -fall
set_global_assignment -name RESERVE_DCLK_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name CYCLONEIII_CONFIGURATION_SCHEME "PASSIVE SERIAL"
set_global_assignment -name FORCE_CONFIGURATION_VCCIO ON
set_global_assignment -name PHYSICAL_SYNTHESIS_EFFORT NORMAL
set_global_assignment -name CYCLONEII_OPTIMIZATION_TECHNIQUE SPEED
set_global_assignment -name SYNTH_TIMING_DRIVEN_SYNTHESIS ON
set_global_assignment -name OPTIMIZE_HOLD_TIMING "ALL PATHS"
set_global_assignment -name OPTIMIZE_MULTI_CORNER_TIMING ON
set_global_assignment -name FITTER_EFFORT "STANDARD FIT"
set_global_assignment -name SEED 1

set_global_assignment -name PRE_FLOW_SCRIPT_FILE "quartus_sh:build_id_verilog.tcl"
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD "3.3-V LVTTL"
set_global_assignment -name ENABLE_SIGNALTAP OFF
set_global_assignment -name USE_SIGNALTAP_FILE output_files/playcity.stp
set_global_assignment -name TIMEQUEST_MULTICORNER_ANALYSIS ON
set_global_assignment -name SMART_RECOMPILE ON
set_instance_assignment -name CURRENT_STRENGTH_NEW 8MA -to VGA_HS
set_instance_assignment -name CURRENT_STRENGTH_NEW 8MA -to VGA_VS
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to UART_TX
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to AUDIO_L
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to AUDIO_R
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to LED
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to SPI_DO
set_global_assignment -name QIP_FILE pll.qip
set_global_assignment -name QIP_FILE "mist-modules/mist.qip"
set_global_assignment -name VERILOG_FILE sigma_delta_dac.v
set_global_assignment -name QIP_FILE T80/T80.qip
set_global_assignment -name SYSTEMVERILOG_FILE GA40010/ga40010.sv
set_global_assignment -name VERILOG_FILE GA40010/syncgen_sync.v
set_global_assignment -name VERILOG_FILE GA40010/casgen_sync.v
set_global_assignment -name SYSTEMVERILOG_FILE GA40010/video.sv
set_global_assignment -name VERILOG_FILE GA40010/rslatch.v
set_global_assignment -name VERILOG_FILE crt_filter.v
set_global_assignment -name SYSTEMVERILOG_FILE u765/u765.sv
set_global_assignment -name VERILOG_FILE sdram.v
set_global_assignment -name VERILOG_FILE i8255.v
set_global_assignment -name SYSTEMVERILOG_FILE color_mix.sv
set_global_assignment -name SYSTEMVERILOG_FILE hid.sv
set_global_assignment -name VERILOG_FILE multiplay_mouse.v
set_global_assignment -name VERILOG_FILE symbiface_mouse.v
set_global_assignment -name VERILOG_FILE kempston_mouse.v
set_global_assignment -name VERILOG_FILE UM6845R.v
set_global_assignment -name VHDL_FILE YM2149.vhd
set_global_assignment -name VHDL_FILE vol_table_array.vhd
set_global_assignment -name VERILOG_FILE Amstrad_MMU.v
set_global_assignment -name VERILOG_FILE Amstrad_motherboard.v
set_global_assignment -name SYSTEMVERILOG_FILE Amstrad.sv
set_global_assignment -name VHDL_FILE tzxplayer.vhd
set_global_assignment -name VHDL_FILE playcity/playcity.vhd
set_global_assignment -name QIP_FILE playcity/Z80CTC/z80ctc.qip
set_global_assignment -name SDC_FILE Amstrad.sdc
set_global_assignment -name SIGNALTAP_FILE output_files/newga.stp
set_global_assignment -name SIGNALTAP_FILE output_files/cpu.stp
set_global_assignment -name SIGNALTAP_FILE output_files/tzxplayer.stp
set_global_assignment -name SIGNALTAP_FILE output_files/playcity.stp
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top