Par Statistics
Total Non-vccgnd Signals=3005
Total Non-vccgnd Design Pins=11992
Total Non-vccgnd Conns=11992
Total Non-vccgnd Timing Constrained Conns=10739
Phase 1 CPU=3.8 sec
Phase 2 CPU=4.2 sec
Phase 3 CPU=8.1 sec
Phase 4 CPU=8.7 sec
Phase 5 CPU=14.0 sec
Phase 6 CPU=14.9 sec
Phase 7 CPU=14.9 sec
Phase 8 CPU=14.9 sec
Phase 9 CPU=15.1 sec
Phase 10 CPU=15.6 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=3.5
AvgWirelenPerPin Fanout 3=3.0
AvgWirelenPerPin Fanout 4=3.3
AvgWirelenPerPin Fanout 10=3.9
AvgWirelenPerPin Fanout 50=3.3
AvgWirelenPerPin Fanout 100=9.1
AvgWirelenPerPin Fanout 500=4.6
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=5.6092