### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:14.7 (WebPack) - P.20131013 | Target Family: | Spartan6
OS Platform: | NT64 | Target Device: | xc6slx16
Project ID (random number) | c5a995aa41e44200b6a177fef6de0406.A73A51172A9E43BA938CDC039F678210.10 | Target Package: | csg324
Registration ID | 211059439_0_0_754 | Target Speed: | -2
Date Generated | 2019-03-04T20:17:22 | Tool Flow | ISE

User Environment
OS Name | Microsoft Windows 7 , 64-bit | OS Release | major release (build 7600)
CPU Name | Intel(R) Core(TM) i7-6700 CPU @ 3.40GHz | CPU Speed | 3408 MHz
OS Name | Microsoft Windows 7 , 64-bit | OS Release | major release (build 7600)
CPU Name | Intel(R) Core(TM) i7-6700 CPU @ 3.40GHz | CPU Speed | 3408 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Accumulators=5

- 4-bit updown loadable accumulator=3
- 7-bit up accumulator=1
- 8-bit down loadable accumulator=1

Adder Trees=6

- 4-bit / 4-inputs adder tree=6

Adders/Subtractors=112

- 10-bit subtractor=1
- 11-bit adder=3
- 12-bit adder=3
- 12-bit subtractor=1
- 14-bit adder=2
- 16-bit adder=3
- 17-bit adder=4
- 18-bit adder=1
- 26-bit adder carry in=52
- 33-bit subtractor=1
- 4-bit adder=12
- 4-bit subtractor=8
- 5-bit adder=5
- 5-bit subtractor=1
- 6-bit adder=1
- 6-bit subtractor=1
- 7-bit adder=1
- 8-bit adder=3
- 8-bit addsub=1
- 8-bit subtractor=4
- 9-bit adder=1
- 9-bit adder carry in=3

Comparators=100

- 1-bit comparator equal=1
- 10-bit comparator greater=6
- 10-bit comparator lessequal=4
- 15-bit comparator equal=1
- 16-bit comparator greater=2
- 16-bit comparator lessequal=4
- 17-bit comparator greater=2
- 26-bit comparator lessequal=32
- 27-bit comparator lessequal=2
- 28-bit comparator lessequal=2
- 29-bit comparator lessequal=2
- 3-bit comparator equal=5
- 30-bit comparator lessequal=2
- 31-bit comparator lessequal=2
- 32-bit comparator lessequal=2
- 33-bit comparator lessequal=2
- 34-bit comparator lessequal=2
- 35-bit comparator lessequal=2
- 36-bit comparator lessequal=2
- 37-bit comparator lessequal=2
- 4-bit comparator equal=1
- 4-bit comparator greater=3
- 5-bit comparator equal=2
- 5-bit comparator greater=6
- 8-bit comparator greater=5
- 8-bit comparator lessequal=2
- 9-bit comparator equal=1
- 9-bit comparator greater=1

Counters=32

- 10-bit up counter=4
- 12-bit up counter=2
- 16-bit up counter=3
- 2-bit up counter=1
- 3-bit up counter=4
- 4-bit down counter=1
- 4-bit up counter=5
- 5-bit up counter=3
- 5-bit updown counter=1
- 8-bit up counter=4
- 9-bit up counter=4

FSMs=11 Logic shifters=1

- 24-bit shifter logical left=1

MACs=2

- 8x8-to-15-bit MAC=2

Multiplexers=2323

- 1-bit 2-to-1 multiplexer=1976
- 1-bit 20-to-1 multiplexer=1
- 1-bit 3-to-1 multiplexer=2
- 1-bit 4-to-1 multiplexer=25
- 1-bit 8-to-1 multiplexer=4
- 10-bit 2-to-1 multiplexer=28
- 11-bit 2-to-1 multiplexer=13
- 11-bit 7-to-1 multiplexer=1
- 12-bit 2-to-1 multiplexer=49
- 15-bit 7-to-1 multiplexer=1
- 16-bit 2-to-1 multiplexer=15
- 17-bit 2-to-1 multiplexer=4
- 2-bit 2-to-1 multiplexer=1
- 20-bit 2-to-1 multiplexer=2
- 21-bit 2-to-1 multiplexer=3
- 24-bit 2-to-1 multiplexer=3
- 26-bit 2-to-1 multiplexer=6
- 3-bit 4-to-1 multiplexer=1
- 32-bit 2-to-1 multiplexer=38
- 4-bit 2-to-1 multiplexer=37
- 5-bit 2-to-1 multiplexer=50
- 5-bit 4-to-1 multiplexer=1
- 6-bit 2-to-1 multiplexer=3
- 7-bit 2-to-1 multiplexer=2
- 8-bit 12-to-1 multiplexer=1
- 8-bit 2-to-1 multiplexer=34
- 8-bit 8-to-1 multiplexer=1
- 9-bit 14-to-1 multiplexer=1
- 9-bit 2-to-1 multiplexer=19
- 9-bit 8-to-1 multiplexer=1

Multipliers=1

- 32x32-bit multiplier=1

RAMs=15

- 128x8-bit single-port distributed RAM=1
- 16x1-bit single-port distributed Read Only RAM=1
- 16x12-bit single-port distributed Read Only RAM=1
- 16x2-bit single-port distributed Read Only RAM=1
- 16x32-bit dual-port distributed RAM=1
- 256x1-bit single-port distributed Read Only RAM=1
- 256x44-bit single-port block Read Only RAM=1
- 256x8-bit single-port distributed Read Only RAM=1
- 32x3-bit single-port distributed Read Only RAM=1
- 4096x32-bit dual-port block RAM=1
- 512x24-bit single-port block Read Only RAM=2
- 8192x1-bit single-port distributed Read Only RAM=1
- 8x1-bit single-port distributed Read Only RAM=1
- 8x8-bit single-port distributed Read Only RAM=1

Registers=2455

- Flip-Flops=2455

Xors=126

- 1-bit xor16=2
- 1-bit xor2=103
- 32-bit xor2=19
- 56-bit xor2=1
- 8-bit xor2=1

MiscellaneousStatistics

- AGG_BONDED_IO=119
- AGG_IO=119
- AGG_LOCED_IO=119
- AGG_SLICE=1115
- NUM_BONDED_IOB=111
- NUM_BONDED_IOBM=4
- NUM_BONDED_IOBS=4
- NUM_BSFULL=1333
- NUM_BSLUTONLY=1742
- NUM_BSREGONLY=299
- NUM_BSUSED=3374
- NUM_BUFG=8
- NUM_BUFIO2=2
- NUM_BUFIO2FB=2
- NUM_DCM=2
- NUM_DPRAM_O5ANDO6=20
- NUM_DPRAM_O6ONLY=4
- NUM_DSP48A1=5
- NUM_IOB_FF=4
- NUM_LOCED_IOB=111
- NUM_LOCED_IOBM=4
- NUM_LOCED_IOBS=4
- NUM_LOGIC_O5ANDO6=484
- NUM_LOGIC_O5ONLY=188
- NUM_LOGIC_O6ONLY=2303
- NUM_LUT_RT_DRIVES_CARRY4=21
- NUM_LUT_RT_DRIVES_FLOP=10
- NUM_LUT_RT_EXO5=10
- NUM_LUT_RT_EXO6=19
- NUM_LUT_RT_O5=6
- NUM_LUT_RT_O5ANDO6=2
- NUM_LUT_RT_O6=188
- NUM_OLOGIC2=4
- NUM_RAMB16BWER=26
- NUM_RAMB8BWER=2
- NUM_SLICEL=193
- NUM_SLICEM=19
- NUM_SLICEX=903
- NUM_SLICE_CARRY4=135
- NUM_SLICE_CONTROLSET=149
- NUM_SLICE_CYINIT=3838
- NUM_SLICE_F7MUX=67
- NUM_SLICE_FF=1748
- NUM_SLICE_LATCH=1
- NUM_SLICE_LATCHLOGIC=17
- NUM_SLICE_UNUSEDCTRL=465
- NUM_SPRAM_O6ONLY=16
- NUM_SRL_O5ANDO6=23
- NUM_SRL_O6ONLY=6
- NUM_UNUSABLE_FF_BELS=483
- Xilinx Core blk_mem_gen_v7_3, Xilinx CORE Generator 14.7=3

NetStatistics

- NumNets_Active=4534
- NumNets_Gnd=1
- NumNets_Vcc=1
- NumNodesOfType_Active_BOUNCEACROSS=104
- NumNodesOfType_Active_BOUNCEIN=694
- NumNodesOfType_Active_BUFGOUT=8
- NumNodesOfType_Active_BUFHINP2OUT=34
- NumNodesOfType_Active_BUFIOINP=4
- NumNodesOfType_Active_CLKPIN=651
- NumNodesOfType_Active_CLKPINFEED=67
- NumNodesOfType_Active_CNTRLPIN=483
- NumNodesOfType_Active_DOUBLE=7098
- NumNodesOfType_Active_GENERIC=109
- NumNodesOfType_Active_GLOBAL=288
- NumNodesOfType_Active_INPUT=1312
- NumNodesOfType_Active_IOBIN2OUT=84
- NumNodesOfType_Active_IOBINPUT=4
- NumNodesOfType_Active_IOBOUTPUT=84
- NumNodesOfType_Active_LUTINPUT=14552
- NumNodesOfType_Active_OUTBOUND=4572
- NumNodesOfType_Active_OUTPUT=4574
- NumNodesOfType_Active_PADINPUT=70
- NumNodesOfType_Active_PADOUTPUT=21
- NumNodesOfType_Active_PINBOUNCE=2771
- NumNodesOfType_Active_PINFEED=16359
- NumNodesOfType_Active_PINFEED1=4
- NumNodesOfType_Active_PINFEED2=10
- NumNodesOfType_Active_QUAD=3678
- NumNodesOfType_Active_REGINPUT=763
- NumNodesOfType_Active_SINGLE=8803
- NumNodesOfType_Gnd_BOUNCEACROSS=1
- NumNodesOfType_Gnd_BOUNCEIN=304
- NumNodesOfType_Gnd_CLKPIN=6
- NumNodesOfType_Gnd_CNTRLPIN=18
- NumNodesOfType_Gnd_DOUBLE=17
- NumNodesOfType_Gnd_GENERIC=21
- NumNodesOfType_Gnd_HGNDOUT=153
- NumNodesOfType_Gnd_INPUT=1947
- NumNodesOfType_Gnd_IOBIN2OUT=21
- NumNodesOfType_Gnd_IOBOUTPUT=21
- NumNodesOfType_Gnd_LUTINPUT=108
- NumNodesOfType_Gnd_OUTBOUND=37
- NumNodesOfType_Gnd_OUTPUT=44
- NumNodesOfType_Gnd_PADINPUT=21
- NumNodesOfType_Gnd_PINBOUNCE=596
- NumNodesOfType_Gnd_PINFEED=1879
- NumNodesOfType_Gnd_REGINPUT=12
- NumNodesOfType_Gnd_SINGLE=49
- NumNodesOfType_Vcc_CLKPIN=8
- NumNodesOfType_Vcc_CNTRLPIN=18
- NumNodesOfType_Vcc_GENERIC=9
- NumNodesOfType_Vcc_HVCCOUT=354
- NumNodesOfType_Vcc_INPUT=37
- NumNodesOfType_Vcc_IOBIN2OUT=9
- NumNodesOfType_Vcc_IOBOUTPUT=9
- NumNodesOfType_Vcc_KVCCOUT=35
- NumNodesOfType_Vcc_LUTINPUT=794
- NumNodesOfType_Vcc_PADINPUT=9
- NumNodesOfType_Vcc_PINBOUNCE=14
- NumNodesOfType_Vcc_PINFEED=852

SiteStatistics

- BUFG-BUFGMUX=8
- IOB-IOBM=48
- IOB-IOBS=63
- SLICEL-SLICEM=79
- SLICEX-SLICEL=180
- SLICEX-SLICEM=198

SiteSummary

- BUFG=8
- BUFG_BUFG=8
- BUFIO2=2
- BUFIO2FB=2
- BUFIO2FB_BUFIO2FB=2
- BUFIO2_BUFIO2=2
- CARRY4=135
- DCM=2
- DCM_DCM=2
- DSP48A1=5
- DSP48A1_DSP48A1=5
- FF_SR=158
- HARD0=26
- HARD1=14
- IOB=111
- IOBM=4
- IOBM_OUTBUF=4
- IOBS=4
- IOB_IMUX=35
- IOB_INBUF=35
- IOB_OUTBUF=84
- LUT5=688
- LUT6=2989
- LUT_OR_MEM5=45
- LUT_OR_MEM6=76
- NULLMUX=4
- OLOGIC2=4
- OLOGIC2_OUTFF=4
- PAD=119
- PULL_OR_KEEP1=25
- RAMB16BWER=26
- RAMB16BWER_RAMB16BWER=26
- RAMB8BWER=2
- RAMB8BWER_RAMB8BWER=2
- REG_SR=1608
- SELMUX2_1=67
- SLICEL=193
- SLICEM=19
- SLICEX=903

Configuration Data
BUFIO2FB_BUFIO2FB

- DIVIDE_BYPASS=[TRUE:2]
- INVERT_INPUTS=[FALSE:2]

BUFIO2_BUFIO2

- DIVIDE=[1:2]
- DIVIDE_BYPASS=[TRUE:2]
- I_INVERT=[FALSE:2]

DCM

- PSCLK=[PSCLK_INV:0] [PSCLK:2]
- PSEN=[PSEN_INV:0] [PSEN:2]
- PSINCDEC=[PSINCDEC:2] [PSINCDEC_INV:0]
- RST=[RST:2] [RST_INV:0]

DCM_DCM

- CLKDV_DIVIDE=[2.0:2]
- CLKIN_DIVIDE_BY_2=[FALSE:2]
- CLKOUT_PHASE_SHIFT=[NONE:2]
- CLK_FEEDBACK=[1X:2]
- DESKEW_ADJUST=[5:2]
- DFS_FREQUENCY_MODE=[LOW:2]
- DLL_FREQUENCY_MODE=[LOW:2]
- DSS_MODE=[NONE:2]
- DUTY_CYCLE_CORRECTION=[TRUE:2]
- PSCLK=[PSCLK_INV:0] [PSCLK:2]
- PSEN=[PSEN_INV:0] [PSEN:2]
- PSINCDEC=[PSINCDEC:2] [PSINCDEC_INV:0]
- RST=[RST:2] [RST_INV:0]
- STARTUP_WAIT=[FALSE:2]
- VERY_HIGH_FREQUENCY=[FALSE:2]

DSP48A1

- CEA=[CEA_INV:0] [CEA:5]
- CEB=[CEB_INV:0] [CEB:5]
- CEC=[CEC:5] [CEC_INV:0]
- CECARRYIN=[CECARRYIN_INV:0] [CECARRYIN:5]
- CED=[CED_INV:0] [CED:5]
- CEM=[CEM_INV:0] [CEM:5]
- CEOPMODE=[CEOPMODE_INV:0] [CEOPMODE:5]
- CEP=[CEP:5] [CEP_INV:0]
- CLK=[CLK:5] [CLK_INV:0]
- RSTA=[RSTA:5] [RSTA_INV:0]
- RSTB=[RSTB:5] [RSTB_INV:0]
- RSTC=[RSTC_INV:0] [RSTC:5]
- RSTCARRYIN=[RSTCARRYIN_INV:0] [RSTCARRYIN:5]
- RSTD=[RSTD_INV:0] [RSTD:5]
- RSTM=[RSTM:5] [RSTM_INV:0]
- RSTOPMODE=[RSTOPMODE_INV:0] [RSTOPMODE:5]
- RSTP=[RSTP_INV:0] [RSTP:5]

DSP48A1_DSP48A1

- A0REG=[0:5]
- A1REG=[0:5]
- B0REG=[0:5]
- B1REG=[0:5]
- B_INPUT=[CASCADE:1] [DIRECT:4]
- CARRYINREG=[0:5]
- CARRYINSEL=[OPMODE5:5]
- CARRYOUTREG=[0:5]
- CEA=[CEA_INV:0] [CEA:5]
- CEB=[CEB_INV:0] [CEB:5]
- CEC=[CEC:5] [CEC_INV:0]
- CECARRYIN=[CECARRYIN_INV:0] [CECARRYIN:5]
- CED=[CED_INV:0] [CED:5]
- CEM=[CEM_INV:0] [CEM:5]
- CEOPMODE=[CEOPMODE_INV:0] [CEOPMODE:5]
- CEP=[CEP:5] [CEP_INV:0]
- CLK=[CLK:5] [CLK_INV:0]
- CREG=[0:4] [1:1]
- DREG=[0:5]
- MREG=[0:5]
- OPMODEREG=[0:5]
- PREG=[0:5]
- RSTA=[RSTA:5] [RSTA_INV:0]
- RSTB=[RSTB:5] [RSTB_INV:0]
- RSTC=[RSTC_INV:0] [RSTC:5]
- RSTCARRYIN=[RSTCARRYIN_INV:0] [RSTCARRYIN:5]
- RSTD=[RSTD_INV:0] [RSTD:5]
- RSTM=[RSTM:5] [RSTM_INV:0]
- RSTOPMODE=[RSTOPMODE_INV:0] [RSTOPMODE:5]
- RSTP=[RSTP_INV:0] [RSTP:5]
- RSTTYPE=[SYNC:5]

FF_SR

- CK=[CK:149] [CK_INV:9]
- SRINIT=[SRINIT0:142] [SRINIT1:16]
- SYNC_ATTR=[ASYNC:144] [SYNC:14]

IOBM_OUTBUF

- SUSPEND=[3STATE:4]

IOB_OUTBUF

- DRIVEATTRBOX=[8:8] [12:74] [16:2]
- SLEW=[SLOW:84]
- SUSPEND=[3STATE:84]

LUT_OR_MEM5

- CLK=[CLK:43] [CLK_INV:0]
- LUT_OR_MEM=[LUT:2] [RAM:43]
- RAMMODE=[SRL16:23] [DPRAM32:20]

LUT_OR_MEM6

- CLK=[CLK:53] [CLK_INV:16]
- LUT_OR_MEM=[LUT:7] [RAM:69]
- RAMMODE=[SPRAM64:16] [SRL16:29] [DPRAM32:20] [DPRAM64:4]

OLOGIC2

- CLK0=[CLK0_INV:0] [CLK0:4]
- CLK1=[CLK1:4] [CLK1_INV:0]

OLOGIC2_OUTFF

- CK0=[CK0_INV:0] [CK0:4]
- CK1=[CK1_INV:0] [CK1:4]
- DDR_ALIGNMENT=[C0:4]
- OUTFFTYPE=[DDR:4]
- SRINIT_OQ=[0:4]
- SRTYPE_OQ=[ASYNC:4]

PULL_OR_KEEP1

- PULLTYPE=[PULLUP:25]

RAMB16BWER

- CLKA=[CLKA_INV:0] [CLKA:26]
- CLKB=[CLKB_INV:0] [CLKB:24]
- ENA=[ENA_INV:8] [ENA:18]
- ENB=[ENB_INV:7] [ENB:17]
- REGCEA=[REGCEA_INV:0] [REGCEA:26]
- REGCEB=[REGCEB_INV:0] [REGCEB:24]
- RSTA=[RSTA:26] [RSTA_INV:0]
- RSTB=[RSTB:24] [RSTB_INV:0]
- WEA0=[WEA0:26] [WEA0_INV:0]
- WEA1=[WEA1:26] [WEA1_INV:0]
- WEA2=[WEA2:26] [WEA2_INV:0]
- WEA3=[WEA3_INV:0] [WEA3:26]
- WEB0=[WEB0:24] [WEB0_INV:0]
- WEB1=[WEB1:24] [WEB1_INV:0]
- WEB2=[WEB2_INV:0] [WEB2:24]
- WEB3=[WEB3:24] [WEB3_INV:0]

RAMB16BWER_RAMB16BWER

- CLKA=[CLKA_INV:0] [CLKA:26]
- CLKB=[CLKB_INV:0] [CLKB:24]
- DATA_WIDTH_A=[1:14] [4:10] [36:2]
- DATA_WIDTH_B=[0:2] [1:14] [4:10]
- DOA_REG=[0:26]
- DOB_REG=[0:26]
- ENA=[ENA_INV:8] [ENA:18]
- ENB=[ENB_INV:7] [ENB:17]
- EN_RSTRAM_A=[FALSE:16] [TRUE:10]
- EN_RSTRAM_B=[FALSE:16] [TRUE:10]
- RAM_MODE=[TDP:26]
- REGCEA=[REGCEA_INV:0] [REGCEA:26]
- REGCEB=[REGCEB_INV:0] [REGCEB:24]
- RSTA=[RSTA:26] [RSTA_INV:0]
- RSTB=[RSTB:24] [RSTB_INV:0]
- RSTTYPE=[SYNC:26]
- RST_PRIORITY_A=[CE:26]
- RST_PRIORITY_B=[CE:26]
- WEA0=[WEA0:26] [WEA0_INV:0]
- WEA1=[WEA1:26] [WEA1_INV:0]
- WEA2=[WEA2:26] [WEA2_INV:0]
- WEA3=[WEA3_INV:0] [WEA3:26]
- WEB0=[WEB0:24] [WEB0_INV:0]
- WEB1=[WEB1:24] [WEB1_INV:0]
- WEB2=[WEB2_INV:0] [WEB2:24]
- WEB3=[WEB3:24] [WEB3_INV:0]
- WRITE_MODE_A=[WRITE_FIRST:26]
- WRITE_MODE_B=[WRITE_FIRST:12] [READ_FIRST:14]

RAMB8BWER

- CLKAWRCLK=[CLKAWRCLK:2] [CLKAWRCLK_INV:0]
- CLKBRDCLK=[CLKBRDCLK_INV:0] [CLKBRDCLK:1]
- ENAWREN=[ENAWREN:1] [ENAWREN_INV:1]
- ENBRDEN=[ENBRDEN_INV:0] [ENBRDEN:1]
- REGCEA=[REGCEA_INV:0] [REGCEA:2]
- REGCEBREGCE=[REGCEBREGCE_INV:0] [REGCEBREGCE:1]
- RSTA=[RSTA:2] [RSTA_INV:0]
- RSTBRST=[RSTBRST:1] [RSTBRST_INV:0]
- WEAWEL0=[WEAWEL0:2] [WEAWEL0_INV:0]
- WEAWEL1=[WEAWEL1_INV:0] [WEAWEL1:2]
- WEBWEU0=[WEBWEU0:1] [WEBWEU0_INV:0]
- WEBWEU1=[WEBWEU1:1] [WEBWEU1_INV:0]

RAMB8BWER_RAMB8BWER

- CLKAWRCLK=[CLKAWRCLK:2] [CLKAWRCLK_INV:0]
- CLKBRDCLK=[CLKBRDCLK_INV:0] [CLKBRDCLK:1]
- DATA_WIDTH_A=[9:1] [18:1]
- DATA_WIDTH_B=[0:1] [18:1]
- DOA_REG=[0:2]
- DOB_REG=[0:2]
- ENAWREN=[ENAWREN:1] [ENAWREN_INV:1]
- ENBRDEN=[ENBRDEN_INV:0] [ENBRDEN:1]
- EN_RSTRAM_A=[FALSE:1] [TRUE:1]
- EN_RSTRAM_B=[FALSE:1] [TRUE:1]
- RAM_MODE=[TDP:2]
- REGCEA=[REGCEA_INV:0] [REGCEA:2]
- REGCEBREGCE=[REGCEBREGCE_INV:0] [REGCEBREGCE:1]
- RSTA=[RSTA:2] [RSTA_INV:0]
- RSTBRST=[RSTBRST:1] [RSTBRST_INV:0]
- RSTTYPE=[SYNC:2]
- RST_PRIORITY_A=[CE:2]
- RST_PRIORITY_B=[CE:2]
- WEAWEL0=[WEAWEL0:2] [WEAWEL0_INV:0]
- WEAWEL1=[WEAWEL1_INV:0] [WEAWEL1:2]
- WEBWEU0=[WEBWEU0:1] [WEBWEU0_INV:0]
- WEBWEU1=[WEBWEU1:1] [WEBWEU1_INV:0]
- WRITE_MODE_A=[WRITE_FIRST:2]
- WRITE_MODE_B=[WRITE_FIRST:2]

REG_SR

- CK=[CK:1439] [CK_INV:169]
- LATCH_OR_FF=[FF:1590] [LATCH:1] [AND2L:17]
- SRINIT=[SRINIT0:1582] [SRINIT1:26]
- SYNC_ATTR=[ASYNC:1367] [SYNC:241]

SLICEL

- CLK=[CLK:98] [CLK_INV:11]

SLICEM

- CLK=[CLK:15] [CLK_INV:4]

SLICEX

- CLK=[CLK:474] [CLK_INV:48]

Pin Data
BUFG

- I0=8
- O=8

BUFG_BUFG

- I0=8
- O=8

BUFIO2

- DIVCLK=2
- I=2

BUFIO2FB

- I=2
- O=2

BUFIO2FB_BUFIO2FB

- I=2
- O=2

BUFIO2_BUFIO2

- DIVCLK=2
- I=2

CARRY4

- CIN=90
- CO0=5
- CO3=95
- CYINIT=45
- DI0=127
- DI1=112
- DI2=109
- DI3=95
- O0=119
- O1=114
- O2=104
- O3=102
- S0=135
- S1=122
- S2=112
- S3=109

DCM

- CLK0=2
- CLKDV=1
- CLKFB=2
- CLKFX=2
- CLKFX180=1
- CLKIN=2
- PSCLK=2
- PSEN=2
- PSINCDEC=2
- RST=2

DCM_DCM

- CLK0=2
- CLKDV=1
- CLKFB=2
- CLKFX=2
- CLKFX180=1
- CLKIN=2
- PSCLK=2
- PSEN=2
- PSINCDEC=2
- RST=2

DSP48A1

- A0=5
- A1=5
- A10=5
- A11=5
- A12=5
- A13=5
- A14=5
- A15=5
- A16=5
- A17=5
- A2=5
- A3=5
- A4=5
- A5=5
- A6=5
- A7=5
- A8=5
- A9=5
- B0=5
- B1=5
- B10=5
- B11=5
- B12=5
- B13=5
- B14=5
- B15=5
- B16=5
- B17=5
- B2=5
- B3=5
- B4=5
- B5=5
- B6=5
- B7=5
- B8=5
- B9=5
- BCIN0=1
- BCIN1=1
- BCIN10=1
- BCIN11=1
- BCIN12=1
- BCIN13=1
- BCIN14=1
- BCIN15=1
- BCIN16=1
- BCIN17=1
- BCIN2=1
- BCIN3=1
- BCIN4=1
- BCIN5=1
- BCIN6=1
- BCIN7=1
- BCIN8=1
- BCIN9=1
- BCOUT0=1
- BCOUT1=1
- BCOUT10=1
- BCOUT11=1
- BCOUT12=1
- BCOUT13=1
- BCOUT14=1
- BCOUT15=1
- BCOUT16=1
- BCOUT17=1
- BCOUT2=1
- BCOUT3=1
- BCOUT4=1
- BCOUT5=1
- BCOUT6=1
- BCOUT7=1
- BCOUT8=1
- BCOUT9=1
- C0=5
- C1=5
- C10=5
- C11=5
- C12=5
- C13=5
- C14=5
- C15=5
- C16=5
- C17=5
- C18=5
- C19=5
- C2=5
- C20=5
- C21=5
- C22=5
- C23=5
- C24=5
- C25=5
- C26=5
- C27=5
- C28=5
- C29=5
- C3=5
- C30=5
- C31=5
- C32=5
- C33=5
- C34=5
- C35=5
- C36=5
- C37=5
- C38=5
- C39=5
- C4=5
- C40=5
- C41=5
- C42=5
- C43=5
- C44=5
- C45=5
- C46=5
- C47=5
- C5=5
- C6=5
- C7=5
- C8=5
- C9=5
- CEA=5
- CEB=5
- CEC=5
- CECARRYIN=5
- CED=5
- CEM=5
- CEOPMODE=5
- CEP=5
- CLK=5
- D0=5
- D1=5
- D10=5
- D11=5
- D12=5
- D13=5
- D14=5
- D15=5
- D16=5
- D17=5
- D2=5
- D3=5
- D4=5
- D5=5
- D6=5
- D7=5
- D8=5
- D9=5
- OPMODE0=5
- OPMODE1=5
- OPMODE2=5
- OPMODE3=5
- OPMODE4=5
- OPMODE5=5
- OPMODE6=5
- OPMODE7=5
- P0=4
- P1=4
- P10=4
- P11=4
- P12=4
- P13=4
- P14=4
- P15=1
- P16=1
- P17=1
- P18=1
- P19=1
- P2=4
- P20=1
- P21=1
- P22=1
- P23=1
- P24=1
- P25=1
- P26=1
- P27=1
- P28=1
- P29=1
- P3=4
- P30=1
- P31=1
- P32=1
- P33=1
- P34=1
- P35=1
- P36=1
- P37=1
- P38=1
- P39=1
- P4=4
- P40=1
- P41=1
- P42=1
- P43=1
- P44=1
- P45=1
- P46=1
- P47=1
- P5=4
- P6=4
- P7=4
- P8=4
- P9=4
- PCIN0=1
- PCIN1=1
- PCIN10=1
- PCIN11=1
- PCIN12=1
- PCIN13=1
- PCIN14=1
- PCIN15=1
- PCIN16=1
- PCIN17=1
- PCIN18=1
- PCIN19=1
- PCIN2=1
- PCIN20=1
- PCIN21=1
- PCIN22=1
- PCIN23=1
- PCIN24=1
- PCIN25=1
- PCIN26=1
- PCIN27=1
- PCIN28=1
- PCIN29=1
- PCIN3=1
- PCIN30=1
- PCIN31=1
- PCIN32=1
- PCIN33=1
- PCIN34=1
- PCIN35=1
- PCIN36=1
- PCIN37=1
- PCIN38=1
- PCIN39=1
- PCIN4=1
- PCIN40=1
- PCIN41=1
- PCIN42=1
- PCIN43=1
- PCIN44=1
- PCIN45=1
- PCIN46=1
- PCIN47=1
- PCIN5=1
- PCIN6=1
- PCIN7=1
- PCIN8=1
- PCIN9=1
- PCOUT0=1
- PCOUT1=1
- PCOUT10=1
- PCOUT11=1
- PCOUT12=1
- PCOUT13=1
- PCOUT14=1
- PCOUT15=1
- PCOUT16=1
- PCOUT17=1
- PCOUT18=1
- PCOUT19=1
- PCOUT2=1
- PCOUT20=1
- PCOUT21=1
- PCOUT22=1
- PCOUT23=1
- PCOUT24=1
- PCOUT25=1
- PCOUT26=1
- PCOUT27=1
- PCOUT28=1
- PCOUT29=1
- PCOUT3=1
- PCOUT30=1
- PCOUT31=1
- PCOUT32=1
- PCOUT33=1
- PCOUT34=1
- PCOUT35=1
- PCOUT36=1
- PCOUT37=1
- PCOUT38=1
- PCOUT39=1
- PCOUT4=1
- PCOUT40=1
- PCOUT41=1
- PCOUT42=1
- PCOUT43=1
- PCOUT44=1
- PCOUT45=1
- PCOUT46=1
- PCOUT47=1
- PCOUT5=1
- PCOUT6=1
- PCOUT7=1
- PCOUT8=1
- PCOUT9=1
- RSTA=5
- RSTB=5
- RSTC=5
- RSTCARRYIN=5
- RSTD=5
- RSTM=5
- RSTOPMODE=5
- RSTP=5

DSP48A1_DSP48A1

- A0=5
- A1=5
- A10=5
- A11=5
- A12=5
- A13=5
- A14=5
- A15=5
- A16=5
- A17=5
- A2=5
- A3=5
- A4=5
- A5=5
- A6=5
- A7=5
- A8=5
- A9=5
- B0=5
- B1=5
- B10=5
- B11=5
- B12=5
- B13=5
- B14=5
- B15=5
- B16=5
- B17=5
- B2=5
- B3=5
- B4=5
- B5=5
- B6=5
- B7=5
- B8=5
- B9=5
- BCIN0=1
- BCIN1=1
- BCIN10=1
- BCIN11=1
- BCIN12=1
- BCIN13=1
- BCIN14=1
- BCIN15=1
- BCIN16=1
- BCIN17=1
- BCIN2=1
- BCIN3=1
- BCIN4=1
- BCIN5=1
- BCIN6=1
- BCIN7=1
- BCIN8=1
- BCIN9=1
- BCOUT0=1
- BCOUT1=1
- BCOUT10=1
- BCOUT11=1
- BCOUT12=1
- BCOUT13=1
- BCOUT14=1
- BCOUT15=1
- BCOUT16=1
- BCOUT17=1
- BCOUT2=1
- BCOUT3=1
- BCOUT4=1
- BCOUT5=1
- BCOUT6=1
- BCOUT7=1
- BCOUT8=1
- BCOUT9=1
- C0=5
- C1=5
- C10=5
- C11=5
- C12=5
- C13=5
- C14=5
- C15=5
- C16=5
- C17=5
- C18=5
- C19=5
- C2=5
- C20=5
- C21=5
- C22=5
- C23=5
- C24=5
- C25=5
- C26=5
- C27=5
- C28=5
- C29=5
- C3=5
- C30=5
- C31=5
- C32=5
- C33=5
- C34=5
- C35=5
- C36=5
- C37=5
- C38=5
- C39=5
- C4=5
- C40=5
- C41=5
- C42=5
- C43=5
- C44=5
- C45=5
- C46=5
- C47=5
- C5=5
- C6=5
- C7=5
- C8=5
- C9=5
- CEA=5
- CEB=5
- CEC=5
- CECARRYIN=5
- CED=5
- CEM=5
- CEOPMODE=5
- CEP=5
- CLK=5
- D0=5
- D1=5
- D10=5
- D11=5
- D12=5
- D13=5
- D14=5
- D15=5
- D16=5
- D17=5
- D2=5
- D3=5
- D4=5
- D5=5
- D6=5
- D7=5
- D8=5
- D9=5
- OPMODE0=5
- OPMODE1=5
- OPMODE2=5
- OPMODE3=5
- OPMODE4=5
- OPMODE5=5
- OPMODE6=5
- OPMODE7=5
- P0=4
- P1=4
- P10=4
- P11=4
- P12=4
- P13=4
- P14=4
- P15=1
- P16=1
- P17=1
- P18=1
- P19=1
- P2=4
- P20=1
- P21=1
- P22=1
- P23=1
- P24=1
- P25=1
- P26=1
- P27=1
- P28=1
- P29=1
- P3=4
- P30=1
- P31=1
- P32=1
- P33=1
- P34=1
- P35=1
- P36=1
- P37=1
- P38=1
- P39=1
- P4=4
- P40=1
- P41=1
- P42=1
- P43=1
- P44=1
- P45=1
- P46=1
- P47=1
- P5=4
- P6=4
- P7=4
- P8=4
- P9=4
- PCIN0=1
- PCIN1=1
- PCIN10=1
- PCIN11=1
- PCIN12=1
- PCIN13=1
- PCIN14=1
- PCIN15=1
- PCIN16=1
- PCIN17=1
- PCIN18=1
- PCIN19=1
- PCIN2=1
- PCIN20=1
- PCIN21=1
- PCIN22=1
- PCIN23=1
- PCIN24=1
- PCIN25=1
- PCIN26=1
- PCIN27=1
- PCIN28=1
- PCIN29=1
- PCIN3=1
- PCIN30=1
- PCIN31=1
- PCIN32=1
- PCIN33=1
- PCIN34=1
- PCIN35=1
- PCIN36=1
- PCIN37=1
- PCIN38=1
- PCIN39=1
- PCIN4=1
- PCIN40=1
- PCIN41=1
- PCIN42=1
- PCIN43=1
- PCIN44=1
- PCIN45=1
- PCIN46=1
- PCIN47=1
- PCIN5=1
- PCIN6=1
- PCIN7=1
- PCIN8=1
- PCIN9=1
- PCOUT0=1
- PCOUT1=1
- PCOUT10=1
- PCOUT11=1
- PCOUT12=1
- PCOUT13=1
- PCOUT14=1
- PCOUT15=1
- PCOUT16=1
- PCOUT17=1
- PCOUT18=1
- PCOUT19=1
- PCOUT2=1
- PCOUT20=1
- PCOUT21=1
- PCOUT22=1
- PCOUT23=1
- PCOUT24=1
- PCOUT25=1
- PCOUT26=1
- PCOUT27=1
- PCOUT28=1
- PCOUT29=1
- PCOUT3=1
- PCOUT30=1
- PCOUT31=1
- PCOUT32=1
- PCOUT33=1
- PCOUT34=1
- PCOUT35=1
- PCOUT36=1
- PCOUT37=1
- PCOUT38=1
- PCOUT39=1
- PCOUT4=1
- PCOUT40=1
- PCOUT41=1
- PCOUT42=1
- PCOUT43=1
- PCOUT44=1
- PCOUT45=1
- PCOUT46=1
- PCOUT47=1
- PCOUT5=1
- PCOUT6=1
- PCOUT7=1
- PCOUT8=1
- PCOUT9=1
- RSTA=5
- RSTB=5
- RSTC=5
- RSTCARRYIN=5
- RSTD=5
- RSTM=5
- RSTOPMODE=5
- RSTP=5

FF_SR

- CE=107
- CK=158
- D=158
- Q=158
- SR=16

HARD0

- 0=26

HARD1

- 1=14

IOB

- I=35
- O=84
- PAD=111
- T=8

IOBM

- DIFFO_OUT=4
- O=4
- PAD=4

IOBM_OUTBUF

- IN=4
- OUT=4
- OUTN=4

IOBS

- DIFFO_IN=4
- PAD=4

IOB_IMUX

- I=35
- OUT=35

IOB_INBUF

- OUT=35
- PAD=35

IOB_OUTBUF

- IN=84
- OUT=84
- TRI=8

LUT5

- A1=234
- A2=289
- A3=347
- A4=317
- A5=309
- O5=688

LUT6

- A1=1548
- A2=2138
- A3=2434
- A4=2704
- A5=2822
- A6=2958
- O6=2989

LUT_OR_MEM5

- A1=44
- A2=44
- A3=44
- A4=45
- A5=45
- CLK=43
- DI1=43
- O5=45
- WA1=20
- WA2=20
- WA3=20
- WA4=20
- WA5=20
- WE=43

LUT_OR_MEM6

- A1=74
- A2=74
- A3=76
- A4=75
- A5=76
- A6=76
- CLK=69
- DI1=20
- DI2=49
- O6=69
- WA1=40
- WA2=40
- WA3=40
- WA4=40
- WA5=40
- WA6=40
- WA7=16
- WE=69

NULLMUX

- 0=4
- OUT=4

OLOGIC2

- CLK0=4
- CLK1=4
- D1=4
- D2=4
- OCE=4
- OQ=4
- SR=4

OLOGIC2_OUTFF

- CE=4
- CK0=4
- CK1=4
- D1=4
- D2=4
- Q=4
- SR=4

PAD

- PAD=119

PULL_OR_KEEP1

- PAD=25

RAMB16BWER

- ADDRA0=16
- ADDRA1=16
- ADDRA10=26
- ADDRA11=26
- ADDRA12=26
- ADDRA13=26
- ADDRA2=24
- ADDRA3=24
- ADDRA4=24
- ADDRA5=26
- ADDRA6=26
- ADDRA7=26
- ADDRA8=26
- ADDRA9=26
- ADDRB0=16
- ADDRB1=16
- ADDRB10=24
- ADDRB11=24
- ADDRB12=24
- ADDRB13=24
- ADDRB2=24
- ADDRB3=24
- ADDRB4=24
- ADDRB5=24
- ADDRB6=24
- ADDRB7=24
- ADDRB8=24
- ADDRB9=24
- CLKA=26
- CLKB=24
- DIA0=26
- DIA1=26
- DIA10=18
- DIA11=18
- DIA12=18
- DIA13=18
- DIA14=18
- DIA15=18
- DIA16=18
- DIA17=18
- DIA18=18
- DIA19=18
- DIA2=26
- DIA20=18
- DIA21=18
- DIA22=18
- DIA23=18
- DIA24=18
- DIA25=18
- DIA26=18
- DIA27=18
- DIA28=18
- DIA29=18
- DIA3=26
- DIA30=18
- DIA31=18
- DIA4=18
- DIA5=18
- DIA6=18
- DIA7=18
- DIA8=18
- DIA9=18
- DIB0=24
- DIB1=24
- DIB10=16
- DIB11=16
- DIB12=16
- DIB13=16
- DIB14=16
- DIB15=16
- DIB16=16
- DIB17=16
- DIB18=16
- DIB19=16
- DIB2=24
- DIB20=16
- DIB21=16
- DIB22=16
- DIB23=16
- DIB24=16
- DIB25=16
- DIB26=16
- DIB27=16
- DIB28=16
- DIB29=16
- DIB3=24
- DIB30=16
- DIB31=16
- DIB4=16
- DIB5=16
- DIB6=16
- DIB7=16
- DIB8=16
- DIB9=16
- DIPA0=18
- DIPA1=18
- DIPA2=18
- DIPA3=18
- DIPB0=16
- DIPB1=16
- DIPB2=16
- DIPB3=16
- DOA0=12
- DOA1=12
- DOA10=2
- DOA11=2
- DOA12=2
- DOA13=2
- DOA14=2
- DOA15=2
- DOA16=2
- DOA17=2
- DOA18=2
- DOA19=2
- DOA2=12
- DOA20=2
- DOA21=2
- DOA22=2
- DOA23=2
- DOA24=1
- DOA25=1
- DOA26=1
- DOA27=1
- DOA28=1
- DOA29=1
- DOA3=12
- DOA30=1
- DOA31=1
- DOA4=2
- DOA5=2
- DOA6=2
- DOA7=2
- DOA8=2
- DOA9=2
- DOB0=22
- DOB1=8
- DOB2=8
- DOB3=8
- DOPA0=1
- DOPA1=1
- DOPA2=1
- DOPA3=1
- ENA=26
- ENB=24
- REGCEA=26
- REGCEB=24
- RSTA=26
- RSTB=24
- WEA0=26
- WEA1=26
- WEA2=26
- WEA3=26
- WEB0=24
- WEB1=24
- WEB2=24
- WEB3=24

RAMB16BWER_RAMB16BWER

- ADDRA0=16
- ADDRA1=16
- ADDRA10=26
- ADDRA11=26
- ADDRA12=26
- ADDRA13=26
- ADDRA2=24
- ADDRA3=24
- ADDRA4=24
- ADDRA5=26
- ADDRA6=26
- ADDRA7=26
- ADDRA8=26
- ADDRA9=26
- ADDRB0=16
- ADDRB1=16
- ADDRB10=24
- ADDRB11=24
- ADDRB12=24
- ADDRB13=24
- ADDRB2=24
- ADDRB3=24
- ADDRB4=24
- ADDRB5=24
- ADDRB6=24
- ADDRB7=24
- ADDRB8=24
- ADDRB9=24
- CLKA=26
- CLKB=24
- DIA0=26
- DIA1=26
- DIA10=18
- DIA11=18
- DIA12=18
- DIA13=18
- DIA14=18
- DIA15=18
- DIA16=18
- DIA17=18
- DIA18=18
- DIA19=18
- DIA2=26
- DIA20=18
- DIA21=18
- DIA22=18
- DIA23=18
- DIA24=18
- DIA25=18
- DIA26=18
- DIA27=18
- DIA28=18
- DIA29=18
- DIA3=26
- DIA30=18
- DIA31=18
- DIA4=18
- DIA5=18
- DIA6=18
- DIA7=18
- DIA8=18
- DIA9=18
- DIB0=24
- DIB1=24
- DIB10=16
- DIB11=16
- DIB12=16
- DIB13=16
- DIB14=16
- DIB15=16
- DIB16=16
- DIB17=16
- DIB18=16
- DIB19=16
- DIB2=24
- DIB20=16
- DIB21=16
- DIB22=16
- DIB23=16
- DIB24=16
- DIB25=16
- DIB26=16
- DIB27=16
- DIB28=16
- DIB29=16
- DIB3=24
- DIB30=16
- DIB31=16
- DIB4=16
- DIB5=16
- DIB6=16
- DIB7=16
- DIB8=16
- DIB9=16
- DIPA0=18
- DIPA1=18
- DIPA2=18
- DIPA3=18
- DIPB0=16
- DIPB1=16
- DIPB2=16
- DIPB3=16
- DOA0=12
- DOA1=12
- DOA10=2
- DOA11=2
- DOA12=2
- DOA13=2
- DOA14=2
- DOA15=2
- DOA16=2
- DOA17=2
- DOA18=2
- DOA19=2
- DOA2=12
- DOA20=2
- DOA21=2
- DOA22=2
- DOA23=2
- DOA24=1
- DOA25=1
- DOA26=1
- DOA27=1
- DOA28=1
- DOA29=1
- DOA3=12
- DOA30=1
- DOA31=1
- DOA4=2
- DOA5=2
- DOA6=2
- DOA7=2
- DOA8=2
- DOA9=2
- DOB0=22
- DOB1=8
- DOB2=8
- DOB3=8
- DOPA0=1
- DOPA1=1
- DOPA2=1
- DOPA3=1
- ENA=26
- ENB=24
- REGCEA=26
- REGCEB=24
- RSTA=26
- RSTB=24
- WEA0=26
- WEA1=26
- WEA2=26
- WEA3=26
- WEB0=24
- WEB1=24
- WEB2=24
- WEB3=24

RAMB8BWER

- ADDRAWRADDR0=1
- ADDRAWRADDR1=1
- ADDRAWRADDR10=2
- ADDRAWRADDR11=2
- ADDRAWRADDR12=2
- ADDRAWRADDR2=1
- ADDRAWRADDR3=2
- ADDRAWRADDR4=2
- ADDRAWRADDR5=2
- ADDRAWRADDR6=2
- ADDRAWRADDR7=2
- ADDRAWRADDR8=2
- ADDRAWRADDR9=2
- ADDRBRDADDR0=1
- ADDRBRDADDR1=1
- ADDRBRDADDR10=1
- ADDRBRDADDR11=1
- ADDRBRDADDR12=1
- ADDRBRDADDR2=1
- ADDRBRDADDR3=1
- ADDRBRDADDR4=1
- ADDRBRDADDR5=1
- ADDRBRDADDR6=1
- ADDRBRDADDR7=1
- ADDRBRDADDR8=1
- ADDRBRDADDR9=1
- CLKAWRCLK=2
- CLKBRDCLK=1
- DIADI0=2
- DIADI1=2
- DIADI10=1
- DIADI11=1
- DIADI12=1
- DIADI13=1
- DIADI14=1
- DIADI15=1
- DIADI2=2
- DIADI3=2
- DIADI4=2
- DIADI5=2
- DIADI6=2
- DIADI7=2
- DIADI8=1
- DIADI9=1
- DIBDI0=1
- DIBDI1=1
- DIBDI10=1
- DIBDI11=1
- DIBDI12=1
- DIBDI13=1
- DIBDI14=1
- DIBDI15=1
- DIBDI2=1
- DIBDI3=1
- DIBDI4=1
- DIBDI5=1
- DIBDI6=1
- DIBDI7=1
- DIBDI8=1
- DIBDI9=1
- DIPADIP0=2
- DIPADIP1=1
- DIPBDIP0=1
- DIPBDIP1=1
- DOADO0=2
- DOADO1=2
- DOADO10=1
- DOADO2=2
- DOADO3=2
- DOADO4=1
- DOADO5=1
- DOADO6=1
- DOADO7=1
- DOADO8=1
- DOADO9=1
- DOBDO0=1
- DOBDO1=1
- DOBDO10=1
- DOBDO2=1
- DOBDO3=1
- DOBDO8=1
- DOBDO9=1
- ENAWREN=2
- ENBRDEN=1
- REGCEA=2
- REGCEBREGCE=1
- RSTA=2
- RSTBRST=1
- WEAWEL0=2
- WEAWEL1=2
- WEBWEU0=1
- WEBWEU1=1

RAMB8BWER_RAMB8BWER

- ADDRAWRADDR0=1
- ADDRAWRADDR1=1
- ADDRAWRADDR10=2
- ADDRAWRADDR11=2
- ADDRAWRADDR12=2
- ADDRAWRADDR2=1
- ADDRAWRADDR3=2
- ADDRAWRADDR4=2
- ADDRAWRADDR5=2
- ADDRAWRADDR6=2
- ADDRAWRADDR7=2
- ADDRAWRADDR8=2
- ADDRAWRADDR9=2
- ADDRBRDADDR0=1
- ADDRBRDADDR1=1
- ADDRBRDADDR10=1
- ADDRBRDADDR11=1
- ADDRBRDADDR12=1
- ADDRBRDADDR2=1
- ADDRBRDADDR3=1
- ADDRBRDADDR4=1
- ADDRBRDADDR5=1
- ADDRBRDADDR6=1
- ADDRBRDADDR7=1
- ADDRBRDADDR8=1
- ADDRBRDADDR9=1
- CLKAWRCLK=2
- CLKBRDCLK=1
- DIADI0=2
- DIADI1=2
- DIADI10=1
- DIADI11=1
- DIADI12=1
- DIADI13=1
- DIADI14=1
- DIADI15=1
- DIADI2=2
- DIADI3=2
- DIADI4=2
- DIADI5=2
- DIADI6=2
- DIADI7=2
- DIADI8=1
- DIADI9=1
- DIBDI0=1
- DIBDI1=1
- DIBDI10=1
- DIBDI11=1
- DIBDI12=1
- DIBDI13=1
- DIBDI14=1
- DIBDI15=1
- DIBDI2=1
- DIBDI3=1
- DIBDI4=1
- DIBDI5=1
- DIBDI6=1
- DIBDI7=1
- DIBDI8=1
- DIBDI9=1
- DIPADIP0=2
- DIPADIP1=1
- DIPBDIP0=1
- DIPBDIP1=1
- DOADO0=2
- DOADO1=2
- DOADO10=1
- DOADO2=2
- DOADO3=2
- DOADO4=1
- DOADO5=1
- DOADO6=1
- DOADO7=1
- DOADO8=1
- DOADO9=1
- DOBDO0=1
- DOBDO1=1
- DOBDO10=1
- DOBDO2=1
- DOBDO3=1
- DOBDO8=1
- DOBDO9=1
- ENAWREN=2
- ENBRDEN=1
- REGCEA=2
- REGCEBREGCE=1
- RSTA=2
- RSTBRST=1
- WEAWEL0=2
- WEAWEL1=2
- WEBWEU0=1
- WEBWEU1=1

REG_SR

- CE=1095
- CK=1608
- D=1608
- Q=1608
- SR=275

SELMUX2_1

- 0=67
- 1=67
- OUT=67
- S0=67

SLICEL

- A=31
- A1=36
- A2=47
- A3=74
- A4=111
- A5=136
- A6=170
- AMUX=73
- AQ=74
- AX=46
- B=44
- B1=29
- B2=44
- B3=64
- B4=105
- B5=129
- B6=161
- BMUX=69
- BQ=67
- BX=44
- C=4
- C1=41
- C2=71
- C3=90
- C4=121
- C5=144
- C6=172
- CE=53
- CIN=90
- CLK=109
- CMUX=91
- COUT=90
- CQ=89
- CX=99
- D=4
- D1=58
- D2=76
- D3=89
- D4=121
- D5=141
- D6=167
- DMUX=57
- DQ=62
- DX=40
- SR=45

SLICEM

- A=6
- A1=19
- A2=19
- A3=19
- A4=19
- A5=19
- A6=19
- AI=13
- AMUX=11
- AQ=13
- AX=15
- B=7
- B1=18
- B2=18
- B3=19
- B4=19
- B5=19
- B6=19
- BI=13
- BMUX=11
- BQ=8
- BX=14
- C=6
- C1=19
- C2=19
- C3=19
- C4=19
- C5=19
- C6=19
- CE=19
- CI=12
- CLK=19
- CMUX=11
- CQ=12
- CX=14
- D=2
- D1=18
- D2=18
- D3=19
- D4=19
- D5=19
- D6=19
- DI=11
- DMUX=12
- DQ=8
- DX=16
- WE=4

SLICEX

- A=470
- A1=471
- A2=635
- A3=675
- A4=704
- A5=715
- A6=716
- AMUX=60
- AQ=413
- AX=153
- B=436
- B1=417
- B2=542
- B3=585
- B4=602
- B5=613
- B6=611
- BMUX=115
- BQ=303
- BX=122
- C=280
- C1=345
- C2=440
- C3=467
- C4=480
- C5=483
- C6=485
- CE=325
- CLK=522
- CMUX=84
- CQ=320
- CX=111
- D=343
- D1=327
- D2=423
- D3=454
- D4=465
- D5=474
- D6=476
- DMUX=102
- DQ=239
- DX=101
- SR=63

Tool Usage
Command Line History

- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd
- xst -intstyle ise -ifn <ise_file>
- ngdbuild -intstyle ise -dd _ngo -sd <dname> -nt timestamp -uc <fname>.ucf -p xc6slx16-csg324-2 <fname>.ngc <fname>.ngd
- map -intstyle ise -p xc6slx16-csg324-2 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -r 4 -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf
- par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf
- trce -intstyle ise -v 3 -s 2 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf
- bitgen -intstyle ise -f <fname>.ut <fname>.ncd

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
XSLTProcess | 200 | 200 | 0 | 0 | 0 | 0 | 0
_impact | 310 | 250 | 0 | 0 | 0 | 0 | 0
bitgen | 821 | 811 | 0 | 0 | 0 | 0 | 0
cpldfit | 230 | 205 | 0 | 0 | 0 | 0 | 0
hprep6 | 144 | 144 | 0 | 0 | 0 | 0 | 0
map | 844 | 816 | 0 | 0 | 0 | 0 | 0
ngcbuild | 13 | 13 | 0 | 0 | 0 | 0 | 0
ngdbuild | 1101 | 1096 | 0 | 0 | 0 | 0 | 0
obngc | 4 | 4 | 0 | 0 | 0 | 0 | 0
par | 820 | 813 | 0 | 0 | 0 | 0 | 0
taengine | 209 | 208 | 0 | 0 | 0 | 0 | 0
trce | 814 | 814 | 0 | 0 | 0 | 0 | 0
tsim | 161 | 161 | 0 | 0 | 0 | 0 | 0
xst | 1616 | 1595 | 0 | 0 | 0 | 0 | 0

Help Statistics
Search words with results
environment variable ( 1 )
Help files
/doc/usenglish/isehelp/dsm_c_design_summary_overview.htm ( 1 ) | /doc/usenglish/isehelp/ise_c_overview.htm ( 1 )
/doc/usenglish/isehelp/ise_r_environment_variables.htm ( 1 ) | /doc/usenglish/isehelp/ite_c_overview.htm ( 1 )
/doc/usenglish/isehelp/pim_c_overview.htm ( 1 ) | /doc/usenglish/isehelp/pp_p_process_manage_config_project_impact.htm ( 1 )

Project Statistics
PROP_Enable_Message_Filtering=false | PROP_FitterReportFormat=HTML
PROP_ImpactProjectFile=changed | PROP_LastAppliedGoal=Balanced
PROP_LastAppliedStrategy=Xilinx Default (unlocked) | PROP_ManualCompileOrderImp=false
PROP_PropSpecInProjFile=Store all values | PROP_Simulator=ISim (VHDL/Verilog)
PROP_SynthTopFile=changed | PROP_Top_Level_Module_Type=HDL
PROP_UseSmartGuide=false | PROP_UserConstraintEditorPreference=Text Editor
PROP_intProjectCreationTimestamp=2018-10-19T20:16:45 | PROP_intWbtProjectID=A73A51172A9E43BA938CDC039F678210
PROP_intWbtProjectIteration=10 | PROP_intWorkingDirLocWRTProjDir=Same
PROP_intWorkingDirUsed=No | PROP_xilxBitgStart_IntDone=true
PROP_AutoTop=true | PROP_DevFamily=Spartan6
PROP_DevDevice=xc6slx16 | PROP_DevFamilyPMName=spartan6
PROP_DevPackage=csg324 | PROP_Synthesis_Tool=XST (VHDL/Verilog)
PROP_DevSpeed=-2 | PROP_PreferredLanguage=VHDL
FILE_COREGEN=7 | FILE_UCF=1
FILE_VERILOG=1 | FILE_VHDL=32

Core Statistics
Core Type=blk_mem_gen_v7_3
c_addra_width=9 | c_addrb_width=9 | c_algorithm=1 | c_axi_id_width=4
c_axi_slave_type=0 | c_axi_type=1 | c_byte_size=9 | c_common_clk=0
c_default_data=0 | c_disable_warn_bhv_coll=0 | c_disable_warn_bhv_range=0 | c_elaboration_dir=masked_value
c_enable_32bit_address=0 | c_family=spartan6 | c_has_axi_id=0 | c_has_ena=0
c_has_enb=0 | c_has_injecterr=0 | c_has_mem_output_regs_a=0 | c_has_mem_output_regs_b=0
c_has_mux_output_regs_a=0 | c_has_mux_output_regs_b=0 | c_has_regcea=0 | c_has_regceb=0
c_has_rsta=0 | c_has_rstb=0 | c_has_softecc_input_regs_a=0 | c_has_softecc_output_regs_b=0
c_init_file=BlankString | c_init_file_name=no_coe_file_loaded | c_inita_val=0 | c_initb_val=0
c_interface_type=0 | c_load_init_file=0 | c_mem_type=2 | c_mux_pipeline_stages=0
c_prim_type=1 | c_read_depth_a=512 | c_read_depth_b=512 | c_read_width_a=7
c_read_width_b=7 | c_rst_priority_a=CE | c_rst_priority_b=CE | c_rst_type=SYNC
c_rstram_a=0 | c_rstram_b=0 | c_sim_collision_check=ALL | c_use_bram_block=0
c_use_byte_wea=0 | c_use_byte_web=0 | c_use_default_data=0 | c_use_ecc=0
c_use_softecc=0 | c_wea_width=1 | c_web_width=1 | c_write_depth_a=512
c_write_depth_b=512 | c_write_mode_a=WRITE_FIRST | c_write_mode_b=WRITE_FIRST | c_write_width_a=7
c_write_width_b=7 | c_xdevicefamily=spartan6
Core Type=blk_mem_gen_v7_3
c_addra_width=15 | c_addrb_width=15 | c_algorithm=1 | c_axi_id_width=4
c_axi_slave_type=0 | c_axi_type=1 | c_byte_size=9 | c_common_clk=1
c_default_data=0 | c_disable_warn_bhv_coll=0 | c_disable_warn_bhv_range=0 | c_elaboration_dir=masked_value
c_enable_32bit_address=0 | c_family=spartan6 | c_has_axi_id=0 | c_has_ena=0
c_has_enb=0 | c_has_injecterr=0 | c_has_mem_output_regs_a=0 | c_has_mem_output_regs_b=0
c_has_mux_output_regs_a=0 | c_has_mux_output_regs_b=0 | c_has_regcea=0 | c_has_regceb=0
c_has_rsta=0 | c_has_rstb=0 | c_has_softecc_input_regs_a=0 | c_has_softecc_output_regs_b=0
c_init_file=BlankString | c_init_file_name=no_coe_file_loaded | c_inita_val=0 | c_initb_val=0
c_interface_type=0 | c_load_init_file=0 | c_mem_type=2 | c_mux_pipeline_stages=0
c_prim_type=1 | c_read_depth_a=32768 | c_read_depth_b=32768 | c_read_width_a=8
c_read_width_b=8 | c_rst_priority_a=CE | c_rst_priority_b=CE | c_rst_type=SYNC
c_rstram_a=0 | c_rstram_b=0 | c_sim_collision_check=ALL | c_use_bram_block=0
c_use_byte_wea=0 | c_use_byte_web=0 | c_use_default_data=0 | c_use_ecc=0
c_use_softecc=0 | c_wea_width=1 | c_web_width=1 | c_write_depth_a=32768
c_write_depth_b=32768 | c_write_mode_a=WRITE_FIRST | c_write_mode_b=READ_FIRST | c_write_width_a=8
c_write_width_b=8 | c_xdevicefamily=spartan6
Core Type=blk_mem_gen_v7_3
c_addra_width=12 | c_addrb_width=12 | c_algorithm=1 | c_axi_id_width=4
c_axi_slave_type=0 | c_axi_type=1 | c_byte_size=9 | c_common_clk=0
c_default_data=0 | c_disable_warn_bhv_coll=0 | c_disable_warn_bhv_range=0 | c_elaboration_dir=masked_value
c_enable_32bit_address=0 | c_family=spartan6 | c_has_axi_id=0 | c_has_ena=0
c_has_enb=0 | c_has_injecterr=0 | c_has_mem_output_regs_a=0 | c_has_mem_output_regs_b=0
c_has_mux_output_regs_a=0 | c_has_mux_output_regs_b=0 | c_has_regcea=0 | c_has_regceb=0
c_has_rsta=0 | c_has_rstb=0 | c_has_softecc_input_regs_a=0 | c_has_softecc_output_regs_b=0
c_init_file=BlankString | c_init_file_name=fname.mif | c_inita_val=0 | c_initb_val=0
c_interface_type=0 | c_load_init_file=1 | c_mem_type=3 | c_mux_pipeline_stages=0
c_prim_type=1 | c_read_depth_a=4096 | c_read_depth_b=4096 | c_read_width_a=8
c_read_width_b=8 | c_rst_priority_a=CE | c_rst_priority_b=CE | c_rst_type=SYNC
c_rstram_a=0 | c_rstram_b=0 | c_sim_collision_check=ALL | c_use_bram_block=0
c_use_byte_wea=0 | c_use_byte_web=0 | c_use_default_data=0 | c_use_ecc=0
c_use_softecc=0 | c_wea_width=1 | c_web_width=1 | c_write_depth_a=4096
c_write_depth_b=4096 | c_write_mode_a=WRITE_FIRST | c_write_mode_b=WRITE_FIRST | c_write_width_a=8
c_write_width_b=8 | c_xdevicefamily=spartan6
Core Type=clk_wiz_v3_6
clkin1_period=20.0 | clkin2_period=20.0 | clock_mgr_type=AUTO | feedback_source=FDBK_AUTO
feedback_type=SINGLE | manual_override=false | num_out_clk=1 | primtype_sel=DCM_SP
use_clk_valid=false | use_dyn_phase_shift=false | use_dyn_reconfig=false | use_freeze=false
use_inclk_stopped=false | use_inclk_switchover=false | use_locked=false | use_max_i_jitter=false
use_min_o_jitter=false | use_phase_alignment=true | use_power_down=false | use_reset=false
use_status=false
Core Type=clk_wiz_v3_6
clkin1_period=20.0 | clkin2_period=20.0 | clock_mgr_type=AUTO | feedback_source=FDBK_AUTO
feedback_type=SINGLE | manual_override=false | num_out_clk=4 | primtype_sel=DCM_SP
use_clk_valid=false | use_dyn_phase_shift=false | use_dyn_reconfig=false | use_freeze=false
use_inclk_stopped=false | use_inclk_switchover=false | use_locked=false | use_max_i_jitter=false
use_min_o_jitter=false | use_phase_alignment=true | use_power_down=false | use_reset=false
use_status=false

Unisim Statistics
XST_UNISIM_SUMMARY
XST_NUM_BUFG=1 | XST_NUM_IBUFG=1 | XST_NUM_OBUFDS=4 | XST_NUM_ODDR2=4
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=8 | NGDBUILD_NUM_DCM_SP=2 | NGDBUILD_NUM_DSP48A1=5 | NGDBUILD_NUM_FD=336
NGDBUILD_NUM_FDC=1 | NGDBUILD_NUM_FDCE=19 | NGDBUILD_NUM_FDE=998 | NGDBUILD_NUM_FDE_1=144
NGDBUILD_NUM_FDPE=1 | NGDBUILD_NUM_FDR=137 | NGDBUILD_NUM_FDRE=132 | NGDBUILD_NUM_FDSE=4
NGDBUILD_NUM_FD_1=8 | NGDBUILD_NUM_GND=4 | NGDBUILD_NUM_IBUF=8 | NGDBUILD_NUM_IBUFG=1
NGDBUILD_NUM_INV=88 | NGDBUILD_NUM_IOBUF=8 | NGDBUILD_NUM_LDP=1 | NGDBUILD_NUM_LUT1=221
NGDBUILD_NUM_LUT2=274 | NGDBUILD_NUM_LUT3=327 | NGDBUILD_NUM_LUT4=388 | NGDBUILD_NUM_LUT5=667
NGDBUILD_NUM_LUT6=1476 | NGDBUILD_NUM_MUXCY=459 | NGDBUILD_NUM_MUXF7=59 | NGDBUILD_NUM_OBUF=76
NGDBUILD_NUM_OBUFDS=4 | NGDBUILD_NUM_ODDR2=4 | NGDBUILD_NUM_RAM128X1S=8 | NGDBUILD_NUM_RAM16X1D=2
NGDBUILD_NUM_RAM32M=5 | NGDBUILD_NUM_RAMB16BWER=29 | NGDBUILD_NUM_RAMB8BWER=2 | NGDBUILD_NUM_SRLC16E=52
NGDBUILD_NUM_VCC=4 | NGDBUILD_NUM_XORCY=456
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=8 | NGDBUILD_NUM_DCM_SP=2 | NGDBUILD_NUM_DSP48A1=5 | NGDBUILD_NUM_FD=336
NGDBUILD_NUM_FDC=1 | NGDBUILD_NUM_FDCE=19 | NGDBUILD_NUM_FDE=998 | NGDBUILD_NUM_FDE_1=144
NGDBUILD_NUM_FDPE=1 | NGDBUILD_NUM_FDR=137 | NGDBUILD_NUM_FDRE=132 | NGDBUILD_NUM_FDSE=4
NGDBUILD_NUM_FD_1=8 | NGDBUILD_NUM_GND=4 | NGDBUILD_NUM_IBUF=34 | NGDBUILD_NUM_IBUFG=1
NGDBUILD_NUM_INV=88 | NGDBUILD_NUM_LDP=1 | NGDBUILD_NUM_LUT1=221 | NGDBUILD_NUM_LUT2=274
NGDBUILD_NUM_LUT3=327 | NGDBUILD_NUM_LUT4=388 | NGDBUILD_NUM_LUT5=667 | NGDBUILD_NUM_LUT6=1476
NGDBUILD_NUM_MUXCY=459 | NGDBUILD_NUM_MUXF7=59 | NGDBUILD_NUM_OBUF=76 | NGDBUILD_NUM_OBUFDS=4
NGDBUILD_NUM_OBUFT=8 | NGDBUILD_NUM_ODDR2=4 | NGDBUILD_NUM_PULLUP=25 | NGDBUILD_NUM_RAM128X1S=8
NGDBUILD_NUM_RAM32M=5 | NGDBUILD_NUM_RAMB16BWER=29 | NGDBUILD_NUM_RAMB8BWER=2 | NGDBUILD_NUM_SRLC16E=52
NGDBUILD_NUM_TS_TIMESPEC=1 | NGDBUILD_NUM_VCC=4 | NGDBUILD_NUM_XORCY=456

XST Command Line Options
XST_OPTION_SUMMARY
-ifn=<fname>.prj | -ofn=<design_top> | -ofmt=NGC | -p=xc6slx16-2-csg324
-top=<design_top> | -opt_mode=Speed | -opt_level=1 | -power=NO
-iuc=NO | -keep_hierarchy=No | -netlist_hierarchy=As_Optimized | -rtlview=Yes
-glob_opt=AllClockNets | -read_cores=YES | -sd=<No customer specific name> | -write_timing_constraints=NO
-cross_clock_analysis=NO | -bus_delimiter=<> | -slice_utilization_ratio=100 | -bram_utilization_ratio=100
-dsp_utilization_ratio=100 | -reduce_control_sets=Auto | -fsm_extract=YES | -fsm_encoding=Auto
-safe_implementation=No | -fsm_style=LUT | -ram_extract=Yes | -ram_style=Auto
-rom_extract=Yes | -shreg_extract=YES | -rom_style=Auto | -auto_bram_packing=NO
-resource_sharing=YES | -async_to_sync=NO | -use_dsp48=Auto | -iobuf=YES
-max_fanout=100000 | -bufg=16 | -register_duplication=YES | -register_balancing=No
-optimize_primitives=NO | -use_clock_enable=Auto | -use_sync_set=Auto | -use_sync_reset=Auto
-iob=Auto | -equivalent_register_removal=YES | -slice_utilization_ratio_maxmargin=5