Par Statistics
Total Non-vccgnd Signals=5589
Total Non-vccgnd Design Pins=23770
Total Non-vccgnd Conns=23770
Total Non-vccgnd Timing Constrained Conns=17082
Phase 1 CPU=11.0 sec
Phase 2 CPU=13.6 sec
Phase 3 CPU=33.4 sec
Phase 4 CPU=43.3 sec
Phase 5 CPU=121.2 sec
Phase 6 CPU=168.9 sec
Phase 7 CPU=169.1 sec
Phase 8 CPU=169.1 sec
Phase 9 CPU=169.7 sec
Phase 10 CPU=172.1 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=2.0
AvgWirelenPerPin Fanout 3=3.0
AvgWirelenPerPin Fanout 4=3.5
AvgWirelenPerPin Fanout 10=3.7
AvgWirelenPerPin Fanout 50=3.0
AvgWirelenPerPin Fanout 100=6.0
AvgWirelenPerPin Fanout 500=3.1
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=9.3143