(kicad_sch (version 20211123) (generator eeschema)

  (uuid afd71847-b437-4031-a90c-b4d7b29147a0)

  (paper "A4")

  (title_block
    (title "Atari 2600 SD/TV Switch Breakout Board")
    (date "2022-06-21")
    (rev "C")
  )

  (lib_symbols
    (symbol "Connector:AudioJack4" (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 8.89 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "AudioJack4" (id 1) (at 0 6.35 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "audio jack receptacle stereo headphones TRRS connector" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Audio Jack, 4 Poles (TRRS)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Jack*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "AudioJack4_0_1"
        (rectangle (start -6.35 -5.08) (end -7.62 -7.62)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 -5.08)
            (xy 0.635 -5.715)
            (xy 1.27 -5.08)
            (xy 2.54 -5.08)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.715 -5.08)
            (xy -5.08 -5.715)
            (xy -4.445 -5.08)
            (xy -4.445 2.54)
            (xy 2.54 2.54)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -5.08)
            (xy -1.27 -5.715)
            (xy -0.635 -5.08)
            (xy -0.635 -2.54)
            (xy 2.54 -2.54)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy -2.54 0)
            (xy -2.54 -5.08)
            (xy -3.175 -5.715)
            (xy -3.81 -5.08)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 2.54 3.81) (end -6.35 -7.62)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "AudioJack4_1_1"
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "R1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "R2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 2.54 180) (length 2.54)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "S" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 -5.08 180) (length 2.54)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "T" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Connector:Conn_01x05_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Conn_01x05_Male" (id 1) (at 0 -7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "connector" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Conn_01x05_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 5.08)
            (xy 0.8636 5.08)
          )
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (rectangle (start 0.8636 5.207) (end 0 4.953)
          (stroke (width 0.1524) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_1" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_2" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_3" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_4" (effects (font (size 1.27 1.27))))
          (number "4" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_5" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:LED_Dual_AAK" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D1" (id 0) (at 8.89 1.27 90)
        (effects (font (size 1.27 1.27)) (justify right))
      )
      (property "Value" "LED_Dual_AAK_SOT" (id 1) (at 8.89 -1.27 90)
        (effects (font (size 1.27 1.27)) (justify right))
      )
      (property "Footprint" "LED_THT:LED_D3.0mm-3" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "LED diode bicolor dual" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Dual LED, common cathode on pin 3" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "LED_Dual_AAK_0_1"
        (circle (center -2.54 0) (radius 0.2794)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.572 0)
            (xy -2.54 0)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 -3.81)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 3.81)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 -2.54)
            (xy 1.905 -2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 2.54)
            (xy 1.905 2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -3.81)
            (xy 1.27 -1.27)
            (xy -1.27 -2.54)
            (xy 1.27 -3.81)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 3.81)
            (xy -1.27 2.54)
            (xy 1.27 1.27)
          )
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 2.54)
            (xy -2.54 2.54)
            (xy -2.54 -2.54)
            (xy 2.032 -2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 5.08)
            (xy 3.556 6.604)
            (xy 2.794 6.604)
            (xy 3.556 6.604)
            (xy 3.556 5.842)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 4.064)
            (xy 4.826 5.588)
            (xy 4.064 5.588)
            (xy 4.826 5.588)
            (xy 4.826 4.826)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (circle (center 0 0) (radius 4.572)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type background))
        )
      )
      (symbol "LED_Dual_AAK_1_1"
        (pin input line (at 7.62 -2.54 180) (length 3.81)
          (name "A2" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at 7.62 2.54 180) (length 3.81)
          (name "A1" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin input line (at -7.62 0 0) (length 3.048)
          (name "K" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:Q_NPN_BEC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "Q_NPN_BEC" (id 1) (at 5.08 -1.27 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 5.08 2.54 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "transistor NPN" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "NPN transistor, base/emitter/collector" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Q_NPN_BEC_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (stroke (width 0.508) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (stroke (width 0.254) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Q_NPN_BEC_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (stroke (width 0.2032) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Jumper:Jumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.794 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "Jumper_2_Open" (id 1) (at 0 -2.286 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Jumper SPST" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Jumper, 2-pole, open" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "Jumper_2_Open_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_0_1"
        (arc (start 1.524 1.27) (mid 0 1.778) (end -1.524 1.27)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "R_Small_1" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Value" "R_Small_1" (id 1) (at 0.762 -1.016 0)
        (effects (font (size 1.27 1.27)) (justify left))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "R_Small_1_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (stroke (width 0.2032) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
      )
    )
    (symbol "Switch:SW_SPDT" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 0 4.318 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "SW_SPDT" (id 1) (at 0 -5.08 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "" (id 2) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "~" (id 3) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "switch single-pole double-throw spdt ON-ON" (id 4) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "Switch, single pole double throw" (id 5) (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "SW_SPDT_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (circle (center 2.032 -2.54) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "SW_SPDT_0_1"
        (polyline
          (pts
            (xy -1.524 0.254)
            (xy 1.651 2.286)
          )
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
        (circle (center 2.032 2.54) (radius 0.508)
          (stroke (width 0) (type default) (color 0 0 0 0))
          (fill (type none))
        )
      )
      (symbol "SW_SPDT_1_1"
        (pin passive line (at 5.08 2.54 180) (length 2.54)
          (name "A" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "B" (effects (font (size 1.27 1.27))))
          (number "2" (effects (font (size 1.27 1.27))))
        )
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "C" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )

  (junction (at 186.69 102.87) (diameter 0) (color 0 0 0 0)
    (uuid 134fce8a-cb3d-4ac1-9efa-7579b0dbac4f)
  )
  (junction (at 149.86 85.09) (diameter 0) (color 0 0 0 0)
    (uuid 6046b781-8b69-4a92-a6a6-1ecfc3afc4ab)
  )
  (junction (at 137.16 92.71) (diameter 0) (color 0 0 0 0)
    (uuid 877d6103-fc1a-468b-aea8-c295d26223f0)
  )
  (junction (at 137.16 100.33) (diameter 0) (color 0 0 0 0)
    (uuid b581ad1f-10a4-4323-81de-a8d09d0a7e3e)
  )
  (junction (at 149.86 100.33) (diameter 0) (color 0 0 0 0)
    (uuid da2d85bd-f4c1-4c65-ba2a-22bee5eab07e)
  )
  (junction (at 170.18 85.09) (diameter 0) (color 0 0 0 0)
    (uuid e15f01b8-ac20-4b2e-981b-14d5e8aab0c8)
  )
  (junction (at 170.18 77.47) (diameter 0) (color 0 0 0 0)
    (uuid e1a2b355-15a4-4378-a82c-389d6c4cdeae)
  )
  (junction (at 173.99 105.41) (diameter 0) (color 0 0 0 0)
    (uuid ee5e0fce-4a14-42aa-a782-3cb9ae10b40f)
  )

  (wire (pts (xy 184.15 107.95) (xy 187.96 107.95))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 220b8307-c0d1-46e9-8244-d15d6b293c30)
  )
  (wire (pts (xy 125.73 97.79) (xy 125.73 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2c0433cc-760a-4636-be80-3cd80c3021f2)
  )
  (wire (pts (xy 173.99 105.41) (xy 187.96 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 2fba980a-4005-45a8-a6a1-109a7f9ed01a)
  )
  (wire (pts (xy 186.69 102.87) (xy 187.96 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 33ad21f6-dae6-49ba-934a-ab22663351b9)
  )
  (wire (pts (xy 170.18 80.01) (xy 177.8 80.01))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 380619a3-36ac-4019-90fa-003bd0dec0de)
  )
  (wire (pts (xy 186.69 100.33) (xy 186.69 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 3beca948-ff0e-4b01-8821-e697ba31e544)
  )
  (polyline (pts (xy 116.84 73.66) (xy 201.93 73.66))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4197380d-9b5e-43e5-9c3d-66af4251884d)
  )

  (wire (pts (xy 120.65 95.25) (xy 125.73 95.25))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 46903072-c0d0-4e25-b501-07217d6e9c55)
  )
  (wire (pts (xy 120.65 100.33) (xy 120.65 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4780cdc4-a85c-430f-b2bb-26cf8e9d7c09)
  )
  (wire (pts (xy 149.86 85.09) (xy 149.86 87.63))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4951ab01-45f3-4930-aa70-3496b6af10ed)
  )
  (wire (pts (xy 123.19 80.01) (xy 160.02 80.01))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4a48bc73-1ae6-4dc2-a076-a55215d94379)
  )
  (polyline (pts (xy 201.93 73.66) (xy 201.93 113.03))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 4e60d943-6f3d-4cd3-8ce3-3e5d6a10a0a1)
  )

  (wire (pts (xy 137.16 85.09) (xy 149.86 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 50608ce3-de93-4d17-91a4-793e9ead5017)
  )
  (wire (pts (xy 182.88 80.01) (xy 189.23 80.01))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 5590ee75-2caa-41fd-b87d-bfdbfacc11f5)
  )
  (wire (pts (xy 173.99 85.09) (xy 170.18 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 616929f4-851b-45aa-ac50-fd69fbf200a0)
  )
  (wire (pts (xy 137.16 102.87) (xy 186.69 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6869c283-84ac-442b-86e5-7341a0ed76fc)
  )
  (wire (pts (xy 120.65 92.71) (xy 123.19 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6b42335c-efc5-463b-9291-4ced42d9eb6c)
  )
  (wire (pts (xy 170.18 82.55) (xy 170.18 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 6e89b249-6f67-403f-9e07-2c65f15b9512)
  )
  (wire (pts (xy 125.73 92.71) (xy 125.73 95.25))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 797a3391-1c71-4448-9856-bb40a80d9f0b)
  )
  (wire (pts (xy 137.16 92.71) (xy 125.73 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 89c9a55d-2023-4e4b-87ce-ba4e41721bf0)
  )
  (wire (pts (xy 137.16 92.71) (xy 142.24 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8b5f2035-af82-4382-8354-8aed1f58b955)
  )
  (wire (pts (xy 144.78 100.33) (xy 149.86 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 8fde39c1-8d76-41f2-9ef9-298c547a1643)
  )
  (wire (pts (xy 137.16 99.06) (xy 137.16 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 932bd5e1-30c1-4a88-889b-52b227d36425)
  )
  (wire (pts (xy 189.23 80.01) (xy 189.23 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 995a62b2-0ffb-45af-934d-c197d3c8958b)
  )
  (polyline (pts (xy 116.84 111.76) (xy 116.84 73.66))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 9be440bc-b7ad-48bc-80bb-95e3245f3719)
  )

  (wire (pts (xy 120.65 74.93) (xy 170.18 74.93))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid 9f33953e-6083-4721-a335-551cdcbbaa5d)
  )
  (wire (pts (xy 120.65 74.93) (xy 120.65 90.17))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a1669057-152d-4fc2-99cb-f2d60ede16af)
  )
  (wire (pts (xy 149.86 100.33) (xy 149.86 110.49))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid a39e8b63-d557-4c47-be62-e4389787407f)
  )
  (wire (pts (xy 137.16 92.71) (xy 137.16 91.44))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ab9c1053-3a0c-46ba-bc50-e84d730293cb)
  )
  (wire (pts (xy 173.99 105.41) (xy 173.99 107.95))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b43cbcea-3e65-4fb6-8eee-d39c6a465950)
  )
  (wire (pts (xy 149.86 110.49) (xy 187.96 110.49))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b7c99f3b-9a6c-4b25-9902-515299665843)
  )
  (wire (pts (xy 170.18 77.47) (xy 170.18 74.93))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b8c26942-e53e-4058-a50c-d9be606372e0)
  )
  (wire (pts (xy 149.86 100.33) (xy 149.86 97.79))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid b8fbca2b-9054-4521-b49a-dec98afd1658)
  )
  (wire (pts (xy 137.16 100.33) (xy 137.16 102.87))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ba709f4c-8a1c-4d4c-9837-bf937f805dc9)
  )
  (wire (pts (xy 123.19 92.71) (xy 123.19 80.01))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid bda70322-79cb-4ec0-8380-e217094218b4)
  )
  (wire (pts (xy 137.16 100.33) (xy 139.7 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid c8a8f903-d43e-47fd-ac65-6974d2b8dbd0)
  )
  (wire (pts (xy 170.18 77.47) (xy 170.18 80.01))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d65cc07a-adbd-485d-9373-69ccb2cb15dd)
  )
  (wire (pts (xy 149.86 85.09) (xy 170.18 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid d99d6e39-35d3-4359-b6c9-da36ad9e22fb)
  )
  (wire (pts (xy 120.65 97.79) (xy 125.73 97.79))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid dc715a72-08c4-474b-b28b-d8d665cfb77a)
  )
  (wire (pts (xy 137.16 93.98) (xy 137.16 92.71))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid df9d2897-814f-495a-af06-5c2fdfb02392)
  )
  (wire (pts (xy 125.73 100.33) (xy 137.16 100.33))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid e7926426-d2c2-44db-b4a9-c0f3480b38d6)
  )
  (wire (pts (xy 179.07 85.09) (xy 184.15 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid ea2e34b0-3c7c-416f-a7ab-cfecb2dc5e0a)
  )
  (wire (pts (xy 120.65 105.41) (xy 173.99 105.41))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f218c05d-4796-4998-a21a-c31e56bc3e3f)
  )
  (wire (pts (xy 137.16 86.36) (xy 137.16 85.09))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f4fafab7-4e0d-41bd-a0fb-c3168522cff9)
  )
  (polyline (pts (xy 116.84 113.03) (xy 201.93 113.03))
    (stroke (width 0) (type default) (color 0 0 0 0))
    (uuid f9d9c016-e112-463c-869e-a29ca0f573ca)
  )

  (symbol (lib_id "Connector:AudioJack4") (at 193.04 105.41 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid 30d81ea9-07bb-4046-b275-554024496a39)
    (property "Reference" "J2" (id 0) (at 201.93 106.0449 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "AudioJack4" (id 1) (at 201.93 108.5849 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "outputboard:54-00177" (id 2) (at 193.04 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 193.04 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Tensility 54-00177" (id 4) (at 193.04 105.41 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "R1" (uuid 0ef30a2c-421f-4864-9b73-404a7a22952f))
    (pin "R2" (uuid e2faefd8-8e81-4519-8a0a-170823d476cb))
    (pin "S" (uuid cf7765cc-7698-43f4-82d8-eb0d0867d13c))
    (pin "T" (uuid 9bc8b39d-e8b2-47b6-ac1f-a571ae6de881))
  )

  (symbol (lib_id "Device:R_Small") (at 137.16 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 4402ebdf-e340-4cee-8e3e-c2900a4b538b)
    (property "Reference" "R1" (id 0) (at 132.08 87.63 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "2k2" (id 1) (at 132.08 90.17 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (id 2) (at 137.16 88.9 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 137.16 88.9 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Yageo RC1206JR-072K2L" (id 4) (at 137.16 88.9 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 0204ecea-35f3-4b88-aca5-6eb2a632cfef))
    (pin "2" (uuid 79fa6c81-c6c7-424d-be84-d949a347aa42))
  )

  (symbol (lib_id "Device:LED_Dual_AAK") (at 186.69 92.71 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 4d18e310-c3a3-43c0-b623-266032271258)
    (property "Reference" "D1" (id 0) (at 185.42 83.82 90)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Value" "LED_Dual_AAK 2.0/2.2V 20mA" (id 1) (at 187.96 83.82 90)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering" (id 2) (at 186.69 92.71 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 186.69 92.71 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Kingbright KM23ESGW" (id 4) (at 186.69 92.71 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4c63732e-faac-4a01-9b6e-b7955ecb03d8))
    (pin "2" (uuid 10843675-f7d1-4785-8ab0-7d2ea6f93e83))
    (pin "3" (uuid aa44367e-d592-442c-8405-0546971ab05b))
  )

  (symbol (lib_id "Device:R_Small") (at 180.34 80.01 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 519f4229-95b3-4e1f-85e9-243c592c7211)
    (property "Reference" "R4" (id 0) (at 181.61 74.93 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "120" (id 1) (at 181.61 77.47 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (id 2) (at 180.34 80.01 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 180.34 80.01 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Yageo RC1206FR-07120RL" (id 4) (at 180.34 80.01 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid fd6d4eab-d17f-4809-9fcf-ba08609c9ff2))
    (pin "2" (uuid 8417063a-cb90-491e-9fb0-910a734616ae))
  )

  (symbol (lib_id "Connector:Conn_01x05_Male") (at 115.57 95.25 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 6c6c7128-3cd5-4146-bd49-7a6fa7da139e)
    (property "Reference" "J1" (id 0) (at 106.68 91.44 0))
    (property "Value" "Conn_01x05_Male" (id 1) (at 106.68 93.98 0))
    (property "Footprint" "Connector_Molex:Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical" (id 2) (at 115.57 95.25 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 115.57 95.25 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Amtek 2542R-05TW-L" (id 4) (at 115.57 95.25 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part (Alt 1)" "JST like JH2.54-5 (Part of X0014J7UB1)" (id 5) (at 115.57 95.25 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid c7732817-37e3-4b4e-a681-55668a40da50))
    (pin "2" (uuid 2d282416-98e2-4823-a68e-edc2380d362b))
    (pin "3" (uuid ce71de60-b0b5-4ca8-8c65-0150e984f8fc))
    (pin "4" (uuid 625669ea-7cb9-4dd1-9a68-e635641820cc))
    (pin "5" (uuid 9666c440-0e7f-4550-a6f8-6a9eec8f0d9e))
  )

  (symbol (lib_id "Device:R_Small") (at 137.16 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid 9177c5b6-b84b-4e4b-9883-dd98d31e4fa6)
    (property "Reference" "R2" (id 0) (at 132.08 95.25 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "3k3" (id 1) (at 132.08 97.79 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (id 2) (at 137.16 96.52 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 137.16 96.52 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Yageo RC1206JR-073K3L" (id 4) (at 137.16 96.52 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 3ab2d67c-465c-4406-ab08-0d9a0a50f9f7))
    (pin "2" (uuid a0ce2cbe-fa20-4e08-9233-5e67092a03be))
  )

  (symbol (lib_id "Switch:SW_SPDT") (at 165.1 80.01 0) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid b5556445-1554-4bc1-8f96-85e48794e2d8)
    (property "Reference" "SW1" (id 0) (at 156.21 78.74 0))
    (property "Value" "SW_SPDT" (id 1) (at 156.21 81.28 0))
    (property "Footprint" "outputboard:WS-SLSU" (id 2) (at 165.1 80.01 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 165.1 80.01 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Würth WS-SLSU 450404015514" (id 4) (at 165.1 80.01 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 466ac436-a1db-4c0b-9232-5edd30c14549))
    (pin "2" (uuid ef59203d-c324-4982-8118-f706ae370ae0))
    (pin "3" (uuid d9c2fdca-44e5-400e-a091-e39345610589))
  )

  (symbol (lib_id "Device:R_Small") (at 176.53 85.09 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid c154a15b-2c7f-4b1f-8af8-df966ec54964)
    (property "Reference" "R5" (id 0) (at 177.8 87.63 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "150" (id 1) (at 177.8 90.17 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (id 2) (at 176.53 85.09 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 176.53 85.09 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Yageo RC1206FR-13150RL" (id 4) (at 176.53 85.09 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 3381bed3-3b34-4628-bf78-f43c6be49f3c))
    (pin "2" (uuid c64d09f7-7745-4882-b153-0f26150e17c3))
  )

  (symbol (lib_id "Device:Q_NPN_BEC") (at 147.32 92.71 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid c72ee2d3-f36a-4d12-a079-c63d404b1af4)
    (property "Reference" "Q1" (id 0) (at 152.4 91.4399 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "2N2222A" (id 1) (at 152.4 93.9799 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23_Handsoldering" (id 2) (at 152.4 90.17 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 147.32 92.71 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Nexperia PMBT2222A" (id 4) (at 147.32 92.71 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid b3b3f5f9-8a85-4366-8ec4-152d86ed9b83))
    (pin "2" (uuid eb68ae3f-33c4-42b4-9a3a-ad0cae73d047))
    (pin "3" (uuid f2cef362-bd76-4a0e-92a4-bb1fcb75f6e3))
  )

  (symbol (lib_name "R_Small_1") (lib_id "Device:R_Small") (at 142.24 100.33 90) (unit 1)
    (in_bom yes) (on_board yes)
    (uuid d1a68f1b-cfb3-400d-a2a0-7bf86a0683c3)
    (property "Reference" "R3" (id 0) (at 142.2463 95.79 90))
    (property "Value" "75" (id 1) (at 142.2463 97.79 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (id 2) (at 142.24 100.33 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 142.24 100.33 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Part" "Yageo RC1206JR-0775RL" (id 4) (at 142.24 100.33 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 555d59b0-d1af-41e4-ac00-f9073f1f4258))
    (pin "2" (uuid 4852b323-54d6-42b7-ac08-67e2239b3004))
  )

  (symbol (lib_id "Jumper:Jumper_2_Open") (at 179.07 107.95 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (uuid fa194964-dbd1-4b39-be5e-3ae84d7e3f19)
    (property "Reference" "JP1" (id 0) (at 179.07 101.6 0))
    (property "Value" "Jumper_2_Open" (id 1) (at 179.07 104.14 0))
    (property "Footprint" "outputboard:Jumper_2_1.27_Open" (id 2) (at 179.07 107.95 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at 179.07 107.95 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 33973b07-49f4-4190-9074-d4386edafcf4))
    (pin "2" (uuid 7b490316-198e-4b1e-82ed-384090e97c17))
  )

  (sheet_instances
    (path "/" (page "1"))
  )

  (symbol_instances
    (path "/4d18e310-c3a3-43c0-b623-266032271258"
      (reference "D1") (unit 1) (value "LED_Dual_AAK 2.0/2.2V 20mA") (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering")
    )
    (path "/6c6c7128-3cd5-4146-bd49-7a6fa7da139e"
      (reference "J1") (unit 1) (value "Conn_01x05_Male") (footprint "Connector_Molex:Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical")
    )
    (path "/30d81ea9-07bb-4046-b275-554024496a39"
      (reference "J2") (unit 1) (value "AudioJack4") (footprint "outputboard:54-00177")
    )
    (path "/fa194964-dbd1-4b39-be5e-3ae84d7e3f19"
      (reference "JP1") (unit 1) (value "Jumper_2_Open") (footprint "outputboard:Jumper_2_1.27_Open")
    )
    (path "/c72ee2d3-f36a-4d12-a079-c63d404b1af4"
      (reference "Q1") (unit 1) (value "2N2222A") (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering")
    )
    (path "/4402ebdf-e340-4cee-8e3e-c2900a4b538b"
      (reference "R1") (unit 1) (value "2k2") (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder")
    )
    (path "/9177c5b6-b84b-4e4b-9883-dd98d31e4fa6"
      (reference "R2") (unit 1) (value "3k3") (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder")
    )
    (path "/d1a68f1b-cfb3-400d-a2a0-7bf86a0683c3"
      (reference "R3") (unit 1) (value "75") (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder")
    )
    (path "/519f4229-95b3-4e1f-85e9-243c592c7211"
      (reference "R4") (unit 1) (value "120") (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder")
    )
    (path "/c154a15b-2c7f-4b1f-8af8-df966ec54964"
      (reference "R5") (unit 1) (value "150") (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder")
    )
    (path "/b5556445-1554-4bc1-8f96-85e48794e2d8"
      (reference "SW1") (unit 1) (value "SW_SPDT") (footprint "outputboard:WS-SLSU")
    )
  )
)
