*MSX Type : MSX System Version 2.0 (MSX2)

*Model Name : CPC-400S

*Manufacturer : Daewoo (Made in 1987)

*Cartridge Slot : 2 Slots (Slot No.1 & Extension Bus Slot No.3)

*Disk Drive Units : 3.5inch 2DD (1ea)

*ROM : 240KB

 1)MSX BIOS & BASIC Version 2.0 (Slot No.0-0 : 0000-7FFF)
   Filename : cpc-400s_basic-bios2.rom
   Filesize : 0x00008000
   XOR : 19
   SUM : 003b5cc1
   CRC32 : 53850907
   MD5 : 6819a1533502261bfdd52436b8346073
 2)MSX Extended BASIC Version 2.0 (Slot No.0-3 : 0000-7FFF)
   Filename : cpc-400s_msx2sub.rom
   Filesize : 0x00008000
   XOR : 6e
   SUM : 002d350e
   CRC32 : 2ba104a3
   MD5 : 30a0b3402a0a13b516af76d39f45a365
 3)MSX Disk BASIC Version 1.0 (Slot No.2 : 4000-7FFF, FDC Type : Fujitsu MB8877A)
   Filename : cpc-400s_disk.rom
   Filesize : 0x00004000
   XOR : cc
   SUM : 001e8092
   CRC32 : 5fa517df
   MD5 : 25128f53e854d4be82b6178bdc2afc78
 4)MSX Hangul Driver (Slot No.0-1 : 4000-BFFF)
   Filename : cpc-400s_hangul.rom
   Filesize : 0x00008000
   XOR : db
   SUM : 00493475
   CRC32 : 975e7a31
   MD5 : 1bf039533043c2860387720278f285db
 5)MSX Hangul Font (I/O Address : &HD8-&HD9)
   Filename : cpc-400s_hangulfont.rom
   Filesize : 0x00020000
   XOR : a7
   SUM : 006f9a31
   CRC32 : fa85368c
   MD5 : 392218c5e7f761066cbf6000ae577060

*RAM : 256KB

 1)Main : 128KB (Slot No.0-2 : 0000-FFFF)
 2)VRAM : 128KB (I/O Address : &H98-&H9F)
