$JOB CCLX.BI
/ Assemble, load, save, and install new CCLX.  Assume all
/ files on DSK: (watch out, the listing file is 600 and
/ some blocks long).  If using CCL or old CCLX, drop the
/ -R from the PAL and LOAD commands.
.PAL CCLX,CCLX1,CCLX2,CCLX3,CCLX4,CCLX5,CCLX6(WELP9)-LS-R
.LOAD CCLX-R
.SA DSK:CCLX
$MSG    Install new CCLX?
.CCLX
.GE DSK:CCLX
.SA SYS:CCL
/ Save in same place as old CCLX.SV.
.SA SYS:CCL
.R CCL
$END
