Hi, All! Its my speccy emulator, enjoin ;-)
Hot key: up, down, left, rigth, Ctrl - kempston joistik, 1,2,3,4,5,6,7,8,9,0 - sinclar joistik
1) run DEBUGZ80.exe
2) press space, space
3) press N, ENTER
4) fann...
5) press ESC to exit in debug mode
6) press q, ENTER to exit from programm
7) Bye...
0) for change disks from default
 insert disk_image (*.trd file) in virtual FDD:
file FREEDISK.FDD - its image for cleared disk, you can copy its with name disk0000.tmp
after it use MAKE_DRV.EXE -
its retranslator from disks_images (*.drv, or *.trd) to virtual FloppyDiskDrive (file disk0000.tmp)
 instruction:
- copy make_drv.exe and disk0000.tmp {<drive A for TR-DOS} in one folder
- type make_drv.exe [filename].trd
or
- DRAG&DROP  [filename].trd on make_drv

WARNING: this programm dont work in Win7 (but work in WinXP and lowes), and I no hawe free time for reprogramming, meibe in future...
- start screen translate - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
                 !! SPECTRUM emulator !! (Demo Ver1.05)


  autor: Solomatin Denis Vladimirovitsch
                            e-mail: denis_2001j@bk.ru
  betta tester: Homyakov Ivan Valerievitsvh
                            e-mail: ogs_webmaster@mail.ru
                               www: skyslayer.narod.ru

myfile:
debugz80.exe 52,399 07-01-04 23:03 - emulator Z80
dos.rom      16,384 23-11-00 11:21 - ROM file with TR-DOS
sos.rom      16,384 21-09-00 16:39 - ROM file with BASIC (from KOMPANION - its one Russian speccy)
help.dat     64,000 18-10-00 15:54 - spectrum keyboard picture, press F1 in graph mode to show it
svga256.bgi   3,660  9-02-91  1:30 - old grafix driver
disk0000.tmp 1,409,024             - file for FDD emulation <A:>
*.drv  - original disks_images (compatible with *.trd !!)
make_drv.exe  4,112 07-01-04 23:01 - utility for insert disk_images in virtual FDD

remarks:
RETURN - go to SOS
RANDOMIZE USR 15616 - go to DOS

press space to cotinue

this programm run in debug Z80 mode
 screen help:
|in rigth down - my logo
|Code - memory dump <addres> <code> <assembler>
 * current position PC
|CPU - registrs Z80
|SpReg - spec registrs
|IntDat - interrupt info
|ROM - current ROM selected
|Command - memo for type texts commants
 cammand :
n - run programm witout stop, from current PC position
t - tracert code (runs cycles)
q - quit
g - for example gFFFF - run to FFFF, grax - run to addres from AX registr
(all address intered in current numeric system!)
r - registrs change, exaple rrax- changed AX
u - disassemble fom address (for example u0000 - disassembled from 0000)
v - show ZX screen
f - change numeric system (HEX/DEC)
ENTER - execute typed command
> - increment PC             < - decrement PC
 hotkey in full screen graph mode:
ECS - return in text debug mode F1 - show speccy keyboard

press space to cotinue

- - - - - - - - - - - -  - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
from Sibirien with Love