DETAILS.TXT rev 1 96-09-15
* * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * *
     THIS DOCUMENT IS COPYRIGHT (C) 1988, 1996 BY HERNE DATA
     SYSTEMS LTD.  THE MATERIAL CONTAINED HEREIN MAY BE FREELY
     USED FOR PERSONAL INFORMATION ONLY.  IF YOU REPRODUCE IT,
     THIS COPYRIGHT NOTICE MUST NOT BE REMOVED.  THIS MATERIAL
     MAY NOT BE EXPLOITED FOR COMMERCIAL PURPOSES.
* * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * *

Herne Data Systems Ltd., 
PO Box 250, Tiverton, ON N0G 2T0 CANADA.  
Voice/fax 519-366-2732, 
e-mail hernedata@mail.bmts.com, 
internet: http://ourworld.compuserve.com/homepages/herne_data

* * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * *

CP/M Disk Format Details

============================================================
Disk Name: A B C - 80              SS      
Type: 5 1/4     Total usable space: 152k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 7 14 5 12 3 10 1 8 15 6 13 4 11 2 9
 
 - Allocation unit size is 1024 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 97 00 3F 00 C0 00 10 00 02 00 01 01 
============================================================
Disk Name: A B Dick Magna III      DS      
Type: 5 1/4     Total usable space: 256k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 17 to 32)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 256 AU's per disk
 - Directory starts at logical track 2;
     has 256 entries and occupies 32 sectors or 8 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 03 07 00 FF 00 FF 00 FF 00 40 00 02 00 01 01 
============================================================
Disk Name: ATR-8000                DS      
Type: 5 1/4     Total usable space: 380k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 190 AU's per disk
 - Directory starts at logical track 4;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 BD 00 7F 00 C0 00 20 00 04 00 03 07 
============================================================
Disk Name: ATR-8000                SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 2 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 BD 00 3F 00 C0 00 10 00 02 00 03 07 
============================================================
Disk Name: Access Matrix           SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 1 4 7 2 5 8
 
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: Actrix                  DS      
Type: 5 1/4     Total usable space: 350k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 1 4 7 2 5 8 9 12 15 10 13 16 11 14 17
 
 - Allocation unit size is 2048 bytes; 175 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    48 00 04 0F 01 AE 00 3F 00 80 00 10 00 01 00 02 03 
============================================================
Disk Name: Actrix                  SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 1 4 7 2 5 8
 
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: Adler Textwriter        SS      
Type: 5 1/4     Total usable space: 160k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 12 15 2 5 8 11 14 1 4 7 10 13
 
 - Allocation unit size is 1024 bytes; 160 AU's per disk
 - Directory starts at logical track 0;
     has 32 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9F 00 1F 00 80 00 08 00 00 00 01 01 
============================================================
Disk Name: Adv. Digt'l Super-6     DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 1024 bytes/sector;   4 per track; numbered 1 to 4 (Side 2 numbered 1 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 00 9B 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Adv. Digt'l Super-6     SS      
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 1024 bytes/sector;   4 per track; numbered 1 to 4  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 78 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 2 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 00 4D 00 3F 00 80 00 10 00 01 00 03 07 
============================================================
Disk Name: Adv. Digt'l T-DOS 312k  DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 1024 bytes/sector;   4 per track; numbered 1 to 4 (Side 2 numbered 1 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 9B 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Adv. Digt'l T-DOS 366k  DS      
Type: 5 1/4     Total usable space: 366k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 183 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 B6 00 7F 00 C0 00 20 00 03 00 03 07 
============================================================
Disk Name: Amigo                   DS      
Type: 5 1/4     Total usable space: 392k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 196 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 C3 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Amigo                   SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 BD 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: Ampro                   SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 95 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 5E 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Ampro                   SS      
Type: 3 1/2     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 1 2 3 4
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 7F 00 C0 00 20 00 02 00 03 07 
============================================================
Disk Name: Amstrad PCW             DS      
Type: 3 1/2     Total usable space: 714k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 357 AU's per disk
 - Directory starts at logical track 0;
     has 256 entries and occupies 16 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    48 00 04 0F 00 64 01 FF 00 F0 00 40 00 00 00 02 03 
============================================================
Disk Name: Amstrad Vortex          DS      
Type: 3 1/2     Total usable space: 708k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 1 2 3 4 5 6 7 8
 
 - Allocation unit size is 4096 bytes; 177 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    48 00 05 1F 03 B0 00 7F 00 80 00 20 00 01 00 02 03 
============================================================
Disk Name: Archive                 DS      
Type: 5 1/4     Total usable space: 360k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 180 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 B3 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Arisia                  SS      
Type: 5 1/4     Total usable space: 148k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 148 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 93 00 7F 00 F0 00 20 00 02 00 01 01 
============================================================
Disk Name: Avatar                  DS      
Type: 5 1/4     Total usable space: 384k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 
 
 - Allocation unit size is 2048 bytes; 192 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 BF 00 7F 00 C0 00 20 00 03 00 02 03 
============================================================
Disk Name: Beehive                 DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C2 00 7F 00 C0 00 20 00 01 00 02 03 
============================================================
Disk Name: Bitelex                 SS      
Type: 5 1/4     Total usable space: 132k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 10 12 14 1 3 5 7 9 11 13 15 
 
 - Allocation unit size is 1024 bytes; 132 AU's per disk
 - Directory starts at logical track 2;
     has 96 entries and occupies 12 sectors or 3 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 83 00 5F 00 E0 00 18 00 02 00 01 01 
============================================================
Disk Name: Bondwell 12             SS      
Type: 5 1/4     Total usable space: 170k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 0 to 17  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 85 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 54 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Bondwell 14             DS      
Type: 5 1/4     Total usable space: 350k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 0 to 17 (Side 2 numbered 0 to 17)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 175 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AE 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Bondwell 2              SS      
Type: 3 1/2     Total usable space: 350k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 0 to 17  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 175 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AE 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Burr-Brown              DS      
Type: 5 1/4     Total usable space: 342k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 9 1 10 2 11 3 12 4 13 5 14 6 15 7 16 8 17 
 
 - Allocation unit size is 2048 bytes; 171 AU's per disk
 - Directory starts at logical track 4;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AA 00 3F 00 80 00 10 00 04 00 01 01 
============================================================
Disk Name: C/WP Cortex             SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 BD 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: CCS (1024 byte/sector)  DS      
Type: 5 1/4     Total usable space: 370k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 1 3 5 7 9 6 8
 
 - Allocation unit size is 2048 bytes; 185 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 2 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 B8 00 3F 00 80 00 10 00 03 00 03 07 
============================================================
Disk Name: CCS (256 byte/sector)   DS      
Type: 5 1/4     Total usable space: 332k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 12 16 2 6 10 14 1 5 9 13 17 3 7 11 15 
 
 - Allocation unit size is 2048 bytes; 166 AU's per disk
 - Directory starts at logical track 6;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 A5 00 3F 00 80 00 10 00 06 00 01 01 
============================================================
Disk Name: CCS (512 byte/sector)   DS      
Type: 5 1/4     Total usable space: 370k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 2 5 8 1 4 7 10 13 16 19 12 15 18 11 14 17
 
 - Allocation unit size is 2048 bytes; 185 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 B8 00 3F 00 80 00 10 00 03 00 02 03 
============================================================
Disk Name: CDI-5000                DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 1 4 2 
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 2 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 3F 00 80 00 10 00 02 00 03 07 
============================================================
Disk Name: Cal PC                  DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 7F 00 C0 00 20 00 02 00 03 07 
============================================================
Disk Name: Coleco ADAM CP/M        SS    
Type: 5 1/4     Total usable space: 148k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      2 7 4 1 6 3 0 5
 
 - Allocation unit size is 1024 bytes; 148 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 93 00 3F 00 C0 00 10 00 03 00 02 03 
============================================================
Disk Name: Compugraphic MCS 5      SS      
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9B 00 3F 00 C0 00 10 00 01 00 01 01 
============================================================
Disk Name: Compustar 30            DS    
Type: 5 1/4     Total usable space: 340k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 170 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 A9 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Cromemco C-10           DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 11 to 20)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 C2 00 7F 00 C0 00 20 00 01 00 02 03 
============================================================
Disk Name: Cromemco CDOS           DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 C2 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Cromemco CDOS           DSSD    
Type: 5 1/4     Total usable space: 173k bytes
  
Sector information: 
 - 128 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 5 10 15 2 7 12 17 4 9 14 1 6 11 16 3 8 13 
 
 - Allocation unit size is 1024 bytes; 173 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    12 00 03 07 00 AC 00 3F 00 C0 00 10 00 03 00 00 00 
============================================================
Disk Name: Cromemco CDOS           SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 
 
 - Allocation unit size is 1024 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 BD 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: Cromemco CDOS           SSSD    
Type: 5 1/4     Total usable space: 83k bytes
  
Sector information: 
 - 128 bytes/sector;  18 per track; numbered 1 to 18  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 5 10 15 2 7 12 17 4 9 14 1 6 11 16 3 8 13 
 
 - Allocation unit size is 1024 bytes; 83 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    12 00 03 07 00 52 00 3F 00 C0 00 10 00 03 00 00 00 
============================================================
Disk Name: Cromemco Int'l Term     DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 2 5 8 1 4 7 10 13 16 19 12 15 18 11 14 17
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C2 00 7F 00 C0 00 20 00 01 00 02 03 
============================================================
Disk Name: Cromemco Int'l Term     SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 2 5 8 1 4 7 
 
 - Allocation unit size is 2048 bytes; 95 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 5E 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Cykey                   DS      
Type: 5 1/4     Total usable space: 308k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 12 1 5 9 13 2 6 10 14 3 7 11 15 
 
 - Allocation unit size is 2048 bytes; 154 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 99 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: DEC Robin               SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 
 
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: DEC VT-180              SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 
 
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: Digilog                 DS      
Type: 5 1/4     Total usable space: 334k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 167 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 2 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 A6 00 3F 00 80 00 10 00 03 00 03 07 
============================================================
Disk Name: Direct 1025             DS      
Type: 5 1/4     Total usable space: 306k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 153 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 00 98 00 7F 00 C0 00 20 00 03 00 01 01 
============================================================
Disk Name: Epson QX-10 (256)       DS     
Type: 5 1/4     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 97 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Epson QX-10 (256-Euro)  DS     
Type: 5 1/4     Total usable space: 280k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 140 AU's per disk
 - Directory starts at logical track 4;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 8B 00 3F 00 80 00 10 00 04 00 01 01 
============================================================
Disk Name: Epson QX-10 (512)       DS     
Type: 5 1/4     Total usable space: 380k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 190 AU's per disk
 - Directory starts at logical track 4;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 BD 00 7F 00 C0 00 20 00 04 00 02 03 
============================================================
Disk Name: Formula 1               DS      
Type: 5 1/4     Total usable space: 346k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 1 4 5 8 9 12 13 16 17 2 3 6 7 10 11 14 15 
 
 - Allocation unit size is 2048 bytes; 173 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AC 00 7F 00 C0 00 20 00 03 00 01 01 
============================================================
Disk Name: Fujitsu  Micro 8        DS      
Type: 5 1/4     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 97 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Fujitsu Micro 16-s      DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9B 00 3F 00 80 00 10 00 01 00 02 03 
============================================================
Disk Name: Gemini                  DS      
Type: 3 1/2     Total usable space: 780k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 4096 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 05 1F 01 C2 00 7F 00 80 00 20 00 02 00 02 03 
============================================================
Disk Name: Glass Typewriter II     DS      
Type: 5 1/4     Total usable space: 380k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 2 5 8 1 4 7 
 
 - Allocation unit size is 2048 bytes; 190 AU's per disk
 - Directory starts at logical track 4;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 BD 00 7F 00 C0 00 20 00 04 00 02 03 
============================================================
Disk Name: Glass Typewrtr          DS      
Type: 3 1/2     Total usable space: 778k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 2 5 8 1 4 7
 
 - Allocation unit size is 2048 bytes; 389 AU's per disk
 - Directory starts at logical track 4;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 84 01 7F 00 C0 00 20 00 04 00 02 03 
============================================================
Disk Name: Gnat Sys. 10            DS      
Type: 5 1/4     Total usable space: 340k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 11 to 20)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 170 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 A9 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Heath Magnolia          DS      
Type: 5 1/4     Total usable space: 346k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 173 AU's per disk
 - Directory starts at logical track 3;
     has 96 entries and occupies 6 sectors or 1.5 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AC 00 5F 00 C0 00 18 00 03 00 02 03 
============================================================
Disk Name: Heath Magnolia          SS      
Type: 5 1/4     Total usable space: 166k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 83 AU's per disk
 - Directory starts at logical track 3;
     has 96 entries and occupies 6 sectors or 1.5 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 52 00 5F 00 C0 00 18 00 03 00 02 03 
============================================================
Disk Name: Hew.-Pack. 125          SS      
Type: 3 1/2     Total usable space: 252k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 0 to 15  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 252 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 16 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 FB 00 7F 00 F0 00 20 00 03 00 01 01 
============================================================
Disk Name: Hewlett Packard 86, 87  DS      
Type: 5 1/4     Total usable space: 252k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 0 to 15 (Side 2 numbered 0 to 15)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 252 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 16 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 FB 00 7F 00 F0 00 20 00 03 00 01 01 
============================================================
Disk Name: IBM-PC (CP/M-86)        DS     
Type: 5 1/4     Total usable space: 316k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 158 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9D 00 3F 00 80 00 10 00 01 00 02 03 
============================================================
Disk Name: IBM-PC (CP/M-86)        SS     
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9B 00 3F 00 C0 00 10 00 01 00 02 03 
============================================================
Disk Name: ICM Turbo DOS           DS      
Type: 5 1/4     Total usable space: 396k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 198 AU's per disk
 - Directory starts at logical track 0;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C5 00 7F 00 C0 00 20 00 00 00 03 07 
============================================================
Disk Name: IMS-5000                DS      
Type: 5 1/4     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 8 16 24 1 9 17 25 2 10 18 26 3 11 19 27 4 12 20 28 5 13 21 29 6 14 22 30 7 15 23 31
 
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 97 00 3F 00 80 00 10 00 02 00 01 01 
============================================================
Disk Name: IMS-5000                SS      
Type: 5 1/4     Total usable space: 148k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 8 1 9 2 10 3 11 4 12 5 13 6 14 7 15 
 
 - Allocation unit size is 1024 bytes; 148 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 93 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Insight Enter.          DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9B 00 3F 00 80 00 10 00 02 00 01 01 
============================================================
Disk Name: Jet-80                  DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 7F 00 C0 00 20 00 02 00 03 07 
============================================================
Disk Name: KayPro 4, 10            DS     
Type: 5 1/4     Total usable space: 394k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 0 to 9 (Side 2 numbered 10 to 19)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 197 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C4 00 3F 00 C0 00 10 00 01 00 02 03 
============================================================
Disk Name: KayPro II, 2            SS     
Type: 5 1/4     Total usable space: 195k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 0 to 9  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 195 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 C2 00 3F 00 F0 00 10 00 01 00 02 03 
============================================================
Disk Name: L.N.W.-2                SS      
Type: 5 1/4     Total usable space: 166k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18  
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 5 10 15 2 7 12 17 4 9 14 1 6 11 16 3 8 13 
 
 - Allocation unit size is 2048 bytes; 83 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 52 00 3F 00 80 00 10 00 03 00 01 01 
============================================================
Disk Name: Labtam                  DS      
Type: 3 1/2     Total usable space: 798k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 399 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 8E 01 7F 00 C0 00 20 00 02 00 03 07 
============================================================
Disk Name: Lexoriter               SS      
Type: 5 1/4     Total usable space: 160k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 12 15 2 5 8 11 14 1 4 7 10 13 
 
 - Allocation unit size is 1024 bytes; 160 AU's per disk
 - Directory starts at logical track 0;
     has 32 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9F 00 1F 00 80 00 0A 00 00 00 01 01 
============================================================
Disk Name: Librarian 1571          DS      
Type: 5 1/4     Total usable space: 402k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 0 to 4 (Side 2 numbered 0 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 201 AU's per disk
 - Directory starts at logical track 0;
     has 256 entries and occupies 8 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C8 00 FF 00 F0 00 40 00 00 00 03 07 
============================================================
Disk Name: Librarian 1581          DS      
Type: 3 1/2     Total usable space: 802k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 0 to 4 (Side 2 numbered 0 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 401 AU's per disk
 - Directory starts at logical track 0;
     has 512 entries and occupies 16 sectors or 8 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 00 90 01 FF 01 FF 00 80 00 00 00 03 07 
============================================================
Disk Name: Lobo Max-80 (256 byte)  DS      
Type: 5 1/4     Total usable space: 346k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 0 to 17 (Side 2 numbered 0 to 17)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 173 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 00 AC 00 7F 00 C0 00 20 00 03 00 01 01 
============================================================
Disk Name: Lobo Max-80 (256 byte)  SS      
Type: 5 1/4     Total usable space: 166k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 0 to 17  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 166 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 A5 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Lobo Max-80 (512 byte)  DS      
Type: 5 1/4     Total usable space: 384k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 0 to 9 (Side 2 numbered 0 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 192 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 BF 00 7F 00 C0 00 20 00 03 00 02 03 
============================================================
Disk Name: MAXI 1571               DS      
Type: 5 1/4     Total usable space: 402k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 0 to 4 (Side 2 numbered 0 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 201 AU's per disk
 - Directory starts at logical track 0;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C8 00 7F 00 C0 00 20 00 00 00 03 07 
============================================================
Disk Name: MAXI 1581               DS      
Type: 3 1/2     Total usable space: 802k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 0 to 4 (Side 2 numbered 0 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 401 AU's per disk
 - Directory starts at logical track 0;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 00 90 01 7F 00 C0 00 20 00 00 00 03 07 
============================================================
Disk Name: MG 1581                 DS      
Type: 3 1/2     Total usable space: 782k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 391 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 00 86 01 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Magic                   DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 C2 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Mega-88 Turbo DOS       DS      
Type: 5 1/4     Total usable space: 308k bytes
  
Sector information: 
 - 1024 bytes/sector;   4 per track; numbered 1 to 4 (Side 2 numbered 1 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 154 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 99 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Micro Source M-6000     DS      
Type: 5 1/4     Total usable space: 380k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 11 to 20)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 10 14 18 12 16 11 15 19 13 17
 
 - Allocation unit size is 2048 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 BD 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: MicroBee                DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      1 4 7 0 3 6 9 2 5 8 
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Micron Quark            DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 1024 bytes/sector;   4 per track; numbered 1 to 4 (Side 2 numbered 1 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 00 9B 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Molecular S-9           DS      
Type: 5 1/4     Total usable space: 360k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 180 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    48 00 04 0F 01 B3 00 7F 00 C0 00 30 00 02 00 02 03 
============================================================
Disk Name: Morrow MD2              SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 1 4 2 
 
 - Allocation unit size is 2048 bytes; 95 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 5E 00 7F 00 C0 00 20 00 02 00 03 07 
============================================================
Disk Name: Morrow MD3,5,11,16,34   DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 1 4 2 
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 192 entries and occupies 6 sectors or 3 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 BF 00 E0 00 30 00 02 00 03 07 
============================================================
Disk Name: Morrow Turbo DOS        DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 1024 bytes/sector;   4 per track; numbered 1 to 4 (Side 2 numbered 1 to 4)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 00 9B 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Mountain Control        DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 10 14 18 12 16 11 15 19 13 17
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C2 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Multiflex               SS      
Type: 5 1/4     Total usable space: 166k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 1 4 7 2 5 8 
 
 - Allocation unit size is 2048 bytes; 83 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 52 00 3F 00 80 00 10 00 03 00 02 03 
============================================================
Disk Name: NCR Decision Mate       DS      
Type: 5 1/4     Total usable space: 308k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled all first side, then second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 154 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 99 00 7F 00 C0 00 20 00 03 00 02 03 
============================================================
Disk Name: NEC PC-8001             SS      
Type: 5 1/4     Total usable space: 152k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 97 00 3F 00 C0 00 10 00 02 00 01 01 
============================================================
Disk Name: NEC PC-8431             SS      
Type: 3 1/2     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 4;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 97 00 7F 00 C0 00 20 00 04 00 01 01 
============================================================
Disk Name: NEC PC-8801             DS      
Type: 5 1/4     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 97 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Nelma Persona           SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 
 
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 02 03 
============================================================
Disk Name: Olivetti 240            SS      
Type: 3 1/2     Total usable space: 320k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 10 12 14 1 3 5 7 9 11 13 15
 
 - Allocation unit size is 2048 bytes; 160 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9F 00 3F 00 80 00 10 00 01 00 01 01 
============================================================
Disk Name: Olivetti ETV-300        SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18  
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 10 12 14 16 1 3 5 7 9 11 13 15 17 
 
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 01 01 
============================================================
Disk Name: Olivetti M20            DS      
Type: 5 1/4     Total usable space: 256k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 256 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 FF 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Olympia ETX-II          SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 7F 00 F0 00 20 00 02 00 02 03 
============================================================
Disk Name: Olympia EX-100          DS      
Type: 5 1/4     Total usable space: 350k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 175 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AE 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Osborne 1               SSSD    
Type: 5 1/4     Total usable space: 92k bytes
  
Sector information: 
 - 256 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 46 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    14 00 04 0F 01 2D 00 3F 00 80 00 10 00 03 00 01 01 
============================================================
Disk Name: Osborne 1/Executive     SS     
Type: 5 1/4     Total usable space: 185k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 185 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 2 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 B8 00 3F 00 C0 00 10 00 03 00 03 07 
============================================================
Disk Name: Osborne G2              DS      
Type: 5 1/4     Total usable space: 380k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 6 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 00 BD 00 7F 00 C0 00 20 00 02 00 03 07 
============================================================
Disk Name: Osborne Nuevo/Vixen     DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 1 3 5 7 9 6 8
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C2 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Otrona Attache          DS      
Type: 5 1/4     Total usable space: 364k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 182 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 B5 00 7F 00 C0 00 20 00 03 00 02 03 
============================================================
Disk Name: PMC MicroMate           DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C2 00 7F 00 C0 00 20 00 01 00 03 07 
============================================================
Disk Name: Panasonic KXE-828       DS      
Type: 5 1/4     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 97 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Pegasus Data Logger     DS      
Type: 5 1/4     Total usable space: 342k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 1 4 7 2 5 8 9 12 15 10 13 16 11 14 17
 
 - Allocation unit size is 2048 bytes; 171 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    48 00 04 0F 00 AA 00 3F 00 80 00 10 00 03 00 02 03 
============================================================
Disk Name: Philips PC-2010         SS      
Type: 5 1/4     Total usable space: 152k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 10 12 14 1 3 5 7 9 11 13 15 
 
 - Allocation unit size is 1024 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 97 00 3F 00 C0 00 10 00 02 00 01 01 
============================================================
Disk Name: Portapak                DS      
Type: 3 1/2     Total usable space: 778k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9
 
 - Allocation unit size is 2048 bytes; 389 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 84 01 7F 00 C0 00 20 00 03 00 02 03 
============================================================
Disk Name: Royal Alphatronic       DS      
Type: 5 1/4     Total usable space: 304k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 04 0F 01 97 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Sage IV                 DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9B 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Sanyo MBC-1000, 1150    DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 12 15 2 5 8 11 14 1 4 7 10 13 
 
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9B 00 3F 00 80 00 10 00 02 00 01 01 
============================================================
Disk Name: Seequa Chameleon        DS      
Type: 5 1/4     Total usable space: 316k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 158 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9D 00 3F 00 80 00 10 00 01 00 02 03 
============================================================
Disk Name: Seequa Chameleon        SS      
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9B 00 3F 00 C0 00 10 00 01 00 02 03 
============================================================
Disk Name: Sharp MZ-80             DS    
Type: 5 1/4     Total usable space: 340k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 170 AU's per disk
 - Directory starts at logical track 1;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 A9 00 7F 00 C0 00 20 00 01 00 02 03 
============================================================
Disk Name: Slicer                  DS     
Type: 5 1/4     Total usable space: 316k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 158 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9D 00 3F 00 80 00 10 00 01 00 02 03 
============================================================
Disk Name: Sony SMC-70             SS      
Type: 3 1/2     Total usable space: 272k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 3 6 9 12 15 2 5 8 11 14 1 4 7 10 13
 
 - Allocation unit size is 2048 bytes; 136 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 87 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Spectravideo SV-328     DS      
Type: 5 1/4     Total usable space: 326k bytes
  
Sector information: 
 - 256 bytes/sector;  17 per track; numbered 1 to 17 (Side 2 numbered 1 to 17)
 - Disk is filled all first side, then second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 163 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    22 00 04 0F 01 A2 00 3F 00 80 00 10 00 03 00 01 01 
============================================================
Disk Name: SuperBrain              DS    
Type: 5 1/4     Total usable space: 340k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 170 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 A9 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: SuperBrain 40 Track     SS    
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 95 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 5E 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: SuperBrain Jr.          SS    
Type: 5 1/4     Total usable space: 164k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 82 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 51 00 3F 00 80 00 10 00 02 00 02 03 
============================================================
Disk Name: Systel 2                SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 7F 00 F0 00 20 00 02 00 02 03 
============================================================
Disk Name: Systel 3                DS      
Type: 5 1/4     Total usable space: 350k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 175 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AE 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: TI Pro. CP/M-86         SS      
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9B 00 3F 00 C0 00 10 00 01 00 02 03 
============================================================
Disk Name: TRS-80 Color Power II   SS      
Type: 5 1/4     Total usable space: 171k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 03 07 00 AA 00 3F 00 C0 00 10 00 02 00 01 01 
============================================================
Disk Name: TRS-80 Mod 3/Holmes     DS      
Type: 5 1/4     Total usable space: 382k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 0 to 9 (Side 2 numbered 10 to 19)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 191 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 BE 00 3F 00 F0 00 10 00 02 00 02 03 
============================================================
Disk Name: TRS-80 Mod 3/M.M.       SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 95 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 5E 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: TRS-80 Mod 4 CP/M+      SS      
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9B 00 3F 00 C0 00 10 00 01 00 02 03 
============================================================
Disk Name: TRS-80 Mod 4/MTZ (256)  DS      
Type: 5 1/4     Total usable space: 350k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 10 12 14 16 1 3 5 7 9 11 13 15 17 
 
 - Allocation unit size is 2048 bytes; 175 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AE 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: TRS-80 Mod 4/MTZ (256)  SS      
Type: 5 1/4     Total usable space: 170k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 10 12 14 16 1 3 5 7 9 11 13 15 17 
 
 - Allocation unit size is 2048 bytes; 85 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 54 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: TRS-80 Mod 4/MTZ (512)  DS      
Type: 5 1/4     Total usable space: 400k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 200 AU's per disk
 - Directory starts at logical track 0;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C7 00 7F 00 C0 00 20 00 00 00 02 03 
============================================================
Disk Name: TRS-80 Mod 4/MTZ (512)  SS      
Type: 5 1/4     Total usable space: 200k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 2 4 6 8 1 3 5 7 9 
 
 - Allocation unit size is 2048 bytes; 100 AU's per disk
 - Directory starts at logical track 0;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 63 00 7F 00 C0 00 20 00 00 00 02 03 
============================================================
Disk Name: TRS-80 Model 1          SSSD    
Type: 5 1/4     Total usable space: 101k bytes
  
Sector information: 
 - 256 bytes/sector;  10 per track; numbered 0 to 9  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 101 AU's per disk
 - Directory starts at logical track 0;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    14 00 03 07 00 64 00 3F 00 C0 00 10 00 00 00 01 01 
============================================================
Disk Name: TRS-80 Model 1/Omicron  SSSD    
Type: 5 1/4     Total usable space: 72k bytes
  
Sector information: 
 - 128 bytes/sector;  18 per track; numbered 1 to 18  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 12 16 2 6 10 14 1 5 9 13 17 3 7 11 15 
 
 - Allocation unit size is 1024 bytes; 72 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    12 00 03 07 00 47 00 3F 00 C0 00 10 00 03 00 00 00 
============================================================
Disk Name: Tektronix 4170          DS      
Type: 5 1/4     Total usable space: 308k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 154 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 00 99 00 3F 00 80 00 20 00 01 00 02 03 
============================================================
Disk Name: TeleVideo   Turbo DOS   DS      
Type: 5 1/4     Total usable space: 400k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5 (Side 2 numbered 1 to 5)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 200 AU's per disk
 - Directory starts at logical track 0;
     has 128 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    50 00 04 0F 01 C7 00 7F 00 C0 00 20 00 00 00 03 07 
============================================================
Disk Name: TeleVideo 801, 806      DS      
Type: 5 1/4     Total usable space: 342k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 171 AU's per disk
 - Directory starts at logical track 4;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 00 AA 00 3F 00 80 00 10 00 04 00 01 01 
============================================================
Disk Name: Telectronics CP/M 68k   DS      
Type: 5 1/4     Total usable space: 346k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 173 AU's per disk
 - Directory starts at logical track 4;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AC 00 3F 00 80 00 10 00 04 00 01 01 
============================================================
Disk Name: Teletek SystemMaster    DS      
Type: 5 1/4     Total usable space: 346k bytes
  
Sector information: 
 - 256 bytes/sector;  18 per track; numbered 1 to 18 (Side 2 numbered 1 to 18)
 - Disk is filled all first side, then second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 6 12 1 7 13 2 8 14 3 9 15 4 10 16 5 11 17 
 
 - Allocation unit size is 2048 bytes; 173 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AC 00 7F 00 C0 00 20 00 03 00 01 01 
============================================================
Disk Name: Tomcat 1800G            DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 2 6 1 5 9 3 7 
 
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 00 C2 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Toshiba T-100           DS      
Type: 5 1/4     Total usable space: 256k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 12 1 5 9 13 2 6 10 14 3 7 11 15 16 20 24 28 17 21 25 29 18 22 26 30 19 23 27 31
 
 - Allocation unit size is 1024 bytes; 256 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    40 00 03 07 00 FF 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Toshiba T-200           DS      
Type: 5 1/4     Total usable space: 256k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 4 8 12 1 5 9 13 2 6 10 14 3 7 11 15 
 
 - Allocation unit size is 1024 bytes; 256 AU's per disk
 - Directory starts at logical track 6;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 FF 00 3F 00 C0 00 10 00 06 00 01 01 
============================================================
Disk Name: Wang-Writer             DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9B 00 7F 00 C0 00 20 00 02 00 01 01 
============================================================
Disk Name: Wavemate Bullet         SS      
Type: 5 1/4     Total usable space: 190k bytes
  
Sector information: 
 - 1024 bytes/sector;   5 per track; numbered 1 to 5  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 190 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 2 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 03 07 00 BD 00 3F 00 C0 00 10 00 02 00 03 07 
============================================================
Disk Name: XOR-5                   DS      
Type: 5 1/4     Total usable space: 384k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 1 to 10)
 - Disk is filled track 0, first side, then track 0, second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 5 1 6 2 7 3 8 4 9 
 
 - Allocation unit size is 2048 bytes; 192 AU's per disk
 - Directory starts at logical track 3;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 BF 00 7F 00 C0 00 20 00 03 00 02 03 
============================================================
Disk Name: Xerox 16/8              DS      
Type: 5 1/4     Total usable space: 342k bytes
  
Sector information: 
 - 512 bytes/sector;   9 per track; numbered 1 to 9 (Side 2 numbered 1 to 9)
 - Disk is filled all first side, then second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 171 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    24 00 04 0F 01 AA 00 7F 00 C0 00 20 00 02 00 02 03 
============================================================
Disk Name: Xerox 820               SSSD    
Type: 5 1/4     Total usable space: 83k bytes
  
Sector information: 
 - 128 bytes/sector;  18 per track; numbered 1 to 18  
 
Logical Layout:
 - Sector order logical fill table (soft skew): 
      0 5 10 15 2 7 12 17 4 9 14 1 6 11 16 3 8 13 
 
 - Allocation unit size is 1024 bytes; 83 AU's per disk
 - Directory starts at logical track 3;
     has 32 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    12 00 03 07 00 52 00 1F 00 80 00 08 00 03 00 00 00 
============================================================
Disk Name: Xerox 820-II            DS      
Type: 5 1/4     Total usable space: 326k bytes
  
Sector information: 
 - 256 bytes/sector;  17 per track; numbered 1 to 17 (Side 2 numbered 1 to 17)
 - Disk is filled all first side, then second side 
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 163 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    22 00 04 0F 01 A2 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Xerox 820-II            SS      
Type: 5 1/4     Total usable space: 157k bytes
  
Sector information: 
 - 256 bytes/sector;  17 per track; numbered 1 to 17  
 - System tracks are formatted differently than data tracks.
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 157 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    22 00 03 07 00 9C 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Xerox/Sunrise Laptop    SS      
Type: 5 1/4     Total usable space: 156k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 156 AU's per disk
 - Directory starts at logical track 1;
     has 64 entries and occupies 4 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 9B 00 3F 00 C0 00 10 00 01 00 02 03 
============================================================
Disk Name: Zenith Z-100            DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8 (Side 2 numbered 1 to 8)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 2;
     has 256 entries and occupies 16 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 01 9B 00 FF 00 F0 00 40 00 02 00 02 03 
============================================================
Disk Name: Zenith Z-100            SS      
Type: 5 1/4     Total usable space: 152k bytes
  
Sector information: 
 - 512 bytes/sector;   8 per track; numbered 1 to 8  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 8 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 97 00 7F 00 F0 00 20 00 02 00 02 03 
============================================================
Disk Name: Zenith Z-37             SSSD    
Type: 5 1/4     Total usable space: 92k bytes
  
Sector information: 
 - 256 bytes/sector;  10 per track; numbered 1 to 10  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 92 AU's per disk
 - Directory starts at logical track 3;
     has 64 entries and occupies 8 sectors or 2 AU's
 
Standard disk parameter table entry (values in HEX):
    14 00 03 07 00 5B 00 3F 00 C0 00 10 00 03 00 01 01 
============================================================
Disk Name: Zenith Z-89/90          DS      
Type: 5 1/4     Total usable space: 312k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16 (Side 2 numbered 1 to 16)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 156 AU's per disk
 - Directory starts at logical track 2;
     has 256 entries and occupies 32 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 04 0F 00 9B 00 FF 00 F0 00 40 00 02 00 01 01 
============================================================
Disk Name: Zenith Z-90             SS      
Type: 5 1/4     Total usable space: 152k bytes
  
Sector information: 
 - 256 bytes/sector;  16 per track; numbered 1 to 16  
 
Logical Layout:
 - Allocation unit size is 1024 bytes; 152 AU's per disk
 - Directory starts at logical track 2;
     has 128 entries and occupies 16 sectors or 4 AU's
 
Standard disk parameter table entry (values in HEX):
    20 00 03 07 00 97 00 7F 00 F0 00 20 00 02 00 01 01 
============================================================
Disk Name: Zorba                   DS      
Type: 5 1/4     Total usable space: 390k bytes
  
Sector information: 
 - 512 bytes/sector;  10 per track; numbered 1 to 10 (Side 2 numbered 11 to 20)
 - Disk is filled track 0, first side, then track 0, second side 
 
Logical Layout:
 - Allocation unit size is 2048 bytes; 195 AU's per disk
 - Directory starts at logical track 2;
     has 64 entries and occupies 4 sectors or 1 AU's
 
Standard disk parameter table entry (values in HEX):
    28 00 04 0F 01 C2 00 3F 00 80 00 10 00 02 00 02 03