(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.58)
  )

  (paper "A4")
  (title_block
    (title "PC/104 80188 CPU Board")
    (rev "0.2")
    (company "Atsuko Ito")
  )

  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.11) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.2) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.11) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "HAL lead-free")
      (dielectric_constraints yes)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 88.519 53.883)
    (grid_origin 162.179 84.328)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "/X2")
  (net 2 "GND")
  (net 3 "/X1")
  (net 4 "VCC")
  (net 5 "XA16")
  (net 6 "~{RD}")
  (net 7 "BCLK")
  (net 8 "~{S2}")
  (net 9 "INT3")
  (net 10 "~{DEN}")
  (net 11 "~{UCS}")
  (net 12 "~{PCS6}")
  (net 13 "~{PCS4}")
  (net 14 "DRQ0")
  (net 15 "A12")
  (net 16 "A13")
  (net 17 "A14")
  (net 18 "A15")
  (net 19 "XA17")
  (net 20 "XA19")
  (net 21 "~{WR}")
  (net 22 "unconnected-(U202-Pad7)")
  (net 23 "INT1")
  (net 24 "DT{slash}~{R}")
  (net 25 "~{LCS}")
  (net 26 "~{PCS5}")
  (net 27 "~{PCS3}")
  (net 28 "~{CS_S}")
  (net 29 "DRQ1")
  (net 30 "A8")
  (net 31 "A9")
  (net 32 "A10")
  (net 33 "A11")
  (net 34 "XA18")
  (net 35 "~{CARDSLCTD}")
  (net 36 "~{SMEMW}")
  (net 37 "~{SMEMR}")
  (net 38 "~{IOW}")
  (net 39 "~{IOR}")
  (net 40 "IR7")
  (net 41 "IR6")
  (net 42 "IR5")
  (net 43 "IR4")
  (net 44 "DB7")
  (net 45 "DB6")
  (net 46 "DB5")
  (net 47 "DB4")
  (net 48 "DB3")
  (net 49 "DB2")
  (net 50 "DB1")
  (net 51 "DB0")
  (net 52 "A19")
  (net 53 "A18")
  (net 54 "A17")
  (net 55 "A16")
  (net 56 "A7")
  (net 57 "A6")
  (net 58 "A5")
  (net 59 "A4")
  (net 60 "A3")
  (net 61 "A2")
  (net 62 "A1")
  (net 63 "A0")
  (net 64 "M{slash}~{IO}")
  (net 65 "~{BEN}")
  (net 66 "Net-(C305-Pad2)")
  (net 67 "unconnected-(Y1-Pad2)")
  (net 68 "unconnected-(Y1-Pad4)")
  (net 69 "~{CS_RTC}")
  (net 70 "unconnected-(J102-Pad10)")
  (net 71 "RESOUT")
  (net 72 "UART1.~{RTS}")
  (net 73 "TMR_OUT_0")
  (net 74 "UART1.IN")
  (net 75 "UART1.OUT")
  (net 76 "UART1.~{CTS}")
  (net 77 "UART2.~{CD}")
  (net 78 "VBAT")
  (net 79 "AD7")
  (net 80 "AD6")
  (net 81 "AD5")
  (net 82 "AD4")
  (net 83 "AD3")
  (net 84 "AD2")
  (net 85 "AD1")
  (net 86 "AD0")
  (net 87 "Net-(SW301-Pad2)")
  (net 88 "USB.~{DCD}")
  (net 89 "USB.~{PWREN}")
  (net 90 "INT2")
  (net 91 "Net-(U303-Pad31)")
  (net 92 "Net-(U303-Pad30)")
  (net 93 "unconnected-(U303-Pad26)")
  (net 94 "unconnected-(U202-Pad8)")
  (net 95 "unconnected-(J201-Pad1)")
  (net 96 "unconnected-(J201-Pad11)")
  (net 97 "unconnected-(J201-Pad13)")
  (net 98 "UART2.RX")
  (net 99 "UART2.TX")
  (net 100 "UART2.~{DTR}")
  (net 101 "unconnected-(U202-Pad9)")
  (net 102 "unconnected-(U202-Pad12)")
  (net 103 "unconnected-(U202-Pad13)")
  (net 104 "unconnected-(U202-Pad14)")
  (net 105 "USB.~{RESET}")
  (net 106 "DCD")
  (net 107 "UART2.~{DSR}")
  (net 108 "unconnected-(U301-Pad6)")
  (net 109 "UART2.~{RTS}")
  (net 110 "unconnected-(U301-Pad9)")
  (net 111 "UART2.~{CTS}")
  (net 112 "unconnected-(U301-Pad12)")
  (net 113 "UART2.~{RI}")
  (net 114 "unconnected-(U301-Pad18)")
  (net 115 "unconnected-(J302-Pad10)")
  (net 116 "~{CS_S2}")
  (net 117 "~{CS_S1}")
  (net 118 "unconnected-(U301-Pad24)")
  (net 119 "unconnected-(U301-Pad25)")
  (net 120 "~{PCS2}")
  (net 121 "unconnected-(U301-Pad31)")
  (net 122 "RTC.~{IRQ}")
  (net 123 "UART1.~{RI}")
  (net 124 "unconnected-(U301-Pad37)")
  (net 125 "unconnected-(U301-Pad43)")
  (net 126 "Net-(C306-Pad1)")
  (net 127 "UART1.~{DTR}")
  (net 128 "UART1.~{DSR}")
  (net 129 "INT0")
  (net 130 "unconnected-(Y301-Pad2)")
  (net 131 "unconnected-(Y301-Pad4)")
  (net 132 "ROM.A9")
  (net 133 "ROM.~{OE}")
  (net 134 "ISP.VCC")
  (net 135 "ROM.~{WE}")
  (net 136 "CS2")
  (net 137 "unconnected-(J101-Pad2)")
  (net 138 "unconnected-(J101-Pad9)")
  (net 139 "unconnected-(J101-Pad13)")
  (net 140 "unconnected-(J101-Pad17)")
  (net 141 "unconnected-(J101-Pad20)")
  (net 142 "unconnected-(J101-Pad22)")
  (net 143 "unconnected-(J101-Pad31)")
  (net 144 "unconnected-(J101-Pad53)")
  (net 145 "Net-(J103-Pad20)")
  (net 146 "Net-(J103-Pad21)")
  (net 147 "Net-(J103-Pad23)")
  (net 148 "NMI")
  (net 149 "unconnected-(J103-Pad35)")
  (net 150 "unconnected-(J103-Pad36)")
  (net 151 "unconnected-(J103-Pad37)")
  (net 152 "unconnected-(J103-Pad38)")
  (net 153 "Net-(J103-Pad47)")
  (net 154 "unconnected-(J103-Pad48)")
  (net 155 "Net-(J103-Pad49)")
  (net 156 "unconnected-(J103-Pad51)")
  (net 157 "unconnected-(J103-Pad52)")
  (net 158 "unconnected-(J103-Pad53)")
  (net 159 "Net-(J103-Pad55)")
  (net 160 "unconnected-(J103-Pad64)")
  (net 161 "unconnected-(J104-Pad1)")
  (net 162 "~{RESET}")
  (net 163 "unconnected-(U101-Pad1)")
  (net 164 "ALE")
  (net 165 "Net-(J304-Pad1)")
  (net 166 "Net-(J304-Pad2)")
  (net 167 "Net-(J304-Pad3)")
  (net 168 "Net-(J304-Pad4)")
  (net 169 "Net-(J304-Pad5)")
  (net 170 "Net-(J304-Pad6)")
  (net 171 "Net-(J304-Pad7)")
  (net 172 "Net-(J304-Pad8)")
  (net 173 "unconnected-(J304-Pad10)")
  (net 174 "Net-(J305-Pad1)")
  (net 175 "Net-(J305-Pad2)")
  (net 176 "Net-(J305-Pad3)")
  (net 177 "Net-(J305-Pad4)")
  (net 178 "Net-(J305-Pad5)")
  (net 179 "Net-(J305-Pad6)")
  (net 180 "Net-(J305-Pad7)")
  (net 181 "Net-(J305-Pad8)")
  (net 182 "unconnected-(J305-Pad10)")
  (net 183 "P2.~{CS}")
  (net 184 "unconnected-(U304-Pad10)")
  (net 185 "unconnected-(U304-Pad11)")
  (net 186 "unconnected-(U304-Pad12)")
  (net 187 "unconnected-(U304-Pad13)")
  (net 188 "unconnected-(U304-Pad14)")
  (net 189 "unconnected-(U304-Pad15)")
  (net 190 "unconnected-(U304-Pad16)")
  (net 191 "P2.~{IRQ}")

  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 00120ce5-cea2-43e7-a366-060498189dc5)
    (at 135.001 100.203 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (path "/fe7305e5-1dd2-49d0-b6b8-d902feb5e0af")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP101" (at 0 -1.448) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a7e4b8a-4aaa-408f-8b79-5b5f1c60c53c)
    )
    (fp_text value "XTAL" (at 0 1.55) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3f8f1c14-a20e-4d87-84f4-f09ea7a51d55)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c52dde4c-4f8b-40b8-8988-34cf3321ab3b)
    )
    (fp_line (start -0.7 -0.7) (end 0.7 -0.7) (layer "F.SilkS") (width 0.12) (tstamp 25322c6b-0d18-4dd6-a890-d3a2aacffcd4))
    (fp_line (start -0.7 0.7) (end -0.7 -0.7) (layer "F.SilkS") (width 0.12) (tstamp 64389b6f-b407-4d57-9445-ffb25c50972a))
    (fp_line (start 0.7 0.7) (end -0.7 0.7) (layer "F.SilkS") (width 0.12) (tstamp bcfda91e-5bcc-4126-8b34-237a9c3f9299))
    (fp_line (start 0.7 -0.7) (end 0.7 0.7) (layer "F.SilkS") (width 0.12) (tstamp d7839a49-3961-48b9-a998-e0e1c6f6c835))
    (fp_line (start -1 -1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp 256b1de5-1bb3-47bc-9b38-d215f4e24be3))
    (fp_line (start 1 1) (end 1 -1) (layer "F.CrtYd") (width 0.05) (tstamp 6a6d246c-5233-4370-a55a-f4395f9bd297))
    (fp_line (start 1 1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp 8cb3c7f9-5937-4e73-9c30-e5ef46a7add8))
    (fp_line (start -1 -1) (end 1 -1) (layer "F.CrtYd") (width 0.05) (tstamp a7cf1266-2560-4c5b-89bd-3489dda5d58f))
    (pad "1" smd rect (at 0 0 180) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 3 "/X1") (pinfunction "1") (pintype "passive") (tstamp 74e0a7da-a1ce-4360-87e4-598e8f98814f))
  )

  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1) (tstamp 0f69863e-85e9-4bea-8c41-d01e3b007b9c)
    (at 101.981 121.666 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Manufacturer_Name" "Texas Instruments")
    (property "Manufacturer_Part_Number" "MC74HCT245ADWG")
    (property "Mouser Part Number" "863-MC74HCT245ADWG")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/f5f5d2d6-51cd-4fef-9a0f-fba48c9f9e37")
    (attr smd)
    (fp_text reference "U203" (at 3.937 -7.223) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f0eca60f-9cbe-42f7-aee1-e168e7e820c2)
    )
    (fp_text value "74LS245" (at 0.0272 7.239) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e06302a1-0cdc-4787-b2f1-2051001738ff)
    )
    (fp_text user "${REFERENCE}" (at 0.381 0.127) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f09d2f72-7224-4aed-93c8-708c17b349b7)
    )
    (fp_line (start 3.86 -6.51) (end 3.86 -6.275) (layer "F.SilkS") (width 0.12) (tstamp 1a435bd2-2652-490d-8cb7-a38dc9e3836b))
    (fp_line (start -3.86 6.51) (end -3.86 6.275) (layer "F.SilkS") (width 0.12) (tstamp 1bb6129a-35cd-4f41-ac2d-f54e5bf0b6f5))
    (fp_line (start 0 6.51) (end -3.86 6.51) (layer "F.SilkS") (width 0.12) (tstamp 45bf6f7a-60f1-40ab-87f6-66627da1a844))
    (fp_line (start -3.86 -6.275) (end -5.675 -6.275) (layer "F.SilkS") (width 0.12) (tstamp 892129b4-6d0c-4876-b64f-9d11fcd28562))
    (fp_line (start 0 -6.51) (end -3.86 -6.51) (layer "F.SilkS") (width 0.12) (tstamp b9b9c9ab-3377-40bd-9065-60efa485046d))
    (fp_line (start 0 6.51) (end 3.86 6.51) (layer "F.SilkS") (width 0.12) (tstamp cddb63cf-406b-42df-a512-3d36a6b6c538))
    (fp_line (start 0 -6.51) (end 3.86 -6.51) (layer "F.SilkS") (width 0.12) (tstamp ec8f9f87-5337-48a0-8872-fdbcf4605790))
    (fp_line (start -3.86 -6.51) (end -3.86 -6.275) (layer "F.SilkS") (width 0.12) (tstamp f603d1f0-5636-426c-b797-3b22febacbc9))
    (fp_line (start 3.86 6.51) (end 3.86 6.275) (layer "F.SilkS") (width 0.12) (tstamp fc546f08-ed25-4881-a75a-2fea1e566f52))
    (fp_line (start -5.93 -6.65) (end -5.93 6.65) (layer "F.CrtYd") (width 0.05) (tstamp 38f92d8e-d70a-4222-86c4-6cd33d6d9a0a))
    (fp_line (start 5.93 -6.65) (end -5.93 -6.65) (layer "F.CrtYd") (width 0.05) (tstamp 649df29d-0113-4a7c-adc5-8a7828f55d24))
    (fp_line (start 5.93 6.65) (end 5.93 -6.65) (layer "F.CrtYd") (width 0.05) (tstamp aa2b5b47-a9c3-495a-a311-46aa720b7dae))
    (fp_line (start -5.93 6.65) (end 5.93 6.65) (layer "F.CrtYd") (width 0.05) (tstamp b9e7ce92-9915-4da5-8de0-e06db2d5ff4a))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer "F.Fab") (width 0.1) (tstamp a15aabb6-c531-4578-a7a6-858a6b477f8c))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer "F.Fab") (width 0.1) (tstamp ad947b2b-a043-4ba0-96c4-f76674535a76))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer "F.Fab") (width 0.1) (tstamp dd5bd0cf-758a-4912-8dcb-94168c8c0bf1))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer "F.Fab") (width 0.1) (tstamp e096383b-fa75-482c-98ed-9d42650bc8f6))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer "F.Fab") (width 0.1) (tstamp f027f58c-90b9-4bd1-8d91-fbbd4a94dba0))
    (pad "1" smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "DT{slash}~{R}") (pinfunction "A->B") (pintype "input") (tstamp 78386820-eb7f-4717-b95e-c082e8b42009))
    (pad "2" smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "AD0") (pinfunction "A0") (pintype "tri_state") (tstamp 6af9802a-d821-4f8d-9596-52657c9d659d))
    (pad "3" smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "AD1") (pinfunction "A1") (pintype "tri_state") (tstamp b0530e2c-26ef-4e09-92d2-859f599cb379))
    (pad "4" smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "AD2") (pinfunction "A2") (pintype "tri_state") (tstamp 0fcdbc03-dccd-415d-ad76-bf4219f51b12))
    (pad "5" smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "AD3") (pinfunction "A3") (pintype "tri_state") (tstamp 6e3718f2-5630-4781-a465-1399c214d8e6))
    (pad "6" smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "AD4") (pinfunction "A4") (pintype "tri_state") (tstamp bf187f20-34c0-4c64-9c9c-d232c218fabe))
    (pad "7" smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "AD5") (pinfunction "A5") (pintype "tri_state") (tstamp 9c95e5d5-dc46-4da7-8945-3550ab49c59a))
    (pad "8" smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "AD6") (pinfunction "A6") (pintype "tri_state") (tstamp 5426355d-3ae6-490b-95e8-d02d9cc0ad27))
    (pad "9" smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "AD7") (pinfunction "A7") (pintype "tri_state") (tstamp b3340c50-db3c-4c5d-aeda-b007a0d0d56b))
    (pad "10" smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7823daf3-3e7d-40f2-84bd-4e09ca4c30f7))
    (pad "11" smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "DB7") (pinfunction "B7") (pintype "tri_state") (tstamp af7613f2-b35d-4fcd-bd60-548fdd25175a))
    (pad "12" smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "DB6") (pinfunction "B6") (pintype "tri_state") (tstamp 4b8262cf-c784-4d7d-bdb1-d85a28592f03))
    (pad "13" smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "DB5") (pinfunction "B5") (pintype "tri_state") (tstamp 5885843b-7c6f-4bdc-8bbd-ea37b1dfd9a9))
    (pad "14" smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "DB4") (pinfunction "B4") (pintype "tri_state") (tstamp 38bebe59-7711-40db-8a4d-dfe0b8eb1e9f))
    (pad "15" smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "DB3") (pinfunction "B3") (pintype "tri_state") (tstamp 2682205e-31b1-4115-9bc3-b5cbf11e6534))
    (pad "16" smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "DB2") (pinfunction "B2") (pintype "tri_state") (tstamp 326393f2-509a-4d7d-a61a-f80287417265))
    (pad "17" smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "DB1") (pinfunction "B1") (pintype "tri_state") (tstamp b109bedc-48ca-408a-9986-4e795f958a8b))
    (pad "18" smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "DB0") (pinfunction "B0") (pintype "tri_state") (tstamp ad307c57-133a-4d38-bb4f-cb67c23b0bf9))
    (pad "19" smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "~{BEN}") (pinfunction "CE") (pintype "input") (tstamp b568e616-e018-4d01-8de2-6d1b9d245fc9))
    (pad "20" smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 3a7783d2-8e0a-4f61-b38c-959910d59cfc))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 12fb8895-395d-4901-9f1b-bca198430a0f)
    (at 135.001 97.028 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "C0805C220J1GACTU")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/c22beccf-154c-471a-a02e-a783efb16894")
    (attr smd)
    (fp_text reference "C101" (at -0.127 -2.159 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a546a891-9b17-4995-887d-31474bfe656d)
    )
    (fp_text value "22p XTAL" (at 0 1.68 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f55be682-7f00-4a6d-9b40-a44b74164700)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp d4908c22-097a-4bb9-b27e-32d2754ea2f7)
    )
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp 36aac805-2ae9-4815-af06-ba12ddc45e00))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 646c3aa7-4c15-4f2a-be4f-56146f8f3c41))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 03f21012-fbc5-461c-9f93-632125f0c73d))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 0a6001db-02ae-4d63-aae4-b0f5da456645))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 4adb21e8-f876-41d7-9dd8-8ca6a1e4f3be))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 66094f1d-800c-49d8-b392-b1e90f09284a))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 5fec07fd-90f1-4f38-b7ad-a76ec3c64058))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp cca6f319-1945-4095-8fbc-d96016808d7d))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp cde0fa3f-eaf7-473b-9135-9f4145caaf3e))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp de76fb4f-788b-4a3b-b664-3946406e63ea))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive") (tstamp 8532190a-2446-45b5-b1b8-27fa0a5d11e1))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "/X1") (pintype "passive") (tstamp 0cdfb605-0053-4621-997d-9fc85dc9c2a3))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3) (tstamp 1692a95b-07a5-4cfa-ad6d-bd609c2e3b32)
    (at 149.479 130.048 180)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/d7c97edb-529c-4b86-9ff7-e8e8e91c8c64")
    (attr through_hole)
    (fp_text reference "J204" (at 0.635 -1.695) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef8f4047-cb55-48f3-a860-37909f8f1ff7)
    )
    (fp_text value "ISPEXT" (at 3.556 3.556 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 046e1274-446d-4276-82d9-0937d3d4ea15)
    )
    (fp_text user "${REFERENCE}" (at 0.635 2.54 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6eec7a3-74c8-446d-9020-61884eab3e22)
    )
    (fp_line (start -1.13 0.76) (end -0.563471 0.76) (layer "F.SilkS") (width 0.12) (tstamp 24506f2d-3035-4df8-b27f-83d5d79b2e33))
    (fp_line (start -1.13 5.775) (end -0.30753 5.775) (layer "F.SilkS") (width 0.12) (tstamp 25da8667-d387-4fcd-8184-ef46d3401d48))
    (fp_line (start -1.13 -0.76) (end 0 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 2a6688dc-a5ba-4cfb-9d08-71c6f880a1cf))
    (fp_line (start 1.57753 5.775) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 3bb965dd-5573-4642-9c63-5cd31e8b66d5))
    (fp_line (start 0.563471 0.76) (end 0.706529 0.76) (layer "F.SilkS") (width 0.12) (tstamp 3bfc3ea2-93ca-4e08-80f1-41c93658da83))
    (fp_line (start 2.4 -0.695) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 48384556-aeb0-4b11-84d7-9d24e8d96e74))
    (fp_line (start -1.13 0.76) (end -1.13 5.775) (layer "F.SilkS") (width 0.12) (tstamp 4fb884c9-dc0a-4c8b-ba2c-e99ab8ded798))
    (fp_line (start 0.30753 5.775) (end 0.96247 5.775) (layer "F.SilkS") (width 0.12) (tstamp 51bd37f9-3964-4bb9-aed5-594001d6da44))
    (fp_line (start 1.57753 -0.695) (end 2.4 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 5d6856ca-11f3-4c42-8239-03daff8b18d0))
    (fp_line (start 0.76 0.706529) (end 0.76 0.563471) (layer "F.SilkS") (width 0.12) (tstamp a5dd618b-2c21-43ff-869c-6eee7b863379))
    (fp_line (start 0.76 -0.695) (end 0.96247 -0.695) (layer "F.SilkS") (width 0.12) (tstamp bb10123a-c65d-4d47-9b15-d1adb8e38d21))
    (fp_line (start -1.13 0) (end -1.13 -0.76) (layer "F.SilkS") (width 0.12) (tstamp d77b2da9-ca8e-40ec-bfb3-aefe28ac915f))
    (fp_line (start 0.76 -0.563471) (end 0.76 -0.695) (layer "F.SilkS") (width 0.12) (tstamp dfc1258a-94e2-4c1d-a0f4-11592f06e3d1))
    (fp_line (start -1.6 6.25) (end 2.85 6.25) (layer "F.CrtYd") (width 0.05) (tstamp 1c6b1f85-f47a-4eee-b1b2-4f2cb91036f9))
    (fp_line (start -1.6 -1.15) (end -1.6 6.25) (layer "F.CrtYd") (width 0.05) (tstamp e8b087ff-4d07-41d4-8bce-6d5151690057))
    (fp_line (start 2.85 6.25) (end 2.85 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp f1072060-32a4-40c0-86ce-311165e40283))
    (fp_line (start 2.85 -1.15) (end -1.6 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp f279077b-e34d-43c6-9a49-a57dfa3970c0))
    (fp_line (start -0.2175 -0.635) (end 2.34 -0.635) (layer "F.Fab") (width 0.1) (tstamp 41012f7d-ba65-4723-a315-4ded91405182))
    (fp_line (start 2.34 -0.635) (end 2.34 5.715) (layer "F.Fab") (width 0.1) (tstamp 7385365f-5cab-40d2-a459-8984db764cf1))
    (fp_line (start 2.34 5.715) (end -1.07 5.715) (layer "F.Fab") (width 0.1) (tstamp 9936586c-e3d9-4296-b675-d4b08645e392))
    (fp_line (start -1.07 0.2175) (end -0.2175 -0.635) (layer "F.Fab") (width 0.1) (tstamp b01ff610-e6f9-49ae-b159-336410d93de2))
    (fp_line (start -1.07 5.715) (end -1.07 0.2175) (layer "F.Fab") (width 0.1) (tstamp e16cef73-05e7-4427-bfd0-44e9d133bcb2))
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 132 "ROM.A9") (pinfunction "Pin_1") (pintype "passive") (tstamp d75a1129-ebe5-47c7-b420-ce60efca8c12))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 135 "ROM.~{WE}") (pinfunction "Pin_2") (pintype "passive") (tstamp 0c3f9258-be2b-48de-9259-170d3e5cce90))
    (pad "3" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 133 "ROM.~{OE}") (pinfunction "Pin_3") (pintype "passive") (tstamp e4946259-4869-499c-8a6c-311ca76a35db))
    (pad "4" thru_hole oval (at 1.27 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 "~{WR}") (pinfunction "Pin_4") (pintype "passive") (tstamp 4dc0ddd7-197a-40cd-8c64-42a87437aa00))
    (pad "5" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "~{RD}") (pinfunction "Pin_5") (pintype "passive") (tstamp d249f484-be7b-4fe1-aa74-bf5965c8a2c2))
    (pad "6" thru_hole oval (at 1.27 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 136 "CS2") (pinfunction "Pin_6") (pintype "passive") (tstamp 3a535556-5e25-4fcf-a17e-bd40bafcf69c))
    (pad "7" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 134 "ISP.VCC") (pinfunction "Pin_7") (pintype "passive") (tstamp 00f595a2-1b5e-4a98-82a4-f83b05ad9825))
    (pad "8" thru_hole oval (at 1.27 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "~{UCS}") (pinfunction "Pin_8") (pintype "passive") (tstamp c729c227-f54f-465a-9b2c-cfdee87f49c5))
    (pad "9" thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 162 "~{RESET}") (pinfunction "Pin_9") (pintype "passive") (tstamp 9f094e99-1ec6-4311-abdd-a9316cf268d1))
    (pad "10" thru_hole oval (at 1.27 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 "~{LCS}") (pinfunction "Pin_10") (pintype "passive") (tstamp 31693bcb-e71c-4eae-ac61-1ee67b70608e))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3) (tstamp 1f8201c0-e94b-40eb-8f4e-26bb744b5874)
    (at 91.8015 97.018)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/adca42af-191e-4401-80fe-2159341409b7")
    (attr through_hole)
    (fp_text reference "J304" (at 0.635 -1.695) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16825289-ec46-408e-a133-54d918a7c136)
    )
    (fp_text value "PB" (at -2.423 0.01 270 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 91d2c54e-e6a7-4f6e-a10e-9f46a4848ec2)
    )
    (fp_text user "${REFERENCE}" (at 0.635 2.54 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f929714-6d79-4737-9a60-5c925e7045a4)
    )
    (fp_line (start 2.4 -0.695) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 020edd20-1505-4efe-a572-614dbe221edf))
    (fp_line (start 0.76 -0.563471) (end 0.76 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 0afba8aa-be14-4234-ae62-42108f7161b6))
    (fp_line (start -1.13 0.76) (end -1.13 5.775) (layer "F.SilkS") (width 0.12) (tstamp 0b037373-9230-4c49-917c-22980c5818db))
    (fp_line (start 0.76 0.706529) (end 0.76 0.563471) (layer "F.SilkS") (width 0.12) (tstamp 1864fbae-4e08-498c-8396-4dc3c2e2a3f7))
    (fp_line (start -1.13 0) (end -1.13 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 416363e5-624e-4194-8ed2-0fbc7bd60eff))
    (fp_line (start -1.13 -0.76) (end 0 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 4df31b09-b046-4426-a132-dcc07bd12661))
    (fp_line (start -1.13 0.76) (end -0.563471 0.76) (layer "F.SilkS") (width 0.12) (tstamp 580a8a9f-b0d2-4c20-bfee-c915fe9de5bf))
    (fp_line (start -1.13 5.775) (end -0.30753 5.775) (layer "F.SilkS") (width 0.12) (tstamp 58c1fba5-9708-478a-9fa4-6a13c87772e9))
    (fp_line (start 1.57753 5.775) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 603a54d7-84b2-4688-93a4-65f2df63ff30))
    (fp_line (start 0.30753 5.775) (end 0.96247 5.775) (layer "F.SilkS") (width 0.12) (tstamp 9f7750af-379d-44c1-9c6c-4c249c3b8b78))
    (fp_line (start 0.563471 0.76) (end 0.706529 0.76) (layer "F.SilkS") (width 0.12) (tstamp ac6b18b3-1bd7-4dfa-92b7-4b7dbf1eb570))
    (fp_line (start 0.76 -0.695) (end 0.96247 -0.695) (layer "F.SilkS") (width 0.12) (tstamp c8836ff9-3eb9-4691-b243-154c2136af50))
    (fp_line (start 1.57753 -0.695) (end 2.4 -0.695) (layer "F.SilkS") (width 0.12) (tstamp d4223d17-b671-45bc-90fc-ee0474fe4294))
    (fp_line (start -1.6 -1.15) (end -1.6 6.25) (layer "F.CrtYd") (width 0.05) (tstamp 12d0b4fd-662d-470c-915c-3a74103e97e0))
    (fp_line (start -1.6 6.25) (end 2.85 6.25) (layer "F.CrtYd") (width 0.05) (tstamp 4ee5b44a-7145-44ff-a40a-e71f9d406dc6))
    (fp_line (start 2.85 -1.15) (end -1.6 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp bee79f7a-9a84-4cda-950c-ab528c18286b))
    (fp_line (start 2.85 6.25) (end 2.85 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp e14b0e3f-4b72-4912-ab1d-a4cc52b96a13))
    (fp_line (start 2.34 -0.635) (end 2.34 5.715) (layer "F.Fab") (width 0.1) (tstamp 139e2c2c-b47b-4bb0-97f9-7beb5a94364c))
    (fp_line (start 2.34 5.715) (end -1.07 5.715) (layer "F.Fab") (width 0.1) (tstamp 635358bc-f649-4300-a365-17c7c531405d))
    (fp_line (start -1.07 0.2175) (end -0.2175 -0.635) (layer "F.Fab") (width 0.1) (tstamp 655d82f1-1eda-4d5f-8208-5d2b47db5e1b))
    (fp_line (start -0.2175 -0.635) (end 2.34 -0.635) (layer "F.Fab") (width 0.1) (tstamp 6e580fdc-59b8-4360-a227-1038290fc578))
    (fp_line (start -1.07 5.715) (end -1.07 0.2175) (layer "F.Fab") (width 0.1) (tstamp 749385c6-d9c2-49a6-8088-107d097ab0bb))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 165 "Net-(J304-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 0b72ab9b-aea7-43e6-bd6e-e5196279eaf6))
    (pad "2" thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 166 "Net-(J304-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp f511800b-f435-4eab-8e7b-0e45c768c279))
    (pad "3" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 167 "Net-(J304-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp 727782a3-7fc7-4d7c-a813-1333f708b8d3))
    (pad "4" thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 168 "Net-(J304-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp eb9c381c-9e6e-47ac-8911-3ada812ebc5c))
    (pad "5" thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 169 "Net-(J304-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp c4a23832-dd6c-449f-be19-5a1cabbeaebf))
    (pad "6" thru_hole oval (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 170 "Net-(J304-Pad6)") (pinfunction "Pin_6") (pintype "passive") (tstamp e74020f8-ab98-47a6-8dbc-cefc7c36aa37))
    (pad "7" thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 171 "Net-(J304-Pad7)") (pinfunction "Pin_7") (pintype "passive") (tstamp 53b855f6-16a9-499b-b615-56bdc6be97c8))
    (pad "8" thru_hole oval (at 1.27 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 172 "Net-(J304-Pad8)") (pinfunction "Pin_8") (pintype "passive") (tstamp 0b68b101-43d4-40be-89ec-69e43c6b6295))
    (pad "9" thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive") (tstamp 6e532fd1-2fee-4ead-8b95-7693c10fa172))
    (pad "10" thru_hole oval (at 1.27 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 173 "unconnected-(J304-Pad10)") (pinfunction "Pin_10") (pintype "passive") (tstamp 8929376f-803b-4214-8b8a-4f87e17296b4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1) (tstamp 1fa5a828-f463-4f99-b234-116f3dfae9ba)
    (at 135.255 123.698 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Manufacturer_Part_Number" "74VHCT573AFT")
    (property "RS" "")
    (property "RS Part Number" "171-3540")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/775615af-9bb8-41b9-8613-75d20ffa627e")
    (attr smd)
    (fp_text reference "U202" (at 0 -7.35) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 345bfc57-f522-4066-b8f1-5f39ae06e70a)
    )
    (fp_text value "74LS573" (at 0 7.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d543f8c9-08c9-44f1-a659-8e4861b5107f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf50dc04-4120-4b41-9c73-eae7246c7adc)
    )
    (fp_line (start 0 6.51) (end 3.86 6.51) (layer "F.SilkS") (width 0.12) (tstamp 0790b5fe-5611-4175-b261-e4e552b94a8d))
    (fp_line (start -3.86 -6.51) (end -3.86 -6.275) (layer "F.SilkS") (width 0.12) (tstamp 10e1025e-9d9f-46bc-a78d-5f263b936f96))
    (fp_line (start 3.86 -6.51) (end 3.86 -6.275) (layer "F.SilkS") (width 0.12) (tstamp 309d1670-708d-4ec4-896a-47824ce39685))
    (fp_line (start 3.86 6.51) (end 3.86 6.275) (layer "F.SilkS") (width 0.12) (tstamp 7978e6e6-40e2-4b2c-b726-863ad4b4f390))
    (fp_line (start 0 -6.51) (end 3.86 -6.51) (layer "F.SilkS") (width 0.12) (tstamp 959ea80f-5201-4104-a212-6f90e8fa6aa3))
    (fp_line (start 0 6.51) (end -3.86 6.51) (layer "F.SilkS") (width 0.12) (tstamp a59c8853-49be-46a4-8375-7ac7442c905f))
    (fp_line (start 0 -6.51) (end -3.86 -6.51) (layer "F.SilkS") (width 0.12) (tstamp b68ce9d3-8407-48e9-b024-342c29205980))
    (fp_line (start -3.86 -6.275) (end -5.675 -6.275) (layer "F.SilkS") (width 0.12) (tstamp b97a932f-69ee-4d18-9eda-a39afca71ef7))
    (fp_line (start -3.86 6.51) (end -3.86 6.275) (layer "F.SilkS") (width 0.12) (tstamp c8b65d03-7c86-4b35-9a22-ff8f62a66b4d))
    (fp_line (start 5.93 6.65) (end 5.93 -6.65) (layer "F.CrtYd") (width 0.05) (tstamp 4437d9f7-a8a1-4d20-92f7-e5b424a70e3c))
    (fp_line (start -5.93 -6.65) (end -5.93 6.65) (layer "F.CrtYd") (width 0.05) (tstamp 5173115e-02e9-4965-8c73-723f0e987399))
    (fp_line (start 5.93 -6.65) (end -5.93 -6.65) (layer "F.CrtYd") (width 0.05) (tstamp 5ef33dad-4ff0-4c14-bda7-00e764341d06))
    (fp_line (start -5.93 6.65) (end 5.93 6.65) (layer "F.CrtYd") (width 0.05) (tstamp 8f82811f-99a8-47f5-8a72-baaf433d73bd))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer "F.Fab") (width 0.1) (tstamp 0af5da6b-a48f-4e31-8947-6fca8951a904))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer "F.Fab") (width 0.1) (tstamp 12de1395-abaa-4353-9b6a-492988a2ca0c))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer "F.Fab") (width 0.1) (tstamp 6abc9f54-56ce-408e-833e-d773b3b7c058))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer "F.Fab") (width 0.1) (tstamp a9766e24-63ed-4927-acbd-292a10098368))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer "F.Fab") (width 0.1) (tstamp c1314411-e15c-4ae8-9e34-3c68554592b7))
    (pad "1" smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "OE") (pintype "input") (tstamp 0f08d987-be43-4644-ab2d-ae2a31122a23))
    (pad "2" smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "XA19") (pinfunction "D0") (pintype "input") (tstamp aa336b57-ee13-49dd-a3a1-0b8aeb27a463))
    (pad "3" smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "XA18") (pinfunction "D1") (pintype "input") (tstamp 6e5dc8e9-f830-45e4-a276-05483be2769c))
    (pad "4" smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "XA17") (pinfunction "D2") (pintype "input") (tstamp 7d208647-f1df-4db0-89f2-cdc9d226bab4))
    (pad "5" smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "XA16") (pinfunction "D3") (pintype "input") (tstamp 18093067-2f55-4090-ac76-85a51170e587))
    (pad "6" smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "~{S2}") (pinfunction "D4") (pintype "input") (tstamp e9169005-386e-40b1-a31f-2f496d04b986))
    (pad "7" smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "unconnected-(U202-Pad7)") (pinfunction "D5") (pintype "input+no_connect") (tstamp d4642e67-c09e-4573-8d77-9bd5492a86c8))
    (pad "8" smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "unconnected-(U202-Pad8)") (pinfunction "D6") (pintype "input+no_connect") (tstamp 56be6108-ecb5-41dc-ad6f-e7ff4ac5fe27))
    (pad "9" smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "unconnected-(U202-Pad9)") (pinfunction "D7") (pintype "input+no_connect") (tstamp 5d130ac5-6bf7-46a5-a9ab-36742482681b))
    (pad "10" smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 12c5e619-e016-4a0b-b978-5cc1d0fbb3a1))
    (pad "11" smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "Load") (pintype "input") (tstamp 110cbd9a-df60-413c-ba70-c7694b28833d))
    (pad "12" smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "unconnected-(U202-Pad12)") (pinfunction "Q7") (pintype "tri_state+no_connect") (tstamp b8daa96b-87cf-4cc2-bb63-2ff9bc0f0268))
    (pad "13" smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "unconnected-(U202-Pad13)") (pinfunction "Q6") (pintype "tri_state+no_connect") (tstamp 5455cc74-dd96-45da-8267-0be0e46fb174))
    (pad "14" smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "unconnected-(U202-Pad14)") (pinfunction "Q5") (pintype "tri_state+no_connect") (tstamp 8a27be9c-4769-434c-846f-81eeaa0cb8c9))
    (pad "15" smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "M{slash}~{IO}") (pinfunction "Q4") (pintype "tri_state") (tstamp 4e60f8d8-53c6-43b1-8711-5ea61522262e))
    (pad "16" smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "A16") (pinfunction "Q3") (pintype "tri_state") (tstamp f9aa0529-c613-4275-b665-dbd326c612db))
    (pad "17" smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "A17") (pinfunction "Q2") (pintype "tri_state") (tstamp fbb0c20d-a019-45ad-8b6a-e17d8c715039))
    (pad "18" smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "A18") (pinfunction "Q1") (pintype "tri_state") (tstamp 8ee92540-4c75-45a1-9806-d5c8eb42f807))
    (pad "19" smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "A19") (pinfunction "Q0") (pintype "tri_state") (tstamp c5d6ae9c-8d91-41fa-9d23-f4a41a1fa039))
    (pad "20" smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 095fbb3a-b857-4d88-bf3b-515352eec78a))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tedit 59FF03AB) (tstamp 23d269d6-d694-442a-bf5d-98bf3544fc31)
    (at 106.172 146.777 180)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/1b46cbbf-836a-4f8f-ae6c-a951e5621002")
    (attr through_hole)
    (fp_text reference "S1" (at 2.54 -5.08) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0110e22f-e4bb-4889-8b02-17ca7cd7ded1)
    )
    (fp_text value "PWR" (at 9.779 -2.921) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.2)))
      (tstamp ea7a9e89-3034-4a11-96e5-9b8ad83c571d)
    )
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 932eba78-2779-4630-989c-52cca8433294)
    )
    (fp_line (start 7.62 2.54) (end -2.54 2.54) (layer "F.SilkS") (width 0.12) (tstamp 02897324-2877-485a-b1ab-7c14c91dd339))
    (fp_line (start 7.62 -3.81) (end -2.54 -3.81) (layer "F.SilkS") (width 0.12) (tstamp 59e5782d-0986-4ad9-ada8-001e9360eb40))
    (fp_line (start 7.62 3.81) (end 7.62 -3.81) (layer "F.SilkS") (width 0.12) (tstamp 7db5d241-0e46-4cfc-9180-8f17decab700))
    (fp_line (start -2.54 -3.81) (end -2.54 3.81) (layer "F.SilkS") (width 0.12) (tstamp 863ecbc3-f44c-483c-9745-84b67db9920e))
    (fp_line (start -2.54 3.81) (end 7.62 3.81) (layer "F.SilkS") (width 0.12) (tstamp a9846687-3ee4-4c04-8f9e-89e36448b2f8))
    (fp_line (start 7.79 4) (end -2.71 4) (layer "F.CrtYd") (width 0.05) (tstamp 20d83ad9-8c3d-454f-9c91-aa198a053459))
    (fp_line (start 7.79 4) (end 7.79 -4) (layer "F.CrtYd") (width 0.05) (tstamp 8f767b2b-1647-4143-ad55-72413a0364f5))
    (fp_line (start -2.71 -4) (end 7.79 -4) (layer "F.CrtYd") (width 0.05) (tstamp a11a3e3f-08ba-448a-98c0-fc1d3ace94df))
    (fp_line (start -2.71 -4) (end -2.71 4) (layer "F.CrtYd") (width 0.05) (tstamp e204d70f-5fb8-48aa-9b67-c9c8513d5799))
    (fp_line (start 7.54 3.75) (end 7.54 -3.75) (layer "F.Fab") (width 0.1) (tstamp 0c66b92e-76b6-4fbd-a608-f7337c59a4b1))
    (fp_line (start 7.54 -3.75) (end -2.46 -3.75) (layer "F.Fab") (width 0.1) (tstamp 3512b4a6-175f-4902-ba63-e7b867ea30cd))
    (fp_line (start -2.46 3.75) (end 7.54 3.75) (layer "F.Fab") (width 0.1) (tstamp 74134f34-8b33-4121-8f63-805f14e3d7a9))
    (fp_line (start -2.41 2.55) (end 7.49 2.55) (layer "F.Fab") (width 0.1) (tstamp 7e6c0139-5342-471d-a070-6aeed401af50))
    (fp_line (start -2.46 -3.75) (end -2.46 3.75) (layer "F.Fab") (width 0.1) (tstamp f1bde16f-44f8-4ccf-bef5-a35d378d7cb5))
    (pad "1" thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 6db14ee1-280f-4860-aaac-6db0cbe6a1f8))
    (pad "2" thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "Pin_2") (pintype "passive") (tstamp 2ff4b21b-7ede-43d3-a7b5-6e08013aafe7))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl" hide
      (offset (xyz 2.54 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl"
      (offset (xyz 5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -180))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x32_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A428) (tstamp 360bedc1-8522-4c8c-bbbd-baca6d69d40e)
    (at 94.996 137.887 90)
    (descr "Through hole straight socket strip, 2x32, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x32 2.54mm double row")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/1c885dcb-2dbe-489b-95f7-4cf2d7f515a3")
    (attr through_hole)
    (fp_text reference "J101" (at -1.27 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bc976f40-ba2d-4fd7-b01e-0273ab8fa8f8)
    )
    (fp_text value "PC/104 ISA" (at -1.27 82.042 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3ea96363-fb7d-4809-bfb4-59b1c930efc0)
    )
    (fp_text user "${REFERENCE}" (at -1.27 39.37) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9b0d8fc-2001-46f2-93b6-1685844080d4)
    )
    (fp_line (start -3.87 -1.33) (end -1.27 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 26c5b077-bae9-4e08-ad7e-dc9f6c66b08d))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 5ff7c37d-a385-4eec-afdb-9325a1879bc9))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 81c1cfb6-811d-43f6-9f77-bce652001f6e))
    (fp_line (start -1.27 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 81d41a13-b1c5-47f4-a172-45abad1c0f96))
    (fp_line (start -3.87 -1.33) (end -3.87 80.07) (layer "F.SilkS") (width 0.12) (tstamp 82df164c-115c-4bb5-9258-da980dd50b82))
    (fp_line (start -3.87 80.07) (end 1.33 80.07) (layer "F.SilkS") (width 0.12) (tstamp bea03a87-d700-42ab-bc56-ad4ecca4241e))
    (fp_line (start 1.33 1.27) (end 1.33 80.07) (layer "F.SilkS") (width 0.12) (tstamp dca29148-b370-4568-b11c-a924fe0324b6))
    (fp_line (start -1.27 -1.33) (end -1.27 1.27) (layer "F.SilkS") (width 0.12) (tstamp f93596f9-3930-4540-b2d6-9fdfdeadcf4d))
    (fp_line (start 1.76 80.55) (end -4.34 80.55) (layer "F.CrtYd") (width 0.05) (tstamp 4349b373-a30b-4dc9-a006-014d2a5231a7))
    (fp_line (start 1.76 -1.8) (end 1.76 80.55) (layer "F.CrtYd") (width 0.05) (tstamp 6fca34d2-3d17-4aea-9248-77f0d882cd45))
    (fp_line (start -4.34 80.55) (end -4.34 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 923075b4-e3af-4d3b-a229-f68a3d0fcaa9))
    (fp_line (start -4.34 -1.8) (end 1.76 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b323a369-d90a-49f4-869b-7ea8d5436e04))
    (fp_line (start 1.27 80.01) (end -3.81 80.01) (layer "F.Fab") (width 0.1) (tstamp 4ef88bf0-2239-400f-b9f2-cd54862db3b7))
    (fp_line (start 1.27 -0.27) (end 1.27 80.01) (layer "F.Fab") (width 0.1) (tstamp 6b7f9d51-5521-4f24-9e4b-5535d0c61f4c))
    (fp_line (start -3.81 -1.27) (end 0.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 91a3ada8-5ea6-489f-ba7d-9ec0c44fa79c))
    (fp_line (start -3.81 80.01) (end -3.81 -1.27) (layer "F.Fab") (width 0.1) (tstamp b75ce88d-99bb-44b4-98a8-90eb3a673946))
    (fp_line (start 0.27 -1.27) (end 1.27 -0.27) (layer "F.Fab") (width 0.1) (tstamp e4c13d41-89f3-4aac-9532-274c5c4aa4ad))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 18c88179-ee7e-494d-9ee6-5ce447419124))
    (pad "2" thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "unconnected-(J101-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect") (tstamp c8d39f66-7b93-42fe-8aff-bad2b4f5528d))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 164 "ALE") (pinfunction "Pin_3") (pintype "passive") (tstamp 25052694-fd9e-4036-bd7b-980dcf6f64b2))
    (pad "4" thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "DB7") (pinfunction "Pin_4") (pintype "passive") (tstamp 441caf2f-b0df-4acc-b4f4-fbf0ce4386a9))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "Pin_5") (pintype "passive") (tstamp 721a48e1-1b66-4a6a-b954-0fcebbf7922c))
    (pad "6" thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "DB6") (pinfunction "Pin_6") (pintype "passive") (tstamp 5057ecce-1ce9-4b78-ad38-43f43656f016))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "INT1") (pinfunction "Pin_7") (pintype "passive") (tstamp 8100ef15-2196-4d84-983c-e71e200a76ae))
    (pad "8" thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "DB5") (pinfunction "Pin_8") (pintype "passive") (tstamp 23cb16fe-2d4f-40cb-a6c9-6516e236b991))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "unconnected-(J101-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect") (tstamp 8a6ffdbe-79dc-4537-b014-2210092ece80))
    (pad "10" thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "DB4") (pinfunction "Pin_10") (pintype "passive") (tstamp a2df36e2-0887-437e-b3cd-87d39937eb6e))
    (pad "11" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "DRQ1") (pinfunction "Pin_11") (pintype "passive") (tstamp e5dc3475-f762-4c97-8145-c7fe232747b5))
    (pad "12" thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "DB3") (pinfunction "Pin_12") (pintype "passive") (tstamp 6d05e6df-ab52-4067-bdbd-63458eb68e1d))
    (pad "13" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 139 "unconnected-(J101-Pad13)") (pinfunction "Pin_13") (pintype "passive+no_connect") (tstamp 0268c12b-a84b-4694-8d0e-da88e0e75135))
    (pad "14" thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "DB2") (pinfunction "Pin_14") (pintype "passive") (tstamp a822fcda-8ebd-4f02-9f11-e235b362417f))
    (pad "15" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "~{CARDSLCTD}") (pinfunction "Pin_15") (pintype "passive") (tstamp 7a15a0c3-19d6-4cb7-aadc-f21cbaabda60))
    (pad "16" thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "DB1") (pinfunction "Pin_16") (pintype "passive") (tstamp f8a5e5bb-b8f6-4e3c-9b68-8c6b8e53d55f))
    (pad "17" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 "unconnected-(J101-Pad17)") (pinfunction "Pin_17") (pintype "passive+no_connect") (tstamp b7cbb9dd-56ff-4e94-b952-5f5ebe851d00))
    (pad "18" thru_hole oval (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "DB0") (pinfunction "Pin_18") (pintype "passive") (tstamp 0d393a6c-d12b-4b93-8723-2c3d2aa40702))
    (pad "19" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_19") (pintype "passive") (tstamp ad8ce4ca-42e0-4275-827b-0185709fb43d))
    (pad "20" thru_hole oval (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 "unconnected-(J101-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect") (tstamp 27055fd3-4b66-4ff5-9aaf-7ef3f7d099c5))
    (pad "21" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "~{SMEMW}") (pinfunction "Pin_21") (pintype "passive") (tstamp dac278dc-046e-4984-bb7f-c7cf097348e2))
    (pad "22" thru_hole oval (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 142 "unconnected-(J101-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect") (tstamp a73e0ac1-86f4-47bf-9c36-32d6fcb14b24))
    (pad "23" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "~{SMEMR}") (pinfunction "Pin_23") (pintype "passive") (tstamp bac9d2e4-bfec-4b8a-8bcc-24b49c19ff65))
    (pad "24" thru_hole oval (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "A19") (pinfunction "Pin_24") (pintype "passive") (tstamp 310016a9-b415-4e9d-a056-af394ffb92c8))
    (pad "25" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "~{IOW}") (pinfunction "Pin_25") (pintype "passive") (tstamp 258b6af9-d0f8-4f0c-aa27-8b48af15c228))
    (pad "26" thru_hole oval (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "A18") (pinfunction "Pin_26") (pintype "passive") (tstamp d3d238f6-acbb-418b-afb1-01fd90cf418a))
    (pad "27" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "~{IOR}") (pinfunction "Pin_27") (pintype "passive") (tstamp e834d7e8-0673-416e-b918-ddb5cb95059d))
    (pad "28" thru_hole oval (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "A17") (pinfunction "Pin_28") (pintype "passive") (tstamp 84560d9d-de88-49d5-bbc7-f1ad14e0da29))
    (pad "29" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "~{PCS6}") (pinfunction "Pin_29") (pintype "passive") (tstamp 03864836-3830-40eb-80ac-1fc17f3de956))
    (pad "30" thru_hole oval (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "A16") (pinfunction "Pin_30") (pintype "passive") (tstamp a3d70c18-bd2d-4d1b-8e1c-af60a2a87742))
    (pad "31" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 "unconnected-(J101-Pad31)") (pinfunction "Pin_31") (pintype "passive+no_connect") (tstamp 8075f7bf-fa15-4c2b-b284-da9a07cb4204))
    (pad "32" thru_hole oval (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "A15") (pinfunction "Pin_32") (pintype "passive") (tstamp 80f4085c-8957-40c8-a793-4d238a26f6ac))
    (pad "33" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "~{PCS4}") (pinfunction "Pin_33") (pintype "passive") (tstamp 1883ecfa-4fda-4251-b877-cdd45bb3cee8))
    (pad "34" thru_hole oval (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "A14") (pinfunction "Pin_34") (pintype "passive") (tstamp f7288403-fd23-4f36-8301-0d453203c172))
    (pad "35" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "DRQ0") (pinfunction "Pin_35") (pintype "passive") (tstamp 756d3fb3-e04a-4119-b239-b63f7e2ba8fb))
    (pad "36" thru_hole oval (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "A13") (pinfunction "Pin_36") (pintype "passive") (tstamp 33d73790-3a2c-43e6-bf17-37dcc9ef689f))
    (pad "37" thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "~{PCS3}") (pinfunction "Pin_37") (pintype "passive") (tstamp 7aa785bc-ec47-4532-a06c-03a4eee6453a))
    (pad "38" thru_hole oval (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "A12") (pinfunction "Pin_38") (pintype "passive") (tstamp 87cadec8-e64a-442f-9330-e5a7a7d86547))
    (pad "39" thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "BCLK") (pinfunction "Pin_39") (pintype "passive") (tstamp 10ca06e0-32e0-420b-94f0-e1a8d3747c3f))
    (pad "40" thru_hole oval (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "A11") (pinfunction "Pin_40") (pintype "passive") (tstamp 41479eef-db4e-41d0-a0eb-b282ed21c5fe))
    (pad "41" thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "IR7") (pinfunction "Pin_41") (pintype "passive") (tstamp de6753e1-e671-4086-9a13-8142aab9b80b))
    (pad "42" thru_hole oval (at -2.54 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "A10") (pinfunction "Pin_42") (pintype "passive") (tstamp 4a04dc41-632c-4267-9bb5-f4166b52fd3f))
    (pad "43" thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "IR6") (pinfunction "Pin_43") (pintype "passive") (tstamp 60b3b385-3297-4356-8e15-7f05e89cf7d0))
    (pad "44" thru_hole oval (at -2.54 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "A9") (pinfunction "Pin_44") (pintype "passive") (tstamp 4f2d19b1-afa4-47c2-a84b-ee9dedf1266b))
    (pad "45" thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "IR5") (pinfunction "Pin_45") (pintype "passive") (tstamp e107140d-7eda-404a-b1ba-ec23464ccedd))
    (pad "46" thru_hole oval (at -2.54 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "A8") (pinfunction "Pin_46") (pintype "passive") (tstamp b922966a-5398-4d6e-bef7-2c2ebbd60302))
    (pad "47" thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "IR4") (pinfunction "Pin_47") (pintype "passive") (tstamp 44c75a31-0cab-4876-b0c1-1b14f9f1f88c))
    (pad "48" thru_hole oval (at -2.54 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "A7") (pinfunction "Pin_48") (pintype "passive") (tstamp e0b5c79a-175d-4a6c-89b5-f4f4e9b51482))
    (pad "49" thru_hole oval (at 0 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "INT3") (pinfunction "Pin_49") (pintype "passive") (tstamp 3dfa0776-c165-43ec-a3e3-04530f824759))
    (pad "50" thru_hole oval (at -2.54 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "A6") (pinfunction "Pin_50") (pintype "passive") (tstamp 8940650e-203d-4e6b-b993-e934067d1326))
    (pad "51" thru_hole oval (at 0 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "~{PCS5}") (pinfunction "Pin_51") (pintype "passive") (tstamp 3a767d27-477d-48cb-a197-80c0a6f566e5))
    (pad "52" thru_hole oval (at -2.54 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "A5") (pinfunction "Pin_52") (pintype "passive") (tstamp 0b64fb89-ed14-4192-a8cf-2148e1b85204))
    (pad "53" thru_hole oval (at 0 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 "unconnected-(J101-Pad53)") (pinfunction "Pin_53") (pintype "passive+no_connect") (tstamp c6e608eb-98e9-4702-bfb1-2c4643c3f1a8))
    (pad "54" thru_hole oval (at -2.54 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "A4") (pinfunction "Pin_54") (pintype "passive") (tstamp 655dd852-6594-4cc3-9c5b-9137e6e47927))
    (pad "55" thru_hole oval (at 0 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 164 "ALE") (pinfunction "Pin_55") (pintype "passive") (tstamp f0c59afa-6294-4bb0-880b-b8f5daca7961))
    (pad "56" thru_hole oval (at -2.54 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "A3") (pinfunction "Pin_56") (pintype "passive") (tstamp a54bf246-bdfc-4f99-9266-a823443f4f85))
    (pad "57" thru_hole oval (at 0 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "Pin_57") (pintype "passive") (tstamp 116a57e4-8215-4c21-a7eb-6f4d068b9d10))
    (pad "58" thru_hole oval (at -2.54 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "A2") (pinfunction "Pin_58") (pintype "passive") (tstamp 43d1fdb8-5e47-4c39-81f4-305fe7c5399d))
    (pad "59" thru_hole oval (at 0 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "TMR_OUT_0") (pinfunction "Pin_59") (pintype "passive") (tstamp bfced798-567b-4940-880c-a76e32fcc15b))
    (pad "60" thru_hole oval (at -2.54 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "A1") (pinfunction "Pin_60") (pintype "passive") (tstamp 0c35ba98-e483-4d8e-a46c-8c149b2e512e))
    (pad "61" thru_hole oval (at 0 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_61") (pintype "passive") (tstamp 223bff2c-cdb0-4e43-8484-a571fe4fd50d))
    (pad "62" thru_hole oval (at -2.54 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "A0") (pinfunction "Pin_62") (pintype "passive") (tstamp 7921058f-3b5e-401d-9661-789c6c702ac1))
    (pad "63" thru_hole oval (at 0 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_63") (pintype "passive") (tstamp 248ab666-e63b-442a-8fab-bf89bc244e90))
    (pad "64" thru_hole oval (at -2.54 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_64") (pintype "passive") (tstamp 53f41000-fc8d-4835-a981-6e1067e3a261))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x32_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 3fce92fa-e607-4dbb-bd27-27baad6dd8ad)
    (at 118.237 60.706 -90)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (path "/0a8f8a4f-8ec9-4b11-be94-fd8e3caf582e")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP103" (at 0 -1.448 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28ebe813-6f9b-4b8c-8f2c-c88d722b3f01)
    )
    (fp_text value "~{UCS}" (at -1.27 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp fc7ee562-6797-47ab-a684-1525c3c2d899)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9466ad6b-b021-415c-923e-52c065fca831)
    )
    (fp_line (start 0.7 -0.7) (end 0.7 0.7) (layer "F.SilkS") (width 0.12) (tstamp 73cea957-3039-4bf2-a942-abaed65b2a40))
    (fp_line (start -0.7 -0.7) (end 0.7 -0.7) (layer "F.SilkS") (width 0.12) (tstamp a9acb48c-ede2-468b-a8b0-7ff68865b703))
    (fp_line (start 0.7 0.7) (end -0.7 0.7) (layer "F.SilkS") (width 0.12) (tstamp ee1cc14e-b2ad-4f2f-a5b2-5969d95843aa))
    (fp_line (start -0.7 0.7) (end -0.7 -0.7) (layer "F.SilkS") (width 0.12) (tstamp f200ea10-e512-4070-99f9-0e9d68dea4bc))
    (fp_line (start -1 -1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp 352061c9-24ee-4eac-ac5f-fd616ab03645))
    (fp_line (start 1 1) (end 1 -1) (layer "F.CrtYd") (width 0.05) (tstamp 795294a5-eb83-4f17-bfbc-79482a667594))
    (fp_line (start -1 -1) (end 1 -1) (layer "F.CrtYd") (width 0.05) (tstamp 97972314-2b8d-40b3-84e1-3c10e698d682))
    (fp_line (start 1 1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp fd372697-aa58-46fa-ba83-81edf6fc2b62))
    (pad "1" smd rect (at 0 0 270) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 11 "~{UCS}") (pinfunction "1") (pintype "passive") (tstamp 5408273b-0242-4f15-857f-a4e59dd51bb9))
  )

  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 4d683f6c-2463-4e86-b710-686926e8a6ee)
    (at 113.157 76.4155 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "80-C1206X104G4HACTU")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/28ca81ea-ec87-4f8a-a904-2091b521a972")
    (attr smd)
    (fp_text reference "C6" (at 0 2.032 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92432eb5-d761-4aea-af2a-1591923febfc)
    )
    (fp_text value "100n/0.1u PWR" (at -0.127 -2.286 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0a39e67-33f9-48f8-b706-0f2f85ee5e48)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 790fe59c-ec37-43f4-8bf9-5bf8067cd970)
    )
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer "F.SilkS") (width 0.12) (tstamp 45097f23-d30c-493a-9a28-25c5d6e679b2))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer "F.SilkS") (width 0.12) (tstamp 7e99aefc-a2e7-4ba5-86b9-aca3c8ae1611))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 3ac2627e-a7cf-40bc-94ce-83585db91817))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 6de0f009-6d99-4930-9d3e-4f361a6026bc))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 84e685af-b0b8-400b-8714-01461d7a9551))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp d8c8e547-7af3-4c5e-b1a0-ca1e9a23f2ab))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 2797ec0f-e0c2-4907-91a3-9184b73c246d))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 59d55a5f-e7af-49f5-aefe-2155d5117d54))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 8f37416b-9d4b-4daf-910b-f5cb3e91ad8e))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp d6df452e-d471-4317-b96f-ac1913afe743))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "VCC") (pintype "passive") (tstamp ce9574fd-c342-4c15-bf74-244422767857))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive") (tstamp 07a97164-a2cc-4ff6-ae12-a3d549867c1c))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 4e9f6b06-3942-47ec-91b6-302ef574306f)
    (at 121.031 60.706 90)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (path "/6b6a224b-335c-4b2f-a4b4-9655c897469e")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP104" (at 0 -1.448 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c504f662-9a9c-4d5a-a4d6-a5505d68e627)
    )
    (fp_text value "~{LCS}" (at 1.27 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 41efec87-38bb-408f-b177-af29ef5dc2f3)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d9e6adb-b4d4-4bd9-b9a0-477922b27d86)
    )
    (fp_line (start -0.7 -0.7) (end 0.7 -0.7) (layer "F.SilkS") (width 0.12) (tstamp 141c0548-65a0-4a62-a095-0177ef65b15e))
    (fp_line (start 0.7 -0.7) (end 0.7 0.7) (layer "F.SilkS") (width 0.12) (tstamp 22385d51-8e87-4a60-b8ca-bd776d8bbfbe))
    (fp_line (start -0.7 0.7) (end -0.7 -0.7) (layer "F.SilkS") (width 0.12) (tstamp b74aac18-6eb8-40df-b2fb-4951ebd2ed3a))
    (fp_line (start 0.7 0.7) (end -0.7 0.7) (layer "F.SilkS") (width 0.12) (tstamp d3363f22-5a83-4e2a-b735-021d7a4fc6a9))
    (fp_line (start -1 -1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp 42a89069-63d6-459c-a334-0cdc07bd9db0))
    (fp_line (start -1 -1) (end 1 -1) (layer "F.CrtYd") (width 0.05) (tstamp b6f35dbe-9749-49af-b786-315c5dde7ca8))
    (fp_line (start 1 1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp b9f7d033-6fc0-4451-9434-e9d14cca044b))
    (fp_line (start 1 1) (end 1 -1) (layer "F.CrtYd") (width 0.05) (tstamp d658b0ea-c035-46d5-a0ee-6b4df308a604))
    (pad "1" smd rect (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 25 "~{LCS}") (pinfunction "1") (pintype "passive") (tstamp 840e96dd-a7c3-46e9-88eb-4253a1e2b944))
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 5264b699-a844-4267-bd47-59a775247fac)
    (at 122.936 97.155 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "C0805C220J1GACTU")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/f44e49a4-625b-411f-95d9-8fa518ceba4e")
    (attr smd)
    (fp_text reference "C102" (at 0 1.778 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a3aa980-4bec-4f92-901f-9b6fe283f31d)
    )
    (fp_text value "20p XTAL" (at 0 -1.651 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 549a640d-9a34-4cef-b01e-63ec03114f88)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp d032c81a-9ef7-4cf1-aa56-d467d57a0258)
    )
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp 20a6f922-d56c-49f6-ae66-27346b6ea591))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp a56f0f43-97ea-441f-80ad-6f233be1a658))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 1559e19b-f2c7-4a83-ad35-e29b379c1703))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp d51c6ab2-9988-4ad4-bcde-2ad76d64aeb0))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp edeffaf5-e160-4e88-9da2-0a775c5a7000))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp f22b754f-d340-43a8-8128-d239a1cb174a))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 07c7ba98-4de7-4723-bbea-408791881c8a))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 33702b76-eb7d-4f15-8f72-5598105aaee0))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 362d7f1e-346c-4e1e-98ab-fe78ad64137a))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp fd7f9cdc-0c0f-4c43-b89f-10708a944aca))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "/X2") (pintype "passive") (tstamp 875c75d1-f71f-46d0-a14f-76d3d36e6666))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive") (tstamp 0130c45a-a237-4830-977a-7eeb6220f060))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 58377f22-fdac-4b4e-959d-9a75f98651c5)
    (at 117.983 146.2532 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "C0805C220J1GACTU")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/b85501ea-403e-4e03-b871-d64d45ce29b3")
    (attr smd)
    (fp_text reference "C205" (at 0 -1.68 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b88e687e-009d-4332-b839-7359007ef5e5)
    )
    (fp_text value "20p" (at 0 1.68 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b686640d-32ec-4652-bfe1-29c3a98876d9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp ce40f4f1-f8fa-48b4-8b27-04017d11bd44)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 0ac868a2-61cb-4b55-b823-31ea796e4a68))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp 40fab401-4130-4def-97d7-9720e61a4ea3))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp ad35f6b8-a74b-4a5d-8f87-06ce33e25a8f))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp c7bf1649-fd6f-48eb-8bcc-d868f89b2959))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp e5c459d3-20b6-4833-8919-085434c3dc4d))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp f2532b53-a19d-49d7-ae1f-5c27329629fb))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 7314c2d2-48e2-4f34-b685-3af47ead6d03))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 967273f1-c09d-4ffb-9418-6d893dd3f41c))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp b8a81b54-4d39-413d-a68c-b4f48be955d5))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp e56d266a-2785-4eaa-96fb-00220a0e095a))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 162 "~{RESET}") (pintype "passive") (tstamp bb7e0362-dec8-417b-9180-d0d46a9a2637))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive") (tstamp e28e424d-8783-4f2a-b106-f7d792422a42))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF) (tstamp 6345ed7f-2d79-4a1f-9931-17f3babe5ae9)
    (at 97.409 59.909 -90)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/e858ca16-5a04-49a5-8adc-6505fc7c6c12")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.7 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56fcd277-d0fa-4045-8c6c-403fa315d96d)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_Pad_Via" (at 0 3.7 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81cfcd67-91cb-4d6b-bba8-0b4beeb24ea5)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15) italic))
      (tstamp 482efefe-4e01-40d2-baba-6ead4c2bce4d)
    )
    (fp_circle (center 0 0) (end 2.7 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 6ff95fbb-7122-49b5-b08e-8ceb838e6c98))
    (fp_circle (center 0 0) (end 2.95 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp ac997c2c-f3e9-40ef-a0bf-c72665c9d9cd))
    (pad "1" thru_hole circle (at 1.431891 -1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 194ee46c-0360-45e4-b2f3-2edf6d743687))
    (pad "1" thru_hole circle (at 0 2.025 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 24c03125-205d-4555-bf2a-4d5acf0f9431))
    (pad "1" thru_hole circle (at -1.431891 -1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 32113010-c2c9-4f22-b5e0-c1af5e67bd15))
    (pad "1" thru_hole circle (at 0 0 270) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 6acac382-3a70-4fe2-a8d0-e5fb81e6d25e))
    (pad "1" thru_hole circle (at 0 -2.025 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 73ed5c8a-efb1-44bb-9b2a-8a0c81ff0bbb))
    (pad "1" thru_hole circle (at 1.431891 1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp b03f40eb-52ca-4ed1-add3-0f257d9af3a8))
    (pad "1" thru_hole circle (at -1.431891 1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp d31d4a5c-bfd4-4756-95b8-4c98dea2387c))
    (pad "1" thru_hole circle (at -2.025 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp da8c8625-aafd-4cdd-8a69-a69db75bbf93))
    (pad "1" thru_hole circle (at 2.025 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp df2c23dc-fccc-44b2-bce4-4104f48202f7))
  )

  (footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D" (layer "F.Cu")
    (tedit 5EBA9318) (tstamp 64854507-f01d-4be6-b962-9e42d4763f70)
    (at 91.059 128.778 90)
    (descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "667-EEF-CS1D100R")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/5729f36b-3341-48f9-9f27-37a050e600e2")
    (attr smd)
    (fp_text reference "C4" (at -0.035 3.429 270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12fc3375-c11f-404d-8efb-6d15cb772414)
    )
    (fp_text value "PPWR" (at 0 3.1 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 73528342-975f-4223-93af-a055c7a982a0)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9abba321-8b14-4359-92cd-6a6d01cfc986)
    )
    (fp_line (start -4.41 2.26) (end 3.65 2.26) (layer "F.SilkS") (width 0.12) (tstamp 7d2115d2-6e26-4d25-bf00-cb52e1cdf8d7))
    (fp_line (start 3.65 -2.26) (end -4.41 -2.26) (layer "F.SilkS") (width 0.12) (tstamp ed370adf-9f2d-4f87-a11e-e03716245cb7))
    (fp_line (start -4.41 -2.26) (end -4.41 2.26) (layer "F.SilkS") (width 0.12) (tstamp ff42a21e-84d4-4142-bcf0-f48b72956361))
    (fp_line (start 4.4 2.4) (end -4.4 2.4) (layer "F.CrtYd") (width 0.05) (tstamp 31d9ff12-65d5-46c5-b37d-36c2a19fb857))
    (fp_line (start 4.4 -2.4) (end 4.4 2.4) (layer "F.CrtYd") (width 0.05) (tstamp 86f7584d-2113-48a5-9a64-24f9c8f6f843))
    (fp_line (start -4.4 2.4) (end -4.4 -2.4) (layer "F.CrtYd") (width 0.05) (tstamp 9711cc6b-336d-40d7-bfa3-3c72bda8b4cb))
    (fp_line (start -4.4 -2.4) (end 4.4 -2.4) (layer "F.CrtYd") (width 0.05) (tstamp e3eaef93-77d8-4968-8945-d44d8284ae1c))
    (fp_line (start 3.65 -2.15) (end -2.65 -2.15) (layer "F.Fab") (width 0.1) (tstamp 057cd663-7fe3-4a66-aaa5-1d64f4c0ba21))
    (fp_line (start -2.65 -2.15) (end -3.65 -1.15) (layer "F.Fab") (width 0.1) (tstamp 4c82a8ed-4e68-4302-a066-de9d0a3e27e7))
    (fp_line (start -3.65 -1.15) (end -3.65 2.15) (layer "F.Fab") (width 0.1) (tstamp 66c30f32-e3a6-4f5b-8a32-9b14be90edae))
    (fp_line (start 3.65 2.15) (end 3.65 -2.15) (layer "F.Fab") (width 0.1) (tstamp 683302a6-dd25-4e04-96e5-04f36d40fc60))
    (fp_line (start -3.65 2.15) (end 3.65 2.15) (layer "F.Fab") (width 0.1) (tstamp 6ad816fc-e830-4fc0-8f53-fd19e3ebb2f4))
    (pad "1" smd roundrect (at -3.1125 0 90) (size 2.075 2.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.120482)
      (net 4 "VCC") (pintype "passive") (tstamp aeda9a8e-b431-4fb6-be74-255bf5cac2d2))
    (pad "2" smd roundrect (at 3.1125 0 90) (size 2.075 2.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.120482)
      (net 2 "GND") (pintype "passive") (tstamp 0cd3172c-7841-445d-abbe-58e09669215f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm_HandSoldering" (layer "F.Cu")
    (tedit 5A0FD1B2) (tstamp 68b51e53-c009-4064-a2c1-7be76452f156)
    (at 102.5652 78.359 180)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (property "Manufacturer_Part_Number" "830105961709")
    (property "Mouser Part Number" "710-830105961709")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/70234080-ace6-4a4c-a3f6-e036166446b1")
    (attr smd)
    (fp_text reference "Y301" (at 0 -3.05) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ef48a67-28cd-4a1a-8ee1-0b2d8b774911)
    )
    (fp_text value "18.432MHz" (at 1.0922 3.556) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a97d836-119d-4c8a-ad1a-90bff445914c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.105)))
      (tstamp 3357d789-313c-4d8a-b51e-c8c4ea05e0ed)
    )
    (fp_line (start -2.7 -2.25) (end -2.7 2.25) (layer "F.SilkS") (width 0.12) (tstamp aa166302-dc53-41c5-bece-95c9a685584e))
    (fp_line (start -2.7 2.25) (end 2.7 2.25) (layer "F.SilkS") (width 0.12) (tstamp bbda7182-2578-42ff-96db-9241b897f918))
    (fp_line (start -2.8 2.3) (end 2.8 2.3) (layer "F.CrtYd") (width 0.05) (tstamp 2edcef01-d7fa-4f41-976d-89aba56b27f6))
    (fp_line (start -2.8 -2.3) (end -2.8 2.3) (layer "F.CrtYd") (width 0.05) (tstamp 5da345e3-3025-47d1-8737-6693293178f5))
    (fp_line (start 2.8 2.3) (end 2.8 -2.3) (layer "F.CrtYd") (width 0.05) (tstamp 73ff78c2-2deb-4aca-953f-d7ac0aee7a02))
    (fp_line (start 2.8 -2.3) (end -2.8 -2.3) (layer "F.CrtYd") (width 0.05) (tstamp d29b25fc-d8c5-4824-84d9-fcc591ac9c00))
    (fp_line (start 1.6 -1.25) (end -1.6 -1.25) (layer "F.Fab") (width 0.1) (tstamp 0f776712-e222-4844-915e-8128f4da5be2))
    (fp_line (start 1.6 1.25) (end 1.6 -1.25) (layer "F.Fab") (width 0.1) (tstamp 1358bdb0-b18e-427b-96b7-83774d435b0f))
    (fp_line (start -1.6 1.25) (end 1.6 1.25) (layer "F.Fab") (width 0.1) (tstamp 292717e7-c866-4f20-9535-35b2587d2c3f))
    (fp_line (start -1.6 -1.25) (end -1.6 1.25) (layer "F.Fab") (width 0.1) (tstamp 92610f02-560d-4acb-a283-7ad7ba1c14ed))
    (fp_line (start -1.6 0.25) (end -0.6 1.25) (layer "F.Fab") (width 0.1) (tstamp e01df626-ea13-4cac-9a20-25d3652fb669))
    (pad "1" smd rect (at -1.45 1.15 180) (size 2.1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(C305-Pad2)") (pinfunction "1") (pintype "passive") (tstamp d9eb33ea-70e4-43f9-8773-bde5f7e8b59a))
    (pad "2" smd rect (at 1.45 1.15 180) (size 2.1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "unconnected-(Y301-Pad2)") (pinfunction "2") (pintype "passive+no_connect") (tstamp eb24fd7a-61ab-4003-bd75-99291d68e55a))
    (pad "3" smd rect (at 1.45 -1.15 180) (size 2.1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(C306-Pad1)") (pinfunction "3") (pintype "passive") (tstamp a9eb3813-b43c-4261-97a6-18a76d199eb5))
    (pad "4" smd rect (at -1.45 -1.15 180) (size 2.1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(Y301-Pad4)") (pinfunction "4") (pintype "passive+no_connect") (tstamp fb6043ba-82c7-4ccc-a4b3-3bf66bf48b37))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm_HandSoldering.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 6913c1ca-4cbf-4cc5-8056-70484c48e06f)
    (at 107.315 78.613 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "C0805C220J1GACTU")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/8f17a306-9316-4c7c-a371-6e4ba4419618")
    (attr smd)
    (fp_text reference "C305" (at -3.937 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f77c8997-06b2-436d-bbca-8a415431fbbf)
    )
    (fp_text value "22p XTAL" (at 0 1.68 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 32f43bbd-8c25-42ce-84de-c8c70ec944cf)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 37971eca-add2-40aa-b854-0deb45e56a20)
    )
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp 6d8b6497-d9c4-4f7a-82b2-1853e27d672c))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp ff86b8c2-fb4f-4630-88e4-2560429ff8e0))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 60cbf02b-63f7-4ff8-9c76-886bf4a1d1cb))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 903d80e6-7940-435e-9db5-070c0569fe61))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp d79a0ac7-5a63-474a-ae5d-b19d231e5650))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp ffdb72f7-3e7d-4997-a9a7-10db0b379a6b))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp 432b5b55-ce38-4314-ae8a-523626940cd5))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp ced0a8eb-7127-4b99-b887-aaa0821a0490))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp e629fb37-2134-4332-953a-617f6beeb791))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp f8aae2b0-1e08-42c3-b662-05e74221d217))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive") (tstamp 88058682-b662-4fef-8a8a-30720bde18b8))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 66 "Net-(C305-Pad2)") (pintype "passive") (tstamp d33627e7-d5a6-447f-814e-8bed46434e85))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 6b7345ec-7638-4606-95fc-02c5893a2ef6)
    (at 97.204 131.064 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "80-C1206X104G4HACTU")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/e8ffec03-0615-498a-be40-87bbf9bc6378")
    (attr smd)
    (fp_text reference "C204" (at -0.0508 1.9812 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ced28f36-cebb-43ee-96b3-0c6ee4cb6552)
    )
    (fp_text value "100n/0.1u PWR" (at 0 1.85 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c31dfd88-12b6-4960-8c70-a3b8655b8a69)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp b5f45711-68b5-48a9-aaf0-5ecea50c774c)
    )
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer "F.SilkS") (width 0.12) (tstamp a07be6de-f7d9-4e9e-b370-e0bce2f3153f))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer "F.SilkS") (width 0.12) (tstamp eea487a1-f656-4a6a-b813-f14553e9caee))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 0a0386fc-529a-4606-8481-fff0f9d0b1be))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 34997f5c-253a-41d0-952e-4a894192677d))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 6f31ced1-c3fa-47ae-ad72-eda6e151b389))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 7ef81c13-885c-4774-a4dc-33d0376dbc03))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 18e8df0f-2b41-4db0-931a-1cfe498d0fda))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 2c04482a-4909-47e6-92a5-56feeef8ddf2))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 51e6b0e0-9b11-47f3-955b-05fa74d48598))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 6b7fd049-3325-46e5-af1a-46ddb53b39dd))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "VCC") (pintype "passive") (tstamp 534f10a9-69b8-4484-a577-f3357d5b3edb))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive") (tstamp 3b622150-65e1-4f81-a02c-b2d961a6acf5))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SSOP-32_11.305x20.495mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1) (tstamp 6c3ee3bd-fdbc-4c5d-962f-29ccff049ac5)
    (at 163.449 91.948 180)
    (descr "SSOP, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (property "Description" "62C1024 128KB SRAM")
    (property "Manufacturer_Name" "ISSI")
    (property "Manufacturer_Part_Number" "IS62C1024AL-35QLI")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/45528828-5eae-43ac-871e-8f3cff158f5d")
    (attr smd)
    (fp_text reference "U101" (at 0 -11.2) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f05875fd-2819-4310-b8fa-4c3a5228a531)
    )
    (fp_text value "128K SRAM" (at 0 11.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e82ce089-247a-48d6-a299-17d086dfea3f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed6c094c-b185-408b-a3bb-e93f32b2bdbc)
    )
    (fp_line (start 0 -10.3575) (end 5.7625 -10.3575) (layer "F.SilkS") (width 0.12) (tstamp 083a1953-92d9-4d0d-a45b-665293bdbbd9))
    (fp_line (start 0 10.3575) (end -5.7625 10.3575) (layer "F.SilkS") (width 0.12) (tstamp 0c01e301-aa11-4976-9783-2986b163bb1d))
    (fp_line (start 5.7625 10.3575) (end 5.7625 10.085) (layer "F.SilkS") (width 0.12) (tstamp 288cce28-0af0-4627-aa09-1e24932f1a03))
    (fp_line (start 0 10.3575) (end 5.7625 10.3575) (layer "F.SilkS") (width 0.12) (tstamp 3ec6db3b-5c64-4e3a-9e5a-5ca5b7204e2d))
    (fp_line (start -5.7625 -10.085) (end -7.575 -10.085) (layer "F.SilkS") (width 0.12) (tstamp 4069af3d-0838-43d5-ad5a-f61bd44e2c45))
    (fp_line (start 0 -10.3575) (end -5.7625 -10.3575) (layer "F.SilkS") (width 0.12) (tstamp ac213fc3-e990-496c-86ca-b127a21863ea))
    (fp_line (start -5.7625 10.3575) (end -5.7625 10.085) (layer "F.SilkS") (width 0.12) (tstamp c6b65fb3-092d-4f71-9525-6a6ae21f70d5))
    (fp_line (start -5.7625 -10.3575) (end -5.7625 -10.085) (layer "F.SilkS") (width 0.12) (tstamp c9e19888-5e18-4445-838f-e239f9099205))
    (fp_line (start 5.7625 -10.3575) (end 5.7625 -10.085) (layer "F.SilkS") (width 0.12) (tstamp e47d9570-ca9c-4637-97aa-f85169c1ed82))
    (fp_line (start -7.83 -10.5) (end -7.83 10.5) (layer "F.CrtYd") (width 0.05) (tstamp 01afd305-398e-4713-9eb9-0acb95028e03))
    (fp_line (start -7.83 10.5) (end 7.83 10.5) (layer "F.CrtYd") (width 0.05) (tstamp 551d4579-ed62-4d92-931d-eb067d1b2ae3))
    (fp_line (start 7.83 10.5) (end 7.83 -10.5) (layer "F.CrtYd") (width 0.05) (tstamp 713ed210-9723-423f-a653-52b2ba008ed6))
    (fp_line (start 7.83 -10.5) (end -7.83 -10.5) (layer "F.CrtYd") (width 0.05) (tstamp 7d29cefc-497d-4626-8174-be321027288b))
    (fp_line (start -4.6525 -10.2475) (end 5.6525 -10.2475) (layer "F.Fab") (width 0.1) (tstamp 37afa257-c16d-4e41-9c25-44802735a340))
    (fp_line (start 5.6525 -10.2475) (end 5.6525 10.2475) (layer "F.Fab") (width 0.1) (tstamp 3f0c2af5-e018-4c4c-8818-6f793420182c))
    (fp_line (start -5.6525 10.2475) (end -5.6525 -9.2475) (layer "F.Fab") (width 0.1) (tstamp 550e75af-bda7-4d8f-b531-3d913fcafe47))
    (fp_line (start -5.6525 -9.2475) (end -4.6525 -10.2475) (layer "F.Fab") (width 0.1) (tstamp a43162fa-0681-4795-a798-63bd9fa5a3d1))
    (fp_line (start 5.6525 10.2475) (end -5.6525 10.2475) (layer "F.Fab") (width 0.1) (tstamp e8dfe2b1-92af-4a6b-a9d5-c7d5b6df74f4))
    (pad "1" smd roundrect (at -6.55 -9.525 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 163 "unconnected-(U101-Pad1)") (pinfunction "NC") (pintype "no_connect") (tstamp 0c4b05c5-d44b-47cf-a457-b2f6ec3024d8))
    (pad "2" smd roundrect (at -6.55 -8.255 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "A16") (pinfunction "A16") (pintype "input") (tstamp e16bbefd-e170-464b-a9d2-5cc4ed9e1d4f))
    (pad "3" smd roundrect (at -6.55 -6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "A14") (pinfunction "A14") (pintype "input") (tstamp fb4a40df-1626-46be-8101-76232ae06c80))
    (pad "4" smd roundrect (at -6.55 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "A12") (pinfunction "A12") (pintype "input") (tstamp 62973d0f-2168-48fc-9a14-d267aca5fdf7))
    (pad "5" smd roundrect (at -6.55 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "A7") (pinfunction "A7") (pintype "input") (tstamp af04e125-bb61-45a6-9d5d-bfe59683d84a))
    (pad "6" smd roundrect (at -6.55 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "A6") (pinfunction "A6") (pintype "input") (tstamp 8ef21b00-4d7f-46d9-96b2-0b0d321995f5))
    (pad "7" smd roundrect (at -6.55 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "A5") (pinfunction "A5") (pintype "input") (tstamp 87ab0d97-93ed-4ced-88eb-b4298de6c5c1))
    (pad "8" smd roundrect (at -6.55 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "A4") (pinfunction "A4") (pintype "input") (tstamp 7fca620f-6df0-445e-afd2-b63f168f5818))
    (pad "9" smd roundrect (at -6.55 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "A3") (pinfunction "A3") (pintype "input") (tstamp fe1a280b-129c-459c-86d5-e24350d2c701))
    (pad "10" smd roundrect (at -6.55 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "A2") (pinfunction "A2") (pintype "input") (tstamp 4ae4bc79-a588-4f06-a480-71971ed6f4fb))
    (pad "11" smd roundrect (at -6.55 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "A1") (pinfunction "A1") (pintype "input") (tstamp 47398519-a87e-45ef-a45d-6e149e5af1b2))
    (pad "12" smd roundrect (at -6.55 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "A0") (pinfunction "A0") (pintype "input") (tstamp e7a5dbf3-ab3d-4ee7-a9a2-d22bd26b9d29))
    (pad "13" smd roundrect (at -6.55 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "AD0") (pinfunction "Q0") (pintype "tri_state") (tstamp 462155b5-4364-4924-bdba-ddb18d26dd3c))
    (pad "14" smd roundrect (at -6.55 6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "AD1") (pinfunction "Q1") (pintype "tri_state") (tstamp a024934c-9919-4380-83f2-e34414984cfc))
    (pad "15" smd roundrect (at -6.55 8.255 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "AD2") (pinfunction "Q2") (pintype "tri_state") (tstamp 7d3e57ca-29ee-4fa7-b767-d557aa6b705e))
    (pad "16" smd roundrect (at -6.55 9.525 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 1f1b26ee-9490-40c0-a02d-9f81c4ea8f1b))
    (pad "17" smd roundrect (at 6.55 9.525 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "AD3") (pinfunction "Q3") (pintype "tri_state") (tstamp 21a9c3cc-dc0f-4727-bb12-90ac2fecdc6f))
    (pad "18" smd roundrect (at 6.55 8.255 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "AD4") (pinfunction "Q4") (pintype "tri_state") (tstamp 0defee75-c756-444d-a5d7-461284b9d7bc))
    (pad "19" smd roundrect (at 6.55 6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "AD5") (pinfunction "Q5") (pintype "tri_state") (tstamp 1d05a25a-6b9d-4af4-b850-63ad97918c6f))
    (pad "20" smd roundrect (at 6.55 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "AD6") (pinfunction "Q6") (pintype "tri_state") (tstamp 009e240e-3c03-4986-88fa-08c4ef52ed2a))
    (pad "21" smd roundrect (at 6.55 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "AD7") (pinfunction "Q7") (pintype "tri_state") (tstamp 80a6cf06-d5d7-4c05-addd-ebf6c16f8a92))
    (pad "22" smd roundrect (at 6.55 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "~{LCS}") (pinfunction "~{CS1}") (pintype "input") (tstamp 84f011a9-3c5b-4ff2-a145-384cff07fea7))
    (pad "23" smd roundrect (at 6.55 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "A10") (pinfunction "A10") (pintype "input") (tstamp 73578583-bed8-4788-accf-27e1f821e818))
    (pad "24" smd roundrect (at 6.55 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "~{RD}") (pinfunction "~{OE}") (pintype "input") (tstamp 7a016e2d-8d3b-4937-830e-e8baeea13501))
    (pad "25" smd roundrect (at 6.55 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "A11") (pinfunction "A11") (pintype "input") (tstamp ac7658e8-593f-4901-a60c-0ce64a8eb9e4))
    (pad "26" smd roundrect (at 6.55 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "A9") (pinfunction "A9") (pintype "input") (tstamp 0c466aa4-9af9-431d-91f3-ef25a3355f47))
    (pad "27" smd roundrect (at 6.55 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "A8") (pinfunction "A8") (pintype "input") (tstamp 56a857f0-f1d0-4dc1-8ef1-4d99c8397544))
    (pad "28" smd roundrect (at 6.55 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "A13") (pinfunction "A13") (pintype "input") (tstamp 69f7ea7d-af9b-403a-9c35-1af646e41b3d))
    (pad "29" smd roundrect (at 6.55 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "~{WR}") (pinfunction "~{WE}") (pintype "input") (tstamp a23e0590-d154-4f78-9cfa-16497238b80e))
    (pad "30" smd roundrect (at 6.55 -6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "CS2") (pintype "input") (tstamp 260c63dc-1912-4e06-8a44-acdac06cb9d3))
    (pad "31" smd roundrect (at 6.55 -8.255 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "A15") (pinfunction "A15") (pintype "input") (tstamp fb418e98-12b9-4acf-8c22-87832c71b7c9))
    (pad "32" smd roundrect (at 6.55 -9.525 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 82d0a43f-93af-4e46-b621-904990910517))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-32_11.305x20.495mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 6daf9014-e686-48eb-b518-1ce417fae5b5)
    (at 162.7376 60.1218 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "80-C1206X104G4HACTU")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/97deb713-c4e5-4709-b0b6-ef3012775b1c")
    (attr smd)
    (fp_text reference "C203" (at 0 -1.85) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad9a29bc-96c6-4fa2-8af4-d44a0f0be43f)
    )
    (fp_text value "100n/0.1u PWR" (at 0 1.85) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2fffa2d-0e3b-4a65-95dc-c57424680946)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 9915c1a0-bbd8-4b02-8bcd-0bb1bf445506)
    )
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer "F.SilkS") (width 0.12) (tstamp 4df0fb2b-9113-4ac3-8026-6ada2ad7e822))
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer "F.SilkS") (width 0.12) (tstamp 995f0aa9-d01d-4209-a7dd-a10465f7e369))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 2e320d6f-1074-4680-bfb7-0eee1845f46c))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 41a3ce65-a6cb-42a9-a812-47c3f0016063))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp a7c17a4d-9460-40f8-94a3-db648ffd44b7))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp f88aab04-41dc-48b3-9f96-3fafa0db7e93))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 4207d3e3-8f50-4acb-8254-c632d33b10d2))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 6c6a8396-37c3-4072-ba85-3c5749f21311))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 6e318e83-f452-4e73-ae23-5fe4460098b8))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 9f743b53-ff15-4c4f-9a1f-4ef2bda97dd0))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "VCC") (pintype "passive") (tstamp c765f56a-d4ec-42b7-9fc5-968ddfdabcc9))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive") (tstamp 13a7fa32-1e5c-4268-8ef5-282d08c77209))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 79632853-f337-465f-b7b8-11ec5ad129ca)
    (at 97.79 78.486 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "C0805C220J1GACTU")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/d87e1d3f-bbc2-464c-b2f2-afa2cd205a26")
    (attr smd)
    (fp_text reference "C306" (at 0 -1.68 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b2e6653-461e-4da3-a187-d3a392c89944)
    )
    (fp_text value "33p XTAL" (at 0 1.68 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d743cbc-b577-4f9b-beba-c1734590bd3a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 7696a8e7-d948-489c-99ac-405bed5fe601)
    )
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp 87d04fb9-b3f2-4433-8678-bcf5be9a748e))
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp f61c0300-8fbf-4219-ade9-50edccd563c1))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 312882d5-597e-4e54-991d-c8a445d85f35))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 3272fc0b-7511-4e3f-8852-76748a5e1574))
    (fp_line (start 1.88 0.98) (end -1.88 0.98) (layer "F.CrtYd") (width 0.05) (tstamp a016d147-eb5e-4fad-a09e-7e477e7ccf32))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp ba20f805-a3bb-4142-b213-7f6a9df6cef8))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 4aa5fe63-504b-46c6-a920-79f0a173ee48))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp bd4b2168-e28b-44c4-9b80-7038bb495999))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp c31e026b-626f-4c0b-904e-a61242794e6f))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp faa7008c-7276-401c-8a18-aeeb2bfbd935))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 126 "Net-(C306-Pad1)") (pintype "passive") (tstamp 21427096-bab2-4c66-b8e1-63aa46ca1d09))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive") (tstamp 3271143a-3944-456f-8d78-cb6e20638a2a))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 7e488800-6741-49ab-a5e1-63c0cb97a137)
    (at 132.4225 132.588)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "80-C1206X104G4HACTU")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/1248cd3a-a3de-49b2-b3f4-551c723ed03b")
    (attr smd)
    (fp_text reference "C202" (at 0 -1.85) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8bfbd64a-8222-4d79-a77e-f8a99d155879)
    )
    (fp_text value "100n/0.1u PWR" (at 0 1.85) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dbef0cee-154f-458d-b601-dcd92efd6b6b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 65efed00-7c2a-4ca8-b9b3-d70c2c61c3e5)
    )
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer "F.SilkS") (width 0.12) (tstamp 34acfe06-bad2-4206-baf1-fecc2c13596a))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer "F.SilkS") (width 0.12) (tstamp 4424a430-3a5a-4b6d-af0a-a9954236a4b0))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 015cbf33-14c4-43c7-8f88-6ed4cc309f4a))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 023bf836-6ca3-47d3-a47e-f0c986bc8b75))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 18699b3c-36f2-48f9-a207-f5c12639fa0d))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp f8e48e2f-8f45-490a-9570-0fe6f630329f))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 1ee43728-e07d-48db-a99c-049170d0498d))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 3463d3d7-2021-47a1-a186-8ada9c5839c4))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 81916a55-1611-4be1-81ba-ab955935035e))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp fc9c6648-faa9-408e-b279-2d669549cde4))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "VCC") (pintype "passive") (tstamp 6b6d54bf-b829-4f0c-9828-5c53244f4872))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive") (tstamp 7bf43ece-a7c6-4852-bc61-527ab13ee747))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3) (tstamp 83150091-9395-4ba1-bd12-102d16071454)
    (at 91.8015 107.188)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/8bd978d5-43ec-41b4-8ec2-ea92c522d1cb")
    (attr through_hole)
    (fp_text reference "J305" (at 0.635 -1.695) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a0869643-c4e1-4d55-81b1-763ee14af085)
    )
    (fp_text value "PA" (at -2.54 0 270 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c84e373-517e-426d-a3d4-c6b9ad110994)
    )
    (fp_text user "${REFERENCE}" (at 0.635 2.54 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d138279-30e9-40cb-8ea1-d53672808234)
    )
    (fp_line (start 2.4 -0.695) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 1f36a177-b51c-4d49-b66e-d1512de00bbd))
    (fp_line (start 0.563471 0.76) (end 0.706529 0.76) (layer "F.SilkS") (width 0.12) (tstamp 246f8185-47e1-4b0f-a7f9-1a4084a43624))
    (fp_line (start -1.13 5.775) (end -0.30753 5.775) (layer "F.SilkS") (width 0.12) (tstamp 35758e09-3ce1-4dc1-be0a-4b1f6de1e1ef))
    (fp_line (start -1.13 0.76) (end -1.13 5.775) (layer "F.SilkS") (width 0.12) (tstamp 46038cd5-bd5b-4ad9-9ac5-553f464615d5))
    (fp_line (start 0.76 -0.695) (end 0.96247 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 46c3dd74-a31b-4b4a-bffc-eb041cf0facc))
    (fp_line (start -1.13 -0.76) (end 0 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 50cf7fae-44ce-45f6-99d8-ab332f16ebae))
    (fp_line (start -1.13 0.76) (end -0.563471 0.76) (layer "F.SilkS") (width 0.12) (tstamp 58adb602-2198-47fb-bf7b-1032d31de762))
    (fp_line (start 0.76 -0.563471) (end 0.76 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 726d8895-2bb4-42f2-a433-3bf68fc06cc8))
    (fp_line (start 1.57753 5.775) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 87f26cbb-4d5f-4437-9d75-d1c029fe8c7d))
    (fp_line (start -1.13 0) (end -1.13 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 8ead793c-d9c5-40dd-8d81-e45c65177c51))
    (fp_line (start 0.76 0.706529) (end 0.76 0.563471) (layer "F.SilkS") (width 0.12) (tstamp 99d966a2-cbc2-4094-9d76-8f5285d3dd5f))
    (fp_line (start 1.57753 -0.695) (end 2.4 -0.695) (layer "F.SilkS") (width 0.12) (tstamp bfa0707d-03b7-47e8-9f01-6ad733ac6d28))
    (fp_line (start 0.30753 5.775) (end 0.96247 5.775) (layer "F.SilkS") (width 0.12) (tstamp e89d48ed-8f1d-4161-af56-209ae5cedaa7))
    (fp_line (start -1.6 -1.15) (end -1.6 6.25) (layer "F.CrtYd") (width 0.05) (tstamp 205d501b-1e39-4e3b-8188-d975d72dd067))
    (fp_line (start -1.6 6.25) (end 2.85 6.25) (layer "F.CrtYd") (width 0.05) (tstamp b1c05292-010d-4837-8c16-a4f9b42e0b5f))
    (fp_line (start 2.85 6.25) (end 2.85 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp f40c3236-a27b-437e-8e68-82c6d4662691))
    (fp_line (start 2.85 -1.15) (end -1.6 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp f5fa76dd-a8fe-442f-b7cc-d2b3e8022d51))
    (fp_line (start -0.2175 -0.635) (end 2.34 -0.635) (layer "F.Fab") (width 0.1) (tstamp 2d45d0bb-1b60-4085-a77e-52fa4e0287c8))
    (fp_line (start -1.07 0.2175) (end -0.2175 -0.635) (layer "F.Fab") (width 0.1) (tstamp 50666e07-2dff-48d9-adb2-03119c396ae3))
    (fp_line (start -1.07 5.715) (end -1.07 0.2175) (layer "F.Fab") (width 0.1) (tstamp a148b7f4-045b-47e4-b8b7-734dafab438e))
    (fp_line (start 2.34 5.715) (end -1.07 5.715) (layer "F.Fab") (width 0.1) (tstamp a2ad6352-e43a-4053-81e6-3c399a9234d6))
    (fp_line (start 2.34 -0.635) (end 2.34 5.715) (layer "F.Fab") (width 0.1) (tstamp a8ffe36c-d956-4caa-874e-6b44e4211ec4))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 174 "Net-(J305-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 2e12f3b8-bb38-45b9-b535-a0dcca2e31e6))
    (pad "2" thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 175 "Net-(J305-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 9c9de7d0-7d08-42e2-ad67-97f8db7efc35))
    (pad "3" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 176 "Net-(J305-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp e9b023d3-dfa2-4e9d-b5b5-f338f9a38dd7))
    (pad "4" thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 177 "Net-(J305-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp e8c08eb9-a2a2-473a-b7a5-3bf1a081158d))
    (pad "5" thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 178 "Net-(J305-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 7843d99e-9438-4a82-823c-ec916a7f2f6c))
    (pad "6" thru_hole oval (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 179 "Net-(J305-Pad6)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7ea304a0-eff2-4f0f-bc9d-1f94a446904d))
    (pad "7" thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 180 "Net-(J305-Pad7)") (pinfunction "Pin_7") (pintype "passive") (tstamp e9da5cc1-c1a8-4cbd-be88-3be1f72c20f1))
    (pad "8" thru_hole oval (at 1.27 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 181 "Net-(J305-Pad8)") (pinfunction "Pin_8") (pintype "passive") (tstamp bbb2a81e-6345-4f77-b205-55cc7e7f721e))
    (pad "9" thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive") (tstamp 54ac7797-a064-4f26-922b-4a8e6fdf754b))
    (pad "10" thru_hole oval (at 1.27 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 182 "unconnected-(J305-Pad10)") (pinfunction "Pin_10") (pintype "passive") (tstamp 48e5e766-2d13-481f-8338-7de921d407d5))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF) (tstamp 85ddabdf-3810-4a33-8d7f-ead1786dc68e)
    (at 173.609 145.634)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/d3a25122-f000-4eca-88bb-dcb4966af1f8")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.7) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33b48673-c959-4510-b6fa-fd3f7bdb00fd)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_Pad_Via" (at 0 3.7) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c78d97f4-1d1b-46c3-bcbb-8424944a8978)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15) italic))
      (tstamp 8e5a3783-142f-42f6-a215-d0f81a05c5c0)
    )
    (fp_circle (center 0 0) (end 2.7 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 1c57f8a5-0a6c-44cd-b514-5b9d5f8cc98b))
    (fp_circle (center 0 0) (end 2.95 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp b7013b78-ce5a-47df-9e6f-e993b6073985))
    (pad "1" thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 2628b16a-8b1e-4398-be45-c147110e73bb))
    (pad "1" thru_hole circle (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 2b1a1d99-4ea2-4cae-846a-5609aadc4265))
    (pad "1" thru_hole circle (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 3497045f-d218-47c9-8fd1-2d0a39585aa6))
    (pad "1" thru_hole circle (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 3bc24d10-b3eb-4abe-836d-a8521ccc4341))
    (pad "1" thru_hole circle (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 3cf0233f-86e3-4b85-ad75-fb8a46f37498))
    (pad "1" thru_hole circle (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 594594ee-9de8-45bc-b621-a9251877b0c2))
    (pad "1" thru_hole circle (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 8cf4e6c7-f213-4dc6-a215-9a85d8791784))
    (pad "1" thru_hole circle (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp a2d090b5-bdc2-4863-87f2-2ea46a246d3d))
    (pad "1" thru_hole circle (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp dd552f19-e379-4dd5-a10b-882b6c8e7a65))
  )

  (footprint "Crystal:Crystal_SMD_0603-4Pin_6.0x3.5mm_HandSoldering" (layer "F.Cu")
    (tedit 5A0FD1B2) (tstamp 89cb84a8-dc89-42ca-b87f-411fe5057f13)
    (at 128.7272 98.7298 90)
    (descr "SMD Crystal SERIES SMD0603/4 http://www.petermann-technik.de/fileadmin/petermann/pdf/SMD0603-4.pdf, hand-soldering, 6.0x3.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (property "Description" "RS PRO 16MHz Crystal ±30ppm SMT 4-Pin 6 x 3.5 x 1mm ")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "~")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/5aa93441-ceab-45d4-a2e7-4bc90307ae2f")
    (attr smd)
    (fp_text reference "Y1" (at 0 -3.6 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e39eab16-9692-4234-bbbd-8565d1135dc1)
    )
    (fp_text value "16MHz" (at -1.3462 9.9568) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aaf19f6f-c66c-4e29-b7e2-f243ffb17cb1)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a5fac40-7677-4a2d-b495-26691ffaf1ef)
    )
    (fp_circle (center 0 0) (end 0.333333 0) (layer "F.Adhes") (width 0.133333) (fill none) (tstamp 562f1037-af08-4159-a58e-63e7e58ef857))
    (fp_circle (center 0 0) (end 0.093333 0) (layer "F.Adhes") (width 0.186667) (fill none) (tstamp 7c701330-45d3-486a-bb57-7465c17ad40b))
    (fp_circle (center 0 0) (end 0.213333 0) (layer "F.Adhes") (width 0.133333) (fill none) (tstamp ae951ff5-c8c5-46f4-a70f-d69a2f09ce7b))
    (fp_circle (center 0 0) (end 0.4 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp caa51d87-f1fa-49ac-9ef3-80c0ae4be085))
    (fp_line (start -1.1 -1.95) (end 1.1 -1.95) (layer "F.SilkS") (width 0.12) (tstamp 2f54e94d-2de6-45c6-8494-1eb4132408e8))
    (fp_line (start -1.1 1.95) (end -1.1 2.8) (layer "F.SilkS") (width 0.12) (tstamp 580c17f7-95bc-4b0a-8d4c-36db427ae677))
    (fp_line (start 3.2 -0.3) (end 3.2 0.3) (layer "F.SilkS") (width 0.12) (tstamp 68f5c86c-661b-4096-a813-702cb68638ed))
    (fp_line (start -3.2 0.3) (end -3.2 -0.3) (layer "F.SilkS") (width 0.12) (tstamp 7df3fd22-de7e-4054-9004-a4746fbf168f))
    (fp_line (start 1.1 1.95) (end -1.1 1.95) (layer "F.SilkS") (width 0.12) (tstamp cd7dd474-65b2-4bfe-8b79-793a2672f389))
    (fp_line (start -4.2 0.3) (end -3.2 0.3) (layer "F.SilkS") (width 0.12) (tstamp f45cdba4-f6ec-4933-9dde-ddb591f15d05))
    (fp_line (start -4.3 2.9) (end 4.3 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 2edee38e-e93a-4281-8495-d62f7125bebf))
    (fp_line (start -4.3 -2.9) (end -4.3 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 46bb9798-24c6-4cf3-9622-ff5a15dda441))
    (fp_line (start 4.3 2.9) (end 4.3 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp b10591d6-69cc-4a30-95b9-936c15a346a0))
    (fp_line (start 4.3 -2.9) (end -4.3 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp c9371e67-e57c-4594-8978-f91170b0640b))
    (fp_line (start -2.9 1.75) (end -3 1.65) (layer "F.Fab") (width 0.1) (tstamp 2326e1fe-e71b-4012-a484-420d21f8d27f))
    (fp_line (start 3 -1.65) (end 3 1.65) (layer "F.Fab") (width 0.1) (tstamp 3078c687-2f6a-48f1-994e-9417fbc3d137))
    (fp_line (start -3 1.65) (end -3 -1.65) (layer "F.Fab") (width 0.1) (tstamp 4992fdb8-1d02-40f9-90d4-e37783fa7b64))
    (fp_line (start -3 -1.65) (end -2.9 -1.75) (layer "F.Fab") (width 0.1) (tstamp 7f52473d-750f-4ec7-ac69-a7d2ed94e2fe))
    (fp_line (start 3 1.65) (end 2.9 1.75) (layer "F.Fab") (width 0.1) (tstamp 9c15d5ee-7e84-45f1-ac0c-d2bb2718c1c2))
    (fp_line (start 2.9 1.75) (end -2.9 1.75) (layer "F.Fab") (width 0.1) (tstamp b3dc6c44-e498-4d65-8b82-29f3ac40c565))
    (fp_line (start 2.9 -1.75) (end 3 -1.65) (layer "F.Fab") (width 0.1) (tstamp be6f2b1c-81da-4095-bbc1-80d016edf23e))
    (fp_line (start -3 0.75) (end -2 1.75) (layer "F.Fab") (width 0.1) (tstamp cd10a77e-9039-48e1-88f1-30e6cff9af6c))
    (fp_line (start -2.9 -1.75) (end 2.9 -1.75) (layer "F.Fab") (width 0.1) (tstamp e4a4c001-d5d5-4327-92f5-42c799a0a3a6))
    (pad "1" smd rect (at -2.65 1.55 90) (size 2.7 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/X1") (pinfunction "1") (pintype "passive") (tstamp 2224db12-f3a9-4881-b883-cec7135cf606))
    (pad "2" smd rect (at 2.65 1.55 90) (size 2.7 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "unconnected-(Y1-Pad2)") (pinfunction "2") (pintype "passive+no_connect") (tstamp 1b553ff5-e547-413f-98c0-3d1e8717dd6e))
    (pad "3" smd rect (at 2.65 -1.55 90) (size 2.7 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/X2") (pinfunction "3") (pintype "passive") (tstamp 3ad5ea81-cf91-400f-b135-639084356039))
    (pad "4" smd rect (at -2.65 -1.55 90) (size 2.7 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "unconnected-(Y1-Pad4)") (pinfunction "4") (pintype "passive+no_connect") (tstamp 9206c728-e100-4dcb-9cc9-08bf4da1bdbb))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_0603-4Pin_6.0x3.5mm_HandSoldering.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_0603-4Pin_6.0x3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 8b3f22e5-204d-4aee-b2c2-4adcea04c22e)
    (at 148.209 76.708 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "80-C1206X104G4HACTU")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/ef7fd3ba-de74-45f3-9cee-66fdbcbaa165")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.85 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92440b76-b7cf-4060-95dc-41f21c3ef28c)
    )
    (fp_text value "100n/0.1u PWR" (at -8.763 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 604c29c0-7642-4722-86b9-7fec60e89440)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp e0d9208c-3f94-422a-b59d-929950076345)
    )
    (fp_line (start -0.711252 0.91) (end 0.711252 0.91) (layer "F.SilkS") (width 0.12) (tstamp 2c684d45-344d-4704-9911-26f14e47dc4f))
    (fp_line (start -0.711252 -0.91) (end 0.711252 -0.91) (layer "F.SilkS") (width 0.12) (tstamp 33f8c30d-7c47-4d7f-992e-23df5eaf4209))
    (fp_line (start -2.48 1.15) (end -2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 1d6507a0-e442-40e1-a834-b73324324745))
    (fp_line (start 2.48 1.15) (end -2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 21c615fb-a396-4ca6-8d9a-e012b530dec4))
    (fp_line (start -2.48 -1.15) (end 2.48 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 7946c26a-780a-4e95-ad68-2d6db6123783))
    (fp_line (start 2.48 -1.15) (end 2.48 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 87e560f5-6ffb-4c49-a0e9-d1b74964e65c))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 32d4a039-06b4-4453-ba34-900e46e7d495))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 46c840d4-5d1c-4a24-9cb4-2d1c43e9d959))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 9746cf91-adbf-4b78-875e-49fac4ed9f9c))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp b5be6fb9-d48e-4c83-a267-365d8c1be5af))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "VCC") (pintype "passive") (tstamp 84df0327-2200-4277-bf69-8b0f6906defd))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive") (tstamp cc561496-ebc1-462a-816e-d7bd4e612f44))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "80C188:PLCC-68_SMD-Socket" (layer "F.Cu")
    (tedit 5A02ECC8) (tstamp 8bb25c3c-5145-4c18-af67-23c7dffe6781)
    (at 130.429 77.978 180)
    (descr "PLCC, 68 pins, surface mount")
    (tags "plcc smt")
    (property "Manufacturer_Part_Number" "8468-11B1-RK-TP")
    (property "Mouser Part Number" "517-8468-11B1-RK-TP ")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/f6983918-fe05-46ea-b355-bc522ec53440")
    (attr smd)
    (fp_text reference "J103" (at 0 -16.475) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f299c486-04eb-45f2-8aef-a06041168065)
    )
    (fp_text value "80188" (at 0 16.764) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 09bedbd5-4105-478e-b030-3435d60a589b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f9272c3-5ead-4533-b27f-b68a8338df8b)
    )
    (fp_line (start -1 -15.625) (end -14.625 -15.625) (layer "F.SilkS") (width 0.12) (tstamp 1e4f2f74-562e-4263-bcc3-a7c01762f510))
    (fp_line (start -12.785 -11.635) (end -12.785 -11.135) (layer "F.SilkS") (width 0.1) (tstamp 2f840ee0-5e60-4b76-b85f-1164669bc3ac))
    (fp_line (start -12.785 12.785) (end -12.785 11.135) (layer "F.SilkS") (width 0.1) (tstamp 337e7581-6eea-4b63-98ae-025a60491853))
    (fp_line (start 15.625 15.625) (end 15.625 -15.625) (layer "F.SilkS") (width 0.12) (tstamp 35a34c79-878f-4962-bfbf-fb295e944808))
    (fp_line (start 12.785 -12.785) (end 12.785 -11.135) (layer "F.SilkS") (width 0.1) (tstamp 3df36015-a94c-4021-9208-eb3e3e0ef9a5))
    (fp_line (start -11.635 -12.785) (end -12.785 -11.635) (layer "F.SilkS") (width 0.1) (tstamp 74d6d9e3-8212-43ae-84f0-1236397bf5ea))
    (fp_line (start -14.625 -15.625) (end -15.625 -14.625) (layer "F.SilkS") (width 0.12) (tstamp 756de05c-279e-494f-a17b-a3fd7dc8e0db))
    (fp_line (start -15.625 -14.625) (end -15.625 15.625) (layer "F.SilkS") (width 0.12) (tstamp 75d03828-d021-440d-8571-66f5f447a83b))
    (fp_line (start 12.785 12.785) (end 12.785 11.135) (layer "F.SilkS") (width 0.1) (tstamp 791355bf-3560-4eae-849c-5edab9c3c927))
    (fp_line (start 15.625 -15.625) (end 1 -15.625) (layer "F.SilkS") (width 0.12) (tstamp 8b5c1863-61d0-440d-8616-d4dd8ee52974))
    (fp_line (start 11.135 12.785) (end 12.785 12.785) (layer "F.SilkS") (width 0.1) (tstamp ac85aca2-bcf5-4b98-8f28-ea96725b0922))
    (fp_line (start -11.135 -12.785) (end -11.635 -12.785) (layer "F.SilkS") (width 0.1) (tstamp b219e84d-1df8-452f-ade1-1a171fa6158f))
    (fp_line (start -11.135 12.785) (end -12.785 12.785) (layer "F.SilkS") (width 0.1) (tstamp b263108f-7024-4780-ac3f-2ab4606f6144))
    (fp_line (start 11.135 -12.785) (end 12.785 -12.785) (layer "F.SilkS") (width 0.1) (tstamp c7d5508c-cd17-4e31-ae47-3220f10500a2))
    (fp_line (start -15.625 15.625) (end 15.625 15.625) (layer "F.SilkS") (width 0.12) (tstamp d1bb5d27-bc72-4e54-b565-d0947b881337))
    (fp_line (start -15.95 15.95) (end 15.95 15.95) (layer "F.CrtYd") (width 0.05) (tstamp 0959216e-8212-4ca9-8f4a-8f6d5dea128f))
    (fp_line (start -15.95 -15.95) (end -15.95 15.95) (layer "F.CrtYd") (width 0.05) (tstamp 4ef840e1-b94b-410e-b354-58bf5ea44071))
    (fp_line (start 15.95 15.95) (end 15.95 -15.95) (layer "F.CrtYd") (width 0.05) (tstamp c3a4bf8d-0412-4578-90ee-dfc21a2abdc6))
    (fp_line (start 15.95 -15.95) (end -15.95 -15.95) (layer "F.CrtYd") (width 0.05) (tstamp d39ad4d6-aeb4-41b1-9550-45ed67ae0ce5))
    (fp_line (start 12.635 -12.635) (end -11.635 -12.635) (layer "F.Fab") (width 0.1) (tstamp 2516655b-6283-4d81-84be-20f8de9cc742))
    (fp_line (start -14.205 -14.205) (end -14.205 14.205) (layer "F.Fab") (width 0.1) (tstamp 2d7dfe64-52a2-4cdc-bed6-b06419af7668))
    (fp_line (start 15.475 -15.475) (end -14.475 -15.475) (layer "F.Fab") (width 0.1) (tstamp 395bee41-6f72-4e4f-ae2f-1ba840ea455c))
    (fp_line (start 15.475 15.475) (end 15.475 -15.475) (layer "F.Fab") (width 0.1) (tstamp 4b75be97-0bb6-4cae-8be0-c93d605ee536))
    (fp_line (start 14.205 -14.205) (end -14.205 -14.205) (layer "F.Fab") (width 0.1) (tstamp 536e3398-3cb9-4f9d-8c30-b336fcbc38fd))
    (fp_line (start -12.635 -11.635) (end -12.635 12.635) (layer "F.Fab") (width 0.1) (tstamp 5b3181e6-9841-4763-855b-98fccdb1a04a))
    (fp_line (start -14.475 -15.475) (end -15.475 -14.475) (layer "F.Fab") (width 0.1) (tstamp 81d78136-f262-4a62-b110-76aea0ad6a57))
    (fp_line (start 12.635 12.635) (end 12.635 -12.635) (layer "F.Fab") (width 0.1) (tstamp 9be93b12-1fe8-4beb-a8ea-0dc4043126b0))
    (fp_line (start -0.5 -15.475) (end 0 -14.475) (layer "F.Fab") (width 0.1) (tstamp 9f3446fa-ab8f-4d10-b34b-dd235cc42737))
    (fp_line (start 0 -14.475) (end 0.5 -15.475) (layer "F.Fab") (width 0.1) (tstamp abb2f1e9-5d37-4bed-973a-abc6c0dc94b7))
    (fp_line (start -12.635 12.635) (end 12.635 12.635) (layer "F.Fab") (width 0.1) (tstamp c32246d0-3637-4bb1-827f-1737d461a14a))
    (fp_line (start -15.475 15.475) (end 15.475 15.475) (layer "F.Fab") (width 0.1) (tstamp da6a94ae-7bf6-44e9-8f07-a477601a2e75))
    (fp_line (start -15.475 -14.475) (end -15.475 15.475) (layer "F.Fab") (width 0.1) (tstamp e2f05b7c-4df5-4f59-b389-b9cdb5be7084))
    (fp_line (start -11.635 -12.635) (end -12.635 -11.635) (layer "F.Fab") (width 0.1) (tstamp e45d5510-7475-4840-8e5b-4687dc1548fa))
    (fp_line (start 14.205 14.205) (end 14.205 -14.205) (layer "F.Fab") (width 0.1) (tstamp ec47fc5f-bae3-4479-be81-486db15ec414))
    (fp_line (start -14.205 14.205) (end 14.205 14.205) (layer "F.Fab") (width 0.1) (tstamp f44d257a-4cf0-4fe3-8669-52fcc785c433))
    (pad "1" smd rect (at -11.6725 -10.16 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "A15") (pinfunction "A15") (pintype "output") (tstamp 3a48d86e-2b93-4963-b69c-9afa6d2b2405))
    (pad "2" smd rect (at -11.6725 -8.89 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "AD7") (pinfunction "AD7") (pintype "bidirectional") (tstamp c214d60b-e393-4b4d-9928-8c487cc5f5f9))
    (pad "3" smd rect (at -11.6725 -7.62 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "A14") (pinfunction "A14") (pintype "output") (tstamp 1b7bbd95-a607-4533-bf05-707ea045ec52))
    (pad "4" smd rect (at -11.6725 -6.35 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "AD6") (pinfunction "AD6") (pintype "bidirectional") (tstamp 25470f4a-7a4c-499f-9a25-78d7a98aa2b6))
    (pad "5" smd rect (at -11.6725 -5.08 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "A13") (pinfunction "A13") (pintype "output") (tstamp 429ebada-f01b-4067-b300-cb5957ede48a))
    (pad "6" smd rect (at -11.6725 -3.81 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "AD5") (pinfunction "AD5") (pintype "bidirectional") (tstamp 841da79a-316f-4aae-9f5d-e99104ac4208))
    (pad "7" smd rect (at -11.6725 -2.54 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "A12") (pinfunction "A12") (pintype "output") (tstamp 5d54df50-b677-4ef2-b007-cc1e4f7afd58))
    (pad "8" smd rect (at -11.6725 -1.27 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "AD4") (pinfunction "AD4") (pintype "bidirectional") (tstamp b1eeecaf-3351-47fe-9d25-bf3f2c8cebd8))
    (pad "9" smd rect (at -11.6725 0 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 51a78e8d-7ec8-407e-844b-e87a632d4e9c))
    (pad "10" smd rect (at -11.6725 1.27 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "A11") (pinfunction "A11") (pintype "output") (tstamp 76afec14-f63b-4e27-bc22-d2536e90eefc))
    (pad "11" smd rect (at -11.6725 2.54 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "AD3") (pinfunction "AD3") (pintype "bidirectional") (tstamp 97f02fa7-fa74-48c9-ba45-297f0eec820e))
    (pad "12" smd rect (at -11.6725 3.81 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "A10") (pinfunction "A10") (pintype "output") (tstamp 994849b0-18a6-4c63-9d26-59e8363a3690))
    (pad "13" smd rect (at -11.6725 5.08 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "AD2") (pinfunction "AD2") (pintype "bidirectional") (tstamp 42db2db5-2296-484a-a4d4-e01811a951f5))
    (pad "14" smd rect (at -11.6725 6.35 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "A9") (pinfunction "A9") (pintype "output") (tstamp 9e867a18-b31a-4330-a940-7c8f2ef18d86))
    (pad "15" smd rect (at -11.6725 7.62 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "AD1") (pinfunction "AD1") (pintype "bidirectional") (tstamp 4dc92a06-2b36-4363-b1a1-bb613da2e9d6))
    (pad "16" smd rect (at -11.6725 8.89 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "A8") (pinfunction "A8") (pintype "output") (tstamp a0be4a6d-2a45-4d92-ada7-9d646e5459dd))
    (pad "17" smd rect (at -11.6725 10.16 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "AD0") (pinfunction "AD0") (pintype "bidirectional") (tstamp 822f7aa6-29d7-4213-bd21-117c2e874fcc))
    (pad "18" smd rect (at -10.16 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "DRQ0") (pinfunction "DRQ0") (pintype "input") (tstamp 9db51f03-431d-4485-9b16-7c4bcc0f64b7))
    (pad "19" smd rect (at -8.89 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "DRQ1") (pinfunction "DRQ1") (pintype "input") (tstamp 145154a3-9016-4258-98cc-481e8e7c0c98))
    (pad "20" smd rect (at -7.62 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "Net-(J103-Pad20)") (pinfunction "TMR_IN_0") (pintype "input") (tstamp b3e1588a-adc7-4a7b-a7c5-dc0986ba4ca9))
    (pad "21" smd rect (at -6.35 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "Net-(J103-Pad21)") (pinfunction "TMR_IN_1") (pintype "input") (tstamp 81d46faf-cd5b-41b7-b115-c18f466d771b))
    (pad "22" smd rect (at -5.08 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "TMR_OUT_0") (pinfunction "TMR_OUT_0") (pintype "output") (tstamp a31dac67-2ce1-4236-8499-17b28c1e344f))
    (pad "23" smd rect (at -3.81 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "Net-(J103-Pad23)") (pinfunction "TMR_OUT_1") (pintype "output") (tstamp 69139118-8ffd-407f-bd52-99c0b8ac3523))
    (pad "24" smd rect (at -2.54 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "~{RESET}") (pinfunction "~{RES}") (pintype "input") (tstamp 73d7881c-6fda-4024-9194-16647d79fb0f))
    (pad "25" smd rect (at -1.27 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "~{CS_S}") (pinfunction "~{PCS0}") (pintype "output") (tstamp 114b3b40-5689-484b-b123-8359900d7eef))
    (pad "26" smd rect (at 0 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp 2dde9ab0-5a48-4ab7-b70e-b8d7be31e8a3))
    (pad "27" smd rect (at 1.27 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "~{CS_RTC}") (pinfunction "~{PCS1}") (pintype "output") (tstamp 94420d36-ded9-4c64-ac5c-a7afff70ec70))
    (pad "28" smd rect (at 2.54 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "~{PCS2}") (pinfunction "~{PCS2}") (pintype "output") (tstamp 90a79c1e-4c0a-407c-8c8e-4b250cd2614b))
    (pad "29" smd rect (at 3.81 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "~{PCS3}") (pinfunction "~{PCS3}") (pintype "output") (tstamp e35a14b6-6fe7-470b-9e41-233adf95b599))
    (pad "30" smd rect (at 5.08 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "~{PCS4}") (pinfunction "~{PCS4}") (pintype "output") (tstamp f68525ea-73f0-4559-9863-e7aba16007a1))
    (pad "31" smd rect (at 6.35 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "~{PCS5}") (pinfunction "~{PCS5}/A1") (pintype "output") (tstamp 1f3f6f02-a53a-4228-92d9-cf81f075e800))
    (pad "32" smd rect (at 7.62 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "~{PCS6}") (pinfunction "~{PCS6}/A2") (pintype "output") (tstamp a6428dcd-1617-460f-817c-e78d5714fa74))
    (pad "33" smd rect (at 8.89 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "~{LCS}") (pinfunction "~{LCS}") (pintype "output") (tstamp 61a375ff-925e-4067-9096-8ea91fcb2be2))
    (pad "34" smd rect (at 10.16 11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "~{UCS}") (pinfunction "~{UCS}") (pintype "output") (tstamp 971bf341-9fc5-44e6-b276-a7326fd13ec4))
    (pad "35" smd rect (at 11.6725 10.16 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "unconnected-(J103-Pad35)") (pinfunction "~{MCS3}") (pintype "output+no_connect") (tstamp 94c068fa-4488-4115-96f0-93332854d642))
    (pad "36" smd rect (at 11.6725 8.89 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "unconnected-(J103-Pad36)") (pinfunction "~{MCS2}") (pintype "output+no_connect") (tstamp 5240cc26-3c21-41f4-87cd-a540887dc3da))
    (pad "37" smd rect (at 11.6725 7.62 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "unconnected-(J103-Pad37)") (pinfunction "~{MCS1}") (pintype "output+no_connect") (tstamp 32d04e14-5104-406e-a86c-ab3c251d4c5f))
    (pad "38" smd rect (at 11.6725 6.35 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "unconnected-(J103-Pad38)") (pinfunction "~{MCS0}") (pintype "output+no_connect") (tstamp a1c712b8-8bd0-4727-872c-7e4ab81c07ea))
    (pad "39" smd rect (at 11.6725 5.08 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "~{DEN}") (pinfunction "~{DEN}") (pintype "output") (tstamp 64446e06-a48d-42da-8606-605a9726ae75))
    (pad "40" smd rect (at 11.6725 3.81 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "DT{slash}~{R}") (pinfunction "DT/~{R}") (pintype "output") (tstamp b93f4568-fd2a-4b85-8f9d-e59a724ecc57))
    (pad "41" smd rect (at 11.6725 2.54 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "INT3") (pinfunction "INT3/~{INTA1}/IRQ") (pintype "bidirectional") (tstamp f90e549f-44b5-4d4e-ab38-60c22c0b8dcf))
    (pad "42" smd rect (at 11.6725 1.27 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "INT2") (pinfunction "INT2/~{INTA0}") (pintype "bidirectional") (tstamp 29d302d8-0c81-4299-b483-e501302fff2c))
    (pad "43" smd rect (at 11.6725 0 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 791170d7-06d7-4a87-8435-3aa917d7961a))
    (pad "44" smd rect (at 11.6725 -1.27 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "INT1") (pinfunction "INT1/~{SELECT}") (pintype "input") (tstamp 4eddb413-ec70-4f2f-94d6-a04809414d89))
    (pad "45" smd rect (at 11.6725 -2.54 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "INT0") (pinfunction "INT0") (pintype "input") (tstamp 0db74f21-3eac-4b9e-8d77-d4a556037300))
    (pad "46" smd rect (at 11.6725 -3.81 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "NMI") (pinfunction "NMI") (pintype "input") (tstamp 472d0607-7da0-4976-b990-1a464a56da15))
    (pad "47" smd rect (at 11.6725 -5.08 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "Net-(J103-Pad47)") (pinfunction "~{TEST}") (pintype "bidirectional") (tstamp 060435d1-f947-4bbf-83d4-5d93ac872d18))
    (pad "48" smd rect (at 11.6725 -6.35 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "unconnected-(J103-Pad48)") (pinfunction "~{LOCK}") (pintype "output+no_connect") (tstamp af0d1d8b-76aa-429e-8bf3-6d7bd30aa1ee))
    (pad "49" smd rect (at 11.6725 -7.62 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(J103-Pad49)") (pinfunction "SRDY") (pintype "input") (tstamp ac56b332-b38a-4799-9b06-cbb8f2747fe9))
    (pad "50" smd rect (at 11.6725 -8.89 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "HOLD") (pintype "input") (tstamp 284e66ce-1952-40c9-9c40-17e24a02f9b8))
    (pad "51" smd rect (at 11.6725 -10.16 180) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "unconnected-(J103-Pad51)") (pinfunction "HLDA") (pintype "output+no_connect") (tstamp bed17c09-861a-4d34-82d8-8a72a79293b1))
    (pad "52" smd rect (at 10.16 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "unconnected-(J103-Pad52)") (pinfunction "~{S0}") (pintype "output+no_connect") (tstamp 17a12fb1-a8fa-4605-921b-0076ca5ef133))
    (pad "53" smd rect (at 8.89 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "unconnected-(J103-Pad53)") (pinfunction "~{S1}") (pintype "output+no_connect") (tstamp 4437c00d-cafa-434d-b06d-47dbcef0b306))
    (pad "54" smd rect (at 7.62 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "~{S2}") (pinfunction "~{S2}") (pintype "output") (tstamp 0b3e63f7-acf6-4f89-bb34-87de3fe9651b))
    (pad "55" smd rect (at 6.35 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(J103-Pad55)") (pinfunction "ARDY") (pintype "input") (tstamp a5ab68af-9fe7-462b-a088-0ee61c47528f))
    (pad "56" smd rect (at 5.08 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "BCLK") (pinfunction "CLKOUT") (pintype "output") (tstamp 2093dacb-f34c-4179-b7c6-e03ddc4412dc))
    (pad "57" smd rect (at 3.81 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "RESOUT") (pinfunction "RESET") (pintype "output") (tstamp c5b831c4-2d27-4aea-81b1-4a795c2c2c90))
    (pad "58" smd rect (at 2.54 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/X2") (pinfunction "X2") (pintype "output") (tstamp e2b27fd6-c058-4c10-8221-776983fa5fc0))
    (pad "59" smd rect (at 1.27 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/X1") (pinfunction "X1") (pintype "input") (tstamp fde482a4-f167-4b54-9240-78f8db16ce84))
    (pad "60" smd rect (at 0 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive") (tstamp 68586402-2b32-464b-8520-09c7cc673b1f))
    (pad "61" smd rect (at -1.27 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "ALE") (pinfunction "ALE/QS0") (pintype "output") (tstamp 9e06876e-115c-44ac-af2c-99a3d9a46b5c))
    (pad "62" smd rect (at -2.54 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "~{RD}") (pinfunction "~{RD}/~{QSMD}") (pintype "bidirectional") (tstamp 4ad738a7-5c8b-4887-98dc-3ca96a89d050))
    (pad "63" smd rect (at -3.81 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "~{WR}") (pinfunction "~{WR}/QS1") (pintype "output") (tstamp 2eaa9847-8349-44db-ba99-632d10411d51))
    (pad "64" smd rect (at -5.08 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "unconnected-(J103-Pad64)") (pinfunction "S7") (pintype "output+no_connect") (tstamp a2083898-f9d7-4906-ac0f-8df11434a306))
    (pad "65" smd rect (at -6.35 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "XA19") (pinfunction "A19/S6") (pintype "output") (tstamp 15f2c487-72e3-4c7f-9da8-ca57e89f6d47))
    (pad "66" smd rect (at -7.62 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "XA18") (pinfunction "A18/S5") (pintype "output") (tstamp ad509dec-838d-420a-a261-cbbf2608e45d))
    (pad "67" smd rect (at -8.89 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "XA17") (pinfunction "A17/S4") (pintype "output") (tstamp b31e01ec-ca12-4ef9-804b-f7a484d62d79))
    (pad "68" smd rect (at -10.16 -11.6725 180) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "XA16") (pinfunction "A16/S3") (pintype "output") (tstamp c95e5b5d-2620-4a91-ae76-555017154f32))
    (model "${KICAD6_3DMODEL_DIR}/Package_LCC.3dshapes/PLCC-68_SMD-Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/plcc68_p1-27_l24-33_w24-33.stp"
      (offset (xyz 0 0 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )

  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1) (tstamp 961f5ed3-0278-4f1a-ada8-01fcaeb55b9d)
    (at 159.131 68.58)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Manufacturer_Part_Number" "74VHCT573AFT")
    (property "RS" "")
    (property "RS Part Number" "171-3540")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/2105a0d7-04f6-4347-ad89-619ecd118196")
    (attr smd)
    (fp_text reference "U201" (at 0 -7.35) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a4652f1b-0c9a-4077-9aeb-68e90dbbd370)
    )
    (fp_text value "74LS573" (at 0 7.35) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92b36872-a6f5-48a4-b66f-42fb1d7d4012)
    )
    (fp_text user "${REFERENCE}" (at 0.254 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a8ba8f8-2301-4c65-8160-d6052709e235)
    )
    (fp_line (start -3.86 -6.51) (end -3.86 -6.275) (layer "F.SilkS") (width 0.12) (tstamp 03a44891-d3d3-42a2-a8fe-9e5d78d0a265))
    (fp_line (start 0 -6.51) (end -3.86 -6.51) (layer "F.SilkS") (width 0.12) (tstamp 0bcd96cf-bcea-4c6a-a153-da3cf905af26))
    (fp_line (start -3.86 -6.275) (end -5.675 -6.275) (layer "F.SilkS") (width 0.12) (tstamp 23987001-bb48-4d49-83e6-be7b96c056e9))
    (fp_line (start 3.86 6.51) (end 3.86 6.275) (layer "F.SilkS") (width 0.12) (tstamp 34a15b3a-aae4-408c-82b1-e9cf8bf45d09))
    (fp_line (start 0 6.51) (end 3.86 6.51) (layer "F.SilkS") (width 0.12) (tstamp 3f07e880-3e98-48b9-964f-49f53c80f443))
    (fp_line (start 0 6.51) (end -3.86 6.51) (layer "F.SilkS") (width 0.12) (tstamp 95f3d22a-a988-4b80-9c44-4531f8d09c31))
    (fp_line (start 0 -6.51) (end 3.86 -6.51) (layer "F.SilkS") (width 0.12) (tstamp 9cdc1589-0a47-464f-9f73-6cfb3c0130a4))
    (fp_line (start -3.86 6.51) (end -3.86 6.275) (layer "F.SilkS") (width 0.12) (tstamp d8fe7664-94ac-4e37-ab62-32c3f70c28fe))
    (fp_line (start 3.86 -6.51) (end 3.86 -6.275) (layer "F.SilkS") (width 0.12) (tstamp f58462a4-4d64-43f5-8a8e-452bec5e893a))
    (fp_line (start -5.93 6.65) (end 5.93 6.65) (layer "F.CrtYd") (width 0.05) (tstamp 2f067069-755c-48cf-a887-5c02b07e55cd))
    (fp_line (start 5.93 6.65) (end 5.93 -6.65) (layer "F.CrtYd") (width 0.05) (tstamp 4de8b33a-4e46-4512-89b7-a8cd75352305))
    (fp_line (start -5.93 -6.65) (end -5.93 6.65) (layer "F.CrtYd") (width 0.05) (tstamp b337d7c9-8ff7-496d-bdee-2dc17d00c809))
    (fp_line (start 5.93 -6.65) (end -5.93 -6.65) (layer "F.CrtYd") (width 0.05) (tstamp bc8cba45-ac66-4aa0-af1f-31f47c672d29))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer "F.Fab") (width 0.1) (tstamp 52c1200d-bf50-477a-9fb1-ea876d001dab))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer "F.Fab") (width 0.1) (tstamp 935b8931-c164-4d1f-ae52-e60fb1bc948f))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer "F.Fab") (width 0.1) (tstamp acd76eb5-984b-4dab-9d06-3e1ad7e8a110))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer "F.Fab") (width 0.1) (tstamp b4cd8bc5-a2af-457e-a3b8-e08293896eff))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer "F.Fab") (width 0.1) (tstamp b5e2fdb9-a60a-48d3-87d9-178a4e2a6abe))
    (pad "1" smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "OE") (pintype "input") (tstamp 24dc8e07-a4ae-4aec-8f0b-c8ecbf705afc))
    (pad "2" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "AD0") (pinfunction "D0") (pintype "input") (tstamp 64eae7fe-f99d-48ce-8e63-6fb4d5c1d7e9))
    (pad "3" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "AD1") (pinfunction "D1") (pintype "input") (tstamp 28612ef5-b15b-4e7f-91e5-36445fb21d6f))
    (pad "4" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "AD2") (pinfunction "D2") (pintype "input") (tstamp cd34799a-1b53-4019-93b6-3b14a3bf8570))
    (pad "5" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "AD3") (pinfunction "D3") (pintype "input") (tstamp 7704e066-e868-40f0-8e32-9811bf8831a2))
    (pad "6" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "AD4") (pinfunction "D4") (pintype "input") (tstamp bdeeeea9-d97a-46d4-a88c-d850057534df))
    (pad "7" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "AD5") (pinfunction "D5") (pintype "input") (tstamp 4b9a77c9-be04-4b4e-8f45-518bb39b3248))
    (pad "8" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "AD6") (pinfunction "D6") (pintype "input") (tstamp e8de81af-977e-4eb7-9b4a-1b5abf3710d5))
    (pad "9" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "AD7") (pinfunction "D7") (pintype "input") (tstamp d1386a33-c54d-4e1e-b927-dc9b50cc0cc2))
    (pad "10" smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 6555ec63-f46a-4905-9716-f0b547014531))
    (pad "11" smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "Load") (pintype "input") (tstamp 48d65cbb-31f5-4a05-af81-5024a215e532))
    (pad "12" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "A7") (pinfunction "Q7") (pintype "tri_state") (tstamp 7f790a28-c89f-47b9-bcf9-f78f431158b8))
    (pad "13" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "A6") (pinfunction "Q6") (pintype "tri_state") (tstamp f09c3495-a651-4a73-a130-32987611d91b))
    (pad "14" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "A5") (pinfunction "Q5") (pintype "tri_state") (tstamp 0e232d15-fa68-49c9-86f3-511d8678705a))
    (pad "15" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "A4") (pinfunction "Q4") (pintype "tri_state") (tstamp 94300b66-0f66-4b71-919b-d00fec2566ad))
    (pad "16" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "A3") (pinfunction "Q3") (pintype "tri_state") (tstamp b588e5bd-98ab-414a-987a-75d509df9bee))
    (pad "17" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "A2") (pinfunction "Q2") (pintype "tri_state") (tstamp 627f1d71-18bf-4bf7-8d4d-f7298c7c8f24))
    (pad "18" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "A1") (pinfunction "Q1") (pintype "tri_state") (tstamp a5b56de6-68de-4218-b010-d9b24530fb74))
    (pad "19" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "A0") (pinfunction "Q0") (pintype "tri_state") (tstamp 41d80508-e4fb-4454-b544-61a2da91c43c))
    (pad "20" smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp ec9d9fa8-e4db-4064-bbf1-f73c5807fa8e))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp a37f1f80-b769-4830-b380-2d8b4ead3bd8)
    (at 106.553 69.596 -90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (property "exclude_from_bom" "")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/ba24a821-97d7-46aa-8988-96e6dcf98f28")
    (attr through_hole exclude_from_bom)
    (fp_text reference "J301" (at 0 -2.33 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 15f94254-065d-41fa-b424-425549b3444b)
    )
    (fp_text value "UART1" (at 2.54 14.224 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 27887463-580f-4f2b-b4cf-2ee6e95f5aa5)
    )
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b16e7b1-8e82-4d56-b285-b9c355086eec)
    )
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 083f9fff-7f71-4550-8a9d-a73e30e6ac35))
    (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 213c92b3-0b4f-4371-aac8-a1d71cb34cdd))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 9dd8871d-6b94-4ff7-8883-5703cc3c9fa6))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp a497b59b-edfc-4f58-9fee-dc35231343ff))
    (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp c6d524df-4eef-4c53-a7f1-c5d3b5dd0ab7))
    (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp fc2b51d2-9db1-4fb1-8aae-961f00848f5d))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 1f761acf-0e97-4d3d-9306-67dfd5a0b1df))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 3a3d5b97-f306-43ba-aef7-9adc080f0096))
    (fp_line (start -1.8 14.5) (end 1.8 14.5) (layer "F.CrtYd") (width 0.05) (tstamp 3b80c39f-f9b1-46eb-aa34-45fb2d7226c4))
    (fp_line (start -1.8 -1.8) (end -1.8 14.5) (layer "F.CrtYd") (width 0.05) (tstamp fef63519-bdd9-4f91-9101-f32dd3c2a109))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 570ca29b-1057-450a-815c-31f4628ed197))
    (fp_line (start -1.27 13.97) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 77ffbf13-f3dc-4a91-8a51-54b13a5475fa))
    (fp_line (start 1.27 -1.27) (end 1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp 86ef6b16-15ed-400a-bb18-a427454eaacd))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp d286ae30-b4b0-463c-853c-98df6e4054b0))
    (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp f2f879f2-5c8d-4f4e-be6a-4462d9e98652))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 49f7aa52-6acd-4a9d-988f-979f22376f5d))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "UART1.~{RTS}") (pinfunction "Pin_2") (pintype "passive") (tstamp 712bc791-6749-43ea-982f-61769955a93f))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "DCD") (pinfunction "Pin_3") (pintype "passive") (tstamp 6b713e87-fab6-4e62-aa34-a6547235ff22))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "UART1.IN") (pinfunction "Pin_4") (pintype "passive") (tstamp 133c4822-a742-4de9-adde-dab4ee5c73da))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "UART1.OUT") (pinfunction "Pin_5") (pintype "passive") (tstamp 140932e5-7bd7-4365-ab3a-dd0f205a23c7))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "UART1.~{CTS}") (pinfunction "Pin_6") (pintype "passive") (tstamp 1f603a0e-3d57-4c6d-ac23-06de012a7524))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:TSSOP-40_6.1x11mm_P0.5mm" (layer "F.Cu")
    (tedit 5E476F32) (tstamp aa805fdf-7892-4ac0-bc95-218d6add9fe1)
    (at 101.3165 103.378 180)
    (descr "TSSOP, 40 Pin (JEDEC MO-153 Var EC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/8aa3d486-1666-410d-b896-ec5decb640e2")
    (attr smd)
    (fp_text reference "U304" (at 0 -6.45) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9e51a163-de95-4ea7-9cb1-ce4f2e21581b)
    )
    (fp_text value "82C55A" (at 0 6.45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13a674ee-12c5-418f-b803-f03c79ed7b3b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9218bc94-862c-4480-9d59-169446a3ce74)
    )
    (fp_line (start 0 -5.61) (end 3.16 -5.61) (layer "F.SilkS") (width 0.12) (tstamp 419da631-d0be-4eec-b5fa-bab5b1554d3c))
    (fp_line (start 3.16 -5.61) (end 3.16 -5.16) (layer "F.SilkS") (width 0.12) (tstamp 49988e13-9da4-4fec-afd0-a6c92e32567a))
    (fp_line (start 0 5.61) (end -3.16 5.61) (layer "F.SilkS") (width 0.12) (tstamp 75c08938-dc5b-40ca-9fca-e94464fb7ea1))
    (fp_line (start 3.16 5.61) (end 3.16 5.16) (layer "F.SilkS") (width 0.12) (tstamp 7cfab01d-2b3f-4319-acb5-4500132e2bd6))
    (fp_line (start -3.16 5.61) (end -3.16 5.16) (layer "F.SilkS") (width 0.12) (tstamp 952b9e41-30a1-4407-b141-aa5fe31284fb))
    (fp_line (start 0 5.61) (end 3.16 5.61) (layer "F.SilkS") (width 0.12) (tstamp a06ccd14-f464-4586-be33-f78100269406))
    (fp_line (start 0 -5.61) (end -3.16 -5.61) (layer "F.SilkS") (width 0.12) (tstamp a3dc3276-af23-44e8-b799-09926e517caa))
    (fp_line (start -3.16 -5.16) (end -4.45 -5.16) (layer "F.SilkS") (width 0.12) (tstamp a746dfd6-ca86-4e10-a64b-fdbb0ab5452f))
    (fp_line (start -3.16 -5.61) (end -3.16 -5.16) (layer "F.SilkS") (width 0.12) (tstamp d657a340-38e0-4bd7-8937-55ddb9044bb0))
    (fp_line (start -4.7 -5.75) (end -4.7 5.75) (layer "F.CrtYd") (width 0.05) (tstamp 36cce645-2cf7-47c1-b408-ff8661a33c35))
    (fp_line (start 4.7 5.75) (end 4.7 -5.75) (layer "F.CrtYd") (width 0.05) (tstamp 52116e87-4a27-4cf4-9464-f7c358aae7ba))
    (fp_line (start -4.7 5.75) (end 4.7 5.75) (layer "F.CrtYd") (width 0.05) (tstamp 87aa915f-d69d-440e-8e05-b8f22e42acfd))
    (fp_line (start 4.7 -5.75) (end -4.7 -5.75) (layer "F.CrtYd") (width 0.05) (tstamp b780fc18-d22d-4bce-9ef1-7cfab19e85d5))
    (fp_line (start -3.05 5.5) (end -3.05 -4.5) (layer "F.Fab") (width 0.1) (tstamp 1e64f44c-3c79-43d7-82c2-f1fead004a4e))
    (fp_line (start -2.05 -5.5) (end 3.05 -5.5) (layer "F.Fab") (width 0.1) (tstamp 22dd2b8c-a848-45ae-a4dd-2ba875eb25ec))
    (fp_line (start 3.05 -5.5) (end 3.05 5.5) (layer "F.Fab") (width 0.1) (tstamp 51c5f14d-ab37-45cd-889c-de87f9fb31b6))
    (fp_line (start 3.05 5.5) (end -3.05 5.5) (layer "F.Fab") (width 0.1) (tstamp 6b3cba98-ab20-4794-b86c-ec70647f0575))
    (fp_line (start -3.05 -4.5) (end -2.05 -5.5) (layer "F.Fab") (width 0.1) (tstamp ad53285a-9923-422d-89e4-44abd219b536))
    (pad "1" smd roundrect (at -3.7125 -4.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 177 "Net-(J305-Pad4)") (pinfunction "PA3") (pintype "bidirectional") (tstamp 74aeee73-e76b-4f7a-98a0-f47dfafa7a7b))
    (pad "2" smd roundrect (at -3.7125 -4.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 176 "Net-(J305-Pad3)") (pinfunction "PA2") (pintype "bidirectional") (tstamp cc85f753-74d0-4a30-a5b0-f78669b8bc65))
    (pad "3" smd roundrect (at -3.7125 -3.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 175 "Net-(J305-Pad2)") (pinfunction "PA1") (pintype "bidirectional") (tstamp 7bbe0916-8fe0-4afe-9935-85c781455ad7))
    (pad "4" smd roundrect (at -3.7125 -3.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 174 "Net-(J305-Pad1)") (pinfunction "PA0") (pintype "bidirectional") (tstamp 4280dd67-e2ff-4555-8f60-ab4a64321e8e))
    (pad "5" smd roundrect (at -3.7125 -2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "~{IOR}") (pinfunction "~{RD}") (pintype "input") (tstamp 8ae91e36-ea83-4e54-b886-4c5b0cdbf164))
    (pad "6" smd roundrect (at -3.7125 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 183 "P2.~{CS}") (pinfunction "~{CS}") (pintype "input") (tstamp 8c0b33d8-8e29-4c9a-83ed-893f97f934f0))
    (pad "7" smd roundrect (at -3.7125 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 16f41780-8378-494f-9acc-8fb6063ad75e))
    (pad "8" smd roundrect (at -3.7125 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "A1") (pinfunction "A1") (pintype "input") (tstamp fd171f87-56f8-4402-8856-bfa4d937cc08))
    (pad "9" smd roundrect (at -3.7125 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "A0") (pinfunction "A0") (pintype "input") (tstamp 7dffd24d-130f-4961-91bb-5d11993fc5ff))
    (pad "10" smd roundrect (at -3.7125 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "unconnected-(U304-Pad10)") (pinfunction "PC7") (pintype "bidirectional") (tstamp 9d1862ba-f935-417c-abf7-a4ac25b8717d))
    (pad "11" smd roundrect (at -3.7125 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 185 "unconnected-(U304-Pad11)") (pinfunction "PC6") (pintype "bidirectional") (tstamp 61be0fd2-1ac6-420b-bcb7-15592f4e8ffa))
    (pad "12" smd roundrect (at -3.7125 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 186 "unconnected-(U304-Pad12)") (pinfunction "PC5") (pintype "bidirectional") (tstamp 102746ae-cdad-4fae-b60d-e8a914dc7a9c))
    (pad "13" smd roundrect (at -3.7125 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 187 "unconnected-(U304-Pad13)") (pinfunction "PC4") (pintype "bidirectional") (tstamp 543ac115-1cc0-4a74-b5f5-d4a6fe430882))
    (pad "14" smd roundrect (at -3.7125 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 188 "unconnected-(U304-Pad14)") (pinfunction "PC0") (pintype "bidirectional") (tstamp 9fbabc39-0841-4a0f-8eb2-57c3ff86fe58))
    (pad "15" smd roundrect (at -3.7125 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 189 "unconnected-(U304-Pad15)") (pinfunction "PC1") (pintype "bidirectional") (tstamp eba06e47-3d25-4001-be84-c4bf15cfd9b0))
    (pad "16" smd roundrect (at -3.7125 2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "unconnected-(U304-Pad16)") (pinfunction "PC2") (pintype "bidirectional") (tstamp eabb7408-227a-4c36-b6b8-01667372d952))
    (pad "17" smd roundrect (at -3.7125 3.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 191 "P2.~{IRQ}") (pinfunction "PC3") (pintype "bidirectional") (tstamp 28077235-c114-4c94-9d8d-7eb3f63ba4f4))
    (pad "18" smd roundrect (at -3.7125 3.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "Net-(J304-Pad1)") (pinfunction "PB0") (pintype "bidirectional") (tstamp 0ec8a8f5-ef82-426b-abef-06cd98bfd37b))
    (pad "19" smd roundrect (at -3.7125 4.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(J304-Pad2)") (pinfunction "PB1") (pintype "bidirectional") (tstamp 7e7168c3-bf50-4119-a067-91ddb7736d49))
    (pad "20" smd roundrect (at -3.7125 4.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 167 "Net-(J304-Pad3)") (pinfunction "PB2") (pintype "bidirectional") (tstamp d8c5d53c-051a-42f1-ae5f-66708a0d35ab))
    (pad "21" smd roundrect (at 3.7125 4.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 168 "Net-(J304-Pad4)") (pinfunction "PB3") (pintype "bidirectional") (tstamp 09463994-bba1-4492-b0f0-70b909d40652))
    (pad "22" smd roundrect (at 3.7125 4.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 169 "Net-(J304-Pad5)") (pinfunction "PB4") (pintype "bidirectional") (tstamp d38400e5-3802-43cf-b199-36927fdd52b2))
    (pad "23" smd roundrect (at 3.7125 3.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 170 "Net-(J304-Pad6)") (pinfunction "PB5") (pintype "bidirectional") (tstamp 6793745d-d371-4294-856f-fdab033b8436))
    (pad "24" smd roundrect (at 3.7125 3.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 171 "Net-(J304-Pad7)") (pinfunction "PB6") (pintype "bidirectional") (tstamp 5c131b80-1636-4e75-a4c1-f2f80ef0d9f8))
    (pad "25" smd roundrect (at 3.7125 2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 172 "Net-(J304-Pad8)") (pinfunction "PB7") (pintype "bidirectional") (tstamp a0c83be5-d60a-48ed-9721-8f344e497da7))
    (pad "26" smd roundrect (at 3.7125 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp a68c7b78-b7d9-430c-9761-26827fe17971))
    (pad "27" smd roundrect (at 3.7125 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "DB7") (pinfunction "D7") (pintype "bidirectional") (tstamp 0d78cf16-7fc5-48d2-aaad-a313512bee73))
    (pad "28" smd roundrect (at 3.7125 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "DB6") (pinfunction "D6") (pintype "bidirectional") (tstamp 56d8b128-7cb2-403a-8495-de8194056dc2))
    (pad "29" smd roundrect (at 3.7125 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "DB5") (pinfunction "D5") (pintype "bidirectional") (tstamp feb51600-ee52-407d-aeeb-3c912b1c28b7))
    (pad "30" smd roundrect (at 3.7125 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "DB4") (pinfunction "D4") (pintype "bidirectional") (tstamp dbf4dd54-5572-4c81-a6ea-cc3db9c62196))
    (pad "31" smd roundrect (at 3.7125 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "DB3") (pinfunction "D3") (pintype "bidirectional") (tstamp a403537f-92e2-497f-9941-7126cc77cb77))
    (pad "32" smd roundrect (at 3.7125 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "DB2") (pinfunction "D2") (pintype "bidirectional") (tstamp 266f4748-3cbe-4901-802c-c914eb90b8ad))
    (pad "33" smd roundrect (at 3.7125 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "DB1") (pinfunction "D1") (pintype "bidirectional") (tstamp 57fc385b-baf1-4989-9e64-ebc63a6d75d6))
    (pad "34" smd roundrect (at 3.7125 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "DB0") (pinfunction "D0") (pintype "bidirectional") (tstamp 4c87be66-4f53-4c61-81f1-e44211337d8a))
    (pad "35" smd roundrect (at 3.7125 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "RESET") (pintype "input") (tstamp a0a96acb-7b2d-46c9-a1e5-810f035c1359))
    (pad "36" smd roundrect (at 3.7125 -2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "~{IOW}") (pinfunction "~{WR}") (pintype "input") (tstamp b82b386e-c93e-4370-9b19-0683df4352e1))
    (pad "37" smd roundrect (at 3.7125 -3.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(J305-Pad8)") (pinfunction "PA7") (pintype "bidirectional") (tstamp d613febf-096b-407b-b1f0-0475b1361c1c))
    (pad "38" smd roundrect (at 3.7125 -3.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(J305-Pad7)") (pinfunction "PA6") (pintype "bidirectional") (tstamp 61c9c156-abc0-49ec-8f71-c62acaf0a6c8))
    (pad "39" smd roundrect (at 3.7125 -4.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(J305-Pad6)") (pinfunction "PA5") (pintype "bidirectional") (tstamp dbe77e5d-dd7b-4866-b0dc-242ad2b09c1e))
    (pad "40" smd roundrect (at 3.7125 -4.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 178 "Net-(J305-Pad5)") (pinfunction "PA4") (pintype "bidirectional") (tstamp da3d9a97-a7e8-4daf-9c9c-92dd2cc2ea87))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-40_6.1x11mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF) (tstamp ad5d2f01-42d8-4a0a-9705-5596e74b97ea)
    (at 93.599 145.634 -90)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/cad37c48-63b4-471b-8712-a03d5b9149d0")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.7 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2d24be9-0a91-4ad8-a6f8-4f606bd871ac)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_Pad_Via" (at 0 3.7 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1354903a-b7d2-4e04-b220-6c6c8f058ef7)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15) italic))
      (tstamp e0660a46-ff2a-4b28-b311-cf71bc999b82)
    )
    (fp_circle (center 0 0) (end 2.7 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 78d3a4a0-e724-44e1-963f-de88a39d4158))
    (fp_circle (center 0 0) (end 2.95 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 4a56ac62-5ec2-46fc-a86c-9adf2d8fead1))
    (pad "1" thru_hole circle (at -1.431891 -1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 6476e233-d260-45fe-84d2-9ade7d0003a0))
    (pad "1" thru_hole circle (at 0 -2.025 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 8dcf40e6-09a5-42e4-8b46-f4738540468d))
    (pad "1" thru_hole circle (at -2.025 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 90207e9d-650a-4c45-b7d5-e506cc85537d))
    (pad "1" thru_hole circle (at 0 0 270) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp a29e1299-22c5-4fd2-9a37-e405785962a9))
    (pad "1" thru_hole circle (at 1.431891 1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp a8cdda0e-7b06-4b92-8078-341b4e32614a))
    (pad "1" thru_hole circle (at 1.431891 -1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp bc408f2c-2338-4a2e-9d30-e90fd4d4f487))
    (pad "1" thru_hole circle (at -1.431891 1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp d6cc98ff-7d68-4734-afa1-c7dd225e08d3))
    (pad "1" thru_hole circle (at 2.025 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp efd79052-e146-4d61-9e0a-ba764a5a966b))
    (pad "1" thru_hole circle (at 0 2.025 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp fdd41a68-206a-4076-b64a-8b7633d428d6))
  )

  (footprint "69802-132LF:69802132LF" (layer "F.Cu")
    (tedit 0) (tstamp ae0418f2-412f-4c9b-b974-9adcb9cccbd6)
    (at 163.957 120.65 180)
    (descr "69802-132LF-2")
    (tags "Connector")
    (property "Manufacturer_Part_Number" "SST39SF020A-70-4C-NHE")
    (property "Mouser Part Number" "804-39SF020A7CNHE ")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/2a8f5e33-ed01-45e7-abb2-3926cf17e285")
    (attr through_hole)
    (fp_text reference "J104" (at 0 -0.37) (layer "F.SilkS") hide
      (effects (font (size 1.27 1.27) (thickness 0.254)))
      (tstamp ed4ca47a-c3c3-4896-a3be-5aa2cee3c182)
    )
    (fp_text value "256K ROM" (at -0.254 11.568) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b3fc2874-f217-48da-a67f-e5b3ca4ca0df)
    )
    (fp_text user "${REFERENCE}" (at 0 -0.37) (layer "F.Fab")
      (effects (font (size 1.27 1.27) (thickness 0.254)))
      (tstamp 0041abb1-146f-4b49-add4-1f555ac49d4b)
    )
    (fp_line (start 8.89 10.16) (end -8.89 10.16) (layer "F.SilkS") (width 0.1) (tstamp 35a4ec84-b069-449d-a08a-6635d34b31c7))
    (fp_line (start -6.985 -10.16) (end 8.89 -10.16) (layer "F.SilkS") (width 0.1) (tstamp 3fd05627-b166-47c3-bddd-c847d3ea980a))
    (fp_line (start 8.89 -10.16) (end 8.89 10.16) (layer "F.SilkS") (width 0.1) (tstamp 4726c0e8-8a39-4634-bbdd-1586892894ff))
    (fp_line (start -8.89 -8.255) (end -6.985 -10.16) (layer "F.SilkS") (width 0.1) (tstamp b5d2f80f-3e6e-4293-9598-0b47f1de816e))
    (fp_line (start -8.89 10.16) (end -8.89 -8.255) (layer "F.SilkS") (width 0.1) (tstamp eeef49b5-b4a2-4494-ade2-96990466e996))
    (fp_line (start 9.89 11.16) (end -9.89 11.16) (layer "F.CrtYd") (width 0.1) (tstamp 6a50fa86-29e4-4132-bfaf-82d6d3513628))
    (fp_line (start 9.89 -11.9) (end 9.89 11.16) (layer "F.CrtYd") (width 0.1) (tstamp 7e372bcd-bebe-440f-b328-430a2879b611))
    (fp_line (start -9.89 11.16) (end -9.89 -11.9) (layer "F.CrtYd") (width 0.1) (tstamp ae94071f-5ce5-4d16-93d9-66da9bd5d2f6))
    (fp_line (start -9.89 -11.9) (end 9.89 -11.9) (layer "F.CrtYd") (width 0.1) (tstamp fa9a939f-a322-495c-8e5a-4c6db17a6d58))
    (fp_line (start 8.89 10.16) (end -8.89 10.16) (layer "F.Fab") (width 0.2) (tstamp 6d3373f6-da41-4db5-bef8-1bf98634ddd8))
    (fp_line (start 8.89 -10.16) (end 8.89 10.16) (layer "F.Fab") (width 0.2) (tstamp 7b702f79-79b8-425e-b8e0-0d699faa190a))
    (fp_line (start -8.89 10.16) (end -8.89 -10.16) (layer "F.Fab") (width 0.2) (tstamp 8927f329-ec2f-4857-ac45-a8b9849444c6))
    (fp_line (start -8.89 -10.16) (end 8.89 -10.16) (layer "F.Fab") (width 0.2) (tstamp c2673077-87eb-4dd3-8bac-3390d2286e20))
    (pad "1" smd rect (at 0 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "unconnected-(J104-Pad1)") (pinfunction "VPP") (pintype "input+no_connect") (tstamp ee466d3f-0e6b-4d88-9c0f-cc95d6d3e711))
    (pad "2" smd rect (at -1.27 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "A16") (pinfunction "A16") (pintype "input") (tstamp 48e4b4dd-cd38-4424-8ca6-4d93976130d2))
    (pad "3" smd rect (at -2.54 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "A15") (pinfunction "A15") (pintype "input") (tstamp 8c517431-e273-4390-adcb-5be46b464044))
    (pad "4" smd rect (at -3.81 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "A12") (pinfunction "A12") (pintype "input") (tstamp f7c8a60b-0f67-42a5-a535-21683b72248e))
    (pad "5" smd rect (at -5.51 -5.08 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "A7") (pinfunction "A7") (pintype "input") (tstamp 01ea9bec-b6ab-4a8a-aeb0-2801e47a054f))
    (pad "6" smd rect (at -5.51 -3.81 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "A6") (pinfunction "A6") (pintype "input") (tstamp 4dc6aa61-4d4e-490e-94d3-bc4a385691ef))
    (pad "7" smd rect (at -5.51 -2.54 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "A5") (pinfunction "A5") (pintype "input") (tstamp abb400a5-c5af-4c33-8e5b-b2ee8645a002))
    (pad "8" smd rect (at -5.51 -1.27 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "A4") (pinfunction "A4") (pintype "input") (tstamp ab99e9f6-936a-4bdf-a56a-00e887508c10))
    (pad "9" smd rect (at -5.51 0 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "A3") (pinfunction "A3") (pintype "input") (tstamp efc3e04d-7717-42ab-b6c9-81242cff7db2))
    (pad "10" smd rect (at -5.51 1.27 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "A2") (pinfunction "A2") (pintype "input") (tstamp 9bfdb72c-e4a4-408c-aa85-8874535e6098))
    (pad "11" smd rect (at -5.51 2.54 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "A1") (pinfunction "A1") (pintype "input") (tstamp 8ba6b1f6-76b4-4097-a063-dda38182e3c5))
    (pad "12" smd rect (at -5.51 3.81 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "A0") (pinfunction "A0") (pintype "input") (tstamp 805479e4-ade7-4ba8-8074-b449fa07de7f))
    (pad "13" smd rect (at -5.51 5.08 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "AD0") (pinfunction "D0") (pintype "tri_state") (tstamp 5369f466-30cf-4886-b50f-805d1b10b246))
    (pad "14" smd rect (at -3.81 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "AD1") (pinfunction "D1") (pintype "tri_state") (tstamp 092be7e7-3c0c-487d-b880-af3017f83971))
    (pad "15" smd rect (at -2.54 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "AD2") (pinfunction "D2") (pintype "tri_state") (tstamp 13dd0491-5fd0-4ba8-97ac-2923189da359))
    (pad "16" smd rect (at -1.27 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp fb85f2bc-61d9-400b-a7ce-61f026533c62))
    (pad "17" smd rect (at 0 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "AD3") (pinfunction "D3") (pintype "tri_state") (tstamp 16f55ffa-8911-43ed-8f46-b2e6854b6e7f))
    (pad "18" smd rect (at 1.27 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "AD4") (pinfunction "D4") (pintype "tri_state") (tstamp 557ba04d-98da-42f8-a5fd-836ba457d65b))
    (pad "19" smd rect (at 2.54 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "AD5") (pinfunction "D5") (pintype "tri_state") (tstamp a2acbda5-f653-41ce-bf00-b64500f69158))
    (pad "20" smd rect (at 3.81 6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "AD6") (pinfunction "D6") (pintype "tri_state") (tstamp 976696cc-706b-4212-9a66-8e9bd79087bd))
    (pad "21" smd rect (at 5.51 5.08 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "AD7") (pinfunction "D7") (pintype "tri_state") (tstamp 2a08b8cf-1a3c-4871-83e2-e8e59119c93d))
    (pad "22" smd rect (at 5.51 3.81 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "~{UCS}") (pinfunction "~{CE}") (pintype "input") (tstamp 588d0598-a782-46bc-ae2c-a5b70002d155))
    (pad "23" smd rect (at 5.51 2.54 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "A10") (pinfunction "A10") (pintype "input") (tstamp 812501d3-f766-40a4-9835-38e65a15960e))
    (pad "24" smd rect (at 5.51 1.27 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "ROM.~{OE}") (pinfunction "~{OE}") (pintype "input") (tstamp 1858932b-ee8a-4797-ab83-ae97c6717776))
    (pad "25" smd rect (at 5.51 0 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "A11") (pinfunction "A11") (pintype "input") (tstamp 9b857b79-3b9f-4120-8d40-8063061af71c))
    (pad "26" smd rect (at 5.51 -1.27 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "ROM.A9") (pinfunction "A9") (pintype "input") (tstamp 2bb75360-83d9-43b6-b479-4564592a7411))
    (pad "27" smd rect (at 5.51 -2.54 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "A8") (pinfunction "A8") (pintype "input") (tstamp 57375b51-807e-45ea-87e5-60374cefe717))
    (pad "28" smd rect (at 5.51 -3.81 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "A13") (pinfunction "A13") (pintype "input") (tstamp ae3d3407-d674-494a-b2b4-872faf69d415))
    (pad "29" smd rect (at 5.51 -5.08 270) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "A14") (pinfunction "A14") (pintype "input") (tstamp a7f93f43-b1cc-447d-8cd9-d6e50bd5d3a3))
    (pad "30" smd rect (at 3.81 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "A17") (pinfunction "A17") (pintype "input") (tstamp 1c49ce73-94d8-4e9e-8390-1ee1486cada6))
    (pad "31" smd rect (at 2.54 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "ROM.~{WE}") (pinfunction "~{PGM}") (pintype "input") (tstamp 9dbdfb1a-6b6e-4882-9f99-aeaf2259c369))
    (pad "32" smd rect (at 1.27 -6.78 180) (size 0.76 1.91) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp f8dfc4f8-a58b-4cc8-b3bc-375129409185))
    (model "69802-132LF.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/plcc32_p1-27_l14-05_w11-51.stp" hide
      (offset (xyz 0 0 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
    (model "${KIPRJMOD}/PLCC32-SMD_Socket_IC.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp bffa6b67-ebcb-4915-bdc9-d24146d74c38)
    (at 121.6914 145.1814)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (property "exclude_from_bom" "")
    (path "/5a8858fb-0732-4069-9675-193078205da8/df1c9cc7-3907-4e0d-8ff1-6d92cfd3bac1")
    (attr through_hole exclude_from_bom)
    (fp_text reference "J203" (at 0 -2.33) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 49f6ce59-aac4-494d-aad3-f29c48227053)
    )
    (fp_text value "~{RESET}" (at -4.1656 4.5262) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 770e8d7b-efa1-4a9b-9825-a3df7b4836b0)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 15666b00-0411-4bc3-9663-2bdc47feff20)
    )
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 23e25a2f-016e-401a-b5b0-4fa15cee2c61))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 71c110c4-3809-4ae4-a9f2-115b6f910377))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp acb8b859-d107-4b94-970a-4670fdfe44d4))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp c1477202-80ec-4241-b9f5-93f857ca6fa3))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp c8752ad7-13d6-4b1b-8c51-b1e30877da66))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp d5636b98-8149-4713-ae53-1ec6175d1ff1))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 5cf87cb0-5a29-4d7d-850b-ba81cf72f1de))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b8fe8208-8946-4d02-a97c-350b3c08b134))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp ba97395e-61fc-43ef-aace-c71396f62a96))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp c06031ed-f625-481d-86f9-e69d18b113f2))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 048786ac-26be-4b40-8be2-ce47bb9aa54c))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 529b1e6c-456c-4b84-8dd8-342f1afeb8a0))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 90b9aa4f-7ffb-44ce-8b9d-28a1a464de09))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp eb5c5e5d-f572-4aad-a0e6-9feb3a58b45f))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp f7459fd6-b57b-4ad6-b45d-5a735a6a9bc3))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp c82448c0-8a04-4ae3-bd03-95f1280926a2))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 162 "~{RESET}") (pinfunction "Pin_2") (pintype "passive") (tstamp a7436c40-154d-4187-915a-76faca7ea514))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_SMD:SW_SPST_EVQP7A" (layer "F.Cu")
    (tedit 5A02FC95) (tstamp c33facdd-072f-48ac-8ec8-1beb2fe7b0fd)
    (at 127.511191 148.431191)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (property "Manufacturer_Part_Number" "EVQ-P7J01P")
    (property "Mouser Part Number" "667-EVQP7J01P")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/bfab7b0e-2080-443e-8b9a-c0dcba2d694a")
    (attr smd)
    (fp_text reference "SW201" (at 0 -2.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 742a8eab-d844-44a2-b601-850d4e2aa31e)
    )
    (fp_text value "RESET" (at -6.35 1.595) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f265f1d2-5d8b-4ebf-9b1f-b3924753d9f5)
    )
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp de7203b3-17f6-489c-8998-ca41007481df)
    )
    (fp_line (start 1.75 1.55) (end -1.75 1.55) (layer "F.SilkS") (width 0.12) (tstamp 7fea5749-c933-4da0-8197-2b0dc558df87))
    (fp_line (start -0.95 2.2) (end -0.95 1.55) (layer "F.SilkS") (width 0.12) (tstamp 98c74728-4019-489f-b401-ef52c58f2f7a))
    (fp_line (start 0.95 1.55) (end 0.95 2.2) (layer "F.SilkS") (width 0.12) (tstamp ca6c37fc-a396-4f41-89f2-f99f82fa09c1))
    (fp_line (start 0.95 2.2) (end -0.95 2.2) (layer "F.SilkS") (width 0.12) (tstamp eef2e19b-c587-4abc-bca6-d282e512c6ec))
    (fp_line (start -1.75 -1.55) (end 1.75 -1.55) (layer "F.SilkS") (width 0.12) (tstamp fa8b77fb-f162-4f07-9f4f-ca2db03aee7f))
    (fp_line (start -1.1 1.7) (end -2.75 1.7) (layer "F.CrtYd") (width 0.05) (tstamp 0fb7a1b1-f9a2-44f6-b1e1-9bb9d87fdfe0))
    (fp_line (start 2.75 1.7) (end 1.1 1.7) (layer "F.CrtYd") (width 0.05) (tstamp 1318f980-8eba-42a5-bf58-bf33a3fe009b))
    (fp_line (start -2.75 -1.7) (end 2.75 -1.7) (layer "F.CrtYd") (width 0.05) (tstamp 2c618605-4f9c-4055-9184-195b36bfc170))
    (fp_line (start 2.75 -1.7) (end 2.75 1.7) (layer "F.CrtYd") (width 0.05) (tstamp 5718792e-d62a-428c-9492-74f0071b0cb4))
    (fp_line (start 1.1 2.35) (end -1.1 2.35) (layer "F.CrtYd") (width 0.05) (tstamp 9c4bd80e-2c2d-4051-b8bf-aaffc158b184))
    (fp_line (start -1.1 2.35) (end -1.1 1.7) (layer "F.CrtYd") (width 0.05) (tstamp baf1eed9-da76-4385-8d0e-954ba4c9eddd))
    (fp_line (start 1.1 1.7) (end 1.1 2.35) (layer "F.CrtYd") (width 0.05) (tstamp e19bd615-a41f-4821-8459-3cc2ad82929e))
    (fp_line (start -2.75 1.7) (end -2.75 -1.7) (layer "F.CrtYd") (width 0.05) (tstamp f2762ffe-8822-40ab-b09b-baa443205417))
    (fp_line (start 0.85 2.1) (end 0.85 1.45) (layer "F.Fab") (width 0.1) (tstamp 28913c7a-a5c2-4878-87f7-8b40b320635e))
    (fp_line (start -1.75 -1.45) (end 1.75 -1.45) (layer "F.Fab") (width 0.1) (tstamp 29b9af3c-631d-41f3-8c5b-135f7c3b6faf))
    (fp_line (start -1.75 1.45) (end -1.75 -1.4) (layer "F.Fab") (width 0.1) (tstamp 38bfd600-69be-4690-8f84-057d5cc4200c))
    (fp_line (start 1.75 1.45) (end -1.75 1.45) (layer "F.Fab") (width 0.1) (tstamp 6428fe23-4d1b-4181-8c1e-bf99a448f4df))
    (fp_line (start -0.85 2.1) (end -0.85 1.45) (layer "F.Fab") (width 0.1) (tstamp 8a6100a7-a020-49ab-a260-6a135b04af11))
    (fp_line (start -0.85 2.1) (end 0.85 2.1) (layer "F.Fab") (width 0.1) (tstamp c67947f2-a9c6-4aa1-9f2e-711ebaa2fd48))
    (fp_line (start 1.75 -1.45) (end 1.75 1.45) (layer "F.Fab") (width 0.1) (tstamp d5318cb0-26f3-48c0-ad7e-dce4c8ad088a))
    (pad "1" smd rect (at 1.8 -0.72) (size 1.4 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "~{RESET}") (pinfunction "1") (pintype "passive") (tstamp 0ecdd667-bb35-4468-b46f-899d75a71cf8))
    (pad "1" smd rect (at -1.8 -0.72) (size 1.4 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "~{RESET}") (pinfunction "1") (pintype "passive") (tstamp 898bd276-c5bf-42b5-aaa8-f6e9c7fb350e))
    (pad "2" smd rect (at 1.8 0.72) (size 1.4 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (tstamp 23fd8581-44df-4392-b5a3-7c269365ca7c))
    (pad "2" smd rect (at -1.8 0.72) (size 1.4 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (tstamp e1013e16-2744-4f3f-beb4-5e13863ccdfa))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP7A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/SW_SPST_EVQP7A/EVQ-P7A01P--3DModel-STEP-269445.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "Package_QFP:TQFP-48_7x7mm_P0.5mm" (layer "F.Cu")
    (tedit 5ECA1038) (tstamp cc54e793-dce6-429d-96d3-7dd100c8b724)
    (at 100.711 87.884 180)
    (descr "TQFP, 48 Pin (https://www.jedec.org/system/files/docs/MS-026D.pdf var ABC), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (property "Description" "UART Interface IC 2CH. UART 64B FIFO")
    (property "Height" "1.6")
    (property "Manufacturer_Name" "NXP")
    (property "Manufacturer_Part_Number" "SC16C752BIB48,157")
    (property "Mouser Part Number" "771-SC16C752BIB48")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/NXP-Semiconductors/SC16C752BIB48157?qs=LOCUfHb8d9sKsb5zIyQ%2FFA%3D%3D")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/8584ccec-a8e1-4678-906b-c55737bd91a5")
    (attr smd)
    (fp_text reference "U301" (at 0 -5.85) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 71f60241-ce55-424d-8a22-198851248c23)
    )
    (fp_text value "SC16C752B" (at -5.842 -0.127 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8d16389d-fe43-4083-80e8-34513d222f00)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 346dd969-1f00-4e6b-bb6a-db6a7b3ef1b6)
    )
    (fp_line (start 3.16 -3.61) (end 3.61 -3.61) (layer "F.SilkS") (width 0.12) (tstamp 105e53ae-3114-472b-9ed6-ebb596b61048))
    (fp_line (start -3.16 3.61) (end -3.61 3.61) (layer "F.SilkS") (width 0.12) (tstamp 281acd51-0a70-49e6-a0b5-3f3ec2d64df4))
    (fp_line (start 3.61 3.61) (end 3.61 3.16) (layer "F.SilkS") (width 0.12) (tstamp 5cc8fdbe-c753-43de-bac1-49d951f90c3f))
    (fp_line (start -3.16 -3.61) (end -3.61 -3.61) (layer "F.SilkS") (width 0.12) (tstamp 73991501-41a7-4ba8-a480-a17e83a736ca))
    (fp_line (start -3.61 -3.61) (end -3.61 -3.16) (layer "F.SilkS") (width 0.12) (tstamp 82c9e2e4-48a9-4d7d-a72d-fcfbc22fc56a))
    (fp_line (start 3.61 -3.61) (end 3.61 -3.16) (layer "F.SilkS") (width 0.12) (tstamp 8e516748-da52-447f-a925-01ad7901b029))
    (fp_line (start -3.61 3.61) (end -3.61 3.16) (layer "F.SilkS") (width 0.12) (tstamp a649814d-e03d-4b08-986f-9c3e80aafd9a))
    (fp_line (start -3.61 -3.16) (end -4.9 -3.16) (layer "F.SilkS") (width 0.12) (tstamp af09d2b3-6475-4486-951a-cc54554b34c9))
    (fp_line (start 3.16 3.61) (end 3.61 3.61) (layer "F.SilkS") (width 0.12) (tstamp ff0d78ba-06ef-4a33-b6d5-8eb9fef13110))
    (fp_line (start 3.15 -5.15) (end 3.15 -3.75) (layer "F.CrtYd") (width 0.05) (tstamp 03299ffd-3eaa-4c41-82d0-0384e7339328))
    (fp_line (start 0 5.15) (end -3.15 5.15) (layer "F.CrtYd") (width 0.05) (tstamp 072ffb12-ec02-4dfa-a0f2-02055c6530a1))
    (fp_line (start -3.75 -3.75) (end -3.75 -3.15) (layer "F.CrtYd") (width 0.05) (tstamp 15e690fa-6f5a-431e-992a-a9dfae6f31b4))
    (fp_line (start 0 -5.15) (end -3.15 -5.15) (layer "F.CrtYd") (width 0.05) (tstamp 1b819185-3087-417a-81ca-771de825399e))
    (fp_line (start 3.75 -3.15) (end 5.15 -3.15) (layer "F.CrtYd") (width 0.05) (tstamp 26d6e849-8105-49a9-9a5c-e15dcec499b8))
    (fp_line (start 0 5.15) (end 3.15 5.15) (layer "F.CrtYd") (width 0.05) (tstamp 34684e29-2987-4809-8309-43a17779f89a))
    (fp_line (start -3.75 3.75) (end -3.75 3.15) (layer "F.CrtYd") (width 0.05) (tstamp 36379c26-cc34-4613-9179-92b638fb7e8d))
    (fp_line (start 5.15 3.15) (end 5.15 0) (layer "F.CrtYd") (width 0.05) (tstamp 36a22a6e-66ee-442b-b19a-5881b5471776))
    (fp_line (start -3.75 3.15) (end -5.15 3.15) (layer "F.CrtYd") (width 0.05) (tstamp 5babd139-9ebe-44ed-bba6-45b3d7f7f1da))
    (fp_line (start 3.75 -3.75) (end 3.75 -3.15) (layer "F.CrtYd") (width 0.05) (tstamp 7214cb88-3a7e-41d3-b5c6-7ebef21587e8))
    (fp_line (start -3.75 -3.15) (end -5.15 -3.15) (layer "F.CrtYd") (width 0.05) (tstamp 8cc71e85-d071-413c-84ad-1fae603340cb))
    (fp_line (start 5.15 -3.15) (end 5.15 0) (layer "F.CrtYd") (width 0.05) (tstamp 9d946f5e-5803-4c94-a6b3-3436c134b1a7))
    (fp_line (start -3.15 -5.15) (end -3.15 -3.75) (layer "F.CrtYd") (width 0.05) (tstamp a6b9745b-93bc-4ad0-acc5-27cbf10a43bc))
    (fp_line (start 3.15 3.75) (end 3.75 3.75) (layer "F.CrtYd") (width 0.05) (tstamp aab84180-a3d0-4d6f-b595-c9fde2ab2a03))
    (fp_line (start 0 -5.15) (end 3.15 -5.15) (layer "F.CrtYd") (width 0.05) (tstamp b0941729-aed5-466e-9820-3c7718af55ec))
    (fp_line (start -5.15 3.15) (end -5.15 0) (layer "F.CrtYd") (width 0.05) (tstamp b34c9740-4a30-4bc1-b319-d7c68b357cd6))
    (fp_line (start -3.15 3.75) (end -3.75 3.75) (layer "F.CrtYd") (width 0.05) (tstamp b47b6938-45ab-4d82-93db-0b747e65a7db))
    (fp_line (start -3.15 5.15) (end -3.15 3.75) (layer "F.CrtYd") (width 0.05) (tstamp c02d5394-8230-4886-a715-914a45cadce2))
    (fp_line (start -5.15 -3.15) (end -5.15 0) (layer "F.CrtYd") (width 0.05) (tstamp d8e321ba-1b34-48b9-8a47-bc3472ed329b))
    (fp_line (start 3.15 -3.75) (end 3.75 -3.75) (layer "F.CrtYd") (width 0.05) (tstamp ea6e712b-53bf-4fc3-8c01-12f27a6b1eb1))
    (fp_line (start 3.15 5.15) (end 3.15 3.75) (layer "F.CrtYd") (width 0.05) (tstamp ebd9bb57-7baf-480a-8e2e-3aac607b004e))
    (fp_line (start 3.75 3.15) (end 5.15 3.15) (layer "F.CrtYd") (width 0.05) (tstamp f0d40f8b-55ef-4179-9b41-315e9625e0d6))
    (fp_line (start -3.15 -3.75) (end -3.75 -3.75) (layer "F.CrtYd") (width 0.05) (tstamp faba573b-6508-4e96-979f-fabe168cdc1d))
    (fp_line (start 3.75 3.75) (end 3.75 3.15) (layer "F.CrtYd") (width 0.05) (tstamp ff83ca9c-9856-4366-81ba-9e20419852ff))
    (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer "F.Fab") (width 0.1) (tstamp 1f8c94de-4edb-483e-9dcc-ca2fe35c170b))
    (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer "F.Fab") (width 0.1) (tstamp 7e13cf59-6f7b-4157-b8ae-edbd4a8377f1))
    (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp 996ac7b4-0c11-4a0e-820f-e52934931fa8))
    (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp bfacca6b-3ef6-41df-b2b6-e6beeddc6014))
    (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer "F.Fab") (width 0.1) (tstamp fbf640cc-020b-4c5a-8ab4-5335ef00945e))
    (pad "1" smd roundrect (at -4.1625 -2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "DB5") (pinfunction "D5") (pintype "passive") (tstamp 29a49488-0ea2-4ecd-840d-8ab433acf8eb))
    (pad "2" smd roundrect (at -4.1625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "DB6") (pinfunction "D6") (pintype "passive") (tstamp 0a7d1dc9-d875-4a8d-9088-0723e3baa095))
    (pad "3" smd roundrect (at -4.1625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "DB7") (pinfunction "D7") (pintype "passive") (tstamp db9a7abd-b0eb-4239-a624-c3c7f00e8237))
    (pad "4" smd roundrect (at -4.1625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "UART2.RX") (pinfunction "RXB") (pintype "passive") (tstamp a1fd7cf2-0fed-4fc8-95ff-67cab909a3b6))
    (pad "5" smd roundrect (at -4.1625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "UART1.IN") (pinfunction "RXA") (pintype "passive") (tstamp f274bbdd-5c0b-4c93-9714-65a029d96f37))
    (pad "6" smd roundrect (at -4.1625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "unconnected-(U301-Pad6)") (pinfunction "~{TXRDYB}") (pintype "passive+no_connect") (tstamp 67991ed0-495b-4f2f-85be-21e952b2cd90))
    (pad "7" smd roundrect (at -4.1625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "UART1.OUT") (pinfunction "TXA") (pintype "passive") (tstamp 527d9d6b-138f-467f-95cd-1441017b1737))
    (pad "8" smd roundrect (at -4.1625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "UART2.TX") (pinfunction "TXB") (pintype "passive") (tstamp 44e7dcf7-d135-4b1b-a2a5-46ffc8609574))
    (pad "9" smd roundrect (at -4.1625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "unconnected-(U301-Pad9)") (pinfunction "~{OPB}") (pintype "passive+no_connect") (tstamp 1f53a79c-081e-40cd-bdfd-4758dc5655dc))
    (pad "10" smd roundrect (at -4.1625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "~{CS_S1}") (pinfunction "~{CSA}") (pintype "passive") (tstamp 24a0918b-0b51-46cc-a335-584bc6ef0e64))
    (pad "11" smd roundrect (at -4.1625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "~{CS_S2}") (pinfunction "~{CSB}") (pintype "passive") (tstamp e9061d70-eee8-4363-b2e3-96e59eb5eba0))
    (pad "12" smd roundrect (at -4.1625 2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "unconnected-(U301-Pad12)") (pinfunction "N.C._1") (pintype "passive+no_connect") (tstamp f02721e7-a8f0-4682-991a-c48b79b810db))
    (pad "13" smd roundrect (at -2.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(C305-Pad2)") (pinfunction "XTAL1") (pintype "passive") (tstamp a89fa66a-2f37-4eed-b4f7-2698a9f302a0))
    (pad "14" smd roundrect (at -2.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(C306-Pad1)") (pinfunction "XTAL2") (pintype "passive") (tstamp 3f4fc3ef-1067-4f6f-9c38-b31bf9f8521c))
    (pad "15" smd roundrect (at -1.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "~{IOW}") (pinfunction "~{IOW}") (pintype "passive") (tstamp e352c549-3bb6-491b-8dfa-17d9ce75219b))
    (pad "16" smd roundrect (at -1.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "UART2.~{CD}") (pinfunction "~{CDB}") (pintype "passive") (tstamp fe3a3a5e-437a-4e3f-8ddc-9cae56813f0d))
    (pad "17" smd roundrect (at -0.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 86020aa9-5c71-4c03-b5ae-8558b5a8d292))
    (pad "18" smd roundrect (at -0.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "unconnected-(U301-Pad18)") (pinfunction "~{RXRDYB}") (pintype "passive+no_connect") (tstamp 7bcf3db3-8ee1-4452-a8de-001bd477876b))
    (pad "19" smd roundrect (at 0.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "~{IOR}") (pinfunction "~{IOR}") (pintype "passive") (tstamp a98c23b2-1576-4689-882f-9dd912d804b3))
    (pad "20" smd roundrect (at 0.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "UART2.~{DSR}") (pinfunction "~{DSRB}") (pintype "passive") (tstamp 3da0219c-9ea8-4ddf-8966-c8423ba10bf2))
    (pad "21" smd roundrect (at 1.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "UART2.~{RI}") (pinfunction "~{RIB}") (pintype "passive") (tstamp c0cbcd98-3c26-4e9c-809f-fa364a43249c))
    (pad "22" smd roundrect (at 1.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "UART2.~{RTS}") (pinfunction "~{RTSB}") (pintype "passive") (tstamp b34b8e20-aed1-426c-b8bb-6d062b33fd5d))
    (pad "23" smd roundrect (at 2.25 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "UART2.~{CTS}") (pinfunction "~{CTSB}") (pintype "passive") (tstamp 7ff2ae19-7a7b-4251-9692-0d917116fcc4))
    (pad "24" smd roundrect (at 2.75 4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "unconnected-(U301-Pad24)") (pinfunction "N.C._2") (pintype "passive+no_connect") (tstamp c1d6cce6-27ae-46b2-9516-49f70f7d4532))
    (pad "25" smd roundrect (at 4.1625 2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "unconnected-(U301-Pad25)") (pinfunction "N.C._3") (pintype "passive+no_connect") (tstamp 7fa7ce08-bbed-4bee-a703-c9ec6d114ea1))
    (pad "26" smd roundrect (at 4.1625 2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "A2") (pinfunction "A2") (pintype "passive") (tstamp e92b0e47-f667-4181-a1bf-33d7565a2a3a))
    (pad "27" smd roundrect (at 4.1625 1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "A1") (pinfunction "A1") (pintype "passive") (tstamp 6486ce24-12cd-4c06-a747-f1f989d87983))
    (pad "28" smd roundrect (at 4.1625 1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "A0") (pinfunction "A0") (pintype "passive") (tstamp ebc1216d-effe-4360-9e4b-17ef16121043))
    (pad "29" smd roundrect (at 4.1625 0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "INT2") (pinfunction "INTB") (pintype "passive") (tstamp cf61d8b7-dcaa-4e59-b5cc-765d64f0dd94))
    (pad "30" smd roundrect (at 4.1625 0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "INT0") (pinfunction "INTA") (pintype "passive") (tstamp f55b9f2e-62fa-4d96-9505-931d9bed076d))
    (pad "31" smd roundrect (at 4.1625 -0.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "unconnected-(U301-Pad31)") (pinfunction "~{RXRDYA}") (pintype "passive+no_connect") (tstamp cf4f2420-284d-4a36-8a3f-9af368ddfed0))
    (pad "32" smd roundrect (at 4.1625 -0.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "USB.~{DCD}") (pinfunction "~{OPA}") (pintype "passive") (tstamp 5e9d500b-0a8a-4952-ab33-8b631b41c06b))
    (pad "33" smd roundrect (at 4.1625 -1.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "UART1.~{RTS}") (pinfunction "~{RTSA}") (pintype "passive") (tstamp 779a1bdb-bff9-4f28-8f0a-6b9a014f08a4))
    (pad "34" smd roundrect (at 4.1625 -1.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "UART1.~{DTR}") (pinfunction "~{DTRA}") (pintype "passive") (tstamp 4685f07a-4b89-4bf7-a876-9e42baf1fda2))
    (pad "35" smd roundrect (at 4.1625 -2.25 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "UART2.~{DTR}") (pinfunction "~{DTRB}") (pintype "passive") (tstamp 019431f6-1428-4b60-a349-dc01bf905e38))
    (pad "36" smd roundrect (at 4.1625 -2.75 180) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "RESET") (pintype "passive") (tstamp e8e80187-1eb5-45d1-bf57-1f6b8200a202))
    (pad "37" smd roundrect (at 2.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "unconnected-(U301-Pad37)") (pinfunction "N.C._4") (pintype "passive+no_connect") (tstamp ae7197d1-ded7-4291-b079-95a9d6543dd4))
    (pad "38" smd roundrect (at 2.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "UART1.~{CTS}") (pinfunction "~{CTSA}") (pintype "passive") (tstamp 4c772ec8-47bd-4eb5-abee-2a48a27dd255))
    (pad "39" smd roundrect (at 1.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "UART1.~{DSR}") (pinfunction "~{DSRA}") (pintype "passive") (tstamp e1a72987-23ea-426d-ab03-050db6c7ff28))
    (pad "40" smd roundrect (at 1.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "USB.~{PWREN}") (pinfunction "~{CDA}") (pintype "passive") (tstamp b1098362-91e3-40d6-8e54-d81540959f36))
    (pad "41" smd roundrect (at 0.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "UART1.~{RI}") (pinfunction "~{RIA}") (pintype "passive") (tstamp 8ed5ee37-baa2-47ad-92b9-9ec1256bdf44))
    (pad "42" smd roundrect (at 0.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "passive") (tstamp 588ceb3d-1852-4ede-bc45-a870db410deb))
    (pad "43" smd roundrect (at -0.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "unconnected-(U301-Pad43)") (pinfunction "~{TXRDYA}") (pintype "passive+no_connect") (tstamp cde708c3-c662-49eb-8b38-37d0db40fe9f))
    (pad "44" smd roundrect (at -0.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "DB0") (pinfunction "D0") (pintype "passive") (tstamp f5319a0b-faae-4d29-90f5-375eea08d41b))
    (pad "45" smd roundrect (at -1.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "DB1") (pinfunction "D1") (pintype "passive") (tstamp a37a3bbf-6f3a-4ec0-aab5-c053451fbf92))
    (pad "46" smd roundrect (at -1.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "DB2") (pinfunction "D2") (pintype "passive") (tstamp 9dcd2904-0df3-49e0-acc6-d47ebfa008a4))
    (pad "47" smd roundrect (at -2.25 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "DB3") (pinfunction "D3") (pintype "passive") (tstamp b9423e6d-13ff-4a98-b9ab-93e7592e4691))
    (pad "48" smd roundrect (at -2.75 -4.1625 180) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "DB4") (pinfunction "D4") (pintype "passive") (tstamp 6d64d522-188c-4a88-9664-385f76bc0d16))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-48_7x7mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3) (tstamp dc63a514-7ce0-49f8-a0ed-4f50f6e2e32a)
    (at 92.837 92.202 180)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/a133e451-a678-4e00-bd48-e8a1675498fb")
    (attr through_hole)
    (fp_text reference "J302" (at 0.635 -1.695) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4708c4cc-3c12-4dea-8497-5fef0d1b9532)
    )
    (fp_text value "UART2" (at 3.419 5.7 270 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 5fa793db-b0cf-4e87-a620-bcd48f701927)
    )
    (fp_text user "${REFERENCE}" (at 0.635 2.54 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0dd7a28-91a6-4e8a-b952-7f84608af926)
    )
    (fp_line (start 2.4 -0.695) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 0539deee-89c2-4960-bfb9-06e757d158a9))
    (fp_line (start 1.57753 -0.695) (end 2.4 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 23471d7b-2825-4974-9cf3-da282a6508eb))
    (fp_line (start 0.76 -0.695) (end 0.96247 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 25c7375f-0f57-4762-b2ac-62e4397a9d82))
    (fp_line (start 1.57753 5.775) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 25e852bb-9676-43ae-83aa-2f59d7d6d041))
    (fp_line (start -1.13 -0.76) (end 0 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 5459cb2e-f7c0-46e3-ba4e-4d27a320d9f2))
    (fp_line (start -1.13 5.775) (end -0.30753 5.775) (layer "F.SilkS") (width 0.12) (tstamp 67cdd909-6440-4708-8ed9-80276a0a77bf))
    (fp_line (start -1.13 0.76) (end -1.13 5.775) (layer "F.SilkS") (width 0.12) (tstamp 73ceaef1-24c4-406f-a2da-50242103dc0f))
    (fp_line (start 0.30753 5.775) (end 0.96247 5.775) (layer "F.SilkS") (width 0.12) (tstamp 8a12d770-705b-4edb-b6b3-cbea76244aff))
    (fp_line (start 0.76 0.706529) (end 0.76 0.563471) (layer "F.SilkS") (width 0.12) (tstamp 9408e2f6-d4bf-47ea-a28c-c5cd4c87d99a))
    (fp_line (start -1.13 0.76) (end -0.563471 0.76) (layer "F.SilkS") (width 0.12) (tstamp 9d346913-b0d3-4fe3-93c0-a2b7ff0f00a1))
    (fp_line (start 0.76 -0.563471) (end 0.76 -0.695) (layer "F.SilkS") (width 0.12) (tstamp a38169a5-46f0-48c5-b6e4-28bea6ecfbd3))
    (fp_line (start 0.563471 0.76) (end 0.706529 0.76) (layer "F.SilkS") (width 0.12) (tstamp e6ce1eab-0d0c-4085-ba3c-6ff0a99c8b94))
    (fp_line (start -1.13 0) (end -1.13 -0.76) (layer "F.SilkS") (width 0.12) (tstamp f8b54619-8455-4208-9ae6-8410d104e57c))
    (fp_line (start 2.85 6.25) (end 2.85 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp a59d76d5-feab-47a5-a27d-994d3722f920))
    (fp_line (start 2.85 -1.15) (end -1.6 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp d5ed6db8-3738-4129-97d7-e4994d318611))
    (fp_line (start -1.6 -1.15) (end -1.6 6.25) (layer "F.CrtYd") (width 0.05) (tstamp f4d3581d-1c0e-4475-a211-5ad9285b018b))
    (fp_line (start -1.6 6.25) (end 2.85 6.25) (layer "F.CrtYd") (width 0.05) (tstamp fb2e9b30-94f9-4e0a-9718-ee5a2b130fb9))
    (fp_line (start -1.07 0.2175) (end -0.2175 -0.635) (layer "F.Fab") (width 0.1) (tstamp 4010a29d-376d-42c6-b3d9-39d199932a85))
    (fp_line (start 2.34 5.715) (end -1.07 5.715) (layer "F.Fab") (width 0.1) (tstamp 9aa4e401-92da-499a-9e62-b34244496726))
    (fp_line (start 2.34 -0.635) (end 2.34 5.715) (layer "F.Fab") (width 0.1) (tstamp b0735f85-fe3a-4f12-8254-65fc1c894cae))
    (fp_line (start -0.2175 -0.635) (end 2.34 -0.635) (layer "F.Fab") (width 0.1) (tstamp cdfef499-dd76-441b-b996-d33b663d5423))
    (fp_line (start -1.07 5.715) (end -1.07 0.2175) (layer "F.Fab") (width 0.1) (tstamp d6edef77-14b9-437f-a3c2-63327251e1f8))
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 77 "UART2.~{CD}") (pinfunction "Pin_1") (pintype "passive") (tstamp 98efbd90-12c4-481d-802e-fa02749709ed))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 98 "UART2.RX") (pinfunction "Pin_2") (pintype "passive") (tstamp b7960f75-ee53-4eab-8239-b7b19ee0f8c3))
    (pad "3" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 99 "UART2.TX") (pinfunction "Pin_3") (pintype "passive") (tstamp c20ec536-ef9a-4e2a-9175-49df8b1aaf67))
    (pad "4" thru_hole oval (at 1.27 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 100 "UART2.~{DTR}") (pinfunction "Pin_4") (pintype "passive") (tstamp f7a15133-2950-4f4d-9b60-96ea30d3fce8))
    (pad "5" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp 77356b53-db4f-4e93-a0b0-2e09c38c2ff1))
    (pad "6" thru_hole oval (at 1.27 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 107 "UART2.~{DSR}") (pinfunction "Pin_6") (pintype "passive") (tstamp 599354d0-47c8-435d-a48f-9b8a6928badf))
    (pad "7" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 109 "UART2.~{RTS}") (pinfunction "Pin_7") (pintype "passive") (tstamp bf06b468-dd14-44f0-ae64-95d72514df3d))
    (pad "8" thru_hole oval (at 1.27 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 111 "UART2.~{CTS}") (pinfunction "Pin_8") (pintype "passive") (tstamp 02ce1c79-e49b-4dcd-a327-c67b8f7ecdc8))
    (pad "9" thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 113 "UART2.~{RI}") (pinfunction "Pin_9") (pintype "passive") (tstamp c4f3a743-7b32-4348-be59-57b246c1bc1a))
    (pad "10" thru_hole oval (at 1.27 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 115 "unconnected-(J302-Pad10)") (pinfunction "Pin_10") (pintype "passive+no_connect") (tstamp 62e51d7e-2bd4-48f3-a2a6-1e526ad202f6))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_Via" (layer "F.Cu")
    (tedit 56DDBBFF) (tstamp e2928b7d-86c1-4d98-942d-4b8bfdd0d498)
    (at 171.069 59.944 -90)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/d9546b4d-8ad5-470a-9199-081184401146")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.7 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 88a7e34c-57e7-48ce-a358-6866b2c01d90)
    )
    (fp_text value "MountingHole_2.7mm_M2.5_Pad_Via" (at 0 3.7 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2b878984-ad62-40d5-87be-d30f465ae2b3)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15) italic))
      (tstamp cce13a3b-854c-49ae-8b19-551eed5c4f96)
    )
    (fp_circle (center 0 0) (end 2.7 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp f5a54919-b960-48fc-8517-e9e32dce0bf0))
    (fp_circle (center 0 0) (end 2.95 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp d22f8c08-7c7a-481b-96ff-cad6b4c95453))
    (pad "1" thru_hole circle (at 0 -2.025 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 04868f85-bc69-4fa9-8e62-d78ffe5ae58e))
    (pad "1" thru_hole circle (at -1.431891 -1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 2792ed93-89db-4e51-99ff-281323e776eb))
    (pad "1" thru_hole circle (at -1.431891 1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 335263d3-7e35-4a9c-83c2-cd71d45f0688))
    (pad "1" thru_hole circle (at 0 0 270) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 4102ae0e-3d75-40cd-957b-0b4db5d3f5ee))
    (pad "1" thru_hole circle (at 1.431891 -1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 84315919-677c-4909-a747-2c92c96d5870))
    (pad "1" thru_hole circle (at 1.431891 1.431891 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp 9a88d63d-f7e5-416d-9807-a8e942aef287))
    (pad "1" thru_hole circle (at -2.025 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp a17368fb-646b-4ffd-9057-0994609f8a46))
    (pad "1" thru_hole circle (at 2.025 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp ad2d033c-4040-4813-b5da-82cf827f9d86))
    (pad "1" thru_hole circle (at 0 2.025 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input") (tstamp cd8c6c53-febf-40c1-af77-5373add0fde7))
  )

  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3) (tstamp f6af98b7-6c68-41cc-9c3f-51f70431c4ea)
    (at 149.479 119.888 180)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/1ea60411-14df-4e7e-a9fa-3b3b00f1524d")
    (attr through_hole)
    (fp_text reference "J102" (at 0.635 -1.695) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 792f9b5b-5b67-4481-8a4a-9abdd127653e)
    )
    (fp_text value "SYSBUS" (at -2.286 2.032 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef9bbb97-1060-4a59-9ddf-dca70e02a3c8)
    )
    (fp_text user "${REFERENCE}" (at 0.635 2.54 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b4736c28-da3d-4a4c-9a29-f91b87fb508b)
    )
    (fp_line (start 1.57753 -0.695) (end 2.4 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 0e42572b-3ca3-4a83-8a26-913805523c92))
    (fp_line (start 0.76 -0.695) (end 0.96247 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 2059bc96-e45f-4bdb-97ac-389ac633a825))
    (fp_line (start 1.57753 5.775) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 4a2212c3-b1c0-4f3c-a817-3d3846b819f4))
    (fp_line (start -1.13 0) (end -1.13 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 4ad896d2-2dad-475e-917e-32c0bb7ff8eb))
    (fp_line (start -1.13 -0.76) (end 0 -0.76) (layer "F.SilkS") (width 0.12) (tstamp 5af9c586-2233-4335-8920-53be70db6960))
    (fp_line (start 0.30753 5.775) (end 0.96247 5.775) (layer "F.SilkS") (width 0.12) (tstamp 7359f971-71b1-46f4-8076-4851e07a14a0))
    (fp_line (start 2.4 -0.695) (end 2.4 5.775) (layer "F.SilkS") (width 0.12) (tstamp 877f384a-9d49-478b-927a-3393fc4900d0))
    (fp_line (start 0.76 -0.563471) (end 0.76 -0.695) (layer "F.SilkS") (width 0.12) (tstamp 91911800-6b0e-49bf-b44d-73e588ecad85))
    (fp_line (start -1.13 0.76) (end -1.13 5.775) (layer "F.SilkS") (width 0.12) (tstamp 9c6840e2-d142-4927-8fd2-1680262caba2))
    (fp_line (start -1.13 0.76) (end -0.563471 0.76) (layer "F.SilkS") (width 0.12) (tstamp 9d07c116-582c-474c-93d9-728a84d8f38c))
    (fp_line (start 0.563471 0.76) (end 0.706529 0.76) (layer "F.SilkS") (width 0.12) (tstamp a927d1e6-0247-43f5-a7e5-84e0c9720c42))
    (fp_line (start -1.13 5.775) (end -0.30753 5.775) (layer "F.SilkS") (width 0.12) (tstamp b6fb3407-0a05-4a3d-b25f-d0c232e443ce))
    (fp_line (start 0.76 0.706529) (end 0.76 0.563471) (layer "F.SilkS") (width 0.12) (tstamp c324a92f-a299-4fe3-8d70-c59f96c38d92))
    (fp_line (start 2.85 -1.15) (end -1.6 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 3f1b46a9-de00-44b6-b302-95ba5d4fc7be))
    (fp_line (start 2.85 6.25) (end 2.85 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp a04ccdcd-a971-4610-922a-93c1b8151d4b))
    (fp_line (start -1.6 6.25) (end 2.85 6.25) (layer "F.CrtYd") (width 0.05) (tstamp a8438cf0-2b94-4a9d-8963-c8f4621cc31d))
    (fp_line (start -1.6 -1.15) (end -1.6 6.25) (layer "F.CrtYd") (width 0.05) (tstamp d318d252-1228-47b3-81b6-14876227d164))
    (fp_line (start -0.2175 -0.635) (end 2.34 -0.635) (layer "F.Fab") (width 0.1) (tstamp 04acb1c6-22e2-4d62-b796-fc79d5317ce7))
    (fp_line (start -1.07 0.2175) (end -0.2175 -0.635) (layer "F.Fab") (width 0.1) (tstamp a58d8a79-53fd-4fe3-992a-01100e8d47c4))
    (fp_line (start -1.07 5.715) (end -1.07 0.2175) (layer "F.Fab") (width 0.1) (tstamp bab16d81-9e60-4aa3-8e5a-6d79dd4ac03e))
    (fp_line (start 2.34 -0.635) (end 2.34 5.715) (layer "F.Fab") (width 0.1) (tstamp dece6949-2c91-4d3e-ae10-0bd6a4692886))
    (fp_line (start 2.34 5.715) (end -1.07 5.715) (layer "F.Fab") (width 0.1) (tstamp e2925fdb-24ac-4d53-94b5-cae9830e46d4))
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 86 "AD0") (pinfunction "Pin_1") (pintype "passive") (tstamp f46028de-f273-490b-8945-833e713eff6b))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 85 "AD1") (pinfunction "Pin_2") (pintype "passive") (tstamp 2f5e7418-10d8-4e50-8906-ff3d6c5c811a))
    (pad "3" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 84 "AD2") (pinfunction "Pin_3") (pintype "passive") (tstamp 302180d1-901c-41bd-9e73-d669be86dfa7))
    (pad "4" thru_hole oval (at 1.27 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 83 "AD3") (pinfunction "Pin_4") (pintype "passive") (tstamp c56d61b6-6b2e-4032-be2a-e7df35196bb8))
    (pad "5" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 82 "AD4") (pinfunction "Pin_5") (pintype "passive") (tstamp 75bf5183-9251-4ee5-aef5-3deaeaf1fc96))
    (pad "6" thru_hole oval (at 1.27 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 81 "AD5") (pinfunction "Pin_6") (pintype "passive") (tstamp 2c67b746-2515-42f9-bcd3-da30c8f7b79d))
    (pad "7" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 80 "AD6") (pinfunction "Pin_7") (pintype "passive") (tstamp 9b7cdf03-2bba-4f6d-b8f1-54e654a62473))
    (pad "8" thru_hole oval (at 1.27 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 79 "AD7") (pinfunction "Pin_8") (pintype "passive") (tstamp 3b99e878-3301-4669-87fe-71b5ed86b3f5))
    (pad "9" thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive") (tstamp 936cfd5d-2f2e-4d78-951b-8989c884e46a))
    (pad "10" thru_hole oval (at 1.27 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 70 "unconnected-(J102-Pad10)") (pinfunction "Pin_10") (pintype "passive+no_connect") (tstamp eea44734-3d62-434e-8fb3-e37828d94e5a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1) (tstamp f75df116-d1cf-4895-851b-434898dd973d)
    (at 120.015 122.682 180)
    (descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "glue.kicad_sch")
    (property "Sheetname" "GLUE")
    (path "/5a8858fb-0732-4069-9675-193078205da8/f399b29e-6048-49e1-9d8d-a11731e251c6")
    (attr smd)
    (fp_text reference "J201" (at 0 -8.65) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 468d1038-100f-4863-bc23-a98e1fe897dc)
    )
    (fp_text value "22V10/16V8" (at 0 8.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 311764c7-b652-45a2-af0b-30d0ba8793a5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfab3268-a833-40c4-be64-c75b1dbdcbb4)
    )
    (fp_line (start -3.86 -7.545) (end -5.675 -7.545) (layer "F.SilkS") (width 0.12) (tstamp 1d2ffbd6-50ff-45a4-b16b-42458ca85232))
    (fp_line (start -3.86 -7.81) (end -3.86 -7.545) (layer "F.SilkS") (width 0.12) (tstamp 1dfdbd68-966a-4a23-a253-bb8fea3cfffb))
    (fp_line (start 3.86 7.81) (end 3.86 7.545) (layer "F.SilkS") (width 0.12) (tstamp 7d22b976-fd98-453a-8761-671a8c082020))
    (fp_line (start 0 7.81) (end 3.86 7.81) (layer "F.SilkS") (width 0.12) (tstamp 8251f48e-f100-41d7-8bd7-71dc05df8bd1))
    (fp_line (start 0 -7.81) (end -3.86 -7.81) (layer "F.SilkS") (width 0.12) (tstamp 92ff2ec1-37e9-40e2-9b6e-7063f769bd5a))
    (fp_line (start 3.86 -7.81) (end 3.86 -7.545) (layer "F.SilkS") (width 0.12) (tstamp 9e676404-057a-454b-a2dc-b3623345ae52))
    (fp_line (start 0 7.81) (end -3.86 7.81) (layer "F.SilkS") (width 0.12) (tstamp d119fc4c-cf3e-40da-93bf-c1ad394f4c4d))
    (fp_line (start 0 -7.81) (end 3.86 -7.81) (layer "F.SilkS") (width 0.12) (tstamp e4b51c88-91c3-445b-8555-07e4de269476))
    (fp_line (start -3.86 7.81) (end -3.86 7.545) (layer "F.SilkS") (width 0.12) (tstamp fa05a290-a267-4b2b-ba39-e2e0ff703b33))
    (fp_line (start 5.93 7.95) (end 5.93 -7.95) (layer "F.CrtYd") (width 0.05) (tstamp 664d9d87-ea76-4e52-be0e-5eba7d60f2b4))
    (fp_line (start -5.93 7.95) (end 5.93 7.95) (layer "F.CrtYd") (width 0.05) (tstamp bd4cdc76-18ea-483a-b198-63c8689bda62))
    (fp_line (start 5.93 -7.95) (end -5.93 -7.95) (layer "F.CrtYd") (width 0.05) (tstamp c44f9361-c658-40f1-a89b-4f79aba60382))
    (fp_line (start -5.93 -7.95) (end -5.93 7.95) (layer "F.CrtYd") (width 0.05) (tstamp e438c729-942f-424e-893e-eb7414ed097c))
    (fp_line (start 3.75 -7.7) (end 3.75 7.7) (layer "F.Fab") (width 0.1) (tstamp 5e91646b-87ff-471c-8e43-27b618a8d529))
    (fp_line (start 3.75 7.7) (end -3.75 7.7) (layer "F.Fab") (width 0.1) (tstamp 65fe90ef-fce0-47be-bfa3-0d63d9ac7567))
    (fp_line (start -2.75 -7.7) (end 3.75 -7.7) (layer "F.Fab") (width 0.1) (tstamp 9ba46100-df69-4024-b18c-bccf1502ffb0))
    (fp_line (start -3.75 7.7) (end -3.75 -6.7) (layer "F.Fab") (width 0.1) (tstamp ea06c712-312b-44a0-ae6f-77344419f42b))
    (fp_line (start -3.75 -6.7) (end -2.75 -7.7) (layer "F.Fab") (width 0.1) (tstamp fdc0e9c4-d340-4ba9-b3ae-8d0d887d3a99))
    (pad "1" smd roundrect (at -4.65 -6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "unconnected-(J201-Pad1)") (pinfunction "OD/CLK") (pintype "passive+no_connect") (tstamp b298cbd3-978c-45ec-b603-b77150df68a3))
    (pad "2" smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "RESOUT") (pinfunction "I0") (pintype "passive") (tstamp 0edce152-4fb0-476b-b732-eaacce1168ff))
    (pad "3" smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "A3") (pinfunction "I1") (pintype "passive") (tstamp bfcde445-8940-4f61-afa5-83e251b26982))
    (pad "4" smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "~{WR}") (pinfunction "I2") (pintype "passive") (tstamp f3f07272-748b-40f9-a33c-d4be871adcd4))
    (pad "5" smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "~{RD}") (pinfunction "I3") (pintype "passive") (tstamp b25067af-388a-48da-b265-2838bb385a37))
    (pad "6" smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "M{slash}~{IO}") (pinfunction "I4") (pintype "passive") (tstamp 8a6157b5-bf1c-4610-b39f-5ba06ade240b))
    (pad "7" smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "~{CS_S}") (pinfunction "I5") (pintype "passive") (tstamp 02653996-6a37-46f2-908c-54b24208c6cd))
    (pad "8" smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "~{CARDSLCTD}") (pinfunction "I6") (pintype "passive") (tstamp 3c44d709-d61a-403f-97d1-b4aae9889d31))
    (pad "9" smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "~{DEN}") (pinfunction "I7") (pintype "passive") (tstamp 159e3f85-ea5f-49ef-89f6-568f87c2d02f))
    (pad "10" smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "DCD") (pinfunction "I8") (pintype "passive") (tstamp d6314a9a-5000-4f8f-953e-1535a673e951))
    (pad "11" smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "unconnected-(J201-Pad11)") (pinfunction "I9") (pintype "passive+no_connect") (tstamp 093e1d39-2d57-492b-9211-db019a7ec890))
    (pad "12" smd roundrect (at -4.65 6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (tstamp 9337ce93-0b07-4b76-bbdd-cf845999da93))
    (pad "13" smd roundrect (at 4.65 6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "unconnected-(J201-Pad13)") (pinfunction "CLK/OD") (pintype "passive+no_connect") (tstamp a5a10aee-bc21-42e8-ab63-8da553e163ee))
    (pad "14" smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "~{CS_S2}") (pinfunction "LR/O4") (pintype "passive") (tstamp 73f95aeb-8766-4d3d-94f7-d626a0133193))
    (pad "15" smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "USB.~{RESET}") (pinfunction "A0/O3") (pintype "passive") (tstamp 88340ab9-b95e-42a1-a397-24fd999ccd21))
    (pad "16" smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "~{BEN}") (pinfunction "A1/O2") (pintype "passive") (tstamp b55ec2a5-f12a-43cf-a1a4-b2d17c917c37))
    (pad "17" smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "~{RESET}") (pinfunction "A2/O1") (pintype "passive") (tstamp 44aca021-bc4a-4f51-bcdc-8d2e711559e5))
    (pad "18" smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "~{SMEMW}") (pinfunction "NC/O0") (pintype "passive") (tstamp 852ea28c-5e15-4755-9039-e2d78b4c2567))
    (pad "19" smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "~{SMEMR}") (pinfunction "O4/NC") (pintype "passive") (tstamp d8b248e3-0713-4fa6-ba4b-8eed4989c3dc))
    (pad "20" smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "~{IOW}") (pinfunction "O3/A2") (pintype "passive") (tstamp 1fb3873c-a2c2-4466-9b9d-9398d9e26ea0))
    (pad "21" smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "~{IOR}") (pinfunction "O2/A1") (pintype "passive") (tstamp 4d2fde0e-d85e-4f78-ac86-afeb76dc7b3c))
    (pad "22" smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "~{CS_S1}") (pinfunction "O1/A0") (pintype "passive") (tstamp 030352fe-69ce-4b15-a163-38e13cceec60))
    (pad "23" smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "ALE") (pinfunction "O0/LR") (pintype "passive") (tstamp d02c9e78-1643-4aab-a48c-21dc36a262fe))
    (pad "24" smd roundrect (at 4.65 -6.985 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "passive") (tstamp 0db3291b-4aab-4512-b804-568fb632f3a4))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 02b8749d-8df5-4032-a24a-2669d0318e48)
    (at 114.046 93.1352)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Description" "1206 SMD 20 Kohms")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "71-RCC120620K0FKEA")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/69356db1-2f6a-4f32-a89c-a56d93e6b077")
    (attr smd)
    (fp_text reference "R2" (at 0 1.82) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9847bc6f-9fb2-4902-a73c-bc6895f4b605)
    )
    (fp_text value "ARDY" (at 2.667 0.009) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
      (tstamp 45fe4a8f-93c2-4701-a471-f3eb61416b7a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 34d5568d-b3be-436d-9eca-5d316928227c)
    )
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91) (layer "B.SilkS") (width 0.12) (tstamp 641ddb57-accc-4a5b-bd09-73574625e5f4))
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91) (layer "B.SilkS") (width 0.12) (tstamp 9660a892-1836-4d22-9d52-9ee5495cd388))
    (fp_line (start -2.45 1.12) (end 2.45 1.12) (layer "B.CrtYd") (width 0.05) (tstamp 177d7db9-29c9-410e-981c-a977f0536bbe))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12) (layer "B.CrtYd") (width 0.05) (tstamp 7ecbad01-a6cb-4ba7-b43c-9d90c6d5ef7b))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12) (layer "B.CrtYd") (width 0.05) (tstamp 7fb86adf-ce68-47a3-8479-54d722c01a47))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12) (layer "B.CrtYd") (width 0.05) (tstamp de8d2ea1-923c-47bd-a301-dbff2089ec53))
    (fp_line (start -1.6 0.8) (end 1.6 0.8) (layer "B.Fab") (width 0.1) (tstamp 2456d4f7-0a42-44f1-98d3-4e733790463b))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8) (layer "B.Fab") (width 0.1) (tstamp 5e4eeb3d-a000-44ef-a000-f6bc316e3c37))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8) (layer "B.Fab") (width 0.1) (tstamp e5f4f84a-88b7-48c8-b83e-562d354302fd))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer "B.Fab") (width 0.1) (tstamp e7e73ee5-6717-4f6d-927a-1afecd5558b9))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 4 "VCC") (pintype "passive") (tstamp 28aa0230-b358-493e-b3f8-57d18dfbda4a))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 159 "Net-(J103-Pad55)") (pintype "passive") (tstamp 17ac10e4-01f5-4d09-8034-25f5c42dc16e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Crystal:Crystal_SMD_EuroQuartz_EQ161-2Pin_3.2x1.5mm_HandSoldering" (layer "B.Cu")
    (tedit 5A0FD1B2) (tstamp 15e041e3-43eb-4998-9031-224a316dd8b0)
    (at 145.796 96.647)
    (descr "SMD Crystal EuroQuartz EQ161 series http://cdn-reichelt.de/documents/datenblatt/B400/PG32768C.pdf, hand-soldering, 3.2x1.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (property "Manufacturer_Part_Number" "ECS-.327-6-34R-TR")
    (property "Mouser Part Number" "520-.327-6-34RT")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/be9fdfa9-dd1a-4381-a422-dcc5c6f7d74a")
    (attr smd)
    (fp_text reference "Y302" (at 0 1.95) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5b3a6369-1c89-44ac-a4f3-23f9a6459e08)
    )
    (fp_text value "32.768kHz" (at 1.162 -2.1908) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 77732c5e-b571-41d1-bc20-72e832032956)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.105)) (justify mirror))
      (tstamp 0f37c109-2d15-49d4-b790-c980ae1bd11e)
    )
    (fp_line (start -0.55 -0.95) (end 0.55 -0.95) (layer "B.SilkS") (width 0.12) (tstamp 15df788a-c0a2-4264-8670-f6a49c26c8a2))
    (fp_line (start -0.55 0.95) (end 0.55 0.95) (layer "B.SilkS") (width 0.12) (tstamp 243f23b4-ca49-4455-94ce-054f96c6598e))
    (fp_line (start -2.7 0.9) (end -2.7 -0.9) (layer "B.SilkS") (width 0.12) (tstamp 5ee14158-af25-4a52-962e-b18488d5f011))
    (fp_line (start -2.8 1.2) (end -2.8 -1.2) (layer "B.CrtYd") (width 0.05) (tstamp 0fbb0ccb-cbb0-4eca-960a-2074a2e3cb40))
    (fp_line (start 2.8 1.2) (end -2.8 1.2) (layer "B.CrtYd") (width 0.05) (tstamp 54bd76ab-1b77-41e9-ad4a-4fe6c6f4e848))
    (fp_line (start -2.8 -1.2) (end 2.8 -1.2) (layer "B.CrtYd") (width 0.05) (tstamp 5adeda94-6ae2-4727-b48c-902af23c3641))
    (fp_line (start 2.8 -1.2) (end 2.8 1.2) (layer "B.CrtYd") (width 0.05) (tstamp 953eda6e-f5c2-4afb-bed0-2a6058928674))
    (fp_line (start -1.6 0.65) (end -1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp 0c7a659e-ed09-4a29-8b1c-6c80fd580b16))
    (fp_line (start 1.5 -0.75) (end -1.5 -0.75) (layer "B.Fab") (width 0.1) (tstamp 11008ca2-9174-46d0-b82f-bc48b0d5c21a))
    (fp_line (start -1.5 0.75) (end 1.5 0.75) (layer "B.Fab") (width 0.1) (tstamp 138c20b4-c82e-4a07-93cc-d2100f948775))
    (fp_line (start 1.5 0.75) (end 1.6 0.65) (layer "B.Fab") (width 0.1) (tstamp 1df34b8b-9197-487b-912a-77b047b75806))
    (fp_line (start 1.6 -0.65) (end 1.5 -0.75) (layer "B.Fab") (width 0.1) (tstamp a459f325-0ca8-483f-b86a-e071732f9b7c))
    (fp_line (start -1.5 -0.75) (end -1.6 -0.65) (layer "B.Fab") (width 0.1) (tstamp d76999fe-6cef-4007-a815-d6b64822a97f))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer "B.Fab") (width 0.1) (tstamp e055a9d3-6260-4e03-8ad3-a80f4e12bbed))
    (fp_line (start 1.6 0.65) (end 1.6 -0.65) (layer "B.Fab") (width 0.1) (tstamp f10f9021-c7cb-42a4-8731-b4fb8223556a))
    (fp_line (start -1.6 -0.25) (end -1.1 -0.75) (layer "B.Fab") (width 0.1) (tstamp faba97c7-7c83-4bac-8816-e979b386287f))
    (pad "1" smd rect (at -1.625 0) (size 1.75 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(U303-Pad30)") (pinfunction "1") (pintype "passive") (tstamp 9c50ebc1-4b6c-4699-a622-5f22dc477396))
    (pad "2" smd rect (at 1.625 0) (size 1.75 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "Net-(U303-Pad31)") (pinfunction "2") (pintype "passive") (tstamp c7021c59-8798-4f4f-94fb-02d46844ac37))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_EuroQuartz_EQ161-2Pin_3.2x1.5mm_HandSoldering.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66) (tstamp 1fbcfd57-a9b0-45ef-89ea-b37a43678369)
    (at 113.65 85.344)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (path "/ffb6c144-63b5-4896-8d94-0a4d8727177f")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP101" (at 0 1.8) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 92d01c07-4a8c-43ea-b3a1-8a373268e9dc)
    )
    (fp_text value "Enhanced" (at 1.92 0) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
      (tstamp ad2de60b-f332-4015-945e-dc6bed2bdefc)
    )
    (fp_line (start -0.7 1) (end 0.7 1) (layer "B.SilkS") (width 0.12) (tstamp 689ecadd-33a6-45aa-a90c-4ee4f264ee0c))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer "B.SilkS") (width 0.12) (tstamp 76adae7d-3a55-4a71-b25d-7872174ee678))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer "B.SilkS") (width 0.12) (tstamp 9cbba8dd-1e4b-4d0a-a759-f16a90881449))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer "B.SilkS") (width 0.12) (tstamp efb84618-4504-44cf-9373-df6a20b19000))
    (fp_arc (start -1.4 -0.3) (mid -1.194975 -0.794975) (end -0.7 -1) (layer "B.SilkS") (width 0.12) (tstamp 703619ca-4c58-4f77-847f-41f591614748))
    (fp_arc (start 1.4 0.3) (mid 1.194975 0.794975) (end 0.7 1) (layer "B.SilkS") (width 0.12) (tstamp 9a32b6b0-498c-4f2a-aa24-84b909a22f23))
    (fp_arc (start 0.7 -1) (mid 1.194975 -0.794975) (end 1.4 -0.3) (layer "B.SilkS") (width 0.12) (tstamp d1f7822c-eadf-4153-9149-fc61d4cef5d7))
    (fp_arc (start -0.7 1) (mid -1.194975 0.794975) (end -1.4 0.3) (layer "B.SilkS") (width 0.12) (tstamp e8644adf-dd26-4e97-bbc1-cba0a96dce87))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp 14580ec3-c360-4ee5-b018-50a8b591f485))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer "B.CrtYd") (width 0.05) (tstamp 4474e066-2e60-44f5-9d0e-59cf69405e57))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer "B.CrtYd") (width 0.05) (tstamp 93288098-18a6-4f0f-8b7f-9d3d7ecc92e2))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer "B.CrtYd") (width 0.05) (tstamp f6731a62-0833-4d3e-a6ba-41d855fe7423))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 71 "RESOUT") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ) (tstamp 9895dfcb-9a8b-456c-9828-66394bc82eb8))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 153 "Net-(J103-Pad47)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ) (tstamp 0f7859da-f418-428a-b1f9-7ad12358f75d))
  )

  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE) (tstamp 2ff3ed75-7181-4c39-9dd5-787707739b13)
    (at 114.046 89.2302)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Description" "1206 SMD 20 Kohms")
    (property "Manufacturer_Part_Number" "~")
    (property "Mouser Part Number" "71-RCC120620K0FKEA")
    (property "Sheetfile" "cpu_card.kicad_sch")
    (property "Sheetname" "")
    (path "/67eaaa26-ec9f-4b91-8fdd-d3b9ec260979")
    (attr smd)
    (fp_text reference "R3" (at 0 1.82) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4fd4d73a-aab0-4fe1-ae18-7841fb07a63a)
    )
    (fp_text value "SRDY" (at 2.667 -0.023) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify right mirror))
      (tstamp 51696ca0-ff70-49dd-bdf8-a95d6edf1152)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
      (tstamp 9915628f-115e-446a-915b-9862b08bc5da)
    )
    (fp_line (start -0.727064 -0.91) (end 0.727064 -0.91) (layer "B.SilkS") (width 0.12) (tstamp 5f5a7e64-236d-4969-8093-b7379838a9cd))
    (fp_line (start -0.727064 0.91) (end 0.727064 0.91) (layer "B.SilkS") (width 0.12) (tstamp ae1d4553-1fc6-49e7-9616-921be66476de))
    (fp_line (start 2.45 1.12) (end 2.45 -1.12) (layer "B.CrtYd") (width 0.05) (tstamp 0200e44d-9929-48ba-9eeb-3b2fe8b824fa))
    (fp_line (start -2.45 1.12) (end 2.45 1.12) (layer "B.CrtYd") (width 0.05) (tstamp 4b789403-4b88-4060-93cd-8b10a1f6622b))
    (fp_line (start 2.45 -1.12) (end -2.45 -1.12) (layer "B.CrtYd") (width 0.05) (tstamp 8aa7d8b6-0f1d-4785-9e5a-c21fc45b1fb6))
    (fp_line (start -2.45 -1.12) (end -2.45 1.12) (layer "B.CrtYd") (width 0.05) (tstamp 8bb7c959-ee05-4bfe-81d6-c05fee2eb774))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer "B.Fab") (width 0.1) (tstamp 298b366f-858b-47b4-b7a9-270db1e7e896))
    (fp_line (start -1.6 0.8) (end 1.6 0.8) (layer "B.Fab") (width 0.1) (tstamp 48877766-26dc-468b-b375-103c52744328))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8) (layer "B.Fab") (width 0.1) (tstamp c585b69a-2f24-4eff-a2f6-2597c1d8963b))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8) (layer "B.Fab") (width 0.1) (tstamp ef4bafb2-8718-4ab6-bd1a-b85ad7e023f5))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 4 "VCC") (pintype "passive") (tstamp 179869d9-ca46-46fa-b710-de8c4675c082))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 155 "Net-(J103-Pad49)") (pintype "passive") (tstamp 232e8801-adb1-4510-88b5-979b871d9ac5))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm" (layer "B.Cu")
    (tedit 5A02F146) (tstamp a61610df-4f9d-44a6-9df1-03d38701caa4)
    (at 144.145 105.156 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "Sheetfile" "peripherals.kicad_sch")
    (property "Sheetname" "Peripherals")
    (path "/5a034e86-668f-4bfc-9ac1-a9dda69533ed/969c4ab8-965b-460b-835d-b57233f35aa3")
    (attr smd)
    (fp_text reference "U303" (at 6.223 0 90) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a670d0a3-9fba-4c85-a4b2-110b0f395de2)
    )
    (fp_text value "DS12885T" (at 0 6.35) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 33a8f2ad-4673-4621-84b4-8ee1fcee60a4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2840686c-44f0-4d61-b961-c9f62cf24cdf)
    )
    (fp_line (start 3.625 -3.625) (end 3.625 -3.3) (layer "B.SilkS") (width 0.15) (tstamp 08aad28d-8ce4-4c3e-b76a-fcaf515e411e))
    (fp_line (start 3.625 -3.625) (end 3.3 -3.625) (layer "B.SilkS") (width 0.15) (tstamp 104ee9c6-4a94-40f7-b78e-aa197c902139))
    (fp_line (start -3.625 3.625) (end -3.625 3.4) (layer "B.SilkS") (width 0.15) (tstamp 1fd12d09-6649-4abc-aae6-35cb28ea9031))
    (fp_line (start 3.625 3.625) (end 3.3 3.625) (layer "B.SilkS") (width 0.15) (tstamp 5fad678f-ee2c-4919-bc28-bb83b7d59273))
    (fp_line (start -3.625 -3.625) (end -3.625 -3.3) (layer "B.SilkS") (width 0.15) (tstamp 6b81941e-4a0c-4a7f-b34f-ebf2d5a24226))
    (fp_line (start -3.625 -3.625) (end -3.3 -3.625) (layer "B.SilkS") (width 0.15) (tstamp afda12f1-dc58-4dec-b178-56f3a5118019))
    (fp_line (start 3.625 3.625) (end 3.625 3.3) (layer "B.SilkS") (width 0.15) (tstamp bf3cf546-dde1-469a-a346-94d433cd9949))
    (fp_line (start -3.625 3.4) (end -5.05 3.4) (layer "B.SilkS") (width 0.15) (tstamp cf270ea1-f088-4ba3-8b16-f4a7044cd9b2))
    (fp_line (start -3.625 3.625) (end -3.3 3.625) (layer "B.SilkS") (width 0.15) (tstamp d37a3f4d-00ee-48bb-94be-d578e5c650ad))
    (fp_line (start -5.3 5.3) (end -5.3 -5.3) (layer "B.CrtYd") (width 0.05) (tstamp 62b9f5bc-c75d-4809-aa2b-863d7a6686c5))
    (fp_line (start 5.3 5.3) (end 5.3 -5.3) (layer "B.CrtYd") (width 0.05) (tstamp 9fe286ab-6a1b-4142-a0a0-5a31d038bcc6))
    (fp_line (start -5.3 -5.3) (end 5.3 -5.3) (layer "B.CrtYd") (width 0.05) (tstamp b661612b-bc7d-4761-a7dd-165c27e7c131))
    (fp_line (start -5.3 5.3) (end 5.3 5.3) (layer "B.CrtYd") (width 0.05) (tstamp c421d40c-1ac4-47fd-837f-90076e21dd48))
    (fp_line (start -3.5 -3.5) (end -3.5 2.5) (layer "B.Fab") (width 0.15) (tstamp 61d0b928-2232-4685-9b9f-4c5c4c7ed1e5))
    (fp_line (start -2.5 3.5) (end 3.5 3.5) (layer "B.Fab") (width 0.15) (tstamp 80071cfb-2121-405b-8603-7a3c3b1e48ff))
    (fp_line (start 3.5 3.5) (end 3.5 -3.5) (layer "B.Fab") (width 0.15) (tstamp b7671bc1-2d11-4bde-8ffb-cd68567f0bdb))
    (fp_line (start 3.5 -3.5) (end -3.5 -3.5) (layer "B.Fab") (width 0.15) (tstamp cd1abc15-9cf0-465b-bc8e-b18c170514f1))
    (fp_line (start -3.5 2.5) (end -2.5 3.5) (layer "B.Fab") (width 0.15) (tstamp d9936f98-a0bb-4194-80f8-2b5a0c6e05bf))
    (pad "1" smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "AD0") (pinfunction "AD0") (pintype "bidirectional") (tstamp c53bcdd8-5df1-4d73-913f-a7cbff8c7486))
    (pad "2" smd rect (at -4.25 2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "AD1") (pinfunction "AD1") (pintype "bidirectional") (tstamp 00f0be4d-316e-4a5e-a76f-07defb5daea8))
    (pad "3" smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "AD2") (pinfunction "AD2") (pintype "bidirectional") (tstamp 5dfdbfe2-e03e-44ab-864c-67b0a74fb064))
    (pad "4" smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp e86dcc7c-9c05-45a8-ba9f-aa2f48f9ae01))
    (pad "5" smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "AD3") (pinfunction "AD3") (pintype "bidirectional") (tstamp 901f3419-1b60-4bfa-9de8-3b53a9da6d77))
    (pad "6" smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 9e46caa1-48ac-4c3b-b9cc-0ea5f7ba47e6))
    (pad "7" smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "AD4") (pinfunction "AD4") (pintype "bidirectional") (tstamp 3bd270ab-82d4-4dfd-852e-6ea46b8b26a7))
    (pad "8" smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "AD5") (pinfunction "AD5") (pintype "bidirectional") (tstamp b8fa43bc-01fa-4953-b452-9423a50573ab))
    (pad "9" smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "AD6") (pinfunction "AD6") (pintype "bidirectional") (tstamp 8d0616d1-0123-4a11-b6df-586c63326f3f))
    (pad "10" smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp e9ebcc52-2122-4767-ad59-58fc4e200555))
    (pad "11" smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "AD7") (pinfunction "AD7") (pintype "bidirectional") (tstamp 169b54a9-8fda-4d56-8b34-4abf5d05409f))
    (pad "12" smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp fa1dbaaa-1f34-45b7-9c13-190783871118))
    (pad "13" smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "~{CS_RTC}") (pinfunction "~{CS}") (pintype "bidirectional") (tstamp af69dfed-e6b9-4e0a-98dd-bc38c9b81037))
    (pad "14" smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 164 "ALE") (pinfunction "AS") (pintype "bidirectional") (tstamp 437b2bb8-560f-4572-a698-1695e6a5f1a7))
    (pad "15" smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp e9d30831-2202-45ef-aae9-858ff83ed1f1))
    (pad "16" smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "~{WR}") (pinfunction "R/*W") (pintype "bidirectional") (tstamp b7ce5b03-fef6-4824-a5e0-b109d17b9977))
    (pad "17" smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 886c16c8-17d6-421c-b998-e5049470c749))
    (pad "18" smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "~{RD}") (pinfunction "DS") (pintype "bidirectional") (tstamp e28f695e-920d-492e-ba32-cf4b95c4a752))
    (pad "19" smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "~{RESET}") (pinfunction "~{RESET}") (pintype "bidirectional") (tstamp 1c674083-1bb5-439a-a693-b754a5827a1c))
    (pad "20" smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 0bc0a581-6036-40f9-85ad-dbbd7fb44356))
    (pad "21" smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "RTC.~{IRQ}") (pinfunction "~{IRQ}") (pintype "bidirectional") (tstamp 5ee708db-2778-4ff3-9954-0a3f1c8dd073))
    (pad "22" smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "VBAT") (pinfunction "VBAT") (pintype "power_in") (tstamp 9c278d7c-a96b-412a-93b8-42b14a89b013))
    (pad "23" smd rect (at 4.25 2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp e0421bcb-6d78-402d-a01b-95c1c6d0d236))
    (pad "24" smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "Net-(SW301-Pad2)") (pinfunction "~{RCLR}") (pintype "bidirectional") (tstamp 23139037-12a2-4b37-8039-58b7fb90dea5))
    (pad "25" smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp d5e0be70-fc5c-420a-83e4-b17b55e4752e))
    (pad "26" smd rect (at 2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "unconnected-(U303-Pad26)") (pinfunction "SQW") (pintype "bidirectional+no_connect") (tstamp 24429498-2ed4-46a6-b9f6-9f66de935e45))
    (pad "27" smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 715cb2f0-d14d-426e-98c4-545e94253364))
    (pad "28" smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 8fa1ef72-2706-4b15-ae80-81f484b8b40e))
    (pad "29" smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "MOT") (pintype "bidirectional") (tstamp e10957fb-6043-4424-930d-65814b365684))
    (pad "30" smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(U303-Pad30)") (pinfunction "X1") (pintype "bidirectional") (tstamp 43a73f0d-b35e-41f6-8f29-e53e24f60c92))
    (pad "31" smd rect (at -2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "Net-(U303-Pad31)") (pinfunction "X2") (pintype "bidirectional") (tstamp c1233278-6d97-4b76-a9e3-d3b7f4b95573))
    (pad "32" smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp b60a9269-2471-4c59-bfce-1cef81f41009))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 93.218 136.2075) (end 96.266 139.1285) (layer "F.SilkS") (width 0.15) (fill solid) (tstamp 1a21a6a8-7838-4271-860f-e1a56471e49d))
  (gr_rect (start 116.586 136.144) (end 119.126 139.192) (layer "F.SilkS") (width 0.15) (fill solid) (tstamp 3ca90e50-ee3f-405a-95f7-449d8602b6f4))
  (gr_rect (start 92.212 90.312) (end 94.244 89.042) (layer "F.SilkS") (width 0.15) (fill solid) (tstamp 929a216a-4d85-4290-b2dd-a745a945155a))
  (gr_rect (start 170.053 136.2075) (end 172.72 139.1285) (layer "F.SilkS") (width 0.15) (fill solid) (tstamp b4505b49-37c1-4b47-89ad-bd27f82b7379))
  (gr_rect (start 175.514 136.2075) (end 172.593 142.1765) (layer "F.SilkS") (width 0.15) (fill solid) (tstamp d367071e-28c2-4b85-9d75-ecfa7eac9eed))
  (gr_arc (start 130.622691 149.828191) (mid 131.251309 150.088573) (end 131.511691 150.717191) (layer "Edge.Cuts") (width 0.1) (tstamp 0ab99d1a-3d17-4969-835d-a2daa47d2cc4))
  (gr_line (start 88.519 150.714) (end 88.519 54.864) (layer "Edge.Cuts") (width 0.1) (tstamp 1a736170-eccd-4a1f-b6dd-ee961e2c0790))
  (gr_line (start 178.689 150.714) (end 178.689 54.864) (layer "Edge.Cuts") (width 0.1) (tstamp 642a8591-6744-4ef0-b7da-a50f40c58413))
  (gr_line (start 130.622691 149.828191) (end 124.393309 149.821809) (layer "Edge.Cuts") (width 0.1) (tstamp 7ecdb2cf-82ea-4859-8dee-55351d648785))
  (gr_arc (start 123.504309 150.710809) (mid 123.764686 150.082186) (end 124.393309 149.821809) (layer "Edge.Cuts") (width 0.1) (tstamp 8332965c-f8e4-4c5a-8515-5aff504d6d8d))
  (gr_line (start 123.504309 150.710809) (end 88.519 150.714) (layer "Edge.Cuts") (width 0.1) (tstamp acd5305b-c339-4645-a326-10bed9198ad0))
  (gr_line (start 178.689 150.714) (end 131.511691 150.717191) (layer "Edge.Cuts") (width 0.1) (tstamp b2cd3aa5-3f4c-476f-bc06-b1b55ceaa0b6))
  (gr_line (start 88.519 54.864) (end 178.689 54.864) (layer "Edge.Cuts") (width 0.1) (tstamp d0329ec8-445c-4422-93a3-2900d5b2695d))
  (gr_text "GND" (at 112.649 149.698) (layer "B.SilkS") (tstamp 13126287-e9cb-4238-b299-7176f08d4c96)
    (effects (font (size 1 1) (thickness 0.2)) (justify left mirror))
  )
  (gr_text "PWR" (at 96.393 149.698) (layer "B.SilkS") (tstamp d1ea7795-8403-4edb-b959-1b29f77ed16f)
    (effects (font (size 1 1) (thickness 0.2)) (justify mirror))
  )
  (gr_text "8 MHz" (at 143.256 136.144 90) (layer "F.SilkS") (tstamp 030f7528-01d8-4f5d-b375-396511a3f702)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (gr_text "GND" (at 106.5276 64.1858 270) (layer "F.SilkS") (tstamp 0b8419d3-ffc6-49ff-968c-e8cee49f2de2)
    (effects (font (size 0.79 0.79) (thickness 0.15)) (justify left))
  )
  (gr_text "GND" (at 109.347 149.698) (layer "F.SilkS") (tstamp 0fc92961-6e51-49df-b0eb-dd1791483003)
    (effects (font (size 1 1) (thickness 0.2)) (justify left))
  )
  (gr_text "GND" (at 94.996 136.017 90) (layer "F.SilkS") (tstamp 19c7c589-8f9c-49b1-992a-aa9697c8afd9)
    (effects (font (size 0.79 0.79) (thickness 0.15)) (justify left))
  )
  (gr_text "~{SMEMW}\n\n~{SMEMR}\n\n~{IOW}\n\n~{IOR}\n" (at 124.2822 136.144 90) (layer "F.SilkS") (tstamp 41f99891-7a2b-4f30-b64b-8a3195d07d40)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (gr_text "A_{0} ______________________ A_{8} _______________________ A_{16} _____ A_{19}" (at 172.466 142.875 180) (layer "F.SilkS") (tstamp 5b176ccc-587a-4308-8c95-991bd5be9b68)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (gr_text "ALE" (at 163.5506 136.144 90) (layer "F.SilkS") (tstamp 6ee72859-595c-4412-88f3-5722eb8289ca)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (gr_text "RESET" (at 97.536 136.144 90) (layer "F.SilkS") (tstamp 7aafb32f-7d1e-405c-a119-d6e845ab6ed7)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (gr_text "VCC" (at 100.076 136.017 90) (layer "F.SilkS") (tstamp 7c5e4fa0-b86b-4eb9-83a8-3a30394566df)
    (effects (font (size 0.79 0.79) (thickness 0.15)) (justify left))
  )
  (gr_text "~{CARDSEL}" (at 112.776 136.144 90) (layer "F.SilkS") (tstamp 9da855b0-f953-4d94-ac15-68c62fcf943f)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (gr_text "~{RTS} O\n\nDCD I\n\nRXD I\n\nTXD O\n\n~{CTS} I" (at 98.9076 64.1858 270) (layer "F.SilkS") (tstamp a2ea50ae-c24f-4a92-9dc1-0435188040bf)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (gr_text "GND" (at 117.9322 135.9408 90) (layer "F.SilkS") (tstamp c221eefe-1cf5-48d5-b941-f08de75c2fe3)
    (effects (font (size 0.79 0.79) (thickness 0.15)) (justify left))
  )
  (gr_text "VCC" (at 166.111 136.144 90) (layer "F.SilkS") (tstamp d01b7809-03fb-4df1-b9c9-faf1b9468903)
    (effects (font (size 0.79 0.79) (thickness 0.15)) (justify left))
  )
  (gr_text "GND" (at 173.741 136.089 90) (layer "F.SilkS") (tstamp d3a51349-28f4-4529-a091-383e21c10a0b)
    (effects (font (size 0.79 0.79) (thickness 0.15)) (justify left))
  )
  (gr_text "D_{0} ___________________ D_{7}" (at 116.205 142.875 180) (layer "F.SilkS") (tstamp de589fca-e528-4d9d-88c3-9fb59d406d80)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (gr_text "OSC" (at 168.6306 136.072 90) (layer "F.SilkS") (tstamp e2059d98-0534-4fea-b2e4-b29b8760876d)
    (effects (font (size 0.79 0.79) (thickness 0.1)) (justify left))
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 50cdd263-04de-4f9c-b0f8-6f77d1f57fd8)
    (pts (xy 88.519 150.714) (xy 178.689 150.714))
    (height 4.445)
    (gr_text "90.1700 mm" (at 133.604 154.009) (layer "Dwgs.User") (tstamp 50cdd263-04de-4f9c-b0f8-6f77d1f57fd8)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp ab4c8f67-4905-4eb6-a8f5-d5e67b3d0627)
    (pts (xy 178.689 150.714) (xy 178.689 54.864))
    (height 6.477)
    (gr_text "95.8500 mm" (at 184.016 102.789 90) (layer "Dwgs.User") (tstamp ab4c8f67-4905-4eb6-a8f5-d5e67b3d0627)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 130.940191 147.711191) (end 121.571191 147.711191) (width 1) (layer "F.Cu") (net 162) (tstamp fd22d1c4-59bd-4634-9f4b-f7bececb8ecd))

  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 191b19ac-b7b2-49e3-b63c-f648f9d72c7a) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.5032 77.6093)
        (xy 111.6838 77.6093)
        (xy 111.6838 75.5011)
        (xy 114.5032 75.5011)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (tstamp 1e3fd3d5-91a2-4915-bf3d-e5e3d46d180b) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.26 142.24)
        (xy 93.599 142.24)
        (xy 93.599 136.144)
        (xy 175.26 136.144)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (tstamp 50a094e9-d2c1-477f-a23e-76fdc0f40352) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.4354 67.7418)
        (xy 105.4354 71.4248)
        (xy 92.0496 71.4248)
        (xy 92.0496 67.7418)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 99aad319-e7cb-4cac-9185-c14a03dce19d) (name "XTAL_UART") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.585 75.438)
        (xy 108.585 80.772)
        (xy 105.664 81.788)
        (xy 104.013 81.788)
        (xy 104.013 85.09)
        (xy 102.997 85.09)
        (xy 102.997 81.788)
        (xy 101.981 80.899)
        (xy 96.52 80.899)
        (xy 96.52 75.438)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp e194095b-bbcd-4c96-89c2-25d13ffb22b2) (name "XTAL") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.254 91.313)
        (xy 127.254 88.011)
        (xy 129.794 88.011)
        (xy 129.794 91.313)
        (xy 136.271 91.313)
        (xy 136.271 104.521)
        (xy 121.666 104.521)
        (xy 121.666 91.313)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "In1.Cu") (tstamp 47c2b278-ae5d-4e95-b5c8-9e4f00c4a0ec) (name "XTAL") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads not_allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.254 91.313)
        (xy 127.254 87.503)
        (xy 129.794 87.503)
        (xy 129.794 91.313)
        (xy 136.271 91.313)
        (xy 136.271 104.521)
        (xy 121.666 104.521)
        (xy 121.666 91.313)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "In1.Cu") (tstamp 4bc286e0-6a16-4d35-a592-670f1762f921) (name "XTAL_UART") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads not_allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.585 75.438)
        (xy 108.585 80.772)
        (xy 105.664 81.788)
        (xy 104.013 81.788)
        (xy 104.013 85.09)
        (xy 102.997 85.09)
        (xy 102.997 81.788)
        (xy 101.981 80.899)
        (xy 96.52 80.899)
        (xy 96.52 75.438)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (tstamp 49a689bc-e71d-4686-9d73-15b3edc7409e) (name "XTAL_RTC") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.704 100.33)
        (xy 146.704 102.9652)
        (xy 146.704 103.2192)
        (xy 146.704 103.886)
        (xy 144.907 103.886)
        (xy 144.907 99.822)
        (xy 142.24 99.822)
        (xy 142.24 94.234)
        (xy 149.479 94.234)
        (xy 149.479 100.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (tstamp 79107591-050e-43e8-911f-f455dcc429f2) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.0366 94.5134)
        (xy 115.0366 87.8586)
        (xy 112.9284 87.8586)
        (xy 112.9284 94.5134)
      )
    )
  )
  (group "" (id 0312d538-5970-4e86-9ea3-b37f042fa4d2)
    (members
      4bc286e0-6a16-4d35-a592-670f1762f921
      68b51e53-c009-4064-a2c1-7be76452f156
      6913c1ca-4cbf-4cc5-8056-70484c48e06f
      79632853-f337-465f-b7b8-11ec5ad129ca
      99aad319-e7cb-4cac-9185-c14a03dce19d
      cc54e793-dce6-429d-96d3-7dd100c8b724
    )
  )
  (group "" (id 449fab23-798a-4827-8235-edc91a3b5fe1)
    (members
      1fa5a828-f463-4f99-b234-116f3dfae9ba
      7e488800-6741-49ab-a5e1-63c0cb97a137
    )
  )
  (group "" (id 57b16bac-2de0-46be-8093-d4401fd55c2f)
    (members
      15e041e3-43eb-4998-9031-224a316dd8b0
      49a689bc-e71d-4686-9d73-15b3edc7409e
      a61610df-4f9d-44a6-9df1-03d38701caa4
    )
  )
  (group "" (id 661b6453-cf17-4959-9a37-145f8165a00a)
    (members
      030f7528-01d8-4f5d-b375-396511a3f702
      0ab99d1a-3d17-4969-835d-a2daa47d2cc4
      0fc92961-6e51-49df-b0eb-dd1791483003
      13126287-e9cb-4238-b299-7176f08d4c96
      19c7c589-8f9c-49b1-992a-aa9697c8afd9
      1a21a6a8-7838-4271-860f-e1a56471e49d
      1a736170-eccd-4a1f-b6dd-ee961e2c0790
      1e3fd3d5-91a2-4915-bf3d-e5e3d46d180b
      23d269d6-d694-442a-bf5d-98bf3544fc31
      360bedc1-8522-4c8c-bbbd-baca6d69d40e
      3ca90e50-ee3f-405a-95f7-449d8602b6f4
      41f99891-7a2b-4f30-b64b-8a3195d07d40
      50cdd263-04de-4f9c-b0f8-6f77d1f57fd8
      58377f22-fdac-4b4e-959d-9a75f98651c5
      5b176ccc-587a-4308-8c95-991bd5be9b68
      6345ed7f-2d79-4a1f-9931-17f3babe5ae9
      642a8591-6744-4ef0-b7da-a50f40c58413
      6ee72859-595c-4412-88f3-5722eb8289ca
      7aafb32f-7d1e-405c-a119-d6e845ab6ed7
      7c5e4fa0-b86b-4eb9-83a8-3a30394566df
      7ecdb2cf-82ea-4859-8dee-55351d648785
      8332965c-f8e4-4c5a-8515-5aff504d6d8d
      85ddabdf-3810-4a33-8d7f-ead1786dc68e
      9da855b0-f953-4d94-ac15-68c62fcf943f
      ab4c8f67-4905-4eb6-a8f5-d5e67b3d0627
      acd5305b-c339-4645-a326-10bed9198ad0
      ad5d2f01-42d8-4a0a-9705-5596e74b97ea
      b2cd3aa5-3f4c-476f-bc06-b1b55ceaa0b6
      b4505b49-37c1-4b47-89ad-bd27f82b7379
      bffa6b67-ebcb-4915-bdc9-d24146d74c38
      c221eefe-1cf5-48d5-b941-f08de75c2fe3
      c33facdd-072f-48ac-8ec8-1beb2fe7b0fd
      d01b7809-03fb-4df1-b9c9-faf1b9468903
      d0329ec8-445c-4422-93a3-2900d5b2695d
      d1ea7795-8403-4edb-b959-1b29f77ed16f
      d367071e-28c2-4b85-9d75-ecfa7eac9eed
      d3a51349-28f4-4529-a091-383e21c10a0b
      de589fca-e528-4d9d-88c3-9fb59d406d80
      e2059d98-0534-4fea-b2e4-b29b8760876d
      e2928b7d-86c1-4d98-942d-4b8bfdd0d498
      fd22d1c4-59bd-4634-9f4b-f7bececb8ecd
    )
  )
  (group "" (id 75d57d7d-4194-4e29-b7dd-a682d6a5c3ae)
    (members
      929a216a-4d85-4290-b2dd-a745a945155a
      dc63a514-7ce0-49f8-a0ed-4f50f6e2e32a
    )
  )
  (group "" (id 91073c99-9290-4466-929a-77ac631b5af1)
    (members
      6daf9014-e686-48eb-b518-1ce417fae5b5
      961f5ed3-0278-4f1a-ada8-01fcaeb55b9d
    )
  )
  (group "" (id 9cc1410f-ee55-4ac2-aaf6-5ff4272c57cf)
    (members
      1f8201c0-e94b-40eb-8f4e-26bb744b5874
      83150091-9395-4ba1-bd12-102d16071454
      aa805fdf-7892-4ac0-bc95-218d6add9fe1
    )
  )
  (group "" (id d82fbaa0-ce37-4864-ac39-f2ecd5691821)
    (members
      0b8419d3-ffc6-49ff-968c-e8cee49f2de2
      50a094e9-d2c1-477f-a23e-76fdc0f40352
      a2ea50ae-c24f-4a92-9dc1-0435188040bf
      a37f1f80-b769-4830-b380-2d8b4ead3bd8
    )
  )
  (group "" (id e2405288-9578-4b7d-811e-78036f0d30c8)
    (members
      0f69863e-85e9-4bea-8c41-d01e3b007b9c
      6b7345ec-7638-4606-95fc-02c5893a2ef6
    )
  )
  (group "" (id f95c26e9-94fc-4584-9620-9c94facd9589)
    (members
      00120ce5-cea2-43e7-a366-060498189dc5
      02b8749d-8df5-4032-a24a-2669d0318e48
      12fb8895-395d-4901-9f1b-bca198430a0f
      191b19ac-b7b2-49e3-b63c-f648f9d72c7a
      1fbcfd57-a9b0-45ef-89ea-b37a43678369
      2ff3ed75-7181-4c39-9dd5-787707739b13
      3fce92fa-e607-4dbb-bd27-27baad6dd8ad
      47c2b278-ae5d-4e95-b5c8-9e4f00c4a0ec
      4d683f6c-2463-4e86-b710-686926e8a6ee
      4e9f6b06-3942-47ec-91b6-302ef574306f
      5264b699-a844-4267-bd47-59a775247fac
      79107591-050e-43e8-911f-f455dcc429f2
      89cb84a8-dc89-42ca-b87f-411fe5057f13
      8b3f22e5-204d-4aee-b2c2-4adcea04c22e
      8bb25c3c-5145-4c18-af67-23c7dffe6781
      e194095b-bbcd-4c96-89c2-25d13ffb22b2
    )
  )
)
