{ "" "" "" "Verilog HDL or VHDL warning at sys_top.v(209): object \"vip_newcfg\" assigned a value but never read" {  } {  } 0 10036 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Verilog HDL information at MC6845.v(280): always construct contains both blocking and non-blocking assignments" {  } {  } 0 10268 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Verilog HDL or VHDL warning at sys_top.v(601): object \"VSET\" assigned a value but never read" {  } {  } 0 10036 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Port \"extclk\" on the entity instantiation of \"cyclonev_pll\" is connected to a signal of width 1. The formal width of the signal in the module is 2.  The extra bits will be left dangling without any fan-out logic." {  } {  } 0 12030 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "RST port on the PLL is not properly connected on instance emu:emu\|pll:pll\|pll_0002:pll_inst\|altera_pll:altera_pll_i\|general\[0\].gpll. The reset port on the PLL should be connected. If the PLL loses lock for any reason, you might need to manually reset the PLL in order to re-establish lock to the reference clock." {  } {  } 0 0 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Dummy RLC values generated in IBIS model files for device 5CSEBA6 with package UFBGA and pin count 672" {  } {  } 0 205009 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored filter at sys_top.sdc(10): vip\|output_inst\|vid_clk could not be matched with a net" {  } {  } 0 332174 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored create_generated_clock at sys_top.sdc(9): Argument <targets> is an empty collection" {  } {  } 0 332049 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored filter at sys_top.sdc(29): VID_CLK could not be matched with a clock" {  } {  } 0 332174 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Timing characteristics of device 5CSEBA6U23I7 are preliminary" {  } {  } 0 334000 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Inferred RAM node \"emu:emu\|rom_map_rtl_0\" from synchronous design logic.  Pass-through logic has been added to match the read-during-write behavior of the original design." {  } {  } 0 276020 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "RST port on the PLL is not properly connected on instance emu:emu\|pll:pll\|pll_0002:pll_inst\|altera_pll:altera_pll_i\|general\[1\].gpll. The reset port on the PLL should be connected. If the PLL loses lock for any reason, you might need to manually reset the PLL in order to re-establish lock to the reference clock." {  } {  } 0 0 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored filter at sys_top.sdc(17): vip\|output_inst\|vid_clk could not be matched with a net" {  } {  } 0 332174 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored create_generated_clock at sys_top.sdc(16): Argument <targets> is an empty collection" {  } {  } 0 332049 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored filter at sys_top.sdc(37): VID_CLK could not be matched with a clock" {  } {  } 0 332174 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "LOCKED port on the PLL is not properly connected on instance \"emu:emu\|pll:pll\|pll_0002:pll_inst\|altera_pll:altera_pll_i\|general\[0\].gpll\". The LOCKED port on the PLL should be connected when the FBOUTCLK port is connected. Although it is unnecessary to connect the LOCKED signal, any logic driven off of an output clock of the PLL will not know when the PLL is locked and ready." {  } {  } 0 21300 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Some pins have incomplete I/O assignments. Refer to the I/O Assignment Warnings report for details" {  } {  } 0 15714 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignoring invalid fast I/O register assignments. See the Ignored Assignments panel in the Fitter Compilation Report for more information." {  } {  } 0 176250 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "Ignored locations or region assignments to the following nodes" {  } {  } 0 15705 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "RST port on the PLL is not properly connected on instance emu:emu\|pll:pll\|pll_0002:pll_inst\|altera_pll:altera_pll_i\|general\[2\].gpll. The reset port on the PLL should be connected. If the PLL loses lock for any reason, you might need to manually reset the PLL in order to re-establish lock to the reference clock." {  } {  } 0 0 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "RST port on the PLL is not properly connected on instance emu:emu\|pll:pll\|pll_0002:pll_inst\|altera_pll:altera_pll_i\|general\[3\].gpll. The reset port on the PLL should be connected. If the PLL loses lock for any reason, you might need to manually reset the PLL in order to re-establish lock to the reference clock." {  } {  } 0 0 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "*" {  } {  } 0 10268 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "*" {  } {  } 0 276027 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "*" {  } {  } 0 276020 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "altera_pll.v" {  } {  } 0 9999 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "altera_cyclonev_pll.v" {  } {  } 0 9999 "" 0 0 "Quartus II" 0 -1 0 ""}
{ "" "" "" "altera_pll_reconfig_core.v" {  } {  } 0 9999 "" 0 0 "Quartus II" 0 -1 0 ""}
