(export (version D)
  (design
    (source C:\Users\hotkey\SparkleShare\documents\electro\KiCad\CPU8085\CPU8085.sch)
    (date "2018-09-02 22:42:26")
    (tool "Eeschema (5.0.0)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source CPU8085.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /CPU/) (tstamps /5B8BFEAE/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source CPU.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /Memory/) (tstamps /5B8BFECF/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Memory.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /UART/) (tstamps /5B955671/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source UART.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /PIT/) (tstamps /5B98C06B/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source PIT.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /IODECODE/) (tstamps /5B96BA20/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IODECODE.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref MK1)
      (value Mounting_Hole_PAD)
      (footprint Mounting_Holes:MountingHole_2.7mm)
      (libsource (lib "") (part Mounting_Hole_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A6CFED2))
    (comp (ref MK2)
      (value Mounting_Hole_PAD)
      (footprint Mounting_Holes:MountingHole_2.7mm)
      (libsource (lib "") (part Mounting_Hole_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A6CFF98))
    (comp (ref MK4)
      (value Mounting_Hole_PAD)
      (footprint Mounting_Holes:MountingHole_2.7mm)
      (libsource (lib "") (part Mounting_Hole_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A6D003F))
    (comp (ref J1)
      (value POWER)
      (footprint Connector_Molex:Molex_SPOX_5267-04A_1x04_P2.50mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8BFF37))
    (comp (ref MK3)
      (value Mounting_Hole_PAD)
      (footprint Mounting_Holes:MountingHole_2.7mm)
      (libsource (lib "") (part Mounting_Hole_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A6CFFFA))
    (comp (ref U1)
      (value 8085)
      (footprint Package_DIP:DIP-40_W15.24mm)
      (libsource (lib 8085) (part 8085) (description ""))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C0686))
    (comp (ref R1)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C07F0))
    (comp (ref R2)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C0915))
    (comp (ref R3)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C094D))
    (comp (ref R4)
      (value 75K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C097C))
    (comp (ref D1)
      (value 1N4004)
      (footprint Diode_THT:D_A-405_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part D_ALT) (description "Diode, alternativ symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C0E93))
    (comp (ref R5)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C235B))
    (comp (ref R7)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C25AD))
    (comp (ref R6)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C2666))
    (comp (ref R8)
      (value 10K)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor US symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C2722))
    (comp (ref SW1)
      (value RESET)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib Switch) (part SW_DIP_x01) (description "1x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C4B7C))
    (comp (ref C1)
      (value 1uF)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP1) (description "Polarised capacitor"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C4CF6))
    (comp (ref X1)
      (value 1.8432)
      (footprint Oscillator:Oscillator_DIP-14)
      (datasheet http://www.golledge.com/pdf/products/tcxos/gtxos14.pdf)
      (libsource (lib Oscillator) (part TCXO-14) (description "Temperature Compensated Crystal Clock Oscillator, DIP14-style metal package"))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8C642F))
    (comp (ref U4)
      (value GLUE_LOGIC)
      (footprint Package_DIP:DIP-20_W7.62mm)
      (libsource (lib 8085) (part GLUE_LOGIC) (description ""))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8CAEEC))
    (comp (ref U2)
      (value A_LOW)
      (footprint Package_DIP:DIP-20_W7.62mm)
      (libsource (lib 8085) (part ALATCH) (description ""))
      (sheetpath (names /CPU/) (tstamps /5B8BFEAE/))
      (tstamp 5B8E65EA))
    (comp (ref U5)
      (value 27C256)
      (footprint Package_DIP:DIP-28_W15.24mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/doc0014.pdf)
      (libsource (lib Memory_EPROM) (part 27C256) (description "OTP EPROM 256 KiBit"))
      (sheetpath (names /Memory/) (tstamps /5B8BFECF/))
      (tstamp 5B945467))
    (comp (ref U6)
      (value IS61C256AH)
      (footprint Package_DIP:DIP-28_W7.62mm)
      (libsource (lib 8085) (part IS61C256AH) (description ""))
      (sheetpath (names /Memory/) (tstamps /5B8BFECF/))
      (tstamp 5B949123))
    (comp (ref U7)
      (value 8250)
      (footprint Package_DIP:DIP-40_W15.24mm)
      (libsource (lib Interface_UART) (part 8250) (description "PC8250A, Universal Asynchronous Receiver/Transmitter, PDIP-40"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B9557FE))
    (comp (ref U8)
      (value MAX232)
      (footprint Package_DIP:DIP-16_W7.62mm)
      (datasheet http://www.ti.com/lit/ds/symlink/max232.pdf)
      (libsource (lib Interface_UART) (part MAX232) (description "Dual RS232 driver/receiver, 5V supply, 120kb/s, 0C-70C"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B955886))
    (comp (ref J2)
      (value DB9_Female_MountingHoles)
      (footprint Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm)
      (datasheet " ~")
      (libsource (lib Connector) (part DB9_Female_MountingHoles) (description "9-pin female D-SUB connector, Mounting Hole"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B9009D3))
    (comp (ref C3)
      (value 0.1uF)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP1) (description "Polarised capacitor"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B909D17))
    (comp (ref C4)
      (value 0.1uF)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP1) (description "Polarised capacitor"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B90C3A4))
    (comp (ref C2)
      (value 0.1uF)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP1) (description "Polarised capacitor"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B919435))
    (comp (ref C5)
      (value 0.1uF)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part CP1) (description "Polarised capacitor"))
      (sheetpath (names /UART/) (tstamps /5B955671/))
      (tstamp 5B9194F1))
    (comp (ref U12)
      (value 82C54)
      (footprint Package_DIP:DIP-24_W15.24mm)
      (datasheet http://download.intel.com/design/archives/periphrl/docs/23124406.pdf)
      (libsource (lib Timer) (part 82C54) (description "CHMOS Programmable Interval Timer, PDIP-24"))
      (sheetpath (names /PIT/) (tstamps /5B98C06B/))
      (tstamp 5B98D78A))
    (comp (ref U9)
      (value 74LS138)
      (footprint Package_DIP:DIP-16_W7.62mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LS138)
      (libsource (lib 74xx) (part 74LS138) (description "Decoder 3 to 8 active low outputs"))
      (sheetpath (names /IODECODE/) (tstamps /5B96BA20/))
      (tstamp 5B96BCB6)))
  (libparts
    (libpart (lib "") (part Mechanical:Mounting_Hole_PAD)
      (footprints
        (fp Mounting?Hole*)
        (fp Hole*))
      (fields
        (field (name Reference) MK)
        (field (name Value) Mechanical:Mounting_Hole_PAD))
      (pins
        (pin (num 1) (name 1) (type input))))
    (libpart (lib 74xx) (part 74LS138)
      (description "Decoder 3 to 8 active low outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS138)
      (footprints
        (fp DIP?16*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS138))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name E1) (type input))
        (pin (num 5) (name E2) (type input))
        (pin (num 6) (name E3) (type input))
        (pin (num 7) (name O7) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name O6) (type output))
        (pin (num 10) (name O5) (type output))
        (pin (num 11) (name O4) (type output))
        (pin (num 12) (name O3) (type output))
        (pin (num 13) (name O2) (type output))
        (pin (num 14) (name O1) (type output))
        (pin (num 15) (name O0) (type output))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib 8085) (part 8085)
      (footprints
        (fp IC_DIP40_600*))
      (fields
        (field (name Reference) U)
        (field (name Value) 8085))
      (pins
        (pin (num 1) (name X1) (type input))
        (pin (num 2) (name X2) (type input))
        (pin (num 3) (name RES_OUT) (type output))
        (pin (num 4) (name SOD) (type output))
        (pin (num 5) (name SID) (type input))
        (pin (num 6) (name TRAP) (type input))
        (pin (num 7) (name RST7_5) (type input))
        (pin (num 8) (name RST6_5) (type input))
        (pin (num 9) (name RST5_5) (type input))
        (pin (num 10) (name INTR) (type input))
        (pin (num 11) (name ~INTA) (type output))
        (pin (num 12) (name AD0) (type 3state))
        (pin (num 13) (name AD1) (type 3state))
        (pin (num 14) (name AD2) (type 3state))
        (pin (num 15) (name AD3) (type 3state))
        (pin (num 16) (name AD4) (type 3state))
        (pin (num 17) (name AD5) (type 3state))
        (pin (num 18) (name AD6) (type 3state))
        (pin (num 19) (name AD7) (type 3state))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name A8) (type 3state))
        (pin (num 22) (name A9) (type 3state))
        (pin (num 23) (name A10) (type 3state))
        (pin (num 24) (name A11) (type 3state))
        (pin (num 25) (name A12) (type 3state))
        (pin (num 26) (name A13) (type 3state))
        (pin (num 27) (name A14) (type 3state))
        (pin (num 28) (name A15) (type 3state))
        (pin (num 29) (name S0) (type output))
        (pin (num 30) (name ALE) (type output))
        (pin (num 31) (name ~WR) (type output))
        (pin (num 32) (name ~RD) (type output))
        (pin (num 33) (name S1) (type output))
        (pin (num 34) (name IO/~M) (type output))
        (pin (num 35) (name READY) (type input))
        (pin (num 36) (name ~RES_IN) (type input))
        (pin (num 37) (name CLK) (type output))
        (pin (num 38) (name HLDA) (type output))
        (pin (num 39) (name HOLD) (type input))
        (pin (num 40) (name VCC) (type power_in))))
    (libpart (lib 8085) (part ALATCH)
      (fields
        (field (name Reference) U)
        (field (name Value) ALATCH))
      (pins
        (pin (num 1) (name CLK) (type input))
        (pin (num 2) (name I0) (type input))
        (pin (num 3) (name I1) (type input))
        (pin (num 4) (name I2) (type input))
        (pin (num 5) (name I3) (type input))
        (pin (num 6) (name I4) (type input))
        (pin (num 7) (name I5) (type input))
        (pin (num 8) (name I6) (type input))
        (pin (num 9) (name I7) (type input))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name OE) (type input))
        (pin (num 12) (name Q7) (type 3state))
        (pin (num 13) (name Q6) (type 3state))
        (pin (num 14) (name Q5) (type 3state))
        (pin (num 15) (name Q4) (type 3state))
        (pin (num 16) (name Q3) (type 3state))
        (pin (num 17) (name Q2) (type 3state))
        (pin (num 18) (name Q1) (type 3state))
        (pin (num 19) (name Q0) (type 3state))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 8085) (part GLUE_LOGIC)
      (fields
        (field (name Reference) U)
        (field (name Value) GLUE_LOGIC))
      (pins
        (pin (num 1) (name IO/~M) (type input))
        (pin (num 2) (name RD) (type input))
        (pin (num 3) (name WR) (type input))
        (pin (num 4) (name ALE) (type input))
        (pin (num 5) (name A15) (type input))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 13) (name RAMCE) (type output))
        (pin (num 14) (name ROMCE) (type output))
        (pin (num 15) (name MEMW) (type output))
        (pin (num 16) (name MEMR) (type output))
        (pin (num 17) (name IOW) (type output))
        (pin (num 18) (name IOR) (type output))
        (pin (num 19) (name ALECLK) (type output))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 8085) (part IS61C256AH)
      (fields
        (field (name Reference) U)
        (field (name Value) IS61C256AH))
      (pins
        (pin (num 1) (name A14) (type input))
        (pin (num 2) (name A12) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A6) (type input))
        (pin (num 5) (name A5) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A1) (type input))
        (pin (num 10) (name A0) (type input))
        (pin (num 11) (name D0) (type BiDi))
        (pin (num 12) (name D1) (type BiDi))
        (pin (num 13) (name D2) (type BiDi))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name D3) (type BiDi))
        (pin (num 16) (name D4) (type BiDi))
        (pin (num 17) (name D5) (type BiDi))
        (pin (num 18) (name D6) (type BiDi))
        (pin (num 19) (name D7) (type BiDi))
        (pin (num 20) (name CE) (type input))
        (pin (num 21) (name A10) (type input))
        (pin (num 22) (name OE) (type input))
        (pin (num 23) (name A11) (type input))
        (pin (num 24) (name A9) (type input))
        (pin (num 25) (name A8) (type input))
        (pin (num 26) (name A13) (type input))
        (pin (num 27) (name WE) (type input))
        (pin (num 28) (name VCC) (type power_in))))
    (libpart (lib Connector) (part DB9_Female_MountingHoles)
      (description "9-pin female D-SUB connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Female*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB9_Female_MountingHoles))
      (pins
        (pin (num 0) (name PAD) (type passive))
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Device) (part CP1)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_ALT)
      (description "Diode, alternativ symbol")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_ALT))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R_US)
      (description "Resistor US symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_US))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Interface_UART) (part 16450)
      (aliases
        (alias 8250))
      (description "PC16450, Universal Asynchronous Receiver/Transmitter, PDIP-40")
      (footprints
        (fp DIP*W15.24mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 16450)
        (field (name Footprint) Package_DIP:DIP-40_W15.24mm))
      (pins
        (pin (num 1) (name D0) (type BiDi))
        (pin (num 2) (name D1) (type BiDi))
        (pin (num 3) (name D2) (type BiDi))
        (pin (num 4) (name D3) (type BiDi))
        (pin (num 5) (name D4) (type BiDi))
        (pin (num 6) (name D5) (type BiDi))
        (pin (num 7) (name D6) (type BiDi))
        (pin (num 8) (name D7) (type BiDi))
        (pin (num 9) (name RCLK) (type input))
        (pin (num 10) (name SIN) (type input))
        (pin (num 11) (name SOUT) (type output))
        (pin (num 12) (name CS0) (type input))
        (pin (num 13) (name CS1) (type input))
        (pin (num 14) (name ~CS2~) (type input))
        (pin (num 15) (name ~BAUDOUT~) (type output))
        (pin (num 16) (name XIN) (type input))
        (pin (num 17) (name XOUT) (type output))
        (pin (num 18) (name ~WR~) (type input))
        (pin (num 19) (name WR) (type input))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name ~RD~) (type input))
        (pin (num 22) (name RD) (type input))
        (pin (num 23) (name DDIS) (type output))
        (pin (num 24) (name CSOUT) (type output))
        (pin (num 25) (name ~ADS~) (type input))
        (pin (num 26) (name A2) (type input))
        (pin (num 27) (name A1) (type input))
        (pin (num 28) (name A0) (type input))
        (pin (num 30) (name INTR) (type output))
        (pin (num 31) (name ~OUT2~) (type output))
        (pin (num 32) (name ~RTS~) (type output))
        (pin (num 33) (name ~DTR~) (type output))
        (pin (num 34) (name ~OUT1~) (type output))
        (pin (num 35) (name MR) (type input))
        (pin (num 36) (name ~CTS~) (type input))
        (pin (num 37) (name ~DSR~) (type input))
        (pin (num 38) (name ~DCD~) (type input))
        (pin (num 39) (name ~RI~) (type input))
        (pin (num 40) (name VCC) (type power_in))))
    (libpart (lib Interface_UART) (part MAX232)
      (aliases
        (alias MAX232I)
        (alias MAX202)
        (alias ADM232A)
        (alias MAX3232)
        (alias ICL3232))
      (description "Dual RS232 driver/receiver, 5V supply, 120kb/s, 0C-70C")
      (docs http://www.ti.com/lit/ds/symlink/max232.pdf)
      (footprints
        (fp SOIC*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MAX232))
      (pins
        (pin (num 1) (name C1+) (type passive))
        (pin (num 2) (name VS+) (type power_out))
        (pin (num 3) (name C1-) (type passive))
        (pin (num 4) (name C2+) (type passive))
        (pin (num 5) (name C2-) (type passive))
        (pin (num 6) (name VS-) (type power_out))
        (pin (num 7) (name T2OUT) (type output))
        (pin (num 8) (name R2IN) (type input))
        (pin (num 9) (name R2OUT) (type output))
        (pin (num 10) (name T2IN) (type input))
        (pin (num 11) (name T1IN) (type input))
        (pin (num 12) (name R1OUT) (type output))
        (pin (num 13) (name R1IN) (type input))
        (pin (num 14) (name T1OUT) (type output))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Memory_EPROM) (part 27C256)
      (aliases
        (alias 27256))
      (description "OTP EPROM 256 KiBit")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/doc0014.pdf)
      (footprints
        (fp DIP*W15.24mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 27C256)
        (field (name Footprint) Package_DIP:DIP-28_W15.24mm))
      (pins
        (pin (num 1) (name VPP) (type input))
        (pin (num 2) (name A12) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A6) (type input))
        (pin (num 5) (name A5) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A1) (type input))
        (pin (num 10) (name A0) (type input))
        (pin (num 11) (name D0) (type 3state))
        (pin (num 12) (name D1) (type 3state))
        (pin (num 13) (name D2) (type 3state))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name D3) (type 3state))
        (pin (num 16) (name D4) (type 3state))
        (pin (num 17) (name D5) (type 3state))
        (pin (num 18) (name D6) (type 3state))
        (pin (num 19) (name D7) (type 3state))
        (pin (num 20) (name ~CE) (type input))
        (pin (num 21) (name A10) (type input))
        (pin (num 22) (name ~OE) (type input))
        (pin (num 23) (name A11) (type input))
        (pin (num 24) (name A9) (type input))
        (pin (num 25) (name A8) (type input))
        (pin (num 26) (name A13) (type input))
        (pin (num 27) (name A14) (type input))
        (pin (num 28) (name VCC) (type power_in))))
    (libpart (lib Oscillator) (part DGOF5S3)
      (aliases
        (alias ACO-xxxMHz)
        (alias GTXO-S14T)
        (alias TCXO-14))
      (description "HCMOS Crystal Clock Oscillator, DIP14-style metal package")
      (docs http://www.conwin.com/datasheets/cx/cx030.pdf)
      (footprints
        (fp Oscillator*DIP*14*))
      (fields
        (field (name Reference) X)
        (field (name Value) DGOF5S3)
        (field (name Footprint) Oscillator:Oscillator_DIP-14))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT) (type output))
        (pin (num 14) (name Vcc) (type power_in))))
    (libpart (lib Switch) (part SW_DIP_x01)
      (description "1x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x1*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x01))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Timer) (part 82C54)
      (aliases
        (alias 8254)
        (alias 8253))
      (description "CHMOS Programmable Interval Timer, PDIP-24")
      (docs http://download.intel.com/design/archives/periphrl/docs/23124406.pdf)
      (footprints
        (fp DIP*W15.24mm*)
        (fp PDIP*W15.24mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 82C54)
        (field (name Footprint) Package_DIP:DIP-24_W15.24mm))
      (pins
        (pin (num 1) (name D7) (type BiDi))
        (pin (num 2) (name D6) (type BiDi))
        (pin (num 3) (name D5) (type BiDi))
        (pin (num 4) (name D4) (type BiDi))
        (pin (num 5) (name D3) (type BiDi))
        (pin (num 6) (name D2) (type BiDi))
        (pin (num 7) (name D1) (type BiDi))
        (pin (num 8) (name D0) (type BiDi))
        (pin (num 9) (name CLK0) (type input))
        (pin (num 10) (name OUT0) (type output))
        (pin (num 11) (name G0) (type input))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name OUT1) (type output))
        (pin (num 14) (name G1) (type input))
        (pin (num 15) (name CLK1) (type input))
        (pin (num 16) (name G2) (type input))
        (pin (num 17) (name OUT2) (type output))
        (pin (num 18) (name CLK2) (type input))
        (pin (num 19) (name A0) (type input))
        (pin (num 20) (name A1) (type input))
        (pin (num 21) (name ~CS~) (type input))
        (pin (num 22) (name ~RD~) (type input))
        (pin (num 23) (name ~WR~) (type input))
        (pin (num 24) (name VCC) (type power_in)))))
  (libraries
    (library (logical 74xx)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/74xx.lib"))
    (library (logical 8085)
      (uri C:\Users\hotkey\SparkleShare\documents\electro\KiCad\CPU8085/8085.lib))
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Interface_UART)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Interface_UART.lib"))
    (library (logical Memory_EPROM)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Memory_EPROM.lib"))
    (library (logical Oscillator)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Oscillator.lib"))
    (library (logical Switch)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Switch.lib"))
    (library (logical Timer)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Timer.lib")))
  (nets
    (net (code 3) (name /CPU/RESET)
      (node (ref U1) (pin 3))
      (node (ref U7) (pin 35)))
    (net (code 7) (name /CPU/~IOR)
      (node (ref U12) (pin 22))
      (node (ref U4) (pin 18))
      (node (ref U7) (pin 21)))
    (net (code 8) (name /CPU/~IOW)
      (node (ref U4) (pin 17))
      (node (ref U12) (pin 23))
      (node (ref U7) (pin 18)))
    (net (code 9) (name /CPU/CLOCK)
      (node (ref U12) (pin 9))
      (node (ref U12) (pin 18))
      (node (ref X1) (pin 8))
      (node (ref U7) (pin 16))
      (node (ref U1) (pin 1))
      (node (ref U12) (pin 15)))
    (net (code 11) (name /CPU/~MEMR)
      (node (ref U5) (pin 22))
      (node (ref U4) (pin 16))
      (node (ref U6) (pin 22)))
    (net (code 12) (name /CPU/~MEMW)
      (node (ref U4) (pin 15))
      (node (ref U6) (pin 27)))
    (net (code 13) (name /CPU/~ROMCE)
      (node (ref U5) (pin 20))
      (node (ref U4) (pin 14)))
    (net (code 14) (name /CPU/~RAMCE)
      (node (ref U4) (pin 13))
      (node (ref U6) (pin 20)))
    (net (code 15) (name GND)
      (node (ref C4) (pin 1))
      (node (ref U8) (pin 15))
      (node (ref U1) (pin 10))
      (node (ref U7) (pin 22))
      (node (ref U1) (pin 5))
      (node (ref U7) (pin 19))
      (node (ref U7) (pin 39))
      (node (ref U7) (pin 20))
      (node (ref X1) (pin 7))
      (node (ref R7) (pin 2))
      (node (ref U2) (pin 10))
      (node (ref U2) (pin 11))
      (node (ref U5) (pin 14))
      (node (ref R8) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref U1) (pin 39))
      (node (ref U1) (pin 20))
      (node (ref U4) (pin 10))
      (node (ref C1) (pin 2))
      (node (ref J2) (pin 0))
      (node (ref J2) (pin 5))
      (node (ref SW1) (pin 1))
      (node (ref U9) (pin 5))
      (node (ref MK4) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref U7) (pin 37))
      (node (ref U7) (pin 38))
      (node (ref J1) (pin 4))
      (node (ref U9) (pin 4))
      (node (ref MK3) (pin 1))
      (node (ref U6) (pin 14))
      (node (ref MK1) (pin 1))
      (node (ref U12) (pin 12))
      (node (ref MK2) (pin 1))
      (node (ref U7) (pin 25))
      (node (ref U9) (pin 8)))
    (net (code 16) (name VCC)
      (node (ref J1) (pin 2))
      (node (ref U12) (pin 24))
      (node (ref U5) (pin 28))
      (node (ref U1) (pin 40))
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U2) (pin 20))
      (node (ref U9) (pin 16))
      (node (ref U9) (pin 6))
      (node (ref J1) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref U6) (pin 28))
      (node (ref X1) (pin 14))
      (node (ref U7) (pin 40))
      (node (ref U7) (pin 12))
      (node (ref U4) (pin 20))
      (node (ref U8) (pin 16))
      (node (ref U7) (pin 13)))
    (net (code 17) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1))
      (node (ref U4) (pin 19)))
    (net (code 19) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 20) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 21) (name "Net-(R8-Pad1)")
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 22) (name "Net-(R6-Pad1)")
      (node (ref U1) (pin 8))
      (node (ref R6) (pin 1)))
    (net (code 23) (name "Net-(R1-Pad1)")
      (node (ref U1) (pin 35))
      (node (ref R1) (pin 1)))
    (net (code 24) (name "Net-(U1-Pad37)")
      (node (ref U1) (pin 37)))
    (net (code 25) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 26) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 27) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 28) (name "Net-(R5-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 9)))
    (net (code 29) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 30) (name "Net-(U1-Pad38)")
      (node (ref U1) (pin 38)))
    (net (code 31) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30))
      (node (ref U4) (pin 4)))
    (net (code 32) (name "Net-(R2-Pad2)")
      (node (ref U1) (pin 32))
      (node (ref U4) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 33) (name "Net-(R3-Pad2)")
      (node (ref U4) (pin 3))
      (node (ref U1) (pin 31))
      (node (ref R3) (pin 2)))
    (net (code 34) (name "Net-(U1-Pad34)")
      (node (ref U4) (pin 1))
      (node (ref U1) (pin 34)))
    (net (code 35) (name "Net-(C1-Pad1)")
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 36))
      (node (ref R4) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref C1) (pin 1)))
    (net (code 36) (name "Net-(X1-Pad1)")
      (node (ref X1) (pin 1)))
    (net (code 39) (name "Net-(U7-Pad33)")
      (node (ref U7) (pin 33)))
    (net (code 40) (name "Net-(U7-Pad31)")
      (node (ref U7) (pin 31)))
    (net (code 41) (name "Net-(U7-Pad34)")
      (node (ref U7) (pin 34)))
    (net (code 42) (name "Net-(U7-Pad23)")
      (node (ref U7) (pin 23)))
    (net (code 43) (name "Net-(U7-Pad24)")
      (node (ref U7) (pin 24)))
    (net (code 44) (name "Net-(U7-Pad15)")
      (node (ref U7) (pin 9))
      (node (ref U7) (pin 15)))
    (net (code 45) (name "Net-(U7-Pad30)")
      (node (ref U7) (pin 30)))
    (net (code 46) (name "Net-(U7-Pad17)")
      (node (ref U7) (pin 17)))
    (net (code 47) (name /UART/RXD)
      (node (ref U8) (pin 9))
      (node (ref U7) (pin 10)))
    (net (code 48) (name /UART/TXD)
      (node (ref U8) (pin 10))
      (node (ref U7) (pin 11)))
    (net (code 49) (name /UART/~RTS)
      (node (ref U8) (pin 11))
      (node (ref U7) (pin 32)))
    (net (code 50) (name "Net-(C5-Pad1)")
      (node (ref U8) (pin 4))
      (node (ref C5) (pin 1)))
    (net (code 51) (name "Net-(C5-Pad2)")
      (node (ref U8) (pin 5))
      (node (ref C5) (pin 2)))
    (net (code 52) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2))
      (node (ref U8) (pin 3)))
    (net (code 53) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref U8) (pin 1)))
    (net (code 54) (name /UART/~CTS)
      (node (ref U7) (pin 36))
      (node (ref U8) (pin 12)))
    (net (code 55) (name "Net-(J2-Pad3)")
      (node (ref U8) (pin 7))
      (node (ref J2) (pin 3)))
    (net (code 56) (name "Net-(J2-Pad7)")
      (node (ref U8) (pin 14))
      (node (ref J2) (pin 7)))
    (net (code 57) (name "Net-(J2-Pad8)")
      (node (ref U8) (pin 13))
      (node (ref J2) (pin 8)))
    (net (code 58) (name "Net-(J2-Pad2)")
      (node (ref U8) (pin 8))
      (node (ref J2) (pin 2)))
    (net (code 59) (name "Net-(J2-Pad9)")
      (node (ref J2) (pin 9)))
    (net (code 60) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 61) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1)))
    (net (code 62) (name "Net-(J2-Pad6)")
      (node (ref J2) (pin 6)))
    (net (code 63) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref U8) (pin 2)))
    (net (code 64) (name "Net-(C4-Pad2)")
      (node (ref U8) (pin 6))
      (node (ref C4) (pin 2)))
    (net (code 65) (name "Net-(U12-Pad16)")
      (node (ref U12) (pin 16)))
    (net (code 66) (name "Net-(U12-Pad17)")
      (node (ref U12) (pin 17)))
    (net (code 67) (name "Net-(U12-Pad14)")
      (node (ref U12) (pin 14)))
    (net (code 68) (name "Net-(U12-Pad13)")
      (node (ref U12) (pin 13)))
    (net (code 69) (name "Net-(U12-Pad11)")
      (node (ref U12) (pin 11)))
    (net (code 70) (name "Net-(U12-Pad10)")
      (node (ref U12) (pin 10)))
    (net (code 71) (name /CPU/D5)
      (node (ref U7) (pin 6))
      (node (ref U2) (pin 7))
      (node (ref U5) (pin 17))
      (node (ref U12) (pin 3))
      (node (ref U6) (pin 17))
      (node (ref U1) (pin 17)))
    (net (code 72) (name /CPU/D0)
      (node (ref U7) (pin 1))
      (node (ref U1) (pin 12))
      (node (ref U6) (pin 11))
      (node (ref U5) (pin 11))
      (node (ref U12) (pin 8))
      (node (ref U2) (pin 2)))
    (net (code 73) (name /CPU/D1)
      (node (ref U12) (pin 7))
      (node (ref U7) (pin 2))
      (node (ref U5) (pin 12))
      (node (ref U6) (pin 12))
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 13)))
    (net (code 74) (name /CPU/D2)
      (node (ref U1) (pin 14))
      (node (ref U6) (pin 13))
      (node (ref U5) (pin 13))
      (node (ref U2) (pin 4))
      (node (ref U12) (pin 6))
      (node (ref U7) (pin 3)))
    (net (code 75) (name /CPU/D3)
      (node (ref U1) (pin 15))
      (node (ref U12) (pin 5))
      (node (ref U2) (pin 5))
      (node (ref U5) (pin 15))
      (node (ref U6) (pin 15))
      (node (ref U7) (pin 4)))
    (net (code 76) (name /CPU/D4)
      (node (ref U5) (pin 16))
      (node (ref U12) (pin 4))
      (node (ref U7) (pin 5))
      (node (ref U1) (pin 16))
      (node (ref U2) (pin 6))
      (node (ref U6) (pin 16)))
    (net (code 77) (name /CPU/D6)
      (node (ref U7) (pin 7))
      (node (ref U5) (pin 18))
      (node (ref U1) (pin 18))
      (node (ref U2) (pin 8))
      (node (ref U6) (pin 18))
      (node (ref U12) (pin 2)))
    (net (code 78) (name /CPU/D7)
      (node (ref U1) (pin 19))
      (node (ref U5) (pin 19))
      (node (ref U6) (pin 19))
      (node (ref U12) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref U7) (pin 8)))
    (net (code 79) (name /CPU/A0)
      (node (ref U12) (pin 19))
      (node (ref U5) (pin 10))
      (node (ref U6) (pin 10))
      (node (ref U2) (pin 19)))
    (net (code 80) (name /CPU/A1)
      (node (ref U12) (pin 20))
      (node (ref U5) (pin 9))
      (node (ref U2) (pin 18))
      (node (ref U6) (pin 9)))
    (net (code 81) (name /CPU/A2)
      (node (ref U6) (pin 8))
      (node (ref U2) (pin 17))
      (node (ref U5) (pin 8)))
    (net (code 82) (name /CPU/A3)
      (node (ref U2) (pin 16))
      (node (ref U5) (pin 7))
      (node (ref U6) (pin 7)))
    (net (code 83) (name /CPU/A4)
      (node (ref U2) (pin 15))
      (node (ref U6) (pin 6))
      (node (ref U5) (pin 6)))
    (net (code 84) (name /CPU/A5)
      (node (ref U2) (pin 14))
      (node (ref U5) (pin 5))
      (node (ref U6) (pin 5)))
    (net (code 85) (name /CPU/A6)
      (node (ref U5) (pin 4))
      (node (ref U2) (pin 13))
      (node (ref U6) (pin 4)))
    (net (code 86) (name /CPU/A7)
      (node (ref U5) (pin 3))
      (node (ref U2) (pin 12))
      (node (ref U6) (pin 3)))
    (net (code 87) (name /CPU/A8)
      (node (ref U7) (pin 28))
      (node (ref U5) (pin 25))
      (node (ref U1) (pin 21))
      (node (ref U6) (pin 25)))
    (net (code 88) (name /CPU/A9)
      (node (ref U1) (pin 22))
      (node (ref U6) (pin 24))
      (node (ref U7) (pin 27))
      (node (ref U5) (pin 24)))
    (net (code 89) (name /CPU/A10)
      (node (ref U1) (pin 23))
      (node (ref U5) (pin 21))
      (node (ref U7) (pin 26))
      (node (ref U6) (pin 21)))
    (net (code 90) (name /CPU/A11)
      (node (ref U5) (pin 23))
      (node (ref U1) (pin 24))
      (node (ref U6) (pin 23)))
    (net (code 91) (name /CPU/A12)
      (node (ref U5) (pin 2))
      (node (ref U1) (pin 25))
      (node (ref U6) (pin 2)))
    (net (code 92) (name /CPU/A15)
      (node (ref U9) (pin 3))
      (node (ref U1) (pin 28))
      (node (ref U4) (pin 5)))
    (net (code 93) (name /IODECODE/IOPAGE0)
      (node (ref U9) (pin 15)))
    (net (code 94) (name /IODECODE/IOPAGE1)
      (node (ref U9) (pin 14)))
    (net (code 95) (name /IODECODE/IOPAGE2)
      (node (ref U9) (pin 13))
      (node (ref U12) (pin 21)))
    (net (code 96) (name /IODECODE/IOPAGE3)
      (node (ref U7) (pin 14))
      (node (ref U9) (pin 12)))
    (net (code 97) (name /IODECODE/IOPAGE4)
      (node (ref U9) (pin 11)))
    (net (code 98) (name /IODECODE/IOPAGE5)
      (node (ref U9) (pin 10)))
    (net (code 99) (name /IODECODE/IOPAGE6)
      (node (ref U9) (pin 9)))
    (net (code 100) (name /IODECODE/IOPAGE7)
      (node (ref U9) (pin 7)))
    (net (code 101) (name /CPU/A13)
      (node (ref U5) (pin 26))
      (node (ref U1) (pin 26))
      (node (ref U9) (pin 1))
      (node (ref U6) (pin 26)))
    (net (code 102) (name /CPU/A14)
      (node (ref U1) (pin 27))
      (node (ref U5) (pin 27))
      (node (ref U6) (pin 1))
      (node (ref U9) (pin 2)))))