(module FTDI_USB (layer F.Cu) (tedit 5EFE3726)
  (descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
  (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
  (fp_text reference REF** (at 7.62 -7.41) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FTDI_USB (at 7.62 25.19) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.255 -6.35) (end 14.985 -6.35) (layer F.Fab) (width 0.1))
  (fp_line (start 14.985 -6.35) (end 14.985 24.13) (layer F.Fab) (width 0.1))
  (fp_line (start 14.985 24.13) (end 0.255 24.13) (layer F.Fab) (width 0.1))
  (fp_line (start 0.255 24.13) (end 0.255 -5.35) (layer F.Fab) (width 0.1))
  (fp_line (start 0.255 -5.35) (end 1.255 -6.35) (layer F.Fab) (width 0.1))
  (fp_line (start 6.62 -2.54) (end 1.16 -2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 -2.54) (end 1.16 24.19) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 24.19) (end 14.08 24.19) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.08 24.19) (end 14.08 -2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.08 -2.54) (end 6.599673 -2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.05 -6.63) (end -1.05 24.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.05 24.42) (end 16.3 24.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.3 24.42) (end 16.3 -6.63) (layer F.CrtYd) (width 0.05))
  (fp_line (start 16.3 -6.63) (end -1.05 -6.63) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 7.62 8.89) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.54 -2.5) (end 2.54 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.54 0) (end 12.7 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.7 0) (end 12.7 -2.5) (layer F.SilkS) (width 0.15))
  (fp_text user USB-B (at 7.75 -1.27) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 16 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 17 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 18 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 19 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 20 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x10_P2.54mm_Vertical.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x10_P2.54mm_Vertical.step
    (offset (xyz 15.24 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
