(footprint "PinHeader_2x03_P2.54mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
  (tags "Through hole pin header THT 2x03 2.54mm double row")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.27 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a1695a9b-d568-49c9-8e32-8f28b43497e3)
  )
  (fp_text value "PinHeader_2x03_P2.54mm_Vertical" (at 1.27 7.41) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 50c05935-62f0-415f-b4e5-9839168ee0d5)
  )
  (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ee98a671-d44c-4e42-bda7-9e61f94d9023)
  )
  (fp_line (start -1.33 -1.33) (end 0 -1.33)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b48285e1-a572-4277-85a1-a6c981cc5890))
  (fp_line (start -1.33 0) (end -1.33 -1.33)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d4246d55-8f68-46f9-b4dd-468f193c22f6))
  (fp_line (start -1.33 1.27) (end -1.33 6.41)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c55bd168-f478-48ca-b3c9-78f7df3b5a6a))
  (fp_line (start -1.33 1.27) (end 1.27 1.27)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c92a235a-6bb1-4090-af85-4878e34d1be0))
  (fp_line (start -1.33 6.41) (end 3.87 6.41)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f6c5cfa-9127-4a4b-9b4b-087a1ba657a4))
  (fp_line (start 1.27 -1.33) (end 3.87 -1.33)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ededb76f-1372-4d7a-b645-c62729570c64))
  (fp_line (start 1.27 1.27) (end 1.27 -1.33)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2a95782f-e382-4add-9bbd-20377a25b1c8))
  (fp_line (start 3.87 -1.33) (end 3.87 6.41)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9bfa780e-e318-43ed-870f-c3247f648c88))
  (fp_line (start -1.8 -1.8) (end -1.8 6.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a95dcb6b-8075-4faa-a98c-325e64c19156))
  (fp_line (start -1.8 6.85) (end 4.35 6.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 70c56f76-cc32-492b-acc1-0738f839bfbd))
  (fp_line (start 4.35 -1.8) (end -1.8 -1.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 78c82f62-0b24-4de4-92cc-2a6156b32119))
  (fp_line (start 4.35 6.85) (end 4.35 -1.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25f85b4b-7735-4801-90f4-eabe278f3087))
  (fp_line (start -1.27 0) (end 0 -1.27)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 812dcc5e-c22c-4acc-af59-6389e38cda86))
  (fp_line (start -1.27 6.35) (end -1.27 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25db3647-3dd6-49c9-8607-401cb6c98869))
  (fp_line (start 0 -1.27) (end 3.81 -1.27)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 758bd54f-220d-4384-a20f-a60777dc3fac))
  (fp_line (start 3.81 -1.27) (end 3.81 6.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6081530c-21a7-45a9-8e28-f1ba9678ba42))
  (fp_line (start 3.81 6.35) (end -1.27 6.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5596ee42-9552-4205-9f4c-72d523195be5))
  (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp ff8720a8-c701-43b7-bc7a-6a6c11d04791))
  (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 93705e7d-73dc-4f61-b875-d8fcdde8067f))
  (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 213e6c43-7a98-43d7-9b82-159f877d37de))
  (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 901745ea-2db8-46b8-a47a-dfbf66358efa))
  (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 023497c7-041e-403d-8f7d-9c2e6e22dee8))
  (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 40df788e-cbea-4ad2-95b7-f0e2511469bb))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
