(footprint "C_Disc_D4.7mm_W2.5mm_P5.00mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
  (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.54 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8a29945a-0ecf-4424-acad-d9ded6a0319e)
  )
  (fp_text value "C_Disc_D4.7mm_W2.5mm_P5.00mm" (at 2.5 2.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a9d8cea7-a648-41ee-8f65-bfbfbe8f7077)
  )
  (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab")
      (effects (font (size 0.94 0.94) (thickness 0.141)))
    (tstamp 427f4e8a-0b74-4b05-a672-121a918859df)
  )
  (fp_line (start 0.0192 -1.1176) (end 0.0192 -0.8534)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1eae0855-ff8a-4712-b823-026e72751a30))
  (fp_line (start 0.0192 -1.1176) (end 4.9592 -1.1176)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 172480d1-f398-43bd-b1ad-07c6fd97c654))
  (fp_line (start 0.0192 0.8636) (end 0.0192 1.0668)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee09ef97-27db-4401-b809-5f5fddb1ed37))
  (fp_line (start 0.0192 1.0668) (end 4.9592 1.0668)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1c539be-8299-4855-bb87-38f278aaba19))
  (fp_line (start 4.9592 -1.1176) (end 4.9592 -0.8534)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8084a5a4-27c4-4a29-bf35-74c62fadac09))
  (fp_line (start 4.9592 0.8636) (end 4.9592 1.0668)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 771305bb-b508-4469-b96b-7eec5b29c37f))
  (fp_line (start -1.016 1.27) (end 6.084 1.27)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d094f600-f11b-40ce-b8c4-6c1d458a96fa))
  (fp_line (start -1.01 -1.27) (end -1.016 1.27)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 78156a4d-f5d4-47b5-b36a-8ab6ea758a77))
  (fp_line (start 6.084 1.27) (end 6.09 -1.27)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b90afc6a-30ae-412a-ba93-8ade9ecf22aa))
  (fp_line (start 6.09 -1.27) (end -1.01 -1.27)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8402880d-6357-4db0-a235-b0365be0b29f))
  (fp_line (start 0.15 -1.25) (end 0.15 1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60db0a73-6809-476c-8516-dfd00030d546))
  (fp_line (start 0.15 1.25) (end 4.85 1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ddfe6022-2267-4e28-a133-f1fd9c1e5c69))
  (fp_line (start 4.85 -1.25) (end 0.15 -1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c04fe8c-9fa3-49fa-990a-05182da485aa))
  (fp_line (start 4.85 1.25) (end 4.85 -1.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6a91993f-bbcf-4018-9675-32544b488640))
  (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 5d2bb97b-b758-4ce7-bee7-ebf810b54e09))
  (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 2aadeb9c-1e02-4a23-80c4-e9019bc2fbe9))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
