(footprint "C_Disc_D4.3mm_W1.9mm_P5.00mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
  (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.5 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 772ad199-eaf7-43d2-be37-101e3f089218)
  )
  (fp_text value "C_Disc_D4.3mm_W1.9mm_P5.00mm" (at 2.5 2.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 463ddb8d-057b-43cb-a463-85ed1f7b9308)
  )
  (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab")
      (effects (font (size 0.86 0.86) (thickness 0.129)))
    (tstamp 9503949c-6e8f-4b72-8a46-0bb1a8454a3d)
  )
  (fp_line (start 0.23 -0.889) (end 4.77 -0.889)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f38acfd0-cac6-4038-af8f-82437f80f5df))
  (fp_line (start 0.23 0.889) (end 4.77 0.889)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fcafc8f1-57ab-4aa3-9a2c-6925ac517247))
  (fp_line (start -1.05 -1.016) (end -1.05 1.016)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 95527da1-d464-4794-a41e-3f3ba72615c7))
  (fp_line (start -1.05 1.016) (end 6.05 1.016)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b783fddc-fa0e-46e9-921f-2a23d8b0240f))
  (fp_line (start 6.05 -1.016) (end -1.05 -1.016)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d396cd51-484c-4b17-b377-12e34757230a))
  (fp_line (start 6.05 1.016) (end 6.05 -1.016)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 54207d36-6efb-4d4d-a170-ee47b9422392))
  (fp_line (start 0.35 -0.95) (end 0.35 0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9511cd86-8b89-4b90-ac7e-5c988249c3af))
  (fp_line (start 0.35 0.95) (end 4.65 0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 856c959d-fba7-4c17-aadf-37c1239f9f96))
  (fp_line (start 4.65 -0.95) (end 0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49b289b1-ab03-4066-90b2-ff10ef8925e5))
  (fp_line (start 4.65 0.95) (end 4.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cb82620d-e0f6-46a3-89ad-7d001610c21e))
  (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp f42f4e37-8cbe-415b-b097-df6334f704cf))
  (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 78d1b917-2809-4f68-9eb6-3382d6479211))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
