(footprint "R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
  (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
  (attr through_hole)
  (fp_text reference "REF**" (at -2.54 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a38aa6bc-0182-43b0-8b35-d3128fd7d52c)
  )
  (fp_text value "R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (at 1.27 2.37) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d72c1421-dc4e-4cbc-90e5-fd2d2d598d9a)
  )
  (fp_text user "${REFERENCE}" (at -2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3244add2-5f11-4c54-9579-ab6914378ed5)
  )
  (fp_line (start 1.37 0) (end 1.44 0)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cf8bf4f7-7a4e-4f25-ba41-ffe3a544759b))
  (fp_circle (center 0 0) (end 1.37 0)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 971bd421-3717-4ae5-ac2e-9a9c19b7f8d8))
  (fp_line (start -1.5 -1.5) (end -1.5 1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c0b88ba4-f3ab-4a2a-ab07-ea4a0048b2f1))
  (fp_line (start -1.5 1.5) (end 3.59 1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dd2a38fc-7f8b-48a8-9e0e-297d8f8854d7))
  (fp_line (start 3.59 -1.5) (end -1.5 -1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3bdb4fdb-59fb-414d-8358-e5cbe163141c))
  (fp_line (start 3.59 1.5) (end 3.59 -1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 326efe26-7628-4c17-9770-a88c05aeaafc))
  (fp_line (start 0 0) (end 2.54 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 842cceaf-9bec-4425-890a-d7c155934e32))
  (fp_circle (center 0 0) (end 1.25 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp f583ab9d-a863-446f-802e-42b20515718f))
  (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp f5c30ff6-6d97-4771-b17a-6c348e357e77))
  (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 1492ab9d-d659-4b94-a384-54aea0a6da57))
  (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
