## AY-3-8910 Dual Audio Card

Provides 6 channels of audio output. Similar chips can be substituted.

* [AY-3-8910 Datasheet](http://map.grauw.nl/resources/sound/generalinstrument_ay-3-8910.pdf)

## GAL (Optional)

There are two options for glue circuitry in this schematic. Option 1 utilizes a GAL16V8D

The code for the GAL is available in this directory.

* [ay38910control.pld](ay38910control.pld) - source definition file
* [ay38910control.jed](ay38910control.jed) - compiled definition file

Compiled using [WinCupl](https://www.microchip.com/en-us/development-tool/WinCUPL)
