(module WSL_6W_HALF (layer F.Cu) (tedit 59CA799D)
  (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
  (tags "Through hole angled pin header THT 2x03 2.54mm double row")
  (fp_text reference J? (at 1.2 -2 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "" (at 4.6 3.6 90) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 5.585 -2.27) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
    (at (xyz 0.05 -0.1 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
