(module C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 59E3C5DC)
  (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
  (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
  (fp_text reference C6 (at -1.524 0 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value 100nF (at 2.5 2.31) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.8 0) (end 4 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 -0.6) (end 2.8 0.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.4 -0.6) (end 2.4 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.4 0.6) (end 2.4 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0) (end 2.4 0) (layer F.SilkS) (width 0.15))
  (fp_text user %R (at 2.5 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -1.25) (end 0 1.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0 1.25) (end 5 1.25) (layer F.Fab) (width 0.1))
  (fp_line (start 5 1.25) (end 5 -1.25) (layer F.Fab) (width 0.1))
  (fp_line (start 5 -1.25) (end 0 -1.25) (layer F.Fab) (width 0.1))
  (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at 0 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
