(module jyd:SPC-FD05-3.5mm-stereo-phone-jack (layer F.Cu)
  (descr "multicomp SPC24110 Farnell 2112339")
  (fp_text reference NAME (at 0 -8) (layer F.SilkS)
    (effects (font (size 0.625 0.625) (thickness 0.1)))
  )
  (fp_text value "" (at 0 0) (layer F.SilkS)
    (effects (font (thickness 0.15)))
  )
  (fp_line (start -5.2 4.5) (end -4.2 4.5) (layer Dwgs.User) (width 0.1))
  (fp_line (start -4.2 4.5) (end -4.2 -4.5) (layer Dwgs.User) (width 0.1))
  (fp_line (start -4.2 -4.5) (end -5.2 -4.5) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.2 -4.5) (end -5.2 4.5) (layer Dwgs.User) (width 0.1))
  (fp_line (start -7 3.6) (end -5.2 3.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.2 3.6) (end -5.2 -3.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start -5.2 -3.6) (end -7 -3.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start -7 -3.6) (end -7 3.6) (layer Dwgs.User) (width 0.1))
  (fp_line (start -4.2 -6) (end -4.2 6) (layer F.SilkS) (width 0.1))
  (fp_line (start -4.2 6) (end 7 6) (layer F.SilkS) (width 0.1))
  (fp_line (start 7 6) (end 7 -6) (layer F.SilkS) (width 0.1))
  (fp_line (start 7 -6) (end -4.2 -6) (layer F.SilkS) (width 0.1))
  (fp_line (start -4.2 -6) (end -4.2 6) (layer F.SilkS) (width 0.1))
  (fp_text user GND (at -1.5 -2.3) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user R (at 2.5 -5) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (fp_text user L (at 2.5 5) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (pad 1 thru_hole circle (at -0.5 0) (size 2.1 2.1) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole circle (at 4.5 -2.5) (size 2.1 2.1) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at 4.5 2.5 180) (size 2.1 2.1) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 4.5 -5) (size 2.1 2.1) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 4.5 5 180) (size 2.1 2.1) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad d1 thru_hole circle (at -3 -5) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
  (pad d2 thru_hole circle (at -3 5 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
  (pad d3 thru_hole circle (at -0.5 -5) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
  (pad d4 thru_hole circle (at -0.5 5 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
  (pad d5 thru_hole circle (at 4.5 0) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
)
