(module jyd:0603_S_R (layer F.Cu)
  (descr "Generic 0603 footprint made slightly smaller for more densely populated boards used for resistor and capacitor")
  (fp_text reference R3 (at 0 -1.4) (layer F.SilkS)
    (effects (font (size 0.625 0.625) (thickness 0.1)))
  )
  (fp_text value 10k (at 0 1.4) (layer F.SilkS) hide
    (effects (font (size 0.625 0.625) (thickness 0.1)))
  )
  (fp_line (start -0.35 -0.45) (end 0.35 -0.45) (layer Dwgs.User) (width 0.1))
  (fp_line (start -0.35 0.45) (end 0.35 0.45) (layer Dwgs.User) (width 0.1))
  (fp_poly (pts (xy -0.85 -0.5) (xy -0.85 0.5) (xy -0.35 0.5) (xy -0.35 -0.5)
    (xy -0.85 -0.5)) (layer Dwgs.User) (width 0.15))
  (fp_poly (pts (xy 0.35 -0.5) (xy 0.35 0.5) (xy 0.85 0.5) (xy 0.85 -0.5)
    (xy 0.35 -0.5)) (layer Dwgs.User) (width 0.15))
  (fp_line (start -1.45 0.7) (end 1.45 0.7) (layer F.SilkS) (width 0.1))
  (fp_line (start 1.45 0.7) (end 1.45 -0.7) (layer F.SilkS) (width 0.1))
  (fp_line (start 1.45 -0.7) (end -1.45 -0.7) (layer F.SilkS) (width 0.1))
  (fp_line (start -1.45 -0.7) (end -1.45 0.7) (layer F.SilkS) (width 0.1))
  (pad 1 smd rect (at -0.85 0) (size 0.7 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.85 0) (size 0.7 1) (layers F.Cu F.Paste F.Mask))
  (model smd/resistors/R0603.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
