# Static Call Graph for image .\Project.axf

#<CALLGRAPH># ARM Linker, 5060020: Last Updated: Mon Feb 13 21:13:00 2017

### Maximum Stack Usage = 1184 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ Main_Menu ⇒ SerialDownload ⇒ Ymodem_Receive ⇒ Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit_ExtMemCtl from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 1184 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ Main_Menu ⇒ SerialDownload ⇒ Ymodem_Receive ⇒ Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  __get_PSP (Thumb, 6 bytes, Stack size 0 bytes, core_cm3.o(.emb_text), UNUSED)

  __set_PSP (Thumb, 6 bytes, Stack size 0 bytes, core_cm3.o(.emb_text), UNUSED)

  __get_MSP (Thumb, 6 bytes, Stack size 0 bytes, core_cm3.o(.emb_text), UNUSED)

  __set_MSP (Thumb, 6 bytes, Stack size 0 bytes, core_cm3.o(.emb_text))
  [Called By]

  - >> Main_Menu

  __REV16 (Thumb, 4 bytes, Stack size 0 bytes, core_cm3.o(.emb_text), UNUSED)

  __REVSH (Thumb, 4 bytes, Stack size 0 bytes, core_cm3.o(.emb_text), UNUSED)

  SystemInit_ExtMemCtl (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  Reset_Handler (Thumb, 14 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_memcpy (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text))
  [Called By]

  - >> Ymodem_Receive

  __rt_memcpy (Thumb, 138 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  _memcpy_lastbytes (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_v6.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memcpy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 0 bytes, indicate_semi.o(.text), UNUSED)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_DisableWriteProtectionPages (Thumb, 178 bytes, Stack size 32 bytes, common.o(i.FLASH_DisableWriteProtectionPages))
  [Stack]

  - Max Depth = 88
  - Call Chain = FLASH_DisableWriteProtectionPages ⇒ FLASH_EnableWriteProtection ⇒ FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> WWDG_Enable
  - >> RCC_APB1PeriphClockCmd
  - >> FLASH_UserOptionByteConfig
  - >> FLASH_GetWriteProtectionOptionByte
  - >> FLASH_GetUserOptionByte
  - >> FLASH_EraseOptionBytes
  - >> FLASH_EnableWriteProtection
  - >> Serial_PutString
  [Called By]
  - >> Main_Menu

  FLASH_EnableWriteProtection (Thumb, 180 bytes, Stack size 32 bytes, stm32f10x_flash.o(i.FLASH_EnableWriteProtection))
  [Stack]

  - Max Depth = 56
  - Call Chain = FLASH_EnableWriteProtection ⇒ FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_DisableWriteProtectionPages

  FLASH_EraseOptionBytes (Thumb, 142 bytes, Stack size 8 bytes, stm32f10x_flash.o(i.FLASH_EraseOptionBytes))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLASH_EraseOptionBytes ⇒ FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_DisableWriteProtectionPages

  FLASH_ErasePage (Thumb, 76 bytes, Stack size 16 bytes, stm32f10x_flash.o(i.FLASH_ErasePage))
  [Stack]

  - Max Depth = 40
  - Call Chain = FLASH_ErasePage ⇒ FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> Ymodem_Receive

  FLASH_GetStatus (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_GetStatus))
  [Called By]

  - >> FLASH_WaitForLastOperation

  FLASH_GetUserOptionByte (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_GetUserOptionByte))
  [Called By]

  - >> FLASH_DisableWriteProtectionPages

  FLASH_GetWriteProtectionOptionByte (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_GetWriteProtectionOptionByte))
  [Called By]

  - >> Main_Menu
  - >> FLASH_DisableWriteProtectionPages

  FLASH_PagesMask (Thumb, 24 bytes, Stack size 8 bytes, common.o(i.FLASH_PagesMask))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLASH_PagesMask
  [Called By]
  - >> Ymodem_Receive

  FLASH_ProgramWord (Thumb, 110 bytes, Stack size 24 bytes, stm32f10x_flash.o(i.FLASH_ProgramWord))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLASH_ProgramWord ⇒ FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> Ymodem_Receive

  FLASH_Unlock (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_Unlock))
  [Called By]

  - >> main

  FLASH_UserOptionByteConfig (Thumb, 90 bytes, Stack size 24 bytes, stm32f10x_flash.o(i.FLASH_UserOptionByteConfig))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLASH_UserOptionByteConfig ⇒ FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_DisableWriteProtectionPages

  FLASH_WaitForLastOperation (Thumb, 42 bytes, Stack size 16 bytes, stm32f10x_flash.o(i.FLASH_WaitForLastOperation))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLASH_WaitForLastOperation ⇒ delay
  [Calls]
  - >> FLASH_GetStatus
  - >> delay
  [Called By]
  - >> FLASH_ProgramWord
  - >> FLASH_ErasePage
  - >> FLASH_UserOptionByteConfig
  - >> FLASH_EraseOptionBytes
  - >> FLASH_EnableWriteProtection

  GPIO_Configuration (Thumb, 60 bytes, Stack size 8 bytes, main.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> IAP_Init

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> GPIO_Configuration

  GetKey (Thumb, 28 bytes, Stack size 8 bytes, common.o(i.GetKey))
  [Stack]

  - Max Depth = 16
  - Call Chain = GetKey ⇒ SerialKeyPressed
  [Calls]
  - >> SerialKeyPressed
  [Called By]
  - >> Main_Menu

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  Int2Str (Thumb, 84 bytes, Stack size 20 bytes, common.o(i.Int2Str))
  [Stack]

  - Max Depth = 20
  - Call Chain = Int2Str
  [Called By]
  - >> SerialDownload

  Main_Menu (Thumb, 230 bytes, Stack size 0 bytes, common.o(i.Main_Menu))
  [Stack]

  - Max Depth = 1184
  - Call Chain = Main_Menu ⇒ SerialDownload ⇒ Ymodem_Receive ⇒ Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> SerialDownload
  - >> FLASH_GetWriteProtectionOptionByte
  - >> Serial_PutString
  - >> GetKey
  - >> FLASH_DisableWriteProtectionPages
  - >> __set_MSP
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> FLASH_DisableWriteProtectionPages

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_Configuration (Thumb, 14 bytes, Stack size 8 bytes, main.o(i.RCC_Configuration))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_Configuration
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> IAP_Init

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SerialDownload (Thumb, 120 bytes, Stack size 24 bytes, download.o(i.SerialDownload))
  [Stack]

  - Max Depth = 1184
  - Call Chain = SerialDownload ⇒ Ymodem_Receive ⇒ Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> Ymodem_Receive
  - >> Serial_PutString
  - >> Int2Str
  [Called By]
  - >> Main_Menu

  SerialKeyPressed (Thumb, 30 bytes, Stack size 8 bytes, common.o(i.SerialKeyPressed))
  [Stack]

  - Max Depth = 8
  - Call Chain = SerialKeyPressed
  [Calls]
  - >> USART_GetFlagStatus
  [Called By]
  - >> Receive_Byte
  - >> GetKey

  SerialPutChar (Thumb, 28 bytes, Stack size 8 bytes, common.o(i.SerialPutChar))
  [Stack]

  - Max Depth = 8
  - Call Chain = SerialPutChar
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> Send_Byte
  - >> Serial_PutString

  Serial_PutString (Thumb, 22 bytes, Stack size 8 bytes, common.o(i.Serial_PutString))
  [Stack]

  - Max Depth = 16
  - Call Chain = Serial_PutString ⇒ SerialPutChar
  [Calls]
  - >> SerialPutChar
  [Called By]
  - >> main
  - >> SerialDownload
  - >> Main_Menu
  - >> FLASH_DisableWriteProtectionPages

  Str2Int (Thumb, 260 bytes, Stack size 16 bytes, common.o(i.Str2Int))
  [Stack]

  - Max Depth = 16
  - Call Chain = Str2Int
  [Called By]
  - >> Ymodem_Receive

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 70 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> USART_Config

  USART_Config (Thumb, 66 bytes, Stack size 8 bytes, main.o(i.USART_Config))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Config ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  [Called By]
  - >> IAP_Init

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> SerialPutChar
  - >> SerialKeyPressed

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> USART_Config

  USART_Init (Thumb, 156 bytes, Stack size 56 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART_Config

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> SerialPutChar

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_Enable (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_wwdg.o(i.WWDG_Enable))
  [Called By]

  - >> FLASH_DisableWriteProtectionPages

  Ymodem_Receive (Thumb, 570 bytes, Stack size 1104 bytes, ymodem.o(i.Ymodem_Receive))
  [Stack]

  - Max Depth = 1160
  - Call Chain = Ymodem_Receive ⇒ Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> FLASH_ProgramWord
  - >> FLASH_ErasePage
  - >> Send_Byte
  - >> Receive_Packet
  - >> Str2Int
  - >> FLASH_PagesMask
  - >> __aeabi_memcpy
  [Called By]
  - >> SerialDownload

  main (Thumb, 68 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 1184
  - Call Chain = main ⇒ Main_Menu ⇒ SerialDownload ⇒ Ymodem_Receive ⇒ Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> FLASH_Unlock
  - >> IAP_Init
  - >> Serial_PutString
  - >> Main_Menu
  - >> SystemInit
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 220 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  IAP_Init (Thumb, 18 bytes, Stack size 8 bytes, main.o(i.IAP_Init))
  [Stack]

  - Max Depth = 84
  - Call Chain = IAP_Init ⇒ USART_Config ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Config
  - >> RCC_Configuration
  - >> GPIO_Configuration
  [Called By]
  - >> main

  Receive_Byte (Thumb, 34 bytes, Stack size 16 bytes, ymodem.o(i.Receive_Byte))
  [Stack]

  - Max Depth = 24
  - Call Chain = Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> SerialKeyPressed
  [Called By]
  - >> Receive_Packet

  Receive_Packet (Thumb, 188 bytes, Stack size 32 bytes, ymodem.o(i.Receive_Packet))
  [Stack]

  - Max Depth = 56
  - Call Chain = Receive_Packet ⇒ Receive_Byte ⇒ SerialKeyPressed
  [Calls]
  - >> Receive_Byte
  [Called By]
  - >> Ymodem_Receive

  Send_Byte (Thumb, 14 bytes, Stack size 8 bytes, ymodem.o(i.Send_Byte))
  [Stack]

  - Max Depth = 16
  - Call Chain = Send_Byte ⇒ SerialPutChar
  [Calls]
  - >> SerialPutChar
  [Called By]
  - >> Ymodem_Receive

  delay (Thumb, 26 bytes, Stack size 8 bytes, stm32f10x_flash.o(i.delay))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay
  [Called By]
  - >> FLASH_WaitForLastOperation

  ### Undefined Global Symbols