# Static Call Graph for image .\OBJ\obj.axf

#<CALLGRAPH># ARM Linker, 5060300: Last Updated: Tue Mar 07 23:02:03 2017

### Maximum Stack Usage = 140 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ eMBInit ⇒ eMBRTUInit ⇒ xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from porttimer.o(i.TIM4_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from portserial.o(i.USART2_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - eMBASCIIReceive from mbascii.o(i.eMBASCIIReceive) referenced from mb.o(i.eMBInit)
  - eMBASCIISend from mbascii.o(i.eMBASCIISend) referenced from mb.o(i.eMBInit)
  - eMBASCIIStart from mbascii.o(i.eMBASCIIStart) referenced from mb.o(i.eMBInit)
  - eMBASCIIStop from mbascii.o(i.eMBASCIIStop) referenced from mb.o(i.eMBInit)
  - eMBFuncReadCoils from mbfunccoils.o(i.eMBFuncReadCoils) referenced from mb.o(.data)
  - eMBFuncReadDiscreteInputs from mbfuncdisc.o(i.eMBFuncReadDiscreteInputs) referenced from mb.o(.data)
  - eMBFuncReadHoldingRegister from mbfuncholding.o(i.eMBFuncReadHoldingRegister) referenced from mb.o(.data)
  - eMBFuncReadInputRegister from mbfuncinput.o(i.eMBFuncReadInputRegister) referenced from mb.o(.data)
  - eMBFuncReadWriteMultipleHoldingRegister from mbfuncholding.o(i.eMBFuncReadWriteMultipleHoldingRegister) referenced from mb.o(.data)
  - eMBFuncReportSlaveID from mbfuncother.o(i.eMBFuncReportSlaveID) referenced from mb.o(.data)
  - eMBFuncWriteCoil from mbfunccoils.o(i.eMBFuncWriteCoil) referenced from mb.o(.data)
  - eMBFuncWriteHoldingRegister from mbfuncholding.o(i.eMBFuncWriteHoldingRegister) referenced from mb.o(.data)
  - eMBFuncWriteMultipleCoils from mbfunccoils.o(i.eMBFuncWriteMultipleCoils) referenced from mb.o(.data)
  - eMBFuncWriteMultipleHoldingRegister from mbfuncholding.o(i.eMBFuncWriteMultipleHoldingRegister) referenced from mb.o(.data)
  - eMBRTUReceive from mbrtu.o(i.eMBRTUReceive) referenced from mb.o(i.eMBInit)
  - eMBRTUSend from mbrtu.o(i.eMBRTUSend) referenced from mb.o(i.eMBInit)
  - eMBRTUStart from mbrtu.o(i.eMBRTUStart) referenced from mb.o(i.eMBInit)
  - eMBRTUStop from mbrtu.o(i.eMBRTUStop) referenced from mb.o(i.eMBInit)
  - xMBASCIIReceiveFSM from mbascii.o(i.xMBASCIIReceiveFSM) referenced from mb.o(i.eMBInit)
  - xMBASCIITimerT1SExpired from mbascii.o(i.xMBASCIITimerT1SExpired) referenced from mb.o(i.eMBInit)
  - xMBASCIITransmitFSM from mbascii.o(i.xMBASCIITransmitFSM) referenced from mb.o(i.eMBInit)
  - xMBRTUReceiveFSM from mbrtu.o(i.xMBRTUReceiveFSM) referenced from mb.o(i.eMBInit)
  - xMBRTUTimerT35Expired from mbrtu.o(i.xMBRTUTimerT35Expired) referenced from mb.o(i.eMBInit)
  - xMBRTUTransmitFSM from mbrtu.o(i.xMBRTUTransmitFSM) referenced from mb.o(i.eMBInit)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls
  - >> abort

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 140 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ eMBInit ⇒ eMBRTUInit ⇒ xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  abort (Thumb, 22 bytes, Stack size 8 bytes, abort.o(.text))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> __rt_lib_shutdown
  - >> __rt_SIGABRT
  - >> _sys_exit
  [Called By]
  - >> xMBUtilSetBits
  - >> prvucMBBIN2CHAR
  - >> xMBRTUTransmitFSM
  - >> xMBRTUTimerT35Expired
  - >> xMBRTUReceiveFSM
  - >> xMBASCIITransmitFSM
  - >> xMBASCIITimerT1SExpired
  - >> xMBASCIIReceiveFSM
  - >> eMBRTUReceive
  - >> eMBASCIIReceive

  __aeabi_memcpy (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text))
  [Called By]

  - >> eMBFuncReportSlaveID

  __rt_memcpy (Thumb, 138 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  _memcpy_lastbytes (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_v6.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit
  - >> __sig_exit
  - >> abort

  __rt_SIGABRT (Thumb, 14 bytes, Stack size 8 bytes, defsig_abrt_outer.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> __rt_SIGABRT_inner
  - >> __sig_exit
  [Called By]
  - >> abort

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memcpy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 0 bytes, indicate_semi.o(.text), UNUSED)

  __sig_exit (Thumb, 10 bytes, Stack size 0 bytes, defsig_exit.o(.text))
  [Calls]

  - >> _sys_exit
  [Called By]
  - >> __rt_SIGABRT

  __rt_SIGABRT_inner (Thumb, 14 bytes, Stack size 8 bytes, defsig_abrt_inner.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> __default_signal_display
  [Called By]
  - >> __rt_SIGABRT

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __default_signal_display (Thumb, 50 bytes, Stack size 16 bytes, defsig_general.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> _ttywrch
  [Called By]
  - >> __rt_SIGABRT_inner

  _ttywrch (Thumb, 14 bytes, Stack size 8 bytes, sys_wrch.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _ttywrch
  [Called By]
  - >> __default_signal_display

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  Button_Poll (Thumb, 38 bytes, Stack size 16 bytes, main.o(i.Button_Poll))
  [Stack]

  - Max Depth = 16
  - Call Chain = Button_Poll
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> main

  GPIO_Init (Thumb, 162 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> LedInit
  - >> KeyInit
  - >> xMBPortSerialInit

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> Button_Poll

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> LED_Poll

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> LedInit
  - >> LED_Poll

  KeyInit (Thumb, 32 bytes, Stack size 8 bytes, key.o(i.KeyInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = KeyInit ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  LED_Poll (Thumb, 74 bytes, Stack size 16 bytes, main.o(i.LED_Poll))
  [Stack]

  - Max Depth = 16
  - Call Chain = LED_Poll
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> main

  LedInit (Thumb, 80 bytes, Stack size 16 bytes, led.o(i.LedInit))
  [Stack]

  - Max Depth = 36
  - Call Chain = LedInit ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> GPIO_SetBits
  [Called By]
  - >> main

  NVIC_Init (Thumb, 94 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> xMBPortTimersInit
  - >> xMBPortSerialInit

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> xMBPortTimersInit
  - >> xMBPortSerialInit

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> xMBPortTimersInit
  - >> xMBPortSerialInit

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> LedInit
  - >> KeyInit
  - >> xMBPortSerialInit

  RCC_GetClocksFreq (Thumb, 128 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  SystemInit (Thumb, 64 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  TIM4_IRQHandler (Thumb, 36 bytes, Stack size 8 bytes, porttimer.o(i.TIM4_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM4_IRQHandler
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM_ARRPreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ARRPreloadConfig))
  [Called By]

  - >> xMBPortTimersInit

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ClearITPendingBit))
  [Called By]

  - >> TIM4_IRQHandler
  - >> xMBPortTimersInit
  - >> vMBPortTimersEnable
  - >> vMBPortTimersDisable

  TIM_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_Cmd))
  [Called By]

  - >> xMBPortTimersInit
  - >> vMBPortTimersEnable
  - >> vMBPortTimersDisable

  TIM_GetITStatus (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_GetITStatus))
  [Called By]

  - >> TIM4_IRQHandler

  TIM_ITConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ITConfig))
  [Called By]

  - >> xMBPortTimersInit
  - >> vMBPortTimersEnable
  - >> vMBPortTimersDisable

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_SetCounter))
  [Called By]

  - >> vMBPortTimersEnable
  - >> vMBPortTimersDisable

  TIM_TimeBaseInit (Thumb, 114 bytes, Stack size 12 bytes, stm32f10x_tim.o(i.TIM_TimeBaseInit))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TimeBaseInit
  [Called By]
  - >> xMBPortTimersInit

  USART2_IRQHandler (Thumb, 70 bytes, Stack size 16 bytes, portserial.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 28
  - Call Chain = USART2_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_GetITStatus
  - >> USART_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART_ClearITPendingBit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ClearITPendingBit))
  [Called By]

  - >> USART2_IRQHandler

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> xMBPortSerialInit

  USART_GetITStatus (Thumb, 62 bytes, Stack size 12 bytes, stm32f10x_usart.o(i.USART_GetITStatus))
  [Stack]

  - Max Depth = 12
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART2_IRQHandler

  USART_ITConfig (Thumb, 48 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ITConfig
  [Called By]
  - >> vMBPortSerialEnable

  USART_Init (Thumb, 166 bytes, Stack size 32 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 44
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> xMBPortSerialInit

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> xMBPortSerialGetByte

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> xMBPortSerialPutByte

  eMBASCIIInit (Thumb, 44 bytes, Stack size 16 bytes, mbascii.o(i.eMBASCIIInit))
  [Stack]

  - Max Depth = 108
  - Call Chain = eMBASCIIInit ⇒ xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> xMBPortTimersInit
  - >> xMBPortSerialInit
  [Called By]
  - >> eMBInit

  eMBASCIIReceive (Thumb, 68 bytes, Stack size 24 bytes, mbascii.o(i.eMBASCIIReceive))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = eMBASCIIReceive ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> prvucMBLRC
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBASCIISend (Thumb, 68 bytes, Stack size 16 bytes, mbascii.o(i.eMBASCIISend))
  [Stack]

  - Max Depth = 40
  - Call Chain = eMBASCIISend ⇒ vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> vMBPortSerialEnable
  - >> prvucMBLRC
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBASCIIStart (Thumb, 24 bytes, Stack size 8 bytes, mbascii.o(i.eMBASCIIStart))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBASCIIStart ⇒ vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> vMBPortSerialEnable
  - >> xMBPortEventPost
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBASCIIStop (Thumb, 18 bytes, Stack size 8 bytes, mbascii.o(i.eMBASCIIStop))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBASCIIStop ⇒ vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> vMBPortTimersDisable
  - >> vMBPortSerialEnable
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBEnable (Thumb, 28 bytes, Stack size 16 bytes, mb.o(i.eMBEnable))
  [Stack]

  - Max Depth = 16
  - Call Chain = eMBEnable
  [Called By]
  - >> main

  eMBFuncReadCoils (Thumb, 110 bytes, Stack size 16 bytes, mbfunccoils.o(i.eMBFuncReadCoils))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = eMBFuncReadCoils ⇒ eMBRegCoilsCB ⇒ xMBUtilSetBits ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> eMBRegCoilsCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncReadDiscreteInputs (Thumb, 110 bytes, Stack size 16 bytes, mbfuncdisc.o(i.eMBFuncReadDiscreteInputs))
  [Stack]

  - Max Depth = 48
  - Call Chain = eMBFuncReadDiscreteInputs ⇒ eMBRegDiscreteCB ⇒ xMBUtilGetBits
  [Calls]
  - >> eMBRegDiscreteCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncReadHoldingRegister (Thumb, 90 bytes, Stack size 16 bytes, mbfuncholding.o(i.eMBFuncReadHoldingRegister))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBFuncReadHoldingRegister ⇒ eMBRegHoldingCB
  [Calls]
  - >> eMBRegHoldingCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncReadInputRegister (Thumb, 94 bytes, Stack size 16 bytes, mbfuncinput.o(i.eMBFuncReadInputRegister))
  [Stack]

  - Max Depth = 28
  - Call Chain = eMBFuncReadInputRegister ⇒ eMBRegInputCB
  [Calls]
  - >> eMBRegInputCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncReadWriteMultipleHoldingRegister (Thumb, 156 bytes, Stack size 24 bytes, mbfuncholding.o(i.eMBFuncReadWriteMultipleHoldingRegister))
  [Stack]

  - Max Depth = 40
  - Call Chain = eMBFuncReadWriteMultipleHoldingRegister ⇒ eMBRegHoldingCB
  [Calls]
  - >> eMBRegHoldingCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncReportSlaveID (Thumb, 26 bytes, Stack size 16 bytes, mbfuncother.o(i.eMBFuncReportSlaveID))
  [Stack]

  - Max Depth = 16
  - Call Chain = eMBFuncReportSlaveID
  [Calls]
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncWriteCoil (Thumb, 82 bytes, Stack size 16 bytes, mbfunccoils.o(i.eMBFuncWriteCoil))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = eMBFuncWriteCoil ⇒ eMBRegCoilsCB ⇒ xMBUtilSetBits ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> eMBRegCoilsCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncWriteHoldingRegister (Thumb, 46 bytes, Stack size 8 bytes, mbfuncholding.o(i.eMBFuncWriteHoldingRegister))
  [Stack]

  - Max Depth = 24
  - Call Chain = eMBFuncWriteHoldingRegister ⇒ eMBRegHoldingCB
  [Calls]
  - >> eMBRegHoldingCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncWriteMultipleCoils (Thumb, 94 bytes, Stack size 24 bytes, mbfunccoils.o(i.eMBFuncWriteMultipleCoils))
  [Stack]

  - Max Depth = 112 + Unknown Stack Size
  - Call Chain = eMBFuncWriteMultipleCoils ⇒ eMBRegCoilsCB ⇒ xMBUtilSetBits ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> eMBRegCoilsCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBFuncWriteMultipleHoldingRegister (Thumb, 74 bytes, Stack size 16 bytes, mbfuncholding.o(i.eMBFuncWriteMultipleHoldingRegister))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBFuncWriteMultipleHoldingRegister ⇒ eMBRegHoldingCB
  [Calls]
  - >> eMBRegHoldingCB
  - >> prveMBError2Exception
  [Address Reference Count : 1]
  - mb.o(.data)

  eMBInit (Thumb, 140 bytes, Stack size 24 bytes, mb.o(i.eMBInit))
  [Stack]

  - Max Depth = 132
  - Call Chain = eMBInit ⇒ eMBRTUInit ⇒ xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> xMBPortEventInit
  - >> eMBRTUInit
  - >> eMBASCIIInit
  [Called By]
  - >> main

  eMBPoll (Thumb, 176 bytes, Stack size 16 bytes, mb.o(i.eMBPoll))
  [Stack]

  - Max Depth = 16
  - Call Chain = eMBPoll
  [Calls]
  - >> xMBPortEventPost
  - >> xMBPortEventGet
  [Called By]
  - >> main

  eMBRTUInit (Thumb, 54 bytes, Stack size 16 bytes, mbrtu.o(i.eMBRTUInit))
  [Stack]

  - Max Depth = 108
  - Call Chain = eMBRTUInit ⇒ xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> xMBPortTimersInit
  - >> xMBPortSerialInit
  [Called By]
  - >> eMBInit

  eMBRTUReceive (Thumb, 70 bytes, Stack size 24 bytes, mbrtu.o(i.eMBRTUReceive))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = eMBRTUReceive ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> usMBCRC16
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBRTUSend (Thumb, 100 bytes, Stack size 16 bytes, mbrtu.o(i.eMBRTUSend))
  [Stack]

  - Max Depth = 40
  - Call Chain = eMBRTUSend ⇒ vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> usMBCRC16
  - >> xMBPortSerialPutByte
  - >> vMBPortSerialEnable
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBRTUStart (Thumb, 24 bytes, Stack size 8 bytes, mbrtu.o(i.eMBRTUStart))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBRTUStart ⇒ vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> vMBPortTimersEnable
  - >> vMBPortSerialEnable
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBRTUStop (Thumb, 18 bytes, Stack size 8 bytes, mbrtu.o(i.eMBRTUStop))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBRTUStop ⇒ vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> vMBPortTimersDisable
  - >> vMBPortSerialEnable
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  eMBRegCoilsCB (Thumb, 110 bytes, Stack size 24 bytes, main.o(i.eMBRegCoilsCB))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = eMBRegCoilsCB ⇒ xMBUtilSetBits ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> xMBUtilSetBits
  - >> xMBUtilGetBits
  [Called By]
  - >> eMBFuncWriteMultipleCoils
  - >> eMBFuncWriteCoil
  - >> eMBFuncReadCoils

  eMBRegDiscreteCB (Thumb, 72 bytes, Stack size 24 bytes, main.o(i.eMBRegDiscreteCB))
  [Stack]

  - Max Depth = 32
  - Call Chain = eMBRegDiscreteCB ⇒ xMBUtilGetBits
  [Calls]
  - >> xMBUtilGetBits
  [Called By]
  - >> eMBFuncReadDiscreteInputs

  eMBRegHoldingCB (Thumb, 108 bytes, Stack size 16 bytes, main.o(i.eMBRegHoldingCB))
  [Stack]

  - Max Depth = 16
  - Call Chain = eMBRegHoldingCB
  [Called By]
  - >> eMBFuncWriteMultipleHoldingRegister
  - >> eMBFuncWriteHoldingRegister
  - >> eMBFuncReadWriteMultipleHoldingRegister
  - >> eMBFuncReadHoldingRegister

  eMBRegInputCB (Thumb, 70 bytes, Stack size 12 bytes, main.o(i.eMBRegInputCB))
  [Stack]

  - Max Depth = 12
  - Call Chain = eMBRegInputCB
  [Called By]
  - >> eMBFuncReadInputRegister

  main (Thumb, 46 bytes, Stack size 8 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 140
  - Call Chain = main ⇒ eMBInit ⇒ eMBRTUInit ⇒ xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> eMBPoll
  - >> eMBInit
  - >> eMBEnable
  - >> LedInit
  - >> KeyInit
  - >> LED_Poll
  - >> Button_Poll
  [Called By]
  - >> __rt_entry_main

  prveMBError2Exception (Thumb, 24 bytes, Stack size 0 bytes, mbutils.o(i.prveMBError2Exception))
  [Called By]

  - >> eMBFuncWriteMultipleHoldingRegister
  - >> eMBFuncWriteMultipleCoils
  - >> eMBFuncWriteHoldingRegister
  - >> eMBFuncWriteCoil
  - >> eMBFuncReadWriteMultipleHoldingRegister
  - >> eMBFuncReadInputRegister
  - >> eMBFuncReadHoldingRegister
  - >> eMBFuncReadDiscreteInputs
  - >> eMBFuncReadCoils

  usMBCRC16 (Thumb, 40 bytes, Stack size 16 bytes, mbcrc.o(i.usMBCRC16))
  [Stack]

  - Max Depth = 16
  - Call Chain = usMBCRC16
  [Called By]
  - >> eMBRTUSend
  - >> eMBRTUReceive

  vMBPortSerialEnable (Thumb, 66 bytes, Stack size 16 bytes, portserial.o(i.vMBPortSerialEnable))
  [Stack]

  - Max Depth = 24
  - Call Chain = vMBPortSerialEnable ⇒ USART_ITConfig
  [Calls]
  - >> USART_ITConfig
  [Called By]
  - >> xMBRTUTransmitFSM
  - >> xMBASCIITransmitFSM
  - >> eMBRTUStop
  - >> eMBRTUStart
  - >> eMBRTUSend
  - >> eMBASCIIStop
  - >> eMBASCIIStart
  - >> eMBASCIISend

  vMBPortTimersDisable (Thumb, 42 bytes, Stack size 8 bytes, porttimer.o(i.vMBPortTimersDisable))
  [Stack]

  - Max Depth = 8
  - Call Chain = vMBPortTimersDisable
  [Calls]
  - >> TIM_SetCounter
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_ClearITPendingBit
  [Called By]
  - >> xMBRTUTimerT35Expired
  - >> xMBASCIITimerT1SExpired
  - >> xMBASCIIReceiveFSM
  - >> eMBRTUStop
  - >> eMBASCIIStop

  vMBPortTimersEnable (Thumb, 42 bytes, Stack size 8 bytes, porttimer.o(i.vMBPortTimersEnable))
  [Stack]

  - Max Depth = 8
  - Call Chain = vMBPortTimersEnable
  [Calls]
  - >> TIM_SetCounter
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_ClearITPendingBit
  [Called By]
  - >> xMBRTUReceiveFSM
  - >> xMBASCIIReceiveFSM
  - >> eMBRTUStart

  xMBASCIIReceiveFSM (Thumb, 222 bytes, Stack size 24 bytes, mbascii.o(i.xMBASCIIReceiveFSM))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = xMBASCIIReceiveFSM ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> xMBPortSerialGetByte
  - >> vMBPortTimersEnable
  - >> vMBPortTimersDisable
  - >> xMBPortEventPost
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  xMBASCIITimerT1SExpired (Thumb, 42 bytes, Stack size 8 bytes, mbascii.o(i.xMBASCIITimerT1SExpired))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = xMBASCIITimerT1SExpired ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> vMBPortTimersDisable
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  xMBASCIITransmitFSM (Thumb, 168 bytes, Stack size 16 bytes, mbascii.o(i.xMBASCIITransmitFSM))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = xMBASCIITransmitFSM ⇒ prvucMBBIN2CHAR ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> xMBPortSerialPutByte
  - >> vMBPortSerialEnable
  - >> prvucMBBIN2CHAR
  - >> xMBPortEventPost
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  xMBPortEventGet (Thumb, 24 bytes, Stack size 0 bytes, portevent.o(i.xMBPortEventGet))
  [Called By]

  - >> eMBPoll

  xMBPortEventInit (Thumb, 10 bytes, Stack size 0 bytes, portevent.o(i.xMBPortEventInit))
  [Called By]

  - >> eMBInit

  xMBPortEventPost (Thumb, 12 bytes, Stack size 0 bytes, portevent.o(i.xMBPortEventPost))
  [Called By]

  - >> eMBPoll
  - >> xMBRTUTransmitFSM
  - >> xMBRTUTimerT35Expired
  - >> xMBASCIITransmitFSM
  - >> xMBASCIIReceiveFSM
  - >> eMBASCIIStart

  xMBPortSerialGetByte (Thumb, 16 bytes, Stack size 8 bytes, portserial.o(i.xMBPortSerialGetByte))
  [Stack]

  - Max Depth = 8
  - Call Chain = xMBPortSerialGetByte
  [Calls]
  - >> USART_ReceiveData
  [Called By]
  - >> xMBRTUReceiveFSM
  - >> xMBASCIIReceiveFSM

  xMBPortSerialInit (Thumb, 188 bytes, Stack size 48 bytes, portserial.o(i.xMBPortSerialInit))
  [Stack]

  - Max Depth = 92
  - Call Chain = xMBPortSerialInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> USART_Init
  - >> USART_Cmd
  [Called By]
  - >> eMBRTUInit
  - >> eMBASCIIInit

  xMBPortSerialPutByte (Thumb, 14 bytes, Stack size 8 bytes, portserial.o(i.xMBPortSerialPutByte))
  [Stack]

  - Max Depth = 8
  - Call Chain = xMBPortSerialPutByte
  [Calls]
  - >> USART_SendData
  [Called By]
  - >> xMBRTUTransmitFSM
  - >> xMBASCIITransmitFSM
  - >> eMBRTUSend

  xMBPortTimersInit (Thumb, 130 bytes, Stack size 32 bytes, porttimer.o(i.xMBPortTimersInit))
  [Stack]

  - Max Depth = 48
  - Call Chain = xMBPortTimersInit ⇒ NVIC_Init
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> RCC_APB1PeriphClockCmd
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_ClearITPendingBit
  - >> TIM_ARRPreloadConfig
  [Called By]
  - >> eMBRTUInit
  - >> eMBASCIIInit

  xMBRTUReceiveFSM (Thumb, 96 bytes, Stack size 16 bytes, mbrtu.o(i.xMBRTUReceiveFSM))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = xMBRTUReceiveFSM ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> xMBPortSerialGetByte
  - >> vMBPortTimersEnable
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  xMBRTUTimerT35Expired (Thumb, 58 bytes, Stack size 16 bytes, mbrtu.o(i.xMBRTUTimerT35Expired))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = xMBRTUTimerT35Expired ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> vMBPortTimersDisable
  - >> xMBPortEventPost
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  xMBRTUTransmitFSM (Thumb, 86 bytes, Stack size 16 bytes, mbrtu.o(i.xMBRTUTransmitFSM))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = xMBRTUTransmitFSM ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  - >> xMBPortSerialPutByte
  - >> vMBPortSerialEnable
  - >> xMBPortEventPost
  [Address Reference Count : 1]
  - mb.o(i.eMBInit)

  xMBUtilGetBits (Thumb, 34 bytes, Stack size 8 bytes, mbutils.o(i.xMBUtilGetBits))
  [Stack]

  - Max Depth = 8
  - Call Chain = xMBUtilGetBits
  [Called By]
  - >> eMBRegDiscreteCB
  - >> eMBRegCoilsCB

  xMBUtilSetBits (Thumb, 50 bytes, Stack size 16 bytes, mbutils.o(i.xMBUtilSetBits))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = xMBUtilSetBits ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  [Called By]
  - >> eMBRegCoilsCB

  ### Local Symbols

  SetSysClockTo72 (Thumb, 160 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SystemInit

  prvucMBBIN2CHAR (Thumb, 28 bytes, Stack size 8 bytes, mbascii.o(i.prvucMBBIN2CHAR))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = prvucMBBIN2CHAR ⇒ abort ⇒ __rt_SIGABRT ⇒ __rt_SIGABRT_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> abort
  [Called By]
  - >> xMBASCIITransmitFSM

  prvucMBLRC (Thumb, 24 bytes, Stack size 0 bytes, mbascii.o(i.prvucMBLRC))
  [Called By]

  - >> eMBASCIISend
  - >> eMBASCIIReceive

  ### Undefined Global Symbols