;#<FEEDBACK># ARM Linker, 5060300: Last Updated: Tue Mar 07 23:01:51 2017
;VERSION 0.2
;FILE core_cm3.o
__REV16 <= USED 0
__REVSH <= USED 0
__get_MSP <= USED 0
__get_PSP <= USED 0
__set_MSP <= USED 0
__set_PSP <= USED 0
;FILE key.o
;FILE led.o
LedTest <= USED 0
delay <= USED 0
;FILE main.o
;FILE mb.o
eMBClose <= USED 0
eMBDisable <= USED 0
eMBRegisterCB <= USED 0
;FILE mbascii.o
;FILE mbcrc.o
;FILE mbfunccoils.o
;FILE mbfuncdisc.o
;FILE mbfuncholding.o
;FILE mbfuncinput.o
;FILE mbfuncother.o
eMBSetSlaveID <= USED 0
;FILE mbrtu.o
;FILE mbutils.o
;FILE misc.o
NVIC_SetVectorTable <= USED 0
NVIC_SystemLPConfig <= USED 0
SysTick_CLKSourceConfig <= USED 0
;FILE portevent.o
;FILE portserial.o
;FILE porttimer.o
;FILE startup_stm32f10x_hd.o
;FILE stm32f10x_adc.o
ADC_AnalogWatchdogCmd <= USED 0
ADC_AnalogWatchdogSingleChannelConfig <= USED 0
ADC_AnalogWatchdogThresholdsConfig <= USED 0
ADC_AutoInjectedConvCmd <= USED 0
ADC_ClearFlag <= USED 0
ADC_ClearITPendingBit <= USED 0
ADC_Cmd <= USED 0
ADC_DMACmd <= USED 0
ADC_DeInit <= USED 0
ADC_DiscModeChannelCountConfig <= USED 0
ADC_DiscModeCmd <= USED 0
ADC_ExternalTrigConvCmd <= USED 0
ADC_ExternalTrigInjectedConvCmd <= USED 0
ADC_ExternalTrigInjectedConvConfig <= USED 0
ADC_GetCalibrationStatus <= USED 0
ADC_GetConversionValue <= USED 0
ADC_GetDualModeConversionValue <= USED 0
ADC_GetFlagStatus <= USED 0
ADC_GetITStatus <= USED 0
ADC_GetInjectedConversionValue <= USED 0
ADC_GetResetCalibrationStatus <= USED 0
ADC_GetSoftwareStartConvStatus <= USED 0
ADC_GetSoftwareStartInjectedConvCmdStatus <= USED 0
ADC_ITConfig <= USED 0
ADC_Init <= USED 0
ADC_InjectedChannelConfig <= USED 0
ADC_InjectedDiscModeCmd <= USED 0
ADC_InjectedSequencerLengthConfig <= USED 0
ADC_RegularChannelConfig <= USED 0
ADC_ResetCalibration <= USED 0
ADC_SetInjectedOffset <= USED 0
ADC_SoftwareStartConvCmd <= USED 0
ADC_SoftwareStartInjectedConvCmd <= USED 0
ADC_StartCalibration <= USED 0
ADC_StructInit <= USED 0
ADC_TempSensorVrefintCmd <= USED 0
;FILE stm32f10x_bkp.o
BKP_ClearFlag <= USED 0
BKP_ClearITPendingBit <= USED 0
BKP_DeInit <= USED 0
BKP_GetFlagStatus <= USED 0
BKP_GetITStatus <= USED 0
BKP_ITConfig <= USED 0
BKP_RTCOutputConfig <= USED 0
BKP_ReadBackupRegister <= USED 0
BKP_SetRTCCalibrationValue <= USED 0
BKP_TamperPinCmd <= USED 0
BKP_TamperPinLevelConfig <= USED 0
BKP_WriteBackupRegister <= USED 0
;FILE stm32f10x_can.o
CAN_CancelTransmit <= USED 0
CAN_ClearFlag <= USED 0
CAN_ClearITPendingBit <= USED 0
CAN_DBGFreeze <= USED 0
CAN_DeInit <= USED 0
CAN_FIFORelease <= USED 0
CAN_FilterInit <= USED 0
CAN_GetFlagStatus <= USED 0
CAN_GetITStatus <= USED 0
CAN_GetLSBTransmitErrorCounter <= USED 0
CAN_GetLastErrorCode <= USED 0
CAN_GetReceiveErrorCounter <= USED 0
CAN_ITConfig <= USED 0
CAN_Init <= USED 0
CAN_MessagePending <= USED 0
CAN_OperatingModeRequest <= USED 0
CAN_Receive <= USED 0
CAN_SlaveStartBank <= USED 0
CAN_Sleep <= USED 0
CAN_StructInit <= USED 0
CAN_TTComModeCmd <= USED 0
CAN_Transmit <= USED 0
CAN_TransmitStatus <= USED 0
CAN_WakeUp <= USED 0
;FILE stm32f10x_cec.o
CEC_ClearFlag <= USED 0
CEC_ClearITPendingBit <= USED 0
CEC_Cmd <= USED 0
CEC_DeInit <= USED 0
CEC_EndOfMessageCmd <= USED 0
CEC_GetFlagStatus <= USED 0
CEC_GetITStatus <= USED 0
CEC_ITConfig <= USED 0
CEC_Init <= USED 0
CEC_OwnAddressConfig <= USED 0
CEC_ReceiveDataByte <= USED 0
CEC_SendDataByte <= USED 0
CEC_SetPrescaler <= USED 0
CEC_StartOfMessage <= USED 0
;FILE stm32f10x_crc.o
CRC_CalcBlockCRC <= USED 0
CRC_CalcCRC <= USED 0
CRC_GetCRC <= USED 0
CRC_GetIDRegister <= USED 0
CRC_ResetDR <= USED 0
CRC_SetIDRegister <= USED 0
;FILE stm32f10x_dac.o
DAC_Cmd <= USED 0
DAC_DMACmd <= USED 0
DAC_DeInit <= USED 0
DAC_DualSoftwareTriggerCmd <= USED 0
DAC_GetDataOutputValue <= USED 0
DAC_Init <= USED 0
DAC_SetChannel1Data <= USED 0
DAC_SetChannel2Data <= USED 0
DAC_SetDualChannelData <= USED 0
DAC_SoftwareTriggerCmd <= USED 0
DAC_StructInit <= USED 0
DAC_WaveGenerationCmd <= USED 0
;FILE stm32f10x_dbgmcu.o
DBGMCU_Config <= USED 0
DBGMCU_GetDEVID <= USED 0
DBGMCU_GetREVID <= USED 0
;FILE stm32f10x_dma.o
DMA_ClearFlag <= USED 0
DMA_ClearITPendingBit <= USED 0
DMA_Cmd <= USED 0
DMA_DeInit <= USED 0
DMA_GetCurrDataCounter <= USED 0
DMA_GetFlagStatus <= USED 0
DMA_GetITStatus <= USED 0
DMA_ITConfig <= USED 0
DMA_Init <= USED 0
DMA_SetCurrDataCounter <= USED 0
DMA_StructInit <= USED 0
;FILE stm32f10x_exti.o
EXTI_ClearFlag <= USED 0
EXTI_ClearITPendingBit <= USED 0
EXTI_DeInit <= USED 0
EXTI_GenerateSWInterrupt <= USED 0
EXTI_GetFlagStatus <= USED 0
EXTI_GetITStatus <= USED 0
EXTI_Init <= USED 0
EXTI_StructInit <= USED 0
;FILE stm32f10x_flash.o
FLASH_ClearFlag <= USED 0
FLASH_EnableWriteProtection <= USED 0
FLASH_EraseAllBank1Pages <= USED 0
FLASH_EraseAllPages <= USED 0
FLASH_EraseOptionBytes <= USED 0
FLASH_ErasePage <= USED 0
FLASH_GetBank1Status <= USED 0
FLASH_GetFlagStatus <= USED 0
FLASH_GetPrefetchBufferStatus <= USED 0
FLASH_GetReadOutProtectionStatus <= USED 0
FLASH_GetStatus <= USED 0
FLASH_GetUserOptionByte <= USED 0
FLASH_GetWriteProtectionOptionByte <= USED 0
FLASH_HalfCycleAccessCmd <= USED 0
FLASH_ITConfig <= USED 0
FLASH_Lock <= USED 0
FLASH_LockBank1 <= USED 0
FLASH_PrefetchBufferCmd <= USED 0
FLASH_ProgramHalfWord <= USED 0
FLASH_ProgramOptionByteData <= USED 0
FLASH_ProgramWord <= USED 0
FLASH_ReadOutProtection <= USED 0
FLASH_SetLatency <= USED 0
FLASH_Unlock <= USED 0
FLASH_UnlockBank1 <= USED 0
FLASH_UserOptionByteConfig <= USED 0
FLASH_WaitForLastBank1Operation <= USED 0
FLASH_WaitForLastOperation <= USED 0
;FILE stm32f10x_fsmc.o
FSMC_ClearFlag <= USED 0
FSMC_ClearITPendingBit <= USED 0
FSMC_GetECC <= USED 0
FSMC_GetFlagStatus <= USED 0
FSMC_GetITStatus <= USED 0
FSMC_ITConfig <= USED 0
FSMC_NANDCmd <= USED 0
FSMC_NANDDeInit <= USED 0
FSMC_NANDECCCmd <= USED 0
FSMC_NANDInit <= USED 0
FSMC_NANDStructInit <= USED 0
FSMC_NORSRAMCmd <= USED 0
FSMC_NORSRAMDeInit <= USED 0
FSMC_NORSRAMInit <= USED 0
FSMC_NORSRAMStructInit <= USED 0
FSMC_PCCARDCmd <= USED 0
FSMC_PCCARDDeInit <= USED 0
FSMC_PCCARDInit <= USED 0
FSMC_PCCARDStructInit <= USED 0
;FILE stm32f10x_gpio.o
GPIO_AFIODeInit <= USED 0
GPIO_DeInit <= USED 0
GPIO_ETH_MediaInterfaceConfig <= USED 0
GPIO_EXTILineConfig <= USED 0
GPIO_EventOutputCmd <= USED 0
GPIO_EventOutputConfig <= USED 0
GPIO_PinLockConfig <= USED 0
GPIO_PinRemapConfig <= USED 0
GPIO_ReadInputData <= USED 0
GPIO_ReadOutputData <= USED 0
GPIO_ReadOutputDataBit <= USED 0
GPIO_StructInit <= USED 0
GPIO_Write <= USED 0
GPIO_WriteBit <= USED 0
;FILE stm32f10x_i2c.o
I2C_ARPCmd <= USED 0
I2C_AcknowledgeConfig <= USED 0
I2C_CalculatePEC <= USED 0
I2C_CheckEvent <= USED 0
I2C_ClearFlag <= USED 0
I2C_ClearITPendingBit <= USED 0
I2C_Cmd <= USED 0
I2C_DMACmd <= USED 0
I2C_DMALastTransferCmd <= USED 0
I2C_DeInit <= USED 0
I2C_DualAddressCmd <= USED 0
I2C_FastModeDutyCycleConfig <= USED 0
I2C_GeneralCallCmd <= USED 0
I2C_GenerateSTART <= USED 0
I2C_GenerateSTOP <= USED 0
I2C_GetFlagStatus <= USED 0
I2C_GetITStatus <= USED 0
I2C_GetLastEvent <= USED 0
I2C_GetPEC <= USED 0
I2C_ITConfig <= USED 0
I2C_Init <= USED 0
I2C_NACKPositionConfig <= USED 0
I2C_OwnAddress2Config <= USED 0
I2C_PECPositionConfig <= USED 0
I2C_ReadRegister <= USED 0
I2C_ReceiveData <= USED 0
I2C_SMBusAlertConfig <= USED 0
I2C_Send7bitAddress <= USED 0
I2C_SendData <= USED 0
I2C_SoftwareResetCmd <= USED 0
I2C_StretchClockCmd <= USED 0
I2C_StructInit <= USED 0
I2C_TransmitPEC <= USED 0
;FILE stm32f10x_iwdg.o
IWDG_Enable <= USED 0
IWDG_GetFlagStatus <= USED 0
IWDG_ReloadCounter <= USED 0
IWDG_SetPrescaler <= USED 0
IWDG_SetReload <= USED 0
IWDG_WriteAccessCmd <= USED 0
;FILE stm32f10x_pwr.o
PWR_BackupAccessCmd <= USED 0
PWR_ClearFlag <= USED 0
PWR_DeInit <= USED 0
PWR_EnterSTANDBYMode <= USED 0
PWR_EnterSTOPMode <= USED 0
PWR_GetFlagStatus <= USED 0
PWR_PVDCmd <= USED 0
PWR_PVDLevelConfig <= USED 0
PWR_WakeUpPinCmd <= USED 0
;FILE stm32f10x_rcc.o
RCC_ADCCLKConfig <= USED 0
RCC_AHBPeriphClockCmd <= USED 0
RCC_APB1PeriphResetCmd <= USED 0
RCC_APB2PeriphResetCmd <= USED 0
RCC_AdjustHSICalibrationValue <= USED 0
RCC_BackupResetCmd <= USED 0
RCC_ClearFlag <= USED 0
RCC_ClearITPendingBit <= USED 0
RCC_ClockSecuritySystemCmd <= USED 0
RCC_DeInit <= USED 0
RCC_GetFlagStatus <= USED 0
RCC_GetITStatus <= USED 0
RCC_GetSYSCLKSource <= USED 0
RCC_HCLKConfig <= USED 0
RCC_HSEConfig <= USED 0
RCC_HSICmd <= USED 0
RCC_ITConfig <= USED 0
RCC_LSEConfig <= USED 0
RCC_LSICmd <= USED 0
RCC_MCOConfig <= USED 0
RCC_PCLK1Config <= USED 0
RCC_PCLK2Config <= USED 0
RCC_PLLCmd <= USED 0
RCC_PLLConfig <= USED 0
RCC_RTCCLKCmd <= USED 0
RCC_RTCCLKConfig <= USED 0
RCC_SYSCLKConfig <= USED 0
RCC_USBCLKConfig <= USED 0
RCC_WaitForHSEStartUp <= USED 0
;FILE stm32f10x_rtc.o
RTC_ClearFlag <= USED 0
RTC_ClearITPendingBit <= USED 0
RTC_EnterConfigMode <= USED 0
RTC_ExitConfigMode <= USED 0
RTC_GetCounter <= USED 0
RTC_GetDivider <= USED 0
RTC_GetFlagStatus <= USED 0
RTC_GetITStatus <= USED 0
RTC_ITConfig <= USED 0
RTC_SetAlarm <= USED 0
RTC_SetCounter <= USED 0
RTC_SetPrescaler <= USED 0
RTC_WaitForLastTask <= USED 0
RTC_WaitForSynchro <= USED 0
;FILE stm32f10x_sdio.o
SDIO_CEATAITCmd <= USED 0
SDIO_ClearFlag <= USED 0
SDIO_ClearITPendingBit <= USED 0
SDIO_ClockCmd <= USED 0
SDIO_CmdStructInit <= USED 0
SDIO_CommandCompletionCmd <= USED 0
SDIO_DMACmd <= USED 0
SDIO_DataConfig <= USED 0
SDIO_DataStructInit <= USED 0
SDIO_DeInit <= USED 0
SDIO_GetCommandResponse <= USED 0
SDIO_GetDataCounter <= USED 0
SDIO_GetFIFOCount <= USED 0
SDIO_GetFlagStatus <= USED 0
SDIO_GetITStatus <= USED 0
SDIO_GetPowerState <= USED 0
SDIO_GetResponse <= USED 0
SDIO_ITConfig <= USED 0
SDIO_Init <= USED 0
SDIO_ReadData <= USED 0
SDIO_SendCEATACmd <= USED 0
SDIO_SendCommand <= USED 0
SDIO_SendSDIOSuspendCmd <= USED 0
SDIO_SetPowerState <= USED 0
SDIO_SetSDIOOperation <= USED 0
SDIO_SetSDIOReadWaitMode <= USED 0
SDIO_StartSDIOReadWait <= USED 0
SDIO_StopSDIOReadWait <= USED 0
SDIO_StructInit <= USED 0
SDIO_WriteData <= USED 0
;FILE stm32f10x_spi.o
I2S_Cmd <= USED 0
I2S_Init <= USED 0
I2S_StructInit <= USED 0
SPI_BiDirectionalLineConfig <= USED 0
SPI_CalculateCRC <= USED 0
SPI_Cmd <= USED 0
SPI_DataSizeConfig <= USED 0
SPI_GetCRC <= USED 0
SPI_GetCRCPolynomial <= USED 0
SPI_I2S_ClearFlag <= USED 0
SPI_I2S_ClearITPendingBit <= USED 0
SPI_I2S_DMACmd <= USED 0
SPI_I2S_DeInit <= USED 0
SPI_I2S_GetFlagStatus <= USED 0
SPI_I2S_GetITStatus <= USED 0
SPI_I2S_ITConfig <= USED 0
SPI_I2S_ReceiveData <= USED 0
SPI_I2S_SendData <= USED 0
SPI_Init <= USED 0
SPI_NSSInternalSoftwareConfig <= USED 0
SPI_SSOutputCmd <= USED 0
SPI_StructInit <= USED 0
SPI_TransmitCRC <= USED 0
;FILE stm32f10x_tim.o
TIM_BDTRConfig <= USED 0
TIM_BDTRStructInit <= USED 0
TIM_CCPreloadControl <= USED 0
TIM_CCxCmd <= USED 0
TIM_CCxNCmd <= USED 0
TIM_ClearFlag <= USED 0
TIM_ClearOC1Ref <= USED 0
TIM_ClearOC2Ref <= USED 0
TIM_ClearOC3Ref <= USED 0
TIM_ClearOC4Ref <= USED 0
TIM_CounterModeConfig <= USED 0
TIM_CtrlPWMOutputs <= USED 0
TIM_DMACmd <= USED 0
TIM_DMAConfig <= USED 0
TIM_DeInit <= USED 0
TIM_ETRClockMode1Config <= USED 0
TIM_ETRClockMode2Config <= USED 0
TIM_ETRConfig <= USED 0
TIM_EncoderInterfaceConfig <= USED 0
TIM_ForcedOC1Config <= USED 0
TIM_ForcedOC2Config <= USED 0
TIM_ForcedOC3Config <= USED 0
TIM_ForcedOC4Config <= USED 0
TIM_GenerateEvent <= USED 0
TIM_GetCapture1 <= USED 0
TIM_GetCapture2 <= USED 0
TIM_GetCapture3 <= USED 0
TIM_GetCapture4 <= USED 0
TIM_GetCounter <= USED 0
TIM_GetFlagStatus <= USED 0
TIM_GetPrescaler <= USED 0
TIM_ICInit <= USED 0
TIM_ICStructInit <= USED 0
TIM_ITRxExternalClockConfig <= USED 0
TIM_InternalClockConfig <= USED 0
TIM_OC1FastConfig <= USED 0
TIM_OC1Init <= USED 0
TIM_OC1NPolarityConfig <= USED 0
TIM_OC1PolarityConfig <= USED 0
TIM_OC1PreloadConfig <= USED 0
TIM_OC2FastConfig <= USED 0
TIM_OC2Init <= USED 0
TIM_OC2NPolarityConfig <= USED 0
TIM_OC2PolarityConfig <= USED 0
TIM_OC2PreloadConfig <= USED 0
TIM_OC3FastConfig <= USED 0
TIM_OC3Init <= USED 0
TIM_OC3NPolarityConfig <= USED 0
TIM_OC3PolarityConfig <= USED 0
TIM_OC3PreloadConfig <= USED 0
TIM_OC4FastConfig <= USED 0
TIM_OC4Init <= USED 0
TIM_OC4PolarityConfig <= USED 0
TIM_OC4PreloadConfig <= USED 0
TIM_OCStructInit <= USED 0
TIM_PWMIConfig <= USED 0
TIM_PrescalerConfig <= USED 0
TIM_SelectCCDMA <= USED 0
TIM_SelectCOM <= USED 0
TIM_SelectHallSensor <= USED 0
TIM_SelectInputTrigger <= US