
 Start     Stop      Length    Name               Class

00000000h 000040DFh 000040E0h _TEXT               CODE
000040E0h 00005B1Bh 00001A3Ch _DATA               DATA
00005B1Ch 00015F1Bh 00010400h STACK               STACK
00015F1Ch 0003C613h 000266F8h _BSS                BSS

Program entry point at 0000006Ah 



      6A: _main            (example.asm)
     264: DebugRun            (debug.asm)
     264: debugrun            (debug.asm)
     264: _DebugRun            (debug.asm)
     264: _debugrun            (debug.asm)
     EAB: remove_BreakPoint            (debug.asm)
    19E7: copy_font_to_video            (debug.asm)
     1BC: _debug            (debug.asm)
     1BC: _Debug            (debug.asm)
   39F1C: registers_save            (debug.asm)
     A30: read_char            (debug.asm)
     E83: get_Jcc_condition            (debug.asm)
     264: _debug_run            (debug.asm)
     264: _Debug_Run            (debug.asm)
     264: debug_run            (debug.asm)
     264: Debug_Run            (debug.asm)
     1BC: debug            (debug.asm)
     1BC: Debug            (debug.asm)
    4130: MOD_RM_flag            (debug.asm)
   3C5F0: JMP_displacement            (decode.asm)
    5A15: ST0_symb            (decode.asm)
    5A65: ES_symb            (decode.asm)
    59F1: EAX_symb            (decode.asm)
   3C601: op_seg_overide            (decode.asm)
   3C600: MOD_RM_size            (decode.asm)
   3C5F8: MOD_RM_EffectiveAddress            (decode.asm)
    2FF0: Decode_instruction            (decode.asm)
    5A3F: ST7_symb            (decode.asm)
   3C5FC: MOD_RM_DefaultSegmentReg            (decode.asm)
    3DFC: print_decimal_80bit_unsigned_real_fixedpoint            (pfloat.asm)
    3CCB: print_float            (pfloat.asm)
