
How to decompess .IT samples:

Basic structure:

Offset  Length                  Meaning
0       2 (word)                <Compressed byte count>
2       <Compressed byte count> Compressed sample data

The size of the uncompressed data is 32kb or the remainder of the sample,
whichever is less.

Code to decompress sample data:

Each procedure is given DS:SI as the compressed buffer, ES:DI points to the
destination buffer for the sample. CX = <Decompressed byte count>

These routines haven't been optimised at all - they are the ones that have
been used in IT itself, so they should be sufficiently fast.

;ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

Proc            D_Decompress16BitData

                PushAD
                Mov     BP, CX
                Mov     CX, 1100h
                ShR     BP, 1
                Xor     DX, DX
                Xor     BX, BX

D_Decompress16BitData1:
                Push    CX

                Mov     EAX, [SI]
                Mov     CL, DL
                ShR     EAX, CL

                Add     DL, CH
                Mov     CX, DX
                ShR     CX, 3
                Add     SI, CX
                And     DL, 7

                Pop     CX

                Cmp     CH, 6
                JA      D_Decompress16BitA

                ShL     EAX, CL
                Cmp     AX, 8000h
                JE      D_Decompress16BitDepthChange1

D_Decompress16BitD:
                SAR     AX, CL

D_Decompress16BitC:
                Add     BX, AX
                Mov     [ES:DI], BX
                Add     DI, 2

                Dec     BP
                JNZ     D_Decompress16BitData1

                PopAD
                Ret

D_Decompress16BitDepthChange1:
                ShR     EAX, 16
                And     AL, 15

                Inc     AX

                Add     DL, 4

D_Decompress16BitDepthChange3:
                Cmp     AL, CH
                SBB     AL, 0FFh
                Mov     CL, 16
                Mov     CH, AL
                Sub     CL, AL
                AdC     CL, 0

                Jmp     D_Decompress16BitData1

D_Decompress16BitA:
                Cmp     CH, 16
                JA      D_Decompress16BitB

                Push    DX
                Mov     EDX, 10000h
                ShR     EDX, CL
                Dec     DX
                And     AX, DX
                ShR     DX, 1
                Add     DX, 8
                Cmp     AX, DX
                JA      D_Decompress16BitE
                Sub     DX, 16
                Cmp     AX, DX
                JBE     D_Decompress16BitE

                Sub     AX, DX
                Pop     DX
                Jmp     D_Decompress16BitDepthChange3

D_Decompress16BitE:
                Pop     DX
                ShL     AX, CL
                Jmp     D_Decompress16BitD

D_Decompress16BitB:
                Test    EAX, 10000h
                JZ      D_Decompress16BitC

                Mov     CL, 16
                Inc     AX

                Sub     CL, AL
                Mov     CH, AL

                Jmp     D_Decompress16BitData1

EndP            D_Decompress16BitData

;ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

Proc            D_Decompress8BitData

                PushA
                Mov     BP, CX

                Mov     BX, 900h
                Xor     CX, CX
                Xor     DX, DX

D_Decompress8BitData1:
                Push    CX
                Mov     AX, [SI]
                Mov     CL, CH

                ShR     AX, CL
                Pop     CX

                Add     CH, BH
                Mov     DL, CH
                And     CH, 7
                ShR     DL, 3
                Add     SI, DX

                Cmp     BH, 6
                JA      D_Decompress8BitA

                ShL     AX, CL

                Cmp     AL, 80h
                JE      D_Decompress8BitDepthChange1

D_Decompress8BitWriteData2:
                SAR     AL, CL

D_Decompress8BitWriteData:
                Add     BL, AL
                Mov     [ES:DI], BL

                Inc     DI
                Dec     BP

                JNZ     D_Decompress8BitData1
                PopA
                Ret

D_Decompress8BitDepthChange1:
                Mov     AL, AH
                Add     CH, 3

                And     AL, 7
                Mov     DL, CH

                And     CH, 7
                ShR     DL, 3

                Add     SI, DX
                Jmp     D_Decompress8BitD

D_Decompress8BitA:
                Cmp     BH, 8
                JA      D_Decompress8BitC
                JE      D_Decompress8BitB

                ShL     AL, 1
                Cmp     AL, 78h
                JB      D_Decompress8BitWriteData2
                Cmp     AL, 86h
                JA      D_Decompress8BitWriteData2

                ShR     AL, 1
                Sub     AL, 3Ch
                Jmp     D_Decompress8BitD

D_Decompress8BitB:
                Cmp     AL, 7Ch
                JB      D_Decompress8BitWriteData
                Cmp     AL, 83h
                JA      D_Decompress8BitWriteData

                Sub     AL, 7Ch

D_Decompress8BitD:
                Mov     CL, 8
                Inc     AX

                Cmp     AL, BH
                SBB     AL, 0FFh
                Mov     BH, AL
                Sub     CL, AL
                AdC     CL, 0

                Jmp     D_Decompress8BitData1

D_Decompress8BitC:
                And     AX, 1FFh

                Test    AX, 100h
                JZ      D_Decompress8BitWriteData

                Jmp     D_Decompress8BitD

EndP            D_Decompress8BitData


