Next: Graphical Spectrum Analyzer Up: Graphic mode functions Previous: Oscilloscopes Contents

## Note dots

`<n>` starts the note dots function. Each channel is displayed on a horizontal row. The current note is represented by a dot or bar. Low notes are placed on the left side. High notes appear on the right side of the screen. By pressing `<Pgup>`, `<Pgdown>` the scale of the rows can be changed. However the default scale fits the usual note scale of modules exactly, so there should be no need to change.

By pressing `<n>` you can alter the output appearance of the dots. In the modes stereo note cones and stereo note dots the current pan position is indicated by the left / right half of the icon.