Next: Graphic mode functions Up: Text mode functions Previous: Module message Contents

## eXtended mode

All four text mode functions can be displayed simultaneously. This function enables channel, instrument, spectrum analyzer, pattern view and volume control function with a good preset in text mode. `<x>` will enable 132 column mode. `<ALT>`+`<x>` will switch to the default 80x25 mode with channel and instrument functions enabled.4.11

#### Footnotes

... enabled.4.11
  If your VESA bios does not support 132 columns a 80x50 mode is used.