Next: Note dots Up: Graphic mode functions Previous: Graphic mode functions Contents

## Oscilloscopes

The oscilloscopes are started with `<o>` and come in 4 different modes: logical (the channels are sorted with the default panning position), physical (channels 1 to n from top to bottom), master (the mixed output channel(s)) and single (the currently selected channel is shown).

By pressing `<Tab>` you can enable/disable triggering of the scopes. If the output is triggered a wave on the screen always starts with the upper halvwave. If triggering is turned off the wave will be drawn from the current position.

The scale of the scopes can be altered with `<Pgup>`, `<Pgdown>`.