Extended MikMod v1.98a ß1 - A HaRDCoDE International Production
---------------------------------------------------------------
Coded by Air Richter, Rao, and MikMak of HaRDCoDE '96
---------------------------------------------------------------
Usage: XMM [switches] <clokwork.mod> <chlidren.mod> ...
       XMM [switches] <*.*> <*.s3m> <chlidren.mod> ...

Available switches (CaSe SeNsItIvE!):

  /d x        Use device-driver #x for output.
	      0 = Autodetect (default)
	      1 = Gravis Ultrasound
	      2 = SoundBlaster / Pro / 16
	      3 = Ensoniq SoundScape
  /ld         List all available device-drivers
  /ll         List all available loaders
  /x          Disables protracker extended speed
  /p          Disables panning effects (9fingers.mod)
		Some older modules used these commands for extended speed and
		panning to trigger timing changes in demos.
  /v xx       Sets volume from 0 (silence) to 100. Default = 80
  /f xxxx     Sets mixing frequency.  Default = 44100
  /c xx       Set maximum number of channels (32-64).  Default = 32
  /m          Force mono output (so sb-pro can mix at 44100)
		Useful for the SB-Pro, which generally sounds better in mono
		mode when it can mix at 44.1khz as opposed to 22.05khz in stereo.
  /8          Force 8 bit output. For mixing cards only [non-GUS].
  /r          Restart a module when it's done playing

Compatability / Interface Options:

  /win        Enable Windows compatability mode (for Win95 especially)
  /vga x      Enable VGA compatability mode (1 thru 3)
  /w          Suppress warning messages
