# Copy Porteus-v1.1-i486.iso and Porteus-v1.1-i486.mnu to the /_ISO/XXX/MNU folder

# Note: paths and filename as Case Sensitive in the Kernel line!
# Note that the ext2 file /porteus.ext2 is all lowercase
# You can easily create the /porteus.ext2 ext2 file using the RMPrepUSB Create Ext2 FS button (must be contiguous)
# IMPORTANT: you MUST run WinContig (Ctrl+F2) before booting E2B.

# MD5: cc3732501aeb03524b890a00b36936d6
# SHA1: c91bb1f39fa6c6378336a9a8cb5ce0120442971e
# CRC32: f91b784d

iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus Graphics mode Persistent (KDE)\nRun Porteus the best way we can. Try to autoconfigure graphics card and use the maximum allowed resolution.\nUse /porteus as changes filesystem.
map $HOME$/porteus-v1.1-i486.iso (0xff) || map --mem $HOME$/porteus-v1.1-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso vga=791 changes=/porteus.ext2
initrd /boot/initrd.xz

iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus Graphics mode Persistent (LXDE)\nLightweight LXDE to be launched as default desktop.\nUse /porteus as changes filesystem.
map $HOME$/porteus-v1.1-i486.iso (0xff) || map --mem $HOME$/porteus-v1.1-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso lxde vga=791 changes=/porteus.ext2
initrd /boot/initrd.xz

iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus as PXE Server Persistent\nRun Porteus and initialize a PXE server\nThis will allow you to boot on other computers over a network
map $HOME$/porteus-v1.1-i486.iso (0xff) || map --mem $HOME$/porteus-v1.1-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso autoexec=pxe-boot vga=791 changes=/porteus.ext2
initrd /boot/initrd.xz

iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus Text Mode Persistent\nRun Porteus and go to Command Prompt
map $HOME$/porteus-v1.1-i486.iso (0xff) || map --mem $HOME$/porteus-v1.1-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso autoexec=telinit~3  vga=791 changes=/porteus.ext2
initrd /boot/initrd.xz

iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus Graphics VESA Mode Persistent\nRun Porteus with KDE, but skip the graphics card autoconfig. \nThis forces 1024x768 resolution using a standard VESA driver
map $HOME$/porteus-v1.1-i486.iso (0xff) || map --mem $HOME$/porteus-v1.1-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso autoexec=vesa-mode  vga=791 changes=/porteus.ext2
initrd /boot/initrd.xz
 
iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus Fresh Mode\nUse this option to start a fresh system, changes are not read from or written to any device
map $HOME$/porteus-v1.1-i486.iso (0xff) || map --mem $HOME$/porteus-v1.1-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso nomagic
initrd /boot/initrd.xz
  
iftitle [if exist $HOME$/Porteus-v1.1-i486.iso] Porteus Copy to RAM Persistent\nUse this option to get a huge increase in speed.\nNeeds >768MB of memory
map $HOME$/porteus-v1.1-i486.iso (0xff) || pause --wait=3 Please run WinContig on $HOME$/Porteus-v1.1-i486.iso && exit
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/vmlinuz from_iso=$HOME$/Porteus-v1.1-i486.iso vga=791 copy2ram changes=/porteus.ext2
initrd /boot/initrd.xz
  
  
    




