# For persistence, create an ext2 file in the root of the boot drive using RMPrepUSB Create ext2 FS button
# Ext2 File Name=BT5-rw   Volume Name=casper-rw
# Place ISO in \_ISO\Mainmenu\MNU or \_ISO\LINUX\MNU (and this .mnu file too)
# DOES NOT WORK UNDER VM!!!
# IMPORTANT: you MUST run WinContig (Ctrl+F2) before booting E2B.

iftitle [if exist $HOME$/BT5R2-GNOME-32.iso] BackTrack 5 (1024x768) Persistent\nType startx to run GUI once booted

set ISO=$HOME$/BT5R2-GNOME-32.iso
set PER=/BT5-rw

if exist CD echo WARNING: Cannot use partnew command! && pause && configfile (bd)/menu.lst
if "%E2BDEV%"=="" set E2BDEV=hd0 && pause E2BDEV forced to hd0!
#enable parttype output
debug 1
# make empty table entry in 3rd position in ptn table
parttype (%E2BDEV%,2) | set check=
debug off
set check=%check:~-5,4%
if "%check%"=="0x00" partnew (%E2BDEV%,2) 0 0 0
if not "%check%"=="0x00" echo WARNING: PTN TABLE 3 IS ALREADY IN USE! && pause
debug 1
#clear ptn 4
if "%check3%"==0x00" partnew (%E2BDEV%,3) 0x0 0 0 0
if not exist %PER% echo WARNING: %PER% persistence file not found! && pause
errorcheck off
if "%check%"=="0x00" partnew (%E2BDEV%,2) 0x0 %PER%
errorcheck on
map %ISO% (0xff)
map --hook
partnew (%E2BDEV%,3) 0x0 %ISO%
root (0xff)
kernel /casper/vmlinuz file=/cdrom/preseed/custom.seed boot=casper persistent text splash noprompt vga=791-- 
initrd /casper/initrd.gz
