# Copy Porteus-v2.0-i486.iso and Porteus-v2.0-i486.mnu to the /_ISO/Linux/MNU folder (or any similar 3rd level folder)
# You can create the /porteus.ext2 file using the RMPrepUSB Create Ext2 FS button (volume name=file name=porteus.ext2
# MD5: 5d07c127bd8731d5d0a8d860f6ad81c4

iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus Graphics mode Persistent (KDE)\nRun Porteus the best way we can. Try to autoconfigure graphics card and use the maximum allowed resolution.\nUse /porteus as changes filesystem.
map $HOME$/porteus-v2.0-i486.iso (0xff) || map --mem $HOME$/porteus-v2.0-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso vga=791 changes=/porteus.ext2
initrd /boot/syslinux/initrd.xz

iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus Graphics mode Persistent (LXDE)\nLightweight LXDE to be launched as default desktop.\nUse /porteus as changes filesystem.
map $HOME$/porteus-v2.0-i486.iso (0xff) || map --mem $HOME$/porteus-v2.0-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso lxde vga=791 changes=/porteus.ext2
initrd /boot/syslinux/initrd.xz

iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus as PXE Server Persistent\nRun Porteus and initialize a PXE server\nThis will allow you to boot on other computers over a network
map $HOME$/porteus-v2.0-i486.iso (0xff) || map --mem $HOME$/porteus-v2.0-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso autoexec=pxe-boot vga=791 changes=/porteus.ext2
initrd /boot/syslinux/initrd.xz

iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus Text Mode Persistent\nRun Porteus and go to Command Prompt
map $HOME$/porteus-v2.0-i486.iso (0xff) || map --mem $HOME$/porteus-v2.0-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso autoexec=telinit~3  vga=791 changes=/porteus.ext2
initrd /boot/syslinux/initrd.xz

iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus Graphics VESA Mode Persistent\nRun Porteus with KDE, but skip the graphics card autoconfig. \nThis forces 1024x768 resolution using a standard VESA driver
map $HOME$/porteus-v2.0-i486.iso (0xff) || map --mem $HOME$/porteus-v2.0-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso autoexec=vesa-mode  vga=791 changes=/porteus.ext2
initrd /boot/syslinux/initrd.xz
 
iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus Fresh Mode\nUse this option to start a fresh system, changes are not read from or written to any device
map $HOME$/porteus-v2.0-i486.iso (0xff) || map --mem $HOME$/porteus-v2.0-i486.iso (0xff)
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso nomagic
initrd /boot/syslinux/initrd.xz
  
iftitle [if exist $HOME$/Porteus-v2.0-i486.iso] Porteus Copy to RAM Persistent\nUse this option to get a huge increase in speed.\nNeeds >768MB of memory
map $HOME$/porteus-v2.0-i486.iso (0xff) || pause --wait=3 Please run WinContig on $HOME$/Porteus-v2.0-i486.iso && exit
map --hook
chainloader (0xff)
root (0xff)
kernel /boot/syslinux/vmlinuz from=$HOME$/Porteus-v2.0-i486.iso vga=791 copy2ram changes=/porteus.ext2
initrd /boot/syslinux/initrd.xz
  
  
    




