# Use for MSDaRT 5 XP-based ISOs (use DPMS2 version of Easy2Boot for AHCI drivers)
# Make new empty folder, e.g. \_ISO\MAINMENU\MSDART
# Copy this .mnu file and the single ERD or PE ISO file to the empty folder (one .iso file per folder)

title XP MSDart ERD (DPMS)\n If DPMS is not installed\n Remember to select an AHCI driver\n AND the FiraDisk driver (using F6).
set MFOLDER=$HOME$
pause --wait=3 Press ENTER 3 times to boot...
/%grub%/XPStep1.g4b
boot

