-dpx
#
                          >>>> AMPRO SYSTEM MENU <<<<
					
            ........Programs.........    ........Utilities........
            :  X - communications   :    :    1 - AMPRODSK       :
            :  F - File management  :    :    2 - CONFIG         :
            :    - (spare)          :    :    3 - SYSGEN         :
            :    - (spare)          :    :    4 - MULTIDSK       :
            :.......................:    :.......................:

                        .........System Aids..........
                        :  D - Directory of a drive  :
                        :  V - View a file           :
                        :  C - Copy a file           :
                        :  R - Rename a file         :
                        :  E - Erase a file          :
                        :  S - Space on a drive      :
                        :  B - set Port B baud rate  :
                        :  M - Manual cp/m command   : 
                        :............................:
# 
B!set port b="Set Port B to what baud rate? (300,600,1200,2400,4800,9600) ",8,a,n,"Handshaking? (Y/N) "; set ?
C!mcopy "DESTINATION Drive/User? (B0,15,C,...) ":="SOURCE Drive/User? (B0,15,C,...) ":"filename.typ? "
D!dir "Directory of which Drive/User? (B0,15,C,...) ":
E!era "Erase a file in which Drive/User? (B0,15,C,...) ":"filename.typ to erase? "
Ffriendly
M!"Enter command> "
R!ren "Rename a file in which Drive/User? (B0,15,C,...) ":"NEW filename.typ? "="OLD filename.typ? "
S!stat "Space on which Drive? (A,B,...) ":
V!type "View a file in which Drive/User? (B0,15,C,...) ":"filename.typ to view? "
Xmdm740;set port b=9600,8,a,n,y
1amprodsk
2config
3sysgen
4multidsk
##
