Welcome to Disk Manager!
To install your hard disk, simply follow these basic steps:

   1) Physically install your hard disk into your computer.
      Disk Manager assumes power, cables, jumpers, etc.,
      are connected and properly installed.  
   2) Insert your DOS diskette in drive A: and boot the machine. 
   3) Make a working copy of the Disk Manager diskette.
      Use the working copy to install your hard disk.
      Keep the original diskette in a safe place.  
   4) Insert your Disk Manager diskette into drive A: and
      type DM for automatic installation of your hard disk.
   5) When the installation has completed, remove the Disk Manager
      diskette from drive A: and boot from the hard disk.  

The instruction manual for this product exists on the diskette.
It is accessed by typing DM/H.  (Example: A> DM/H)
It can also be accessed by pressing F1 twice from anywhere inside DM.

For the latest information about updates, revisions, and products
from ONTRACK, call the bulletin board at 612-937-0860.
