0770:01*05
PORT=
0771:01*05
 IRQ=
0772:01*05
 DMA=
0773:01*09
C:\EVTAPE
0774:01*11
A:\FILELIST
0775:01*03
A:\
0001:02*60
*            Program already loaded in memory              *
*           Type exit to return to the program             *
0002:02*60
*                Cannot execute COMMAND.COM                *
*          Not enough memory or program not found          *
0003:03*60
*                  Memory allocation error                 *
*   You have invoked a program still resident in memory    *
*             Cannot execute the tape software             *
0004:02*60
*               Hit Enter key to confirm EXIT              *
*                Hit any other key to resume               *
0720:01*60
*            Operation completed with no errors            *
0721:01*60
*                    Operation failed                      *
0722:03*60
*            Not enough RAM memory to proceed              *
*          Minimum of 128K main memory required            *
*                 Operation aborted                        *
0723:03*60
*     Cannot install tape software into the hard disk      *
*             The hard disk is probably full               *
*   Hit F9 to abort and clear some space for the software  *
0724:05*60
*     Cannot find the tape software from the diskette      *
*          You may be using the wrong diskette             *
*   You should start with the first diskette and insert    *
*      the rest according to their numerical order         *
*               Hit Enter key to continue                  *
0725:03*60
*      Cannot seek tape software file, please check        *
*           You may have a damaged diskette                *
*               Hit Enter key to continue                  *
0726:03*60
*     Cannot read the tape software from the diskette      *
*      Please check, you may have a damaged diskette       *
*               Hit Enter key to continue                  *
0727:03*60
*  Unsuccessful in writing the tape software to the hard   *
*  drive. Your hard drive is probably full. Please check   *
*               Hit Enter key to continue                  *
0728:01*60
*                      Disk is full !                      *
0729:02*60
*     Invalid character(s) in pathname, please re-enter    *
*               Hit Enter key to continue                  *
072A:02*60
*           Invalid drive name, please re-enter.           *
*               Hit Enter key to continue                  *
072B:02*60
*        Invalid directory name, please re-enter.          *
*               Hit Enter key to continue                  *
072C:02*60
*    Extra '.' detected from pathname, please re-enter.    *
*               Hit Enter key to continue                  *
072D:02*60
*          Cannot change directory, please check.          *
*               Hit Enter key to continue                  *
072E:03*60
* You cannot have a directory with the same name as a file *
*         Please re-enter another directory name           *
*               Hit Enter key to continue                  *
072F:02*60
*   Wrong diskette, please insert the correct diskette.    *
*                 Hit F8 key to continue                   *
0730:02*60
*   Incorrect number of tape software files in diskette    *
*               Hit Enter key to continue                  *
0731:01*60
*  No fixed disk drive detected (cannot install software). *
0732:01*60
*  No floppy drive detected (must install from drive A).   *
0733:01*60
*          Invalid "TAPE.CFG" file, please check.          *
0741:02*60
*         Port address ranges from 000-3FE HEX             *
*               Hit Enter key to continue                  *
0742:02*60
*         Port address ranges from 000-3FE HEX             *
*               Hit Enter key to continue                  *
0743:02*60
*      The first port address must be an even number       *
*               Hit Enter key to continue                  *
0744:02*60
*   Interrupt must be one of the following: 2,3,4,5 or 7   *
*               Hit Enter key to continue                  *
0745:02*60
*   Interrupt must be one of the following: 2,3,4,5 or 7   *
*               Hit Enter key to continue                  *
0746:02*60
*   Interrupt must be one of the following: 2,3,4,5 or 7   *
*               Hit Enter key to continue                  *
0747:02*60
*    Invalid DMA channel. It can only be 1,2 or 3          *
*               Hit Enter key to continue                  *
0748:02*60
*    Invalid DMA channel. It can only be 1,2 or 3          *
*               Hit Enter key to continue                  *
0749:01*60
*       Cannot create file "TAPE.CFG", please check.       *
074A:01*60
*       Cannot  open  file "TAPE.CFG", please check.       *
074B:01*60
*       Cannot  seek  file "TAPE.CFG", please check.       *
074C:01*60
*       Cannot  read  file "TAPE.CFG", please check.       *
074D:01*60
*       Cannot write  file "TAPE.CFG", please check.       *
074E:01*60
*           Incorrect "TAPE.CFG", please check.            *
074F:01*60
* Do you really want to abort Software Installation (Y/N)? *
0751:02*60
*        All tape software has been installed              *
*             Hit Enter key to continue                    *
0752:02*60
*     Check if tape software has been installed            *
*             Hit Enter key to continue                    *
0753:01*60
*    Please reconfigure DMA channel, and hit F8 to save.   *
0754:01*60
*    Please reconfigure IRQ level, and hit F8 to save.     *
0755:01*60
* Insert diskette #%% in drive A:, and hit %%% to continue.*
0756:02*60
*           Interrupt must be 3, 4, 5, 6 or 7              *
*               Hit Enter key to continue                  *
0757:02*60
*           DMA channel must be 0, 1, 2, or 3              *
*               Hit Enter key to continue                  *
0758:02*60
*               Failed to create ADF file                  *
*               Hit Enter key to continue                  *
FFFF:01*03
EOF

