0001:02*58
*           Program already loaded in memory             *
*          Type EXIT to return to the program            *
0002:03*58
*              Cannot execute COMMAND.COM                *
*         Not enough memory or program not found         *
*               Hit Enter key to continue                *
0003:05*58
*                Memory allocation error                 *
*     Less memory reallocated after return from DOS      *
*  You have invoked a program still resident in memory   *
*            Cannot execute the tape software            *
*                 Hit Enter key to EXIT                  *
0004:02*58
*             Hit Enter key to confirm EXIT              *
*              Hit any other key to resume               *
0005:01*10
Standard  
0006:01*10
Extended  
0007:01*10
Unknown   
0008:01*58
*  Insert cartridge in drive and hit return to continue  *
0600:02*58
*       Not enough memory to run FTFORMAT program        *
*                 Hit Enter key to EXIT                  *
0601:01*58
*   Fatal error: initializing messages. Please check.    *
0602:02*58
*             Please mount a tape in drive &             *
*               Hit Enter key to continue                *
0603:02*58
*              The tape has been formatted.              *
*         Do you want to reformat the tape (Y/N)?        *
0604:02*58
*              There is valid data on tape.              *
*         Do you want to reformat the tape (Y/N)?        *
0605:02*58
*      Please turn off the write protect mechanism       *
* Re-insert tape in drive and hit Enter key to continue  *
0606:02*58
*                 Checking tape content                  *
*                      Please wait                       *
0607:02*58
*                Physical format in progress             *
*                      Please wait                       *
0608:02*58
*            Format read check in progress               *
*                      Please wait                       *
0609:02*58
*        Initializing tape for DOS device driver         *
*                      Please wait                       *
060A:02*58
*                   Format completed.                    *
*               Hit Enter key to continue.               *
060B:02*58
*       WARNING: Tape content will be overwritten.       *
*             Do you want to continue (Y/N)?             *
060C:01*58
*               Closing tape. Please wait.               *
060D:02*58
*       WARNING: This tape only can be formatted as      *
*         40 Megabyte.  Hit Enter key to continue.       *
0630:01*58
*  Error: No header. Hit Enter key to continue.          *
0631:01*58
*  Error: Time out. Hit Enter key to continue.           *
0632:01*58
*  Error: Seek failed. Hit Enter key to continue.        *
0633:02*58
*  Error: NEC controller failed. Hit Enter key to        *
*         continue.                                      *
0634:01*58
*  Error: Bad CRC. Hit Enter key to continue.            *
0635:01*58
*  Error: Bad DMA. Hit Enter key to continue.            *
0636:01*58
*  Error: DMA overrun. Hit Enter key to continue.        *
0637:01*58
*  Error: Media removed. Hit Enter key to continue.      *
0638:02*58
*  Error: Select Stream timing error. Hit Enter key to   *
*         continue.                                      *
0639:01*58
*  Error: Sector not found. Hit Enter key to continue.   *
063A:01*58
*  Error: Write protect. Hit Enter key to continue.      *
063B:01*58
*  Error: No address mark. Hit Enter key to continue.    *
063C:01*58
*  Error: Bad I/O command. Hit Enter key to continue.    *
063E:02*58
*  Error: Too many bad sectors. Hit Enter key to         *
*         continue.                                      *
063F:01*58
*  Error: Unknown error. Hit Enter key to continue.      *
0640:02*58
*  Error: Bad disk I/O command. Hit Enter key to         *
*         continue.                                      *
0641:01*58
*  Error: Tape not found. Hit Enter key to continue.     *
0642:02*58
*  Error: Tape operation time out, probably a bad tape   *
*         in drive. Hit Enter key to continue.           *
06A0:01*14
Total Segments
06B0:01*58
*                     Opening Tape                       *
06B1:01*58
*                Updating Bad Sector Map                 *
06B2:01*58
*     No tape in drive.  Hit Enter key to return.        *
06B3:01*58
*    Tape is not formatted.  Hit Enter key to return.    *
06B4:01*58
*   Tape is write protected.  Hit Enter key to return.   *
06B5:01*58
*      Read tape error.  Hit Enter key to return.        *
06B6:01*58
*     Write tape error.  Hit Enter key to return.        *
06B7:03*58
*    WARNING: There is valid data on tape. Update bad    *
*             sector map may destroy tape data.          *
*             Do you want to continue (Y/N)?             *
06B8:02*58
*       WARNING: Bad sector map will be overwritten.     *
*             Do you want to continue (Y/N)?             *
06B9:01*58
*         Continue formatting the next tape (Y/N)?       *
06BA:01*58
*                 Checking tape capacity                 *
06BB:02*58
*                  Checking tape drive                   *
*                      Please wait                       *
06BC:02*58
*      The tape has been formatted.(QIC-40 standard).    *
*         Do you want to reformat the tape (Y/N)?        *
06BD:02*58
*      The tape has been formatted.(QIC-80 standard).    *
*         Do you want to reformat the tape (Y/N)?        *
06BE:02*58
*      There is valid data on tape.(QIC-40 standard).    *
*         Do you want to reformat the tape (Y/N)?        *
06BF:02*58
*      There is valid data on tape.(QIC-80 standard).    *
*         Do you want to reformat the tape (Y/N)?        *
06C0:01*58
*   Drive number 1                                       *
06C1:01*58
*   Drive number 2                                       *
06C2:01*58
*   Drive number 3                                       *
06C3:01*58
*   Drive number 4                                       *
06C6:02*58
*    ERROR: Hardware error. Failure to communicate       *
*           with drive.  Hit Enter key to continue.      *
06C7:02*58
*           ERROR: Select stream or seek error           *
*               Hit Enter key to continue.               *
06C8:02*58
*         ERROR: Cartridge length detection error        *
*               Hit Enter key to continue.               *
06D0:02*58
*               Error: Tape not formatted                *
*               Hit Enter key to continue.               *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000

