03FD:01*07
No More
03FE:01*07
More...
03FF:01*12
# of Sectors
0001:02*58
*           Program already loaded in memory.            *
*          Type exit to return to the program.           *
0002:03*58
*               Cannot execute COMMAND.COM.              *
*         Not enough memory or program not found.        *
*                Hit Enter key to return.                *
0003:04*58
*                Memory allocation error.                *
*     Less memory reallocated after return from DOS.     *
*  You have invoked a program still resident in memory.  *
*           Hit Enter key to EXIT the program.           *
0004:02*58
*             Hit Enter key to confirm EXIT.             *
*              Hit any other key to resume.              *
0300:01*58
*  Do you really want to abort current operation (Y/N)?  *
0301:02*58
*   Checking the selected target drive for bad sectors.  *
*           Hit F9 key to abort the operation.           *
0305:02*58
*      Advancing the tape to the specified dataset.      *
*           Hit F9 key to abort the operation.           *
0306:02*58
*       Do you want to restore this dataset? (Y/N)       *
*           Hit F9 key to abort the operation.           *
0307:02*58
*       Do you want to compare this dataset? (Y/N)       *
*           Hit F9 key to abort the operation.           *
0308:05*58
* Only part of your dataset image backup is present on   *
* this tape.  You may have used a tape out of the group  *
* sequence.                                              *
*       Do you want to restore this dataset? (Y/N)       *
*           Hit F9 key to abort the operation.           *
0309:05*58
* Only part of your dataset image backup is present on   *
* this tape.  You may have used a tape out of the qroup  *
* sequence.                                              *
*       Do you want to compare this dataset? (Y/N)       *
*           Hit F9 key to abort the operation            *
030A:02*58
*  Restoring the tape data to the selected target drive. *
*           Hit F9 key to abort the operation.           *
030B:02*58
* Comparing the tape data with the selected target drive.*
*           Hit F9 key to abort the operation.           *
030C:02*58
*                Image compare completed.                *
*                Hit Enter key to return.                *
030D:02*58
*         Image restore completed with no errors.        *
*                Hit Enter key to return.                *
030E:02*58
*                Image restore completed.                *
*                Hit Enter key to return.                *
030F:06*58
*   FIXED DISK IMAGE RESTORE COMPLETED WITH NO ERRORS    *
*                                                        *
* The system may not recognize the newly restored fixed  *
* disk image until a system reboot.                      *
*                                                        *
*        Do you want to reboot the system? (Y/N)         *
03F0:06*58
*         THE FIXED DISK IMAGE HAS BEEN MODIFIED         *
*                                                        *
* The system may not recognize the modified fixed disk   *
* image until a system reboot.                           *
*                                                        *
*        Do you want to reboot the system? (Y/N)         *
0310:01*58
*                     Error occurred                     *
0311:01*58
*                   Error in menu file                   *
0312:01*58
*   Not enough memory to perform IMAGE RESTORE/COMPARE.  *
0313:01*58
*       No valid drives for IMAGE RESTORE/COMPARE.       *
0314:02*58
*     The specified target drive is a diskette drive.    *
*     Please enter a non-diskette logical drive name.    *
0315:02*58
*        Invalid logical drive name specification.       *
*        Please enter a valid logical drive name.        *
0316:02*58
*     Invalid fixed disk drive number specification.     *
*      Please enter a valid fixed disk drive number.     *
0317:01*58
*   Failed to get the fixed disk drive type parameters.  *
0318:01*58
*       Error in the disk type file (DSKTYP8?.CFG).      *
0319:03*58
*         Cannot read cylinder 0 head 0 sector 1.        *
*    Selected fixed disk may not have been physically    *
*        formatted or `bad track 0' disk unusable.       *
031A:01*58
*           Failed to read the DOS BOOT record.          *
031B:01*58
*      Failed to read the DOS File Allocation Table.     *
031C:01*58
*     Failed to write the DOS File Allocation Table.     *
031D:02*58
*      The selected drive has too many bad sectors.      *
*   May not be able to recover some of the bad sectors.  *
031E:02*58
*  Failed to modify the number of hidden sectors in the  *
*  DOS BOOT record.                                      *
031F:01*58
*   Failed to read the EXTENDED PARTITION BOOT record.   *
0320:01*58
*      Failed to read the NOVELL volume information.     *
0321:01*58
*         NOVELL volume information is corrupted.        *
0322:01*58
*    Failed to read the NOVELL File Allocation Table.    *
0323:02*58
*    There are bad sectors inside NOVELL system region.  *
*            NOVELL may not be able to reboot.           *
0324:02*58
* NOVELL file system is full (all good blocks are in use)*
*  Cannot relocate some bad sectors (data will be lost). *
0325:01*58
*       Failed to read the NOVELL Directory Table.       *
0326:02*58
*     Failed to perform NOVELL bad sector relocation.    *
*                 Some data may be lost.                 *
0330:01*58
*     The selected fixed disk has no partition table.    *
0331:01*58
*  Partitions are out of the fixed disk physical limit.  *
0332:01*58
*                 Partitions overlap.                    *
0333:01*58
*   The selected fixed disk has no DOS partition found.  *
0334:02*58
* There are non DOS partitions in the selected fixed disk*
*  Cannot perform bad sector relocation for non DOS O/S. *
0335:03*58
*     There are extra partition entries found in the     *
*        logical drive table. Bad sectors in the         *
*     EXTENDED DOS partition may not be able to map.     *
0336:01*58
*  Failed to perform EXTENDED DOS bad sector relocation. *
0337:01*58
*      EXTENDED DOS PARTITION BOOT record not found.     *
0340:01*58
*                   DOS BOOT: bad data                   *
0341:01*58
*             DOS BOOT: incorrect media type             *
0342:01*58
*          DOS BOOT: incorrect disk head count           *
0343:01*58
*          DOS BOOT: incorrect disk track size           *
0344:01*58
*    DOS BOOT: inconsistent with the partition table     *
0345:01*58
*           DOS BOOT: incompatible sector size           *
0346:01*58
* Error in the DOS File Allocation Table size computation*
0347:05*58
* WARNING: Target disk drive has different number of     *
* sectors from the source disk drive. This may cause     *
* problems if you modify data on target drive after the  *
* source image is restored to the target drive.          *
* Do you still want to restore the image? (Y/N)          *
0350:01*58
* Not enough memory to process DOS File Allocation Table.*
0358:01*58
*      Compare error; Do you wish to continue? (Y/N)     *
0360:02*58
* Too many bad clusters (bad sector map buffer is full). *
*      May not be able to recover some bad clusters.     *
0361:02*58
*   There are bad sectors inside the DOS table region.   *
*                 Some data may be lost.                 *
0362:02*58
* DOS file system is full (all good clusters are in use).*
*  Cannot relocate some bad sectors (data will be lost). *
0363:02*58
*     Not enough memory to process the DOS directory.    *
*        Cannot complete the bad sector recovery.        *
0364:02*58
* Crossed links detected in the DOS File Allocation Table*
*       May result in incorrect sector relocation.       *
0370:03*58
*     The first cluster of the file has bad sectors.     *
*          The cluster has been relocated and            *
*            the directory entry corrected.              *
0371:03*58
*      The n-th cluster of the file has bad sectors.     *
*          The cluster has been relocated and            *
*            the directory entry corrected.              *
0372:02*58
*     The first cluster of the file has bad sectors.     *
*    The cluster was not relocated (data may be lost).   *
0373:02*58
*      The n-th cluster of the file has bad sectors.     *
*    The cluster was not relocated (data may be lost).   *
0374:02*58
*             Invalid directory entry found.             *
*  The first cluster of the file is not a valid cluster. *
0375:02*58
*      Invalid cluster chain detected (no EOF mark).     *
*  The last cluster of the file is not a valid cluster.  *
0376:02*58
*             Invalid directory entry found.             *
*   The first cluster of the file was marked as unused.  *
0377:02*58
*             Invalid cluster chain detected.            *
*         Cannot recover the cluster chain error.        *
0378:02*58
*      Invalid cluster chain detected (no EOF mark).     *
*     The cluster chain of the file contains a loop.     *
0380:02*58
*    Tape is not formatted, please change the tape.      *
*                Hit Enter key to return.                *
0381:02*58
*       Tape is not in drive or Drive is not ready.      *
*                Hit Enter key to return.                *
0382:01*58
*      Opening tape error, hit Enter key to return.      *
0383:02*58
*       Tape was removed from drive during restore       *
*  Operation has been aborted. Hit Enter key to return.  *
0384:01*58
*       Reading tape error, hit Enter to return.         *
0385:01*58
*            Error on opening tape channel.              *
0386:02*58
*      Bad compression data format detected.             *
*           Hit Enter key to EXIT                        *
03A0:02*58
*       Incorrect tape: wrong backup date or time.       *
*              Hit Enter key to continue.                *
03A1:02*58
*            Incorrect tape: wrong dataset.              *
*              Hit Enter key to continue.                *
03A2:02*58
*          Incorrect tape: dataset not found.            *
*              Hit Enter key to continue.                *
03A3:02*58
*      Incorrect tape: wrong tape sequence number.       *
*              Hit Enter key to continue.                *
03B0:03*58
*                Dataset label unmatched.                *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03B1:03*58
*            Dataset is not found in the tape.           *
*                Please change the tape.                 *
*                Hit Enter key to return.                *
03B2:03*58
*    The specified dataset is not found on this tape.    *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03B3:02*58
*          Password unmatched, please re-enter.          *
*                Hit Enter key to return.                *
03B4:02*58
*            Incorrect tape sequence number.             *
*                Hit Enter key to return.                *
03B5:03*58
*     The specified dataset is not an IMAGE dataset.     *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03B6:01*58
*   No dataset was specified, hit Enter key to return.   *
03C0:03*58
*       The specified dataset is not on this tape.       *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C1:03*58
*   The specified dataset was not backed up in IMAGE.    *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C2:04*58
*       The specified  dataset is a logical IMAGE,       *
*    but the selected drive is a physical fixed disk.    *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C3:04*58
*       The specified  dataset is a physical IMAGE,      *
*       but the selected drive is a logical drive.       *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C4:04*58
*     The target drive has different number of heads     *
*      than the source drive backed up on the tape.      *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C5:04*58
*   The target drive has different track size than the   *
*          source drive backed up on the tape.           *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C6:04*58
*  The target drive has different sector size than the   *
*          source drive backed up on the tape.           *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C7:04*58
*   The target drive is smaller than the source drive    *
*                 backed up on the tape.                 *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C8:04*58
* The target logical drive has different hidden sectors  *
*      than the source drive backed up on the tape.      *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03C9:04*58
*Only part of your dataset image is present on this tape.*
*   You may have used a tape out of the group sequence.  *
*  Please re-specify another dataset or change the tape. *
*                Hit Enter key to return.                *
03CA:02*58
*                Compare error detected.                 *
*                Hit Enter key to return.                *
03D0:02*58
*           Open tape error.                             *
*           Do you want to retry ? (Y/N)                 *
03D1:02*58
*            Reading tape timeout.                       *
*            Do you want to retry ? (Y/N)                *
03D2:02*58
*            Reading tape error.                         *
*            Do you want to retry ? (Y/N)                *
03F1:01*58
*          Do you want to run CHECKDIR? (Y=YES)          *
03F2:01*58
*     Do you want to list directory entries? (Y=YES)     *
03F3:01*58
*    Do you want to list the bad sector map? (Y=YES)     *
03F4:10*30
* -a  same as -smrfdp        *
* -s  show system info       *
* -m  show bad sector map    *
* -r  show relocation        *
* -f  exam DOS FAT           *
* -d  exam directories       *
* -p  list all file names    *
* -q  dump tape que          *
* -w  disable all disk write *
* -n  NOVELL bad sector map  *
03F5:01*58
*                      Opening Tape                      *
03F6:03*58
*        Please insert tape number # in drive &          *
*        Hit F8 key to continue; or                      *
*        Hit F9 key to abort operation                   *
03F7:04*58
*       Cross tape !!  Please wait for rewind            *
*       Then, insert tape number # in drive &            *
*       Hit F8 key to continue; or                       *
*       Hit F9 key to abort operation                    *
03F8:01*58
*                Exiting; Please wait...                 *
03F9:01*58
*             Closing tape; Please wait...               *
0400:01*58
*       Drive number 1                                   *
0401:01*58
*       Drive number 2                                   *
0402:01*58
*       Drive number 3                                   *
0403:01*58
*       Drive number 4                                   *
0410:01*10
  Yes     
0411:01*10
  No      
0412:01*11
  File     
0413:01*11
  Image    
0414:01*11
  Unknown  
0800:01*58
*       HALT !!!                                         *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000

