0770:01*05
PORT=
0771:01*05
 IRQ=
0772:01*05
 DMA=
0773:01*09
C:\EVTAPE
0774:01*11
A:\FILELIST
0775:01*03
A:\
0776:01*08
C:\STAPE
0001:02*58
*           Program already loaded in memory             *
*          Type exit to return to the program            *
0002:02*58
*               Cannot execute COMMAND.COM               *
*         Not enough memory or program not found         *
0003:03*58
*                 Memory allocation error                *
*  You have invoked a program still resident in memory   *
*            Cannot execute the tape software            *
0004:02*58
*             Press Enter key to confirm EXIT            *
*              Press any other key to resume             *
0720:01*58
*           Operation completed with no errors           *
0721:01*58
*                   Operation failed                     *
0722:03*58
*           Not enough RAM memory to proceed             *
*         Minimum of 128K main memory required           *
*                Operation aborted                       *
0723:03*58
*    Cannot install tape software into the hard disk     *
*            The hard disk is probably full              *
* Press F9 to abort and clear some space for the software*
0724:05*58
*    Cannot find the tape software from the diskette     *
*         You may be using the wrong diskette            *
*  You should start with the first diskette and insert   *
*     the rest according to their numerical order        *
*             Press Enter key to continue                *
0725:03*58
*     Cannot seek tape software file, please check       *
*          You may have a damaged diskette               *
*             Press Enter key to continue                *
0726:03*58
*    Cannot read the tape software from the diskette     *
*     Please check, you may have a damaged diskette      *
*             Press Enter key to continue                *
0727:03*58
* Unsuccessful in writing the tape software to the hard  *
* drive. Your hard drive is probably full. Please check  *
*             Press Enter key to continue                *
0728:01*58
*                     Disk is full !                     *
0729:02*58
*    Invalid character(s) in pathname, please re-enter   *
*             Press Enter key to continue                *
072A:02*58
*          Invalid drive name, please re-enter.          *
*             Press Enter key to continue                *
072B:02*58
*       Invalid directory name, please re-enter.         *
*             Press Enter key to continue                *
072C:02*58
*   Extra '.' detected from pathname, please re-enter.   *
*             Press Enter key to continue                *
072D:02*58
*         Cannot change directory, please check.         *
*             Press Enter key to continue                *
072E:03*58
*You cannot have a directory with the same name as a file*
*        Please re-enter another directory name          *
*             Press Enter key to continue                *
072F:02*58
*  Wrong diskette, please insert the correct diskette.   *
*             Press Enter key to continue                *
0730:02*58
*  Incorrect number of tape software files in diskette   *
*             Press Enter key to continue                *
0731:01*58
* No fixed disk drive detected (cannot install software).*
0732:01*58
* No floppy drive detected (must install from drive A).  *
0733:01*58
*         Invalid "TAPE.CFG" file, please check.         *
0741:02*58
*        Port address ranges from 000-3FE HEX            *
*             Press Enter key to continue                *
0742:02*58
*        Port address ranges from 000-3FE HEX            *
*             Press Enter key to continue                *
0743:02*58
*     The first port address must be an even number      *
*             Press Enter key to continue                *
0744:02*58
*  Interrupt must be one of the following: 2,3,4,5 or 7  *
*             Press Enter key to continue                *
0745:02*58
*  Interrupt must be one of the following: 2,3,4,5 or 7  *
*             Press Enter key to continue                *
0746:02*58
*  Interrupt must be one of the following: 2,3,4,5 or 7  *
*             Press Enter key to continue                *
0747:02*58
*   Invalid DMA channel. It can only be 1,2 or 3         *
*             Press Enter key to continue                *
0748:02*58
*   Invalid DMA channel. It can only be 1,2 or 3         *
*             Press Enter key to continue                *
0749:01*58
*      Cannot create file "TAPE.CFG", please check.      *
074A:01*58
*      Cannot  open  file "TAPE.CFG", please check.      *
074B:01*58
*      Cannot  seek  file "TAPE.CFG", please check.      *
074C:01*58
*      Cannot  read  file "TAPE.CFG", please check.      *
074D:01*58
*      Cannot write  file "TAPE.CFG", please check.      *
074E:01*58
*          Incorrect "TAPE.CFG", please check.           *
074F:01*60
* Do you really want to abort Software Installation (Y/N)? *
0751:02*58
*       All tape software has been installed             *
*           Press Enter key to continue                  *
0752:02*58
*    Check if tape software has been installed           *
*           Press Enter key to continue                  *
0753:01*58
*  Please reconfigure DMA channel, and Press F8 to save. *
0754:01*58
*   Please reconfigure IRQ level, and Press F8 to save.  *
0755:01*60
*Insert diskette #%% in drive A:, and Press %%% to continue*
0756:02*58
*           Interrupt must be 3, 4, 5, or 7              *
*             Press Enter key to continue                *
0757:02*58
*          DMA channel must be 0, 1, 2, or 3             *
*             Press Enter key to continue                *
0758:02*58
*              Failed to create ADF file                 *
*             Press Enter key to continue                *
0759:02*58
*          Drive number must be 0, 1, 2, or 3            *
*             Press Enter key to continue                *
075A:02*58
*         More than one unit has the same channel        *
*             Press Enter key to continue                *
075B:03*58
* Press F5 again to specify configuration of multi-unit. *
* Press F4 to cancel the operation.                      *
* Press F1 to get more information about multi-unit.     *
0800:02*58
*       SCSI tape block size must be 512, or 1024        *
*             Press Enter key to continue                *
0801:02*58
*         SCSI host id must be between 0 and 7           *
*             Press Enter key to continue                *
0802:02*58
*         SCSI tape id must be between 0 and 7           *
*             Press Enter key to continue                *
0803:02*58
*        SCSI DMA channel must be 0, 5, 6, or 7          *
*             Press Enter key to continue                *
0804:02*58
*        SCSI Interrupt must be 10, 11, 12, or 15        *
*             Press Enter key to continue                *
0805:02*58
* SCSI tape buffer size must be 16, 32, 64, 128, or 256  *
*             Press Enter key to continue                *
0806:02*58
*      SCSI host id and tape id's must all be unique     *
*             Press Enter key to continue                *
0807:02*58
*    SCSI tape buffer size must be same for all units    *
*             Press Enter key to continue                *
0808:02*58
*     SCSI tape format can be QIC, DAT, or CASsette      *
*             Press Enter key to continue                *
0809:02*58
* SCSI QIC tape format must be 60, 120, 150, 320, or 525 *
*             Press Enter key to continue                *
0900:01*01
2
0901:01*18
DIGITAL AUDIO TAPE
0902:01*14
STREAMING TAPE
1000:01*58
*                SCSI bus poll.  Please wait...          *
1001:02*58
*                SCSI bus poll failed.                   *
*             Press Enter key to continue                *
1002:02*58
*        No EXCEL tape drive found to configure.         *
*             Press Enter key to continue                *
1003:09*12
Disk        
Tape        
Printer     
Processor   
WORM        
CD-ROM      
Scanner     
Memory      
Jukeboxes   
1004:01*12
Host Adapter
1005:01*12
Others      
1006:02*58
*              Corrupted INSTALL.ERR File.               *
*                 Press ENTER to exit.                   *
1007:04*58
*        No host adapter card found on the system.       *
* In order to auto config or scan SCSI bus, host adapter *
*  card and tape drive must be installed on the system.  *
*              Press Enter key to continue               *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000
