0851:05*77
TAPE SYSTEM TEST REPORT                       DATE: @@-@@-@@  TIME: @@:@@:@@ 
-----------------------------------------------------------------------------
CONTROLLER: @@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@ 
TAPE DRIVE: @@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@ 
TAPE      : @@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@ 
0852:04*77
=============================================================================
@@@@@@@@@@@@@@@  @@@@   DMA=@ IRQ=@ PORT=@@@ DRV=@    | under- |status| test 
No.     sub-test      | block cnt | pattern  |softerr |  runs  | code |result
----------------------+-----------+----------+--------+--------+------+------
0853:01*77
@@ @@@@@@@@@@@@@@@@@@ | @@@@@@@@@ | @@@@@@@@ | @@@@@@ | @@@@@@ | @@@@ | @@@@ 
0854:05*33
TEST RESULT SUMMARY   :      @@@@
   # of blocks written: @@@@@@@@@
   # of blocks read   : @@@@@@@@@
   # of writes failed : @@@@@@@@@
   # of reads  failed : @@@@@@@@@
0855:05*33
   # of hard errors   : @@@@@@@@@
   # of soft errors   : @@@@@@@@@
   # of underruns     : @@@@@@@@@
   total testing time : @@@@@@@@@
   total elapsed time : @@@@@@@@@
0856:02*04
pass
fail
0001:02*56
*          Program already loaded in memory            *
*         Type EXIT to return to the program           *
0002:03*56
*             Cannot execute COMMAND.COM               *
*        Not enough memory or program not found        *
*             Press ENTER key to continue              *
0003:05*56
*               Memory allocation error                *
*    Less memory reallocated after return from DOS     *
*  You have invoked a program still resident in memory *
*           Cannot execute the tape software           *
*               Press ENTER key to EXIT                *
0004:02*56
*           Press ENTER key to confirm EXIT            *
*            Press any other key to resume             *
0820:02*56
*       Not enough memory to do tape system test       *
*               Press ENTER key to EXIT                *
0821:02*56
*   You have entered an invalid tape test selection    *
*             Press ENTER key to continue              *
0823:02*56
*    File name is too long in command line argument    *
*             Press ENTER key to continue              *
0860:03*56
*   Invalid message file (0840) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0861:03*56
*   Invalid message file (0841) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0862:03*56
*   Invalid message file (0842) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0863:03*56
*   Invalid message file (0843) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0864:03*56
*   Invalid message file (0844) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0865:03*56
*   Invalid message file (0845) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0866:03*56
*   Invalid message file (0846) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0867:03*56
*   Invalid message file (0847) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0868:03*56
*   Invalid message file (0848) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0869:03*56
*   Invalid message file (0849) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
082A:03*56
*  Invalid message file (0851) - abort report summary  *
*   There is a problem with your TAPETEST.ERR file     *
*             Press ENTER key to continue              *
082B:03*56
*  Invalid message file (0852) - abort report summary  *
*   There is a problem with your TAPETEST.ERR file     *
*             Press ENTER key to continue              *
082C:03*56
*  Invalid message file (0853) - abort report summary  *
*   There is a problem with your TAPETEST.ERR file     *
*             Press ENTER key to continue              *
082D:03*56
*  Invalid message file (0854) - abort report summary  *
*   There is a problem with your TAPETEST.ERR file     *
*             Press ENTER key to continue              *
082E:03*56
*  Invalid message file (0855) - abort report summary  *
*   There is a problem with your TAPETEST.ERR file     *
*             Press ENTER key to continue              *
082F:03*56
*  Invalid message file (0856) - abort report summary  *
*   There is a problem with your TAPETEST.ERR file     *
*             Press ENTER key to continue              *
0862:03*56
*   Invalid message file (0860) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0863:03*56
*   Invalid message file (0861) - unable to continue   *
*   There is a problem with your TAPETEST.ERR file     *
*               Press ENTER key to EXIT                *
0831:02*56
*      No logging data in memory to write to file      *
*             Press ENTER key to continue              *
0832:02*56
*             Logging data found in memory             *
*          Do you want to overwrite it? (Y/N)          *
0833:02*56
*            Specified file already exists             *
*          Do you want to overwrite it? (Y/N)          *
0834:02*56
*    Specified log file not found - please re-enter    *
*             Press ENTER key to continue              *
0835:02*56
*    User aborted operation - write to file aborted    *
*             Press ENTER key to continue              *
0836:02*56
*    Cannot create file (invalid name or disk full)    *
*             Press ENTER key to continue              *
0837:02*56
*  Cannot open file (invalid name or file not found)   *
*             Press ENTER key to continue              *
0838:02*56
*          Cannot write to file (disk full?)           *
*             Press ENTER key to continue              *
0839:02*56
*              Cannot read from log file               *
*             Press ENTER key to continue              *
083A:02*56
*                Error seeking log file                *
*             Press ENTER key to continue              *
083B:02*56
*           Specified file is not a log file           *
*             Press ENTER key to continue              *
083C:02*56
*    Specified log file is bad (has been modified?)    *
*             Press ENTER key to continue              *
0857:02*56
*        Testing Tape Controller, please wait.         *
*                Press F9 to abort test                *
0870:02*56
*     Tape system test is completed with no errors.    *
*             Press ENTER key to continue              *
0871:04*56
*   WARNING: Tape system test will destroy tape data   *
*                                                      *
*                Press F10 key to exit                 *
*             Press ENTER key to continue              *
0872:02*56
*   No test has been issued,  cannot go to TEST MENU   *
*             Press ENTER key to continue              *
0873:02*56
*       Tape system test completed with errors.        *
*             Press ENTER key to continue              *
0840:06*32
ABDGGDHHDPQRSTUIZ%%%%%%%%%%%%%%%
ABDEGGGDHHHDPQRSTUXYFOIZ%%%%%%%%
ABDEGGGDHHHDPQRSTUXYFONIZ%%%%%%%
ABDPQIZ%%%%%%%%%%%%%%%%%%%%%%%%%
ABDFOIZ%%%%%%%%%%%%%%%%%%%%%%%%%
ABDEIZ%%%%%%%%%%%%%%%%%%%%%%%%%%
0841:40*08
01234567
AF5005FA
AAAAAAAA
55555555
F0A55A0F
AA55FF00
FEDCBA98
89ABCDEF
00008000
00000400
00001000
00000400
99999999
00020000
00003200
00001600
00001000
00000200
00000400
00000200
00020000
00020000
00001600
00000800
99999999
00000800
00001000
00000400
99999999
00020000
00006400
00003200
00008000
00000400
00001000
00000400
99999999
00020000
00003200
00001600
0842:06*16
 COMPLETE TEST%%
  SHORT  TEST%%%
   TAPE TEST%%%%
CONTINUOUS TEST%
  ERASE  TEST%%%
RETENSION  TEST%
0843:16*19
%%%%%%%%%%%%%%%%%%%
open channel%%%%%%%
select tape drive%%
reset tape drive%%%
rewind tape%%%%%%%%
retension tape%%%%%
erase tape%%%%%%%%%
write file mark%%%%
read file mark%%%%%
close channel%%%%%%
start read%%%%%%%%%
end read%%%%%%%%%%%
start write%%%%%%%%
end write%%%%%%%%%%
controller test%%%%
read after erase%%%
0844:16*19
streaming write%%%%
streaming read%%%%%
start-stop write%%%
start-stop read%%%%
dual DMA write%%%%%
dual DMA read%%%%%%
dual DMA write 2?%%
dual DMA read  2?%%
track change write%
track change read%%
test T F X W%%%%%%%
test T F X R%%%%%%%
test T D S W%%%%%%%
test T D S R%%%%%%%
test T D X W%%%%%%%
test T D X R%%%%%%%
0845:16*26
power on/reset occurred%%%
end of recorded media%%%%%
bus parity error%%%%%%%%%%
beginning of media%%%%%%%%
marginal block detected%%%
no data detected%%%%%%%%%%
illegal command%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%
file mark detected%%%%%%%%
bad block not located%%%%%
unrecoverable data error%%
end of media%%%%%%%%%%%%%%
write protected cartridge%
unselected drive%%%%%%%%%%
cartridge not in place%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%
0846:07*09
  READY%%
 TESTING%
   READ%%
  WRITE%%
  REWIND%
 TENSION%
  ERASE%%
0847:03*15
%%%%%%%%%%%%%%%
STATUS 1 ERROR%
STATUS 2 ERROR%
0848:17*26
TEST OK%%%%%%%%%%%%%%%%%%%
TEST RUNNING%%%%%%%%%%%%%%
TEST FAILED%%%%%%%%%%%%%%%
TEST ABORTED BY USER%%%%%%
ERROR: initialize%%%%%%%%%
ERROR: open channel%%%%%%%
ERROR: reset drive%%%%%%%%
ERROR: select drive%%%%%%%
ERROR: rewind tape%%%%%%%%
ERROR: retension%%%%%%%%%%
ERROR: erase tape%%%%%%%%%
ERROR: read mark%%%%%%%%%%
ERROR: write mark%%%%%%%%%
ERROR: close channel%%%%%%
ERROR: terminate%%%%%%%%%%
ERROR: read start%%%%%%%%%
ERROR: write start%%%%%%%%
0849:17*26
ERROR: read%%%%%%%%%%%%%%%
ERROR: write%%%%%%%%%%%%%%
ERROR: read tape%%%%%%%%%%
ERROR: write tape%%%%%%%%%
ERROR: read end%%%%%%%%%%%
ERROR: write end%%%%%%%%%%
ERROR: check drive%%%%%%%%
ERROR: check buffer%%%%%%%
** SYSTEM ERROR%%%%%%%%%%%
** EXCEPTION%%%%%%%%%%%%%%
** EXCEPTION (read/write)%
** NO FREE RAM%%%%%%%%%%%%
** READ DISK ERROR%%%%%%%%
ERROR: MISCOMPARE%%%%%%%%%
ERROR: BAD BLOCK COUNTS%%%
ERROR: tape is not erased%
Bad ID in configuration%%%
0850:16*19
streaming write%%%%
streaming read%%%%%
start-stop write%%%
start-stop read%%%%
dual DMA write%%%%%
dual DMA read%%%%%%
dual DMA write 2?%%
dual DMA read  2?%%
complete tape write
complete tape read%
test T F X W%%%%%%%
test T F X R%%%%%%%
test T D S W%%%%%%%
test T D S R%%%%%%%
test T D X W%%%%%%%
test T D X R%%%%%%%
0900:04*77
=============================================================================
@@@@@@@@@@@@@@@  @@@@                        TID=@    | under- |status| test 
No.     sub-test      | block cnt | pattern  |softerr |  runs  | code |result
----------------------+-----------+----------+--------+--------+------+------
0E02:08*58
*      Tape drive SCSI ID for unit & not responding.     *
*                                                        *
*      Probable cause(s) can be one of the following:    *
*         1) Drive has no power : check power.           *
*         2) Cable not connected: check cable.           *
*         3) Wrong SCSI ID      : run INSTALL/CONFIG.    *
*                                                        *
*                Press Enter key to exit.                *
0E03:03*58
*     Tape drive SCSI ID for unit & not a tape device.   *
*       Please run INSTALL/CONFIG to correct the ID.     *
*                Press Enter key to exit.                *
0E04:02*58
*      SCSI host adapter for unit & does not exist.      *
*                Press Enter key to exit.                *
0E05:03*58
*  Illegal base segment of SCSI host adapter for unit &. *
*  Please run INSTALL/CONFIG to correct the base segment.*
*                Press Enter key to exit.                *
0E07:02*58
*   Tape unit & is not compatible with STAPE software.   *
*               Press Enter key to exit.                 *
0E20:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E21:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E22:02*58
*         Please insert tape cartridge in unit &.        *
*              Press Enter to continue.                  *
0E23:01*58
*           Checking tape unit, please wait.             *
0E25:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E26:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0D00:01*58
*              Rewinding tape, please wait.              *
0D01:01*58
*  Eject cartridge/cassette to terminate the operation.  *
0D02:02*58
*         This operation may take several hours.         *
*             Do you want to proceed (Y/N) ?             *
DA02:02*59
*            Error: Fail to change partition.             *
*                Press Enter key to EXIT.                 *
DA0C:02*59
*               Erasing dataset directory.                *
*  Eject cartridge/cassette to terminate the operation.   *
DA0D:02*59
*                   Erasing data area.                    *
*  Eject cartridge/cassette to terminate the operation.   *
DA0B:01*59
*        Clearing dataset directory, please wait...       *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000
