0100:01*12
Tape Blocks:
0101:01*12
# of Sectors
0001:02*57
*           Program already loaded in memory            *
*              Please type exit to return               *
0002:03*57
*              Cannot execute COMMAND.COM               *
*        Not enough memory or program not found         *
*              Press Enter key to continue              *
0003:03*57
*                Memory allocation error                *
*  You have invoked a program still resident in memory  *
*           Cannot execute the tape software            *
0004:02*57
*            Press Enter key to confirm EXIT            *
*             Press any other key to resume             *
0140:04*57
* Invalid input in easy menu:                           *
*     - A to Append data at the end of existing data    *
*     - O to Overwrite data at the beginning of tape    *
*             Press Enter key to continue               *
0141:04*57
* Invalid input in drive menu:                          *
*     - D to backup Dos   data image                    *
*     - W to backup Whole disk image                    *
*             Press Enter key to continue               *
0142:02*57
*             Too many drive specifications             *
*              Press Enter key to continue              *
0143:03*57
*     Cannot change tape spec unless tape is at BOT     *
*           Press F9 key to rewind tape to BOT          *
*              Press Enter key to continue              *
0150:02*57
*             There is no data on this tape             *
*     Do you want to proceed with this tape? (Y/N)      *
0151:02*57
*             This tape contains valid data.            *
*     Do you want to append data to this tape? (Y/N)    *
0152:07*57
* Warning: you may be using the wrong tape              *
*                                                       *
*  The specified tape ID or label does not match        *
*  that on the tape. The recorded tape ID and label     *
*  cannot be changed at this point.                     *
*                                                       *
*     Do you want to append data to this tape? (Y/N)    *
0153:02*57
*             This tape contains valid data             *
*     Do you want to backup data to this tape? (Y/N)    *
0154:07*57
* Warning: you may be using the wrong tape              *
*                                                       *
*  The specified tape ID or label does not match        *
*  that on the tape. The recorded tape ID and label     *
*  cannot be changed at this point.                     *
*                                                       *
*     Do you want to backup data to this tape? (Y/N)    *
0155:02*57
*             This tape contains valid data             *
*        Do you want to OVERWRITE this tape? (Y/N)      *
0156:07*57
* Warning: you may be using a wrong tape                *
*                                                       *
*  The specified tape ID or label does not match with   *
*  those on the tape.    The tape will be overwritten   *
*  with the newly specified tape ID and label.          *
*                                                       *
*        Do you want to OVERWRITE this tape? (Y/N)      *
0157:02*57
*                  Unknown tape format                  *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0158:02*57
*                  Unknown tape format                  *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0159:02*57
*   This tape has EVEREX version 2 or 3 IMAGE backup    *
*       Do you want to OVERWRITE this tape? (Y/N)       *
015A:02*57
*      This tape has EVEREX version 1 FILE backup       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
015B:02*57
*    This tape has EVEREX version 2 or 3 FILE backup    *
*       Do you want to OVERWRITE this tape? (Y/N)       *
015C:02*57
*     This tape has EVEREX version 3.5 FILE backup      *
*       Do you want to OVERWRITE this tape? (Y/N)       *
015D:02*57
*   This tape was used by TAPETEST (has no valid data)  *
*       Do you want to OVERWRITE this tape? (Y/N)       *
015E:02*57
* Bad data (015E): unknown tape header type             *
*       Do you want to OVERWRITE this tape? (Y/N)       *
015F:02*57
* Bad data (015F): error in the first tape block        *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0160:08*57
* Warning: you may be using the wrong tape              *
*                                                       *
* (1) Specified Dataset is not on this tape.            *
* (2) Specified tape ID or label does not match         *
*     that on the tape. Tape will be overwritten        *
*     with a new ID and label.                          *
*                                                       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0161:05*57
* Warning: you may be using the wrong tape              *
*                                                       *
*       The specified Dataset is not on this tape.      *
*                                                       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0162:06*57
* Warning: you may be using the wrong tape              *
*                                                       *
*       This tape does not look like the correct        *
*       continuation tape of the previous tape.         *
*                                                       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0163:02*57
* Bad data (0164): error when locating the Dataset      *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0164:02*57
* Bad data (0165): missing header block                 *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0165:02*57
* Bad data (0166): header block has incorrect ID        *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0166:03*57
*           End of tape (File Mark Detected)            *
*       The specified Dataset is not on this tape       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0167:03*57
*          End of tape (End of Media Detected)          *
*       The specified Dataset is not on this tape       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0168:03*57
*            End of tape (EOT Mark Detected)            *
*       The specified Dataset is not on this tape       *
*       Do you want to OVERWRITE this tape? (Y/N)       *
0169:03*57
*                  Tape is not mounted                  *
*   Do you want to continue tape unit checking? (Y/N)   *
*          Mount tape in unit & before continue         *
016A:03*57
*               Tape is write-protected                 *
*    Do you want to continue tape unit checking? (Y/N)  *
*    Mount unprotected tape in unit & before continue   *
0170:02*57
*        Invalid logical disk drive specification       *
*              Press Enter key to continue              *
0171:02*57
*         Invalid fixed disk drive specification        *
*              Press Enter key to continue              *
0172:03*57
*    Cannot backup the logical image of this drive.     *
*           The disk BOOT record has bad data.          *
*              Press Enter key to continue              *
0173:02*57
* Error reading disk: %                                 *
*               Retry or Ignore ? (R/I)                 *
0174:03*57
*                    DO NOT SUPPORT                     *
*Logical sector size less than 512 or more than 4K bytes*
*              Press Enter key to continue              *
0180:02*57
*  Cannot read the partition table from the fixed disk  *
*  Do you want to do a RAW backup of this drive? (Y/N)  *
0181:02*57
*     No partition table on the selected fixed disk     *
*  Do you want to do a RAW backup of this drive? (Y/N)  *
0182:02*57
*    No valid DOS partition found on the fixed disk     *
*  Do you want to do a RAW backup of this drive? (Y/N)  *
0183:02*57
*    Not enough memory to process the disk directory    *
*  Do you want to do a RAW backup of this drive? (Y/N)  *
0184:02*57
*   All of the DOS File Allocation Tables are damaged   *
*  Do you want to do a RAW backup of this drive? (Y/N)  *
0190:02*57
*     The fixed disk has partition out of disk limit    *
*              Press Enter key to continue              *
0191:02*57
*      The fixed disk partition table has bad data      *
*              Press Enter key to continue              *
0192:02*57
*         Unable to read BOOT record from drive         *
*              Press Enter key to continue              *
0193:02*57
*                BOOT record has bad data               *
*              Press Enter key to continue              *
0194:02*57
*             Bad BOOT: incorrect head count            *
*              Press Enter key to continue              *
0195:02*57
*             Bad BOOT: incorrect track size            *
*              Press Enter key to continue              *
0196:02*57
*            Bad BOOT: sector size is not 512           *
*              Press Enter key to continue              *
0197:02*57
*   Bad BOOT: incorrect DOS File Allocation Table type  *
*              Press Enter key to continue              *
0198:02*57
*             Multiple DOS partitions found             *
*              Press Enter key to continue              *
0199:02*57
*   All of the DOS File Allocation Tables are damaged   *
*              Press Enter key to continue              *
019A:02*57
*     Damaged DOS File Allocation Table is detected     *
*              Press Enter key to continue              *
019B:02*57
*            Failed to read directory sector            *
*              Press Enter key to continue              *
019C:02*57
*             Bad cluster chain was detected            *
*              Press Enter key to continue              *
019D:02*57
*           Marginal partition sector detected          *
*              Press Enter key to continue              *
019E:02*57
*            Marginal BOOT sector was detected          *
*              Press Enter key to continue              *
019F:02*57
*     Marginal DOS File Allocation Table was detected   *
*              Press Enter key to continue              *
01A0:02*57
*         Marginal directory sector was detected        *
*              Press Enter key to continue              *
01A1:02*57
*         Bad first cluster number in directory         *
*              Press Enter key to continue              *
01A2:02*57
*        Bad cluster chain: no END-OF-CHAIN mark        *
*              Press Enter key to continue              *
01A3:02*57
*        Bad cluster chain: cross link detected         *
*              Press Enter key to continue              *
01C0:01*57
*    Preparing the disk for image backup, please wait   *
01C1:01*57
*        Backing up the disk image, please wait...      *
01C2:01*57
*     Checking the tape information, please wait...     *
01C3:01*57
*           Rewinding the tape, please wait...          *
01C4:01*57
*  Advancing the tape to the end of existing tape data  *
01C5:01*57
*  Advancing tape to specified Dataset, please wait...  *
01C6:01*57
*    End of tape, rewinding the tape, please wait...    *
01C7:01*57
*          Checking tape unit, please wait...           *
01D0:02*57
*               Image backup is completed               *
*              Press Enter key to continue              *
01D1:03*57
*                  Tape is not mounted                  *
*            Please mount the tape in unit &            *
*              Press Enter key to continue              *
01D2:03*57
*               Tape is write-protected                 *
*      Please mount the unprotected tape in unit &      *
*             Press Enter key to continue               *
01D3:02*57
*           Please change the tape in unit &            *
*              Press Enter key to continue              *
01D4:04*57
* A non zero tape ID is required, please:               *
* (1) Press Enter key to go to the tape spec menu       *
* (2) Enter a non zero tape ID                          *
* (3) Press F8 key to continue                          *
01D5:05*57
* End of tape, please:                                  *
* (1) Mount the continuation tape                       *
* (2) Press Enter key to go to the tape spec menu       *
* (3) Enter the continuation tape ID and label          *
* (4) Press F8 key to continue                          *
01D6:02*57
*  End of tape, please change to the continuation tape  *
*              Press Enter key to continue              *
01E0:02*57
* ERROR 01E0: no free memory to do an image backup      *
*                               Press Enter key to exit *
01E1:02*57
* ERROR 01E1: tape was removed during backup            *
*                               Press Enter key to exit *
01E2:02*57
* ERROR 01E2: directory backup failed                   *
*                               Press Enter key to exit *
01E3:02*57
* ERROR 01E3: disk image backup failed                  *
*                               Press Enter key to exit *
01E4:02*57
* ERROR 01E4: cannot open tape channel                  *
*                               Press Enter key to exit *
01E5:02*57
* ERROR 01E5: cannot reset the tape system              *
*                               Press Enter key to exit *
01E6:02*57
* ERROR 01E6: cannot select the tape drive              *
*                               Press Enter key to exit *
01E7:02*57
* ERROR 01E7: cannot read the tape I/O status           *
*                               Press Enter key to exit *
01E8:02*57
* ERROR 01E8: cannot start the write tape command       *
*                                Press Enter key to exit*
01E9:02*57
* ERROR 01E9: write operation failed                    *
*                               Press Enter key to exit *
01EA:02*57
* ERROR 01EA: cannot write the tape file mark           *
*                               Press Enter key to exit *
01EB:02*57
* ERROR 01EB: cannot write the EOT block                *
*                               Press Enter key to exit *
01EC:02*57
* ERROR 01EC: unexpected EOM (tape is too short?)       *
*                               Press Enter key to exit *
01F0:01*57
* INTERNAL ERROR 01F0           Press Enter key to exit *
01F1:01*57
* INTERNAL ERROR 01F1           Press Enter key to exit *
01F2:01*57
* INTERNAL ERROR 01F2           Press Enter key to exit *
01F3:01*57
* INTERNAL ERROR 01F3           Press Enter key to exit *
01F4:04*57
*                                                       *
*      Tape is write-protected!  Can not continue.      *
*                Press Enter key to exit                *
*                                                       *
0200:01*57
* Drive number = 1                                      *
0201:01*57
* Drive number = 2                                      *
0202:03*57
*  There are too many files and subdirectories in the   *
*  data set. You can not restore the data set by file.  *
*              Press Enter key to continue.             *
0E02:08*58
*      Tape drive SCSI ID for unit & not responding.     *
*                                                        *
*      Probable cause(s) can be one of the following:    *
*         1) Drive has no power : check power.           *
*         2) Cable not connected: check cable.           *
*         3) Wrong SCSI ID      : run INSTALL/CONFIG.    *
*                                                        *
*                Press Enter key to exit.                *
0E03:03*58
*     Tape drive SCSI ID for unit & not a tape device.   *
*       Please run INSTALL/CONFIG to correct the ID.     *
*                Press Enter key to exit.                *
0E04:02*58
*      SCSI host adapter for unit & does not exist.      *
*                Press Enter key to exit.                *
0E05:03*58
*  Illegal base segment of SCSI host adapter for unit &. *
*  Please run INSTALL/CONFIG to correct the base segment.*
*                Press Enter key to exit.                *
0E07:02*58
*   Tape unit & is not compatible with STAPE software.   *
*               Press Enter key to exit.                 *
0E20:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E21:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E22:02*58
*         Please insert tape cartridge in unit &.        *
*              Press Enter to continue.                  *
0E23:01*58
*          Checking tape unit. Please wait...            *
0E25:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E26:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E27:03*59
* Can not append data to tape. Incorrect tape drive type. *
*Please run INSTALL/CONFIG to correct the tape drive type.*
*                Press Enter key to exit.                 *
DA00:01*59
*        Updating dataset directory, please wait...       *
DA01:02*59
*        Error: fail to update dataset directory.         *
*                Press Enter key to EXIT.                 *
DA02:02*59
*            Error: fail to change partition.             *
*                Press Enter key to EXIT.                 *
DA03:02*59
*         Error: fail to create dataset directory.        *
*                Press Enter key to EXIT.                 *
DA04:01*59
* Overwriting specified dataset directory, please wait... *
DA05:01*59
*         Reading dataset directory, please wait...       *
DA06:02*59
*           Error: fail to read dataset directory.        *
*                Press Enter key to EXIT.                 *
DA07:02*59
*  Dataset is not in this tape.  Please mount next tape.  *
*              Press Enter key to continue.               *
DA08:02*59
*        Error: fail to get back end of data area.        *
*                Press Enter key to EXIT.                 *
DA09:02*59
*         Creating dataset directory, please wait...      *
*              Approximate Time:  3 minutes.              *
DA0A:01*59
*  Advancing to end of existing tape data, please wait... *
DA0B:01*59
*        Clearing dataset directory, please wait...       *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000
