03FD:01*07
More...
03FE:01*12
Tape Blocks:
03FF:01*12
# of Sectors
0001:02*58
*            Program already loaded in memory            *
*           Type exit to return to the program           *
0002:03*58
*               Cannot execute COMMAND.COM               *
*         Not enough memory or program not found         *
*              Press Enter key to continue               *
0003:04*58
*                Memory allocation error                 *
*     Less memory reallocated after return from DOS      *
*  You have invoked a program still resident in memory   *
*          Press Enter key to EXIT the program           *
0004:02*58
*            Press Enter key to confirm EXIT             *
*             Press any other key to resume              *
0300:03*58
*       DO YOU REALLY WANT TO ABORT THE OPERATION?       *
*       Press F9 key again to abort the operation        *
*        Press any other key to cancel the abort         *
0301:02*58
*   Checking the selected target drive for bad sectors   *
*          Press F9 key to abort the operation           *
0302:02*58
*                Checking the tape header                *
*          Press F9 key to abort the operation           *
0303:02*58
*         Advancing the tape to the next dataset         *
*          Press F9 key to abort the operation           *
0304:02*58
*      Advancing the tape to the next VALID dataset      *
*          Press F9 key to abort the operation           *
0305:02*58
*      Advancing the tape to the specified dataset       *
*          Press F9 key to abort the operation           *
0306:02*58
*       Do you want to restore this dataset? (Y/N)       *
*          Press F9 key to abort the operation           *
0307:02*58
*       Do you want to compare this dataset? (Y/N)       *
*          Press F9 key to abort the operation           *
0308:05*58
* Only part of your dataset image backup is present on   *
* this tape.  You may have used a tape out of the group  *
* sequence.                                              *
*       Do you want to restore this dataset? (Y/N)       *
*          Press F9 key to abort the operation           *
0309:05*58
* Only part of your dataset image backup is present on   *
* this tape.  You may have used a tape out of the group  *
* sequence.                                              *
*       Do you want to compare this dataset? (Y/N)       *
*          Press F9 key to abort the operation           *
030A:02*58
*  Restoring the tape data to the selected target drive  *
*          Press F9 key to abort the operation           *
030B:02*58
* Comparing the tape data with the selected target drive *
*          Press F9 key to abort the operation           *
030C:02*58
*                Image compare completed                 *
*              Press Enter key to continue               *
030D:02*58
*         Image restore completed with no errors         *
*              Press Enter key to continue               *
030E:02*58
*                Image restore completed                 *
*              Press Enter key to continue               *
030F:06*58
*   FIXED DISK IMAGE RESTORE COMPLETED WITH NO ERRORS    *
*                                                        *
* The system may not recognize the newly restored fixed  *
* disk image until a system reboot.                      *
*                                                        *
*        Do you want to reboot the system? (Y/N)         *
03F0:06*58
*         THE FIXED DISK IMAGE HAS BEEN MODIFIED         *
*                                                        *
* The system may not recognize the modified fixed disk   *
* image until a system reboot.                           *
*                                                        *
*        Do you want to reboot the system? (Y/N)         *
0310:01*58
*                     Error occurred                     *
0311:01*58
*                   Error in menu file                   *
0312:01*58
*   Not enough memory to perform IMAGE RESTORE/COMPARE   *
0313:01*58
*       No valid drives for IMAGE RESTORE/COMPARE        *
0314:02*58
*     The specified target drive is a diskette drive     *
*     Please enter a non-diskette logical drive name     *
0315:02*58
*        Invalid logical drive name specification        *
*        Please enter a valid logical drive name         *
0316:02*58
*     Invalid fixed disk drive number specification      *
*      Please enter a valid fixed disk drive number      *
0317:01*58
*   Failed to get the fixed disk drive type parameters   *
0318:01*58
*       Error in the disk type file (DSKTYP8?.CFG)       *
0319:03*58
*         Cannot read cylinder 0 head 0 sector 1         *
*    Selected fixed disk may not have been physically    *
*        formatted or `bad track 0' disk unusable        *
031A:01*58
*           Failed to read the DOS BOOT record           *
031B:01*58
*      Failed to read the DOS File Allocation Table      *
031C:01*58
*     Failed to write the DOS File Allocation Table      *
031D:02*58
*      The selected drive has too many bad sectors       *
*   May not be able to recover some of the bad sectors   *
031E:02*58
*  Failed to modify the number of hidden sectors in the  *
*  DOS BOOT record.                                      *
031F:02*58
*         Tape was removed during the operation          *
* Operation has been aborted.Press Enter key to continue *
0320:01*58
*      Failed to read the NOVELL volume information      *
0321:01*58
*         NOVELL volume information is corrupted         *
0322:01*58
*    Failed to read the NOVELL File Allocation Table     *
0323:02*58
*    There are bad sectors inside NOVELL system region   *
*            NOVELL may not be able to reboot            *
0324:02*58
* NOVELL file system is full (all good blocks are in use)*
*  Cannot relocate some bad sectors (data will be lost)  *
0325:01*58
*       Failed to read the NOVELL Directory Table        *
0326:02*58
*     Failed to perform NOVELL bad sector relocation     *
*                 Some data may be lost                  *
0327:05*60
* Error writing Hot Fix Redirection Table to target disk!  *
* The target disk contains marginally bad sectors and will *
* not be safe to use.                                      *
* Please change a new disk for restoring the NetWare 386!  *
* Press Enter to Exit.                                     *
0328:05*60
* Error reading Hot Fix Redirection Table from target disk!*
* The target disk contains marginal bad sectors and will   *
* not be safe to use.                                      *
* Please use a new disk for restoring the NetWare 386!     *
* Press Enter to Exit.                                     *
0329:05*60
* Error writing Hot Fix Information to target disk!        *
* Too many Bad Sectors located in the Hot Fix information  *
* area.                                                    *
* Please use a new disk for restoring the NetWare 386!     *
* Press Enter to Exit.                                     *
032A:03*60
* Error in checking NetWare 386 Hot Fix Signature!         *
* Tape data may not be NetWare 386 partition data.         *
* Press Enter to Exit.                                     *
032B:05*60
* Error reading sectors from target disk!                  *
* The target disk contains marginal bad sectors and will   *
* not be safe to use.                                      *
* Please use a new disk for restoring the tape image!      *
* Press Enter to Exit.                                     *
032C:02*60
* Hot Fix Redirection Block index is out of bound!         *
* Press Enter to Exit.                                     *
032D:04*60
* Hot Fix Redirection Table is FULL!                       *
* The target disk contains too many bad sectors.           *
* Please use a new disk for restoring the tape image!      *
*  Press Enter to Exit.                                    *
032E:05*60
* Error processing temporary relocations!                  *
* The target disk contains too many bad sectors in the Hot *
* Fix Redirection Area.                                    *
* Please use a new disk for restoring the tape image!      *
* Press Enter to Exit.                                     *
032F:03*60
* Novell 286 Image data is found on tape.                  *
* Please use NVL286IR to restore this image.               *
* Press Enter to Exit.                                     *
0330:01*58
*     The selected fixed disk has no partition table     *
0331:01*58
*  Partitions are out of the fixed disk physical limit   *
0332:01*58
*                 Partitions overlap                     *
0333:01*58
*   The selected fixed disk has no DOS partition found   *
0334:03*58
*  Non-DOS partitions found in the selected fixed disk.  *
*      Bad sector relocation WILL NOT be performed       *
*             on these non-DOS partitions.               *
0335:03*58
*     There are extra partition entries found in the     *
*        logical drive table. Bad sectors in the         *
*     EXTENDED DOS partition may not be able to map.     *
0336:01*58
*  Failed to perform EXTENDED DOS bad sector relocation  *
0337:01*58
*      EXTENDED DOS PARTITION BOOT record not found      *
0338:01*58
*   Failed to read the EXTENDED PARTITION BOOT record    *
0340:01*58
*                   DOS BOOT: bad data                   *
0341:01*58
*             DOS BOOT: incorrect media type             *
0342:01*58
*          DOS BOOT: incorrect disk head count           *
0343:01*58
*          DOS BOOT: incorrect disk track size           *
0344:01*58
*    DOS BOOT: inconsistent with the partition table     *
0345:01*58
*           DOS BOOT: incompatible sector size           *
0346:01*58
* Error in the DOS File Allocation Table size computation*
0350:01*58
* Not enough memory to process DOS File Allocation Table *
0358:01*58
*      Compare error; Do you wish to continue? (Y/N)     *
0360:02*58
* Too many bad clusters (bad sector map buffer is full)  *
*      May not be able to recover some bad clusters      *
0361:02*58
*   There are bad sectors inside the DOS table region    *
*                 Some data may be lost                  *
0362:02*58
* DOS file system is full (all good clusters are in use) *
*  Cannot relocate some bad sectors (data will be lost)  *
0363:02*58
*     Not enough memory to process the DOS directory     *
*        Cannot complete the bad sector recovery         *
0364:02*58
* Crossed links detected in the DOS File Allocation Table*
*       May result in incorrect sector relocation        *
0370:03*58
*     The first cluster of the file has bad sectors      *
* The cluster has been relocated and the directory entry *
* corrected                                              *
0371:03*58
*      The nth cluster of the file has bad sectors       *
* The cluster has been relocated and the directory entry *
* corrected                                              *
0372:02*58
*     The first cluster of the file has bad sectors      *
*    The cluster was not relocated (data may be lost)    *
0373:02*58
*      The nth cluster of the file has bad sectors       *
*    The cluster was not relocated (data may be lost)    *
0374:02*58
*             Invalid directory entry found              *
*  The first cluster of the file is not a valid cluster  *
0375:02*58
*      Invalid cluster chain detected (no EOF mark)      *
*  The last cluster of the file is not a valid cluster   *
0376:02*58
*             Invalid directory entry found              *
*   The first cluster of the file was marked as unused   *
0377:02*58
*             Invalid cluster chain detected             *
*         Cannot recover the cluster chain error         *
0378:02*58
*      Invalid cluster chain detected (no EOF mark)      *
*     The cluster chain of the file contains a loop      *
0380:01*58
*          Failed to initialize tape operation           *
0381:01*58
*              Failed to open tape channel               *
0382:01*58
*              Failed to reset tape system               *
0383:01*58
*               Failed to get tape status                *
0384:01*58
*            Failed to select the tape drive             *
0385:01*58
*               Failed to rewind the tape                *
0386:01*58
*         Failed to start the read-tape command          *
0387:01*58
*       Failed to terminate the read-tape command        *
0388:01*58
*                Failed to read the tape                 *
0389:01*58
*            Failed to read the tape queue               *
038A:01*58
*          Tape drive not installed or no power          *
038B:01*58
*         Unexpected tape error status detected          *
03A0:03*58
*                  Tape is not mounted                   *
*      Do you want to continue the operation ? (Y/N)     *
*    Please mount the tape in unit & before continue     *
03A1:03*58
*          Incorrect Tape: no data on the tape           *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A2:03*58
*          Incorrect Tape: unknown tape format           *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A3:03*58
*    This tape has EVEREX version 2 or 3 IMAGE backup    *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A4:03*58
*       This tape has EVEREX version 1 FILE backup       *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A5:03*58
*    This tape has EVEREX version 2 or 3 FILE backup     *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A6:03*58
*     This tape has EVEREX version 3.5 FILE backup       *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A7:03*58
*          Incorrect tape: unknown tape version          *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A8:04*58
*       Incorrect tape: no valid data on the tape        *
*      The tape has been used for diagnostic tests       *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03A9:03*58
*          Incorrect tape: unknown header type           *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03AA:03*58
*        Incorrect tape: wrong tape group number         *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03AB:03*58
*        Incorrect tape: wrong tape order number         *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03AC:03*58
*           Incorrect tape: wrong backup date            *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03AD:03*58
*           Incorrect tape: wrong backup time            *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03AE:03*58
*          Incorrect tape: wrong dataset number          *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03AF:03*58
*        Incorrect tape: unexpected EOT mark read        *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03B0:03*58
*                No more data on the tape                *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03B1:03*58
*                Failed to read the tape                 *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03B2:03*58
*             Incorrect tape header content              *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03B3:03*58
*                 Tape is not mounted                    *
*   Do you want to continue tape unit checking? (Y/N)    *
*   Please change the tape in unit & before continue     *
03C0:04*58
*       The specified dataset is not on this tape        *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C1:04*58
*    The specified dataset was not backed up in IMAGE    *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C2:05*58
*       The specified  dataset is a logical  IMAGE       *
*    but the selected drive is a physical fixed disk     *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C3:05*58
*       The specified  dataset is a physical IMAGE       *
*       but the selected drive is a logical drive        *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C4:05*58
*     The target drive has different number of heads     *
*      than the source drive backed up on the tape       *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C5:05*58
*   The target drive has different track size than the   *
*           source drive backed up on the tape           *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C6:05*58
*  The target drive has different sector size than the   *
*           source drive backed up on the tape           *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C7:05*58
*   The target drive is smaller than the source drive    *
*                 backed up on the tape                  *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C8:05*58
* The target logical drive has different hidden sectors  *
*      than the source drive backed up on the tape       *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03C9:05*58
* Only part of your dataset image is present on this tape*
*   You may have used a tape out of the group sequence   *
*      Please rewind and change the tape in unit &;      *
*          or re-specify another dataset number          *
*              Press Enter key to continue               *
03CA:02*58
*                Compare error detected                  *
*              Press Enter key to continue               *
03CB:03*58
*  Warning!  The target drive is larger than the source  *
*              drive backed up on the tape               *
*      Press Enter key to continue or F10 to abort       *
03D0:03*58
*  Tape was removed during the IMAGE RESTORE operation   *
*            Do you want to continue ? (Y/N)             *
*    Please mount the tape in unit & before continue     *
03D1:03*58
*                Failed to read the tape                 *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03D2:03*58
*         Bad tape data: unexpected end of tape          *
*            Do you want to continue ? (Y/N)             *
*    Please change the tape in unit & before continue    *
03D3:03*58
*   End of tape, please get the next tape of the group   *
*        Change the tape and Press 'Y' to continue;      *
*           or Press 'N' to abort the operation          *
03E0:01*58
*           Bad tape data: missing tape header           *
03E1:01*58
*         Bad tape data: missing dataset header          *
03E2:01*58
*       Bad tape data: incorrect tape block count        *
03E3:01*58
*          Bad tape data: incorrect dataset ID           *
03E4:01*58
*           Bad tape data: incorrect header ID           *
03E5:02*58
*         ERROR 03E5: failed to read tape data           *
*              Do you want to retry? (Y/N)               *
03E6:02*58
*         ERROR 03E6: failed to read tape data           *
*              Do you want to retry? (Y/N)               *
03F1:01*58
*          Do you want to run CHECKDIR? (Y=YES)          *
03F2:01*58
*     Do you want to list directory entries? (Y=YES)     *
03F3:01*58
*    Do you want to list the bad sector map? (Y=YES)     *
03F4:10*30
* -a  same as -smrfdp        *
* -s  show system info       *
* -m  show bad sector map    *
* -r  show relocation        *
* -f  exam DOS FAT           *
* -d  exam directories       *
* -p  list all file names    *
* -q  dump tape que          *
* -w  disable all disk write *
* -n  novell bad sector map  *
03F5:01*58
*            Rewinding tape, please wait...              *
03F6:02*58
*                  Checking tape unit                    *
*          Press F9 key to abort the operation           *
03FC:01*07
No More
0E02:08*58
*      Tape drive SCSI ID for unit & not responding.     *
*                                                        *
*      Probable cause(s) can be one of the following:    *
*         1) Drive has no power : check power.           *
*         2) Cable not connected: check cable.           *
*         3) Wrong SCSI ID      : run INSTALL/CONFIG.    *
*                                                        *
*                Press Enter key to exit.                *
0E03:03*58
*     Tape drive SCSI ID for unit & not a tape device.   *
*       Please run INSTALL/CONFIG to correct the ID.     *
*                Press Enter key to exit.                *
0E04:02*58
*      SCSI host adapter for unit & does not exist.      *
*                Press Enter key to exit.                *
0E05:03*58
*  Illegal base segment of SCSI host adapter for unit &. *
*  Please run INSTALL/CONFIG to correct the base segment.*
*                Press Enter key to exit.                *
0E07:02*58
*   Tape unit & is not compatible with STAPE software.   *
*               Press Enter key to exit.                 *
0E20:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E21:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E22:02*58
*         Please insert tape cartridge in unit &.        *
*              Press Enter to continue.                  *
0E23:01*58
*          Checking tape unit. Please wait...            *
0E25:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E26:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E27:03*59
* Can not append data to tape. Incorrect tape drive type. *
*Please run INSTALL/CONFIG to correct the tape drive type.*
*                Press Enter key to exit.                 *
0EE0:07*20
*NO LABEL*          
Image               
File                
 B                  
 KB                 
 MB                 
 GB                 
0EE1:01*58
*             Corrupted IRESTORE.ERR File.               *
0EE2:01*13
List Datasets
DA00:01*59
*        Updating dataset directory, please wait.         *
DA01:02*59
*        Error: Fail to update dataset directory.         *
*                Press Enter key to EXIT.                 *
DA02:02*59
*            Error: Fail to change partition.             *
*                Press Enter key to EXIT.                 *
DA03:02*59
*         Error: Fail to create dataset directory.        *
*                Press Enter key to EXIT.                 *
DA04:01*59
*  Overwriting specified dataset directory, please wait.  *
DA05:01*59
*         Reading dataset directory, please wait.         *
DA06:02*59
*           Error: Fail to read dataset directory.        *
*                Press Enter key to EXIT.                 *
DA07:02*59
*  Dataset is not in this tape.  Please mount next tape.  *
*              Press Enter key to continue.               *
DA08:02*59
*        Error: Fail to get back end of data area.        *
*                Press Enter key to EXIT.                 *
DA09:02*59
*         Creating dataset directory, please wait.        *
*              Approximate time:  3 minutes.              *
DA0A:01*59
*   Advancing to end of existing tape data, please wait.  *
DA0B:01*59
*        Clearing dataset directory, please wait.         *
DA0C:01*59
*  Advancing tape to the specified dataset, please wait.  *
DA40:01*59
*   No dataset information. Press Enter key to continue.  *
DA41:03*60
* Novell 386 Image data is found on tape.                  *
* Please use NVL386IR to restore this image.               *
* Press Enter to Exit.                                     *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000
