05C3:01*12
Total Blocks
05C4:01*33
***** Failed to open file-------^
05C5:01*33
***** Failed to read file-------^
05C6:01*03
PRN
05C7:01*08
00011100
0001:02*58
*           Program already loaded in memory             *
*          Type EXIT to return to the program            *
0002:03*58
*              Cannot execute COMMAND.COM                *
*         Not enough memory or program not found         *
*              Press Enter key to continue               *
0003:05*58
*                Memory allocation error                 *
*     Less memory reallocated after return from DOS      *
*  You have invoked a program still resident in memory   *
*            Cannot execute the tape software            *
*                Press Enter key to EXIT                 *
0004:02*58
*            Press Enter key to confirm EXIT             *
*             Press any other key to resume              *
0500:02*58
*     Invalid file specification input in EASY MENU.     *
*              Press Enter key to continue.              *
0501:02*58
*   Invalid input for backing up sub-directory option.   *
*              Press Enter key to continue.              *
0502:02*58
*   Please enter 'A' for append and 'O' for overwrite.   *
*              Press Enter key to continue.              *
0520:02*58
*   Invalid file specification input in FILE SPEC MENU.  *
*              Press Enter key to continue.              *
052D:02*58
*  Invalid input for backup include and exclude option.  *
*              Press Enter key to continue.              *
052E:03*58
*     Invalid value for file attribute option in the     *
*             FBACKUP.MEN file. Please check.            *
*                Press Enter key to EXIT.                *
052F:03*58
*    Invalid value for backup selection option in the    *
*             FBACKUP.MEN file. Please check.            *
*                Press Enter key to EXIT.                *
0531:02*58
*      Need a file specification, please re-enter.       *
*              Press Enter key to continue.              *
0532:02*58
*     Invalid drive specification, please re-enter.      *
*              Press Enter key to continue.              *
0533:02*58
*   File specification is too long, please re-enter.     *
*              Press Enter key to continue.              *
0534:02*58
*   Invalid dot in file specification, please re-enter.  *
*              Press Enter key to continue.              *
0535:02*58
* Too many dots in file specification, please re-enter.  *
*              Press Enter key to continue.              *
0536:02*58
* Too many slashes in file specification, please re-enter*
*              Press Enter key to continue.              *
0537:02*58
*   Invalid option specification, please re-enter.       *
*              Press Enter key to continue.              *
0538:02*58
*   Pathname cannot have wildcard, please re-enter.      *
*              Press Enter key to continue.              *
0539:02*58
*   Invalid date specification, please re-enter.         *
*              Press Enter key to continue.              *
053A:02*58
*   Starting date cannot be greater than Ending date.    *
*              Press Enter key to continue.              *
053B:02*58
*   Input year is out of range, please re-enter.         *
*              Press Enter key to continue.              *
053C:02*58
*   Input month is out of range, please re-enter.        *
*              Press Enter key to continue.              *
053D:02*58
*   Input day is out of range, please re-enter.          *
*              Press Enter key to continue.              *
053E:02*58
*   Invalid file name specification, please re-enter.    *
*              Press Enter key to continue.              *
0551:02*58
*   Too many file specifications, please re-enter.       *
*              Press Enter key to continue.              *
0552:02*58
*   Starting backup date is greater than Ending date.    *
*              Press Enter key to continue.              *
0560:02*58
*             Error: initialize tape operation.          *
*                Press Enter key to EXIT.                *
0561:02*58
*                Error: open tape channel.               *
*                Press Enter key to EXIT.                *
0562:02*58
*               Error: select tape drive.                *
*                Press Enter key to EXIT.                *
0563:02*58
*                Error: reset tape drive.                *
*                Press Enter key to EXIT.                *
0564:02*58
*                Error: read tape status.                *
*                Press Enter key to EXIT.                *
0565:02*58
*                   Error: rewindtape.                   *
*                Press Enter key to EXIT.                *
0566:02*58
*                   Error: read start.                   *
*                Press Enter key to EXIT.                *
0567:02*58
*                   Error: write start.                  *
*                Press Enter key to EXIT.                *
0568:02*58
*                    Error: read tape.                   *
*                Press Enter key to EXIT.                *
0569:02*58
*                   Error: write tape.                   *
*                Press Enter key to EXIT.                *
056A:02*58
*                    Error: read end.                    *
*                Press Enter key to EXIT.                *
056B:02*58
*                    Error: write end.                   *
*                Press Enter key to EXIT.                *
056C:02*58
*                 Error: read file mark.                 *
*                Press Enter key to EXIT.                *
056D:02*58
*                Error: write file mark.                 *
*                Press Enter key to EXIT.                *
056E:02*58
*               Error: close tape channel.               *
*                Press Enter key to EXIT.                *
056F:02*58
*            Error: terminate tape operation.            *
*                Press Enter key to EXIT.                *
0570:02*58
*   Error: exception occurred during tape read/write.    *
*                Press Enter key to EXIT.                *
0571:01*58
*  File specification is too long in file "FBACKUP.CFG"  *
0572:03*58
*Tape was removed from drive during continuation backup. *
*                  Unable to continue.                   *
*                Press Enter key to EXIT.                *
0575:02*58
*                   Tape write error.                    *
*                Press Enter key to EXIT.                *
0576:07*58
* ***** FATAL BACKUP ERROR:  FAILED TO OPEN FILE ******* *
*                                                        *
* This file was not backed up and cannot be restored.    *
* You should manually re-backup this file later.         *
*                                                        *
* Press F9 to abort backup operation and rewind the tape.*
* Press F6 to continue to backup other files.            *
0577:10*58
* ***** FATAL BACKUP ERROR:  FAILED TO READ FILE ******* *
*                                                        *
* This file has incorrect data on the tape and should    *
* not be restored. You must manually exclude this file   *
* during the FILE RESTORE operation to prevent incorrect *
* data from being restored to this file.                 *
* You must manually re-backup this file later.           *
*                                                        *
* Press F9 to abort backup operation and rewind the tape.*
* Press F6 to continue to backup other files.            *
0578:03*58
*               No file found for backup.                *
*           Please re-enter file specification.          *
*               Press Enter to continue.                 *
0579:03*58
*   This tape is full - unable to backup this dataset.   *
*   Please remove this tape after rewind                 *
*   Insert next tape, and press any key when ready.      *
057B:04*58
*   Unknown tape format detected.                        *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
057C:03*58
*   Please enter the tape number and the tape label      *
*   for the continuation tape.                           *
*   Press F8 to continue backing up the rest of the data.*
057E:03*58
*   Tape number/tape label does not match that on the    *
*   tape.  The specified tape number and label will be   *
*   used instead.  Press Y to continue, N to restart.    *
057F:03*58
*   Tape number/tape label does not match that on the    *
*   tape. The number and label on the tape will be used. *
*   Press Y to continue and N to change tape or restart. *
0580:04*58
*   Bad block number detected on this tape.              *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
0581:04*58
*   Bad file number detected on this tape.               *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
0582:04*58
*   Bad dataset identification number is detected.       *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
0583:04*58
*   There is no file mark at the end of data.            *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
0584:04*58
*   Missing header block is detected on this tape.       *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
0586:01*58
*                    Start to backup                     *
0587:01*58
*                   Continue to backup                   *
0588:01*58
*              Rewinding tape, please wait.              *
058A:03*58
*        Please mount a tape in the tape unit &          *
*             Press any key to continue.                 *
*            Press F9 to abort operation.                *
058B:01*58
*          Checking tape header, please wait.            *
058C:01*58
*         Skipping past an IMAGE backup dataset.         *
058D:01*58
*        Skipping past existing data on the tape.        *
058E:02*58
*    Advancing to the specified dataset of the tape.     *
*  Press F5 to turn on listing for FILE backup dataset.  *
058F:01*58
*     Cannot create log file, press Enter to continue.   *
0590:01*58
*    Cannot write to log file, press Enter to continue.  *
0591:02*58
*   There were file access errors during file backup.    *
*     Backup completed.  Please press F3 to return.      *
0592:01*58
*   End of Tape is detected.  Please wait for rewind.    *
0593:01*58
*               Proceed to backup (Y/N)?                 *
0594:02*58
*              There is valid data on tape.              *
*      Overwrite the existing tape contents (Y/N)?       *
0595:01*58
*   There is no data on tape, proceed to backup (Y/N)?   *
0596:01*58
*        Proceed to append data onto tape (Y/N)?         *
0597:01*58
*       Preparing files for backup, please wait.         *
0598:01*58
*      Backup completed.  Please press F2 to return.     *
0599:01*58
*  Do you really want to abort current operation (Y/N)?  *
05A0:02*58
*     There is no file specification to be processed.    *
*              Press Enter key to return.                *
05A1:02*58
*  Directory specification is invalid, please re-enter.  *
*               Press Enter key to return.               *
05A2:04*58
*     Please turn off the write protect mechanism        *
*            on the tape in the unit                     *
*   Re-insert the tape, and press any key to continue.   *
*            Press F9 to abort operation.                *
05A3:02*58
*     Tape number must not be zero, please re-enter.     *
*              Press Enter key to return.                *
05A4:04*58
*   This tape has EVEREX version 1 IMAGE backup.         *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05A5:04*58
*   This tape has EVEREX version 1 FILE backup.          *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05A6:04*58
*   This tape has EVEREX version 2 FILE backup.          *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05A7:04*58
*   This tape has EVEREX version 3 FILE backup.          *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05A8:04*58
*   Unknown tape type is detected on tape.               *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05AA:04*58
*   Unknown header type is detected on tape.             *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05AB:02*58
*   Tape has been removed from drive.                    *
*   Please re-insert tape and press Enter to return.     *
05AC:03*58
*   Tape has been removed from drive.                    *
*   Please re-insert tape and press any key to continue. *
*   Press F9 to abort operation.                         *
05AD:03*58
*   Please check/re-enter the tape number/tape label     *
*   to start a new tape.  Press F8 to start backup.      *
*   Press F9 to abort operation.                         *
05AE:01*58
*   Logging file listing, please wait. Press F9 to abort.*
05B0:02*58
*Please insert the next tape to continue backing up data.*
*                Press any key to start.                 *
05B1:04*58
*   This tape had been erased by TAPETEST program.       *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05B3:02*60
* Please insert another tape and press any key to continue.*
* Press F9 to abort operation.                             *
05B5:02*58
*              Backing up files into tape.               *
*           Press F5 to turn on file listing.            *
05B7:02*58
*       Cannot reset buffer status after exception.      *
*                Press Enter key to EXIT                 *
05B8:04*58
*   First block identification number is incorrect.      *
*   Can only overwrite data from the beginning of tape.  *
*   Press Y to continue, N to change tape.               *
*   Press F9 to abort operation.                         *
05B9:03*58
* Selected dataset is not found on this tape.            *
* Please insert next tape, and press any key to continue.*
* Press F9 to abort operation.                           *
05BA:04*58
* An extra file mark is detected on tape.                *
* Can only overwrite data from the beginning of tape.    *
* Press Y to continue, N to change tape.                 *
* Press F9 to abort operation.                           *
05BB:04*58
* Bad data detected on tape (please check).              *
* Can only overwrite data from the beginning of tape.    *
* Press Y to continue, N to change tape.                 *
* Press F9 to abort operation.                           *
05BC:02*58
*                 Error in FBACKUP.ERR.                  *
*                Press Enter key to EXIT                 *
05BD:02*58
*       Not enough memory to run FBACKUP program         *
*                Press Enter key to EXIT                 *
05BE:02*58
*   Fatal error: unable to write dataset header on       *
*   the continuation tape.                               *
05BF:03*58
*   Fatal error: data in memory buffer and backed up     *
*   data on tape does not match during cross tape        *
*   computation.                                         *
05C0:02*58
*   Fatal error: directory data blocks exceed the        *
*   total number of available buffer blocks.             *
05C1:02*58
*   Fatal error: directory data buffers exceed the       *
*   total number of available buffers.                   *
05C2:03*58
*       This tape is full.  Please wait for rewind.      *
*      Then insert the next tape to continue backup.     *
*             Press F8 to start backup again.            *
05C8:03*58
*     These tapes are full.  Please wait for rewind.     *
*  Then insert continuation tapes starting from unit 1.  *
*             Press F8 to start backup again.            *
05C9:02*58
*      Backup completed.                                 *
*      Please press F2 to return to tape menu.           *
05CA:03*58
*     Tape is not mounted, do you want to continue       *
*             tape unit checking (Y/N)?                  *
*       Mount a tape in the unit & before continue       *
05CB:03*58
*     Tape is protected, do you want to continue         *
*             tape unit checking (Y/N)?                  *
*  Mount unprotected tape in the unit & before continue  *
05CC:01*58
*          Checking tape unit, please wait.              *
05CD:04*58
*       Please check your backup source disk.            *
*       There are some files with open/read error.       *
*       Broadcast to notify users to logout.             *
*       Backup will resume momentarily.                  *
05D0:01*58
*        Backing up files into tape, please wait.        *
05D1:01*58
*        Skipping past existing data on the tape.        *
05D2:01*58
*     Advancing to the specified dataset of the tape.    *
05D3:10*58
*            ***** FATAL BACKUP ERROR *****              *
*                                                        *
*  Incorrect total number of files backed up.            *
*                                                        *
*  You can no longer append data to this tape.           *
*  You can either start with a new tape or overwrite the *
*  whole tape (starting from dataset 1) and thus lose    *
*  all existing data on this tape.                       *
*                                                        *
*             Press Enter key to continue.               *
05D4:10*58
*            ***** FATAL BACKUP ERROR *****              *
*                                                        *
*  Incorrect total file size count detected.             *
*                                                        *
*  You can no longer append data to this tape.           *
*  You can either start with a new tape or overwrite the *
*  whole tape (starting from dataset 1) and thus lose    *
*  all existing data on this tape.                       *
*                                                        *
*             Press Enter key to continue.               *
05D5:10*58
*            ***** FATAL BACKUP ERROR *****              *
*                                                        *
* Open or read file errors detected during backup.       *
*                                                        *
* You must manually exclude read error files from the    *
* FILE RESTORE operation to prevent incorrect data from  *
* being restored to the existing files.                  *
* You must manually re-backup all error files.           *
*                                                        *
*             Press Enter key to continue.               *
05D6:03*58
*  There are too many files and subdirectories in the    *
*  data set.                                             *
*             Press Enter key to continue.               *
0D00:05*58
* ***** WAITING FOR RETRY: FAILED TO OPEN FILE ********* *
*                                                        *
* Broadcast to notify users to release file.             *
* Backup will resume after wait time expires.            *
* Press F6 to resume immediately.                        *
0E02:08*58
*      Tape drive SCSI ID for unit & not responding.     *
*                                                        *
*      Probable cause(s) can be one of the following:    *
*         1) Drive has no power : check power.           *
*         2) Cable not connected: check cable.           *
*         3) Wrong SCSI ID      : run INSTALL/CONFIG.    *
*                                                        *
*                Press Enter key to EXIT.                *
0E03:03*58
*     Tape drive SCSI ID for unit & not a tape device.   *
*       Please run INSTALL/CONFIG to correct the ID.     *
*                Press Enter key to EXIT.                *
0E04:02*58
*      SCSI host adapter for unit & does not exist.      *
*                Press Enter key to EXIT.                *
0E05:03*58
*  Illegal base segment of SCSI host adapter for unit &. *
*  Please run INSTALL/CONFIG to correct the base segment.*
*                Press Enter key to EXIT.                *
0E07:02*58
*   Tape unit & is not compatible with STAPE software.   *
*                Press Enter key to EXIT.                *
0E20:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E21:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*             Press Enter key to continue.               *
0E22:02*58
*         Please insert tape cartridge in unit &.        *
*             Press Enter key to continue.               *
0E23:01*58
*           Checking tape unit, please wait.             *
0E25:04*58
*  Tape cartridge capacity must be one of the following: *
*               60, 120, 150, or 250 MBs.                *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E26:04*58
*  Tape cartridge capacity must be one of the following: *
*                   320 or 525 MBs.                      *
*       Please insert correct cartridge in unit &.       *
*   Press Enter to continue or N to skip to next drive.  *
0E27:03*59
* Can not append data to tape. Incorrect tape drive type. *
*Please run INSTALL/CONFIG to correct the tape drive type.*
*                Press Enter key to EXIT.                 *
DA00:01*59
*        Updating dataset directory, please wait.         *
DA01:02*59
*        Error: Fail to update dataset directory.         *
*                Press Enter key to EXIT.                 *
DA02:02*59
*            Error: Fail to change partition.             *
*                Press Enter key to EXIT.                 *
DA03:02*59
*         Error: Fail to create dataset directory.        *
*                Press Enter key to EXIT.                 *
DA04:01*59
*  Overwriting specified dataset directory, please wait.  *
DA05:01*59
*         Reading dataset directory, please wait.         *
DA06:02*59
*           Error: Fail to read dataset directory.        *
*                Press Enter key to EXIT.                 *
DA07:02*59
*  Dataset is not in this tape.  Please mount next tape.  *
*              Press Enter key to continue.               *
DA08:02*59
*        Error: Fail to get back end of data area.        *
*                Press Enter key to EXIT.                 *
DA09:02*59
*         Creating dataset directory, please wait.        *
*              Approximate time:  3 minutes.              *
DA0A:01*59
*   Advancing to end of existing tape data, please wait.  *
DA0B:01*59
*        Clearing dataset directory, please wait.         *
FFFF:01*68
01807::01871::00112::00012::03847::03087::00000::00000::00000::00000
