IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.17: 12/10/2011 12:50:28

Required cylinders: 2
Required heads    : 2
Data rate         : 250kbps
Est. maximum track: 5458 bytes

Possible drives/options to write ASSEMBLE.IMD :

 5.25" DD 40-track
   Double-step: OFF

 5.25" QD 80-track
   Double-step: ON

 5.25" HD 80-track
   Double-step: ON
   250 kbps -> 300 kbps

 3.5" DD 80-track   NOTE: *1
   Double-step: OFF

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

*1 40 track image will use only first 1/2 of 80-track drive.



IMageDisk Utility 1.18 / Mar 07 2012
IMD 1.17: 12/10/2011 12:50:28

Assuming 1:1 for Binary output
 0/0 250 kbps DD  9x512
      1   2   3   4   5   6   7   8   9  
      U   D   D   D   D   U   U   U   U  
 0/1 250 kbps DD  8x512
      1   2   3   4   5   6   7   9  
      U   U   U   U   U   U   U   U  
 1/0 250 kbps DD  9x512
      1   2   3   4   5   6   7   8   9  
      D   D   D   D   D   D   D   D   D  
3 tracks(2/1), 26 sectors (13 Unavail)



