IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.18: 28/04/2013  4:32:23

Software Production Associates

AIRBORNE!

(C)1985

Double Density / 480z

Required cylinders: 40
Required heads    : 1
Data rate         : 250kbps
Est. maximum track: 5458 bytes

Possible drives/options to write AIRBORNE.IMD :

 5.25" DD 40-track
   Double-step: OFF

 5.25" QD 80-track
   Double-step: ON

 5.25" HD 80-track
   Double-step: ON
   250 kbps -> 300 kbps

 3.5" DD 80-track   NOTE: *1
   Double-step: OFF

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

*1 40 track image will use only first 1/2 of 80-track drive.



IMageDisk Utility 1.18 / Mar 07 2012
IMD 1.18: 28/04/2013  4:32:23

Software Production Associates

AIRBORNE!

(C)1985

Double Density / 480z

Assuming 1:1 for Binary output
 0/0 250 kbps SD  16x128
      1   2   3   4   5   6   7   8   9   10  11  12  13  14  15  16 
      D   DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 1/0 250 kbps DD  9x512
      1   2   3   4   5   6   7   8   9  
      DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 2/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 3/0  D   DE5 D   D   D   DE5 DE5 D   D  
 4/0  D   D   D   D   D   D   D   D   D  
 5/0  D   D   D   D   D   D   D   D   D  
 6/0  D   D   D   D   D   D   D   D   D  
 7/0  D   D   D   D   DE5 D   D   D   D  
 8/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 9/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
10/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
11/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
12/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
13/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
14/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
15/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
16/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
17/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
18/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
19/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
20/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
21/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
22/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
23/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
24/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
25/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
26/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
27/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
28/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
29/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
30/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
31/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
32/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
33/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
34/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
35/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
36/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
37/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
38/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
39/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
40 tracks(40/0), 367 sectors (325 Compressed)



