IMageDisk Analyzer 1.18 / Mar 12 2012
IMD TD 1.5 5.25 LD FM S-step, 1 sides

Required cylinders: 40
Required heads    : 1
Data rate         : 250kbps
Est. maximum track: 3493 bytes

Possible drives/options to write DDWRI.IMD :

 5.25" DD 40-track
   Double-step: OFF

 5.25" QD 80-track
   Double-step: ON

 5.25" HD 80-track
   Double-step: ON
   250 kbps -> 300 kbps

 3.5" DD 80-track   NOTE: *1
   Double-step: OFF

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

*1 40 track image will use only first 1/2 of 80-track drive.



IMageDisk Utility 1.18 / Mar 07 2012
IMD TD 1.5 5.25 LD FM S-step, 1 sides

Assuming 1:1 for Binary output
 0/0 250 kbps SD  16x128
      1   2   3   4   5   6   7   8   9   10  11  12  13  14  15  16 
      D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 1/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 2/0  D   D   D   D   D   D   D   D   D   D00 D00 D   D   D   D   D  
 3/0  D   DE5 DE5 D   DE5 DE5 D   DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 4/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 5/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 6/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 7/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 8/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 9/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
10/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
11/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
12/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
13/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
14/0  D   D   D   D   D   D   D   DE5 D   D   DE5 D   D   DE5 D   D  
15/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
16/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
17/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
18/0  D   D   DE5 D   D   DE5 D   D   D   D   D   D   DE5 D   D   DE5
19/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
20/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
21/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
22/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
23/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
24/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
25/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
26/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
27/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
28/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
29/0  D   DE5 DE5 D   DE5 DE5 D   DE5 D   D   DE5 D   D   DE5 DE5 D  
30/0  D   DE5 DE5 D   DE5 DE5 DE5 DE5 D   DE5 DE5 DE5 DE5 DE5 DE5 DE5
31/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
32/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
33/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
34/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
35/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
36/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
37/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
38/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
39/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
40 tracks(40/0), 640 sectors (187 Compressed)



$ cpmls -f rm-sd -D DDWRI.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
        .    136888330286K 1095106642286 RS   29-Aug-867318 19:45
29/10/85.S11     0K      0    
TEST    .BAK     1K      1    
TEST    .TXT     1K      1    
TEST2   .TXT     1K      1    
WRCON   .COM     7K     52 R  
WRITE   .COM    22K    173 R  
WRITE   .COM    22K    173 R  



