IMageDisk Analyzer 1.18 / Mar 12 2012
IMD 1.17: 25/08/2011 21:38:07

Required cylinders: 15
Required heads    : 1
Data rate         : 250kbps
Est. maximum track: 3706 bytes

Possible drives/options to write BOOT56K.IMD :

 5.25" DD 40-track
   Double-step: OFF

 5.25" QD 80-track
   Double-step: ON

 5.25" HD 80-track
   Double-step: ON
   250 kbps -> 300 kbps

 3.5" DD 80-track   NOTE: *1
   Double-step: OFF

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

*1 40 track image will use only first 1/2 of 80-track drive.



IMageDisk Utility 1.18 / Mar 07 2012
IMD 1.17: 25/08/2011 21:38:07

Assuming 1:1 for Binary output
 0/0 250 kbps SD  17x128
      1   2   3   4   5   6   7   8   9   10  11  12  13  14  15  16  0  
      D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
 1/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
 2/0  D   D   D   D   D00 D00 D00 D00 D   D   D   D   D   D   D   D   U  
 3/0  D   DE5 DE5 D   DE5 DE5 D   DE5 DE5 D   DE5 DE5 D   DE5 DE5 D   U  
 4/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
 5/0  D   D00 D00 D   D00 D00 D   D00 D00 D   D   D00 D   D   D00 D   U  
 6/0  D00 D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
 7/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
 8/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
 9/0  D   D   D00 D   D   D00 D   D   D   D   D   D   D   D   D   D00 U  
10/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
11/0  D   D   DE5 D   D   DE5 D   D   D   D   D   D   D   D   D   D   U  
12/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   U  
13/0  D   DE5 D   D   DE5 D   D   DE5 D   D   DE5 D   D   DE5 D   D   U  
14/0  D   D   DE5 D   D   DE5 D   D   D   D   D   D   DE5 DE5 D   DE5 U  
15 tracks(15/0), 255 sectors (38 Compressed, 15 Unavail)



