


      4014(1)                       (DWB)                       4014(1)



      NAME
           4014 - paginator for the TEKTRONIX 4014 terminal

      SYNTAX
           4014 [ -t ] [ -n ] [ -cN ] [ -pL ] [ file ]

      DESCRIPTION
           The output of 4014 is intended for a TEKTRONIX 4014-type
           terminal; 4014 arranges for 66 lines to fit on the screen,
           divides the screen into N columns, and contributes an
           eight-space page offset in the (default) single-column case.
           Tabs, spaces, and backspaces are collected and plotted when
           necessary.  TELETYPE(Reg.) Model 37 half- and reverse-line
           sequences are interpreted and plotted.  At the end of each
           page, 4014 waits for a new-line (empty line) from the
           keyboard before continuing on to the next page.  In this
           wait state, the command !cmd will send the cmd to the shell.

           The command line options are:

           -t   Do not wait between pages (useful for directing output
                into a file).

           -n   Start printing at the current cursor position and never
                erase the screen.

           -cN  Divide the screen into N columns and wait after the
                last column.

           -pL  Set page length to L; L accepts the scale factors i
                (inches) and l (lines); default is lines.

      SEE ALSO
           troff(1).
           In ROS Reference Manual, pr(1), and settek(1).




















      Page 1                                          (73 A2 02MT REV1)



